{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Daten","Datenüberprüfung"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Daten","index":0,"n_rows":2115,"n_cols":35,"rows_kept":2115,"cut":false,"hidden":false,"merged":[]}
["Höchste ID",50002301]
["ID","Marke","Type","Nennwirkleistung\n(Maximalleistung)\nbei cosPhi = 1\n[kW]","Nennscheinleistung\n(Maximalleistung)\n[kVA]","Phasenzahl","Art Betriebsmittel","Zulässig ","Datum letzte Änderung","Geändert von","Datum Zulassung","ab Firmware","Datum befristet bis","Datum Entzug Zulassung","Grund nicht zulässig","Notstrom-/Inselbetriebsfähig","Externe Notstromumschaltung notwendig","USV-Fähig","OVE R25 Prüfbericht","Geprüft von","Nummer Prüfbericht","Datum OVE R25 Prüfbericht","VDE-AR-N 4110 Zertifikat","AUT Setting Typ A vorhanden","Hersteller Parametrieranleitung","Musterreport vorhanden","Datum Musterreport","Nur mit externem Entkupplungsschutz","Info","Produktion ausgelaufen","E-Mobilität","Kommentar für HP","Kommentar intern","Zulässigkeit","Zusatztext"]
[50002006,"acrevpower","SP-400",0.4,0.4,1,"PV-Wechselrichter","Nein","2024-01-02","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H3,1)=\"J\",LEFT(H3,2),LEFT(H3,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H3,1)=\"J\",RIGHT(H3,LEN(H3)-4),RIGHT(H3,LEN(H3)-6)),\"\"))","v":""}]
[50002007,"acrevpower","SP-600",0.6,0.6,1,"PV-Wechselrichter","Nein","2024-01-02","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H4,1)=\"J\",LEFT(H4,2),LEFT(H4,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H4,1)=\"J\",RIGHT(H4,LEN(H4)-4),RIGHT(H4,LEN(H4)-6)),\"\"))","v":""}]
[50002008,"acrevpower","SP-700",0.7,0.7,1,"PV-Wechselrichter","Nein","2024-01-02","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H5,1)=\"J\",LEFT(H5,2),LEFT(H5,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H5,1)=\"J\",RIGHT(H5,LEN(H5)-4),RIGHT(H5,LEN(H5)-6)),\"\"))","v":""}]
[50002009,"acrevpower","SP-800",0.8,0.8,1,"PV-Wechselrichter","Nein","2024-01-02","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H6,1)=\"J\",LEFT(H6,2),LEFT(H6,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H6,1)=\"J\",RIGHT(H6,LEN(H6)-4),RIGHT(H6,LEN(H6)-6)),\"\"))","v":""}]
[50002010,"acrevpower","SP-1200",1.2,1.2,1,"PV-Wechselrichter","Nein","2024-01-02","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H7,1)=\"J\",LEFT(H7,2),LEFT(H7,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H7,1)=\"J\",RIGHT(H7,LEN(H7)-4),RIGHT(H7,LEN(H7)-6)),\"\"))","v":""}]
[50002011,"acrevpower","SP-1400",1.4,1.4,1,"PV-Wechselrichter","Nein","2024-01-02","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H8,1)=\"J\",LEFT(H8,2),LEFT(H8,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H8,1)=\"J\",RIGHT(H8,LEN(H8)-4),RIGHT(H8,LEN(H8)-6)),\"\"))","v":""}]
[50002012,"acrevpower","SP-1600",1.6,1.6,1,"PV-Wechselrichter","Nein","2024-01-02","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H9,1)=\"J\",LEFT(H9,2),LEFT(H9,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H9,1)=\"J\",RIGHT(H9,LEN(H9)-4),RIGHT(H9,LEN(H9)-6)),\"\"))","v":""}]
[50002013,"acrevpower","SP-2000",2,2,1,"PV-Wechselrichter","Nein","2024-01-02","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H10,1)=\"J\",LEFT(H10,2),LEFT(H10,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H10,1)=\"J\",RIGHT(H10,LEN(H10)-4),RIGHT(H10,LEN(H10)-6)),\"\"))","v":""}]
[50000037,"AE CONVERSION","INV250-45EU ",null,0.24,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"VDE4105/4110",null,null,null,"Vorhanden","nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H11,1)=\"J\",LEFT(H11,2),LEFT(H11,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H11,1)=\"J\",RIGHT(H11,LEN(H11)-4),RIGHT(H11,LEN(H11)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000038,"AE CONVERSION","INV315-50 ",null,0.3,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"VDE4105/4110",null,null,null,"Vorhanden","nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H12,1)=\"J\",LEFT(H12,2),LEFT(H12,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H12,1)=\"J\",RIGHT(H12,LEN(H12)-4),RIGHT(H12,LEN(H12)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000039,"AE CONVERSION","INV350-60EU ",null,0.33,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"VDE4105/4110",null,null,null,"Vorhanden","nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H13,1)=\"J\",LEFT(H13,2),LEFT(H13,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H13,1)=\"J\",RIGHT(H13,LEN(H13)-4),RIGHT(H13,LEN(H13)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000040,"AE CONVERSION","INV350-90EU ",null,0.33,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"VDE4105/4110",null,null,null,"Vorhanden","nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H14,1)=\"J\",LEFT(H14,2),LEFT(H14,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H14,1)=\"J\",RIGHT(H14,LEN(H14)-4),RIGHT(H14,LEN(H14)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000041,"AE CONVERSION","INV500-90EU ",null,0.48,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"VDE4105/4110",null,null,null,"Vorhanden","nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H15,1)=\"J\",LEFT(H15,2),LEFT(H15,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H15,1)=\"J\",RIGHT(H15,LEN(H15)-4),RIGHT(H15,LEN(H15)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001678,"AFORE","AF3K-TH",3,3.3,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H16,1)=\"J\",LEFT(H16,2),LEFT(H16,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H16,1)=\"J\",RIGHT(H16,LEN(H16)-4),RIGHT(H16,LEN(H16)-6)),\"\"))","v":"mit Einschränkung"}]
[50001692,"AFORE","AF3K-THP",3,3.3,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H17,1)=\"J\",LEFT(H17,2),LEFT(H17,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H17,1)=\"J\",RIGHT(H17,LEN(H17)-4),RIGHT(H17,LEN(H17)-6)),\"\"))","v":"mit Einschränkung"}]
[50001681,"AFORE","AF4K-TH",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H18,1)=\"J\",LEFT(H18,2),LEFT(H18,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H18,1)=\"J\",RIGHT(H18,LEN(H18)-4),RIGHT(H18,LEN(H18)-6)),\"\"))","v":"mit Einschränkung"}]
[50001693,"AFORE","AF4K-THP",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H19,1)=\"J\",LEFT(H19,2),LEFT(H19,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H19,1)=\"J\",RIGHT(H19,LEN(H19)-4),RIGHT(H19,LEN(H19)-6)),\"\"))","v":"mit Einschränkung"}]
[50001682,"AFORE","AF5K-TH",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H20,1)=\"J\",LEFT(H20,2),LEFT(H20,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H20,1)=\"J\",RIGHT(H20,LEN(H20)-4),RIGHT(H20,LEN(H20)-6)),\"\"))","v":"mit Einschränkung"}]
[50001694,"AFORE","AF5K-THP",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H21,1)=\"J\",LEFT(H21,2),LEFT(H21,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H21,1)=\"J\",RIGHT(H21,LEN(H21)-4),RIGHT(H21,LEN(H21)-6)),\"\"))","v":"mit Einschränkung"}]
[50001683,"AFORE","AF6K-TH",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H22,1)=\"J\",LEFT(H22,2),LEFT(H22,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H22,1)=\"J\",RIGHT(H22,LEN(H22)-4),RIGHT(H22,LEN(H22)-6)),\"\"))","v":"mit Einschränkung"}]
[50001695,"AFORE","AF6K-THP",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H23,1)=\"J\",LEFT(H23,2),LEFT(H23,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H23,1)=\"J\",RIGHT(H23,LEN(H23)-4),RIGHT(H23,LEN(H23)-6)),\"\"))","v":"mit Einschränkung"}]
[50001684,"AFORE","AF8K-TH",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H24,1)=\"J\",LEFT(H24,2),LEFT(H24,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H24,1)=\"J\",RIGHT(H24,LEN(H24)-4),RIGHT(H24,LEN(H24)-6)),\"\"))","v":"mit Einschränkung"}]
[50001696,"AFORE","AF8K-THP",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H25,1)=\"J\",LEFT(H25,2),LEFT(H25,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H25,1)=\"J\",RIGHT(H25,LEN(H25)-4),RIGHT(H25,LEN(H25)-6)),\"\"))","v":"mit Einschränkung"}]
[50001685,"AFORE","AF10K-TH",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H26,1)=\"J\",LEFT(H26,2),LEFT(H26,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H26,1)=\"J\",RIGHT(H26,LEN(H26)-4),RIGHT(H26,LEN(H26)-6)),\"\"))","v":"mit Einschränkung"}]
[50001697,"AFORE","AF10K-THP",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H27,1)=\"J\",LEFT(H27,2),LEFT(H27,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H27,1)=\"J\",RIGHT(H27,LEN(H27)-4),RIGHT(H27,LEN(H27)-6)),\"\"))","v":"mit Einschränkung"}]
[50001686,"AFORE","AF12K-TH",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H28,1)=\"J\",LEFT(H28,2),LEFT(H28,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H28,1)=\"J\",RIGHT(H28,LEN(H28)-4),RIGHT(H28,LEN(H28)-6)),\"\"))","v":"mit Einschränkung"}]
[50001698,"AFORE","AF12K-THP",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H29,1)=\"J\",LEFT(H29,2),LEFT(H29,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H29,1)=\"J\",RIGHT(H29,LEN(H29)-4),RIGHT(H29,LEN(H29)-6)),\"\"))","v":"mit Einschränkung"}]
[50001687,"AFORE","AF15K-TH",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H30,1)=\"J\",LEFT(H30,2),LEFT(H30,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H30,1)=\"J\",RIGHT(H30,LEN(H30)-4),RIGHT(H30,LEN(H30)-6)),\"\"))","v":"mit Einschränkung"}]
[50001688,"AFORE","AF17K-TH",17,18.7,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H31,1)=\"J\",LEFT(H31,2),LEFT(H31,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H31,1)=\"J\",RIGHT(H31,LEN(H31)-4),RIGHT(H31,LEN(H31)-6)),\"\"))","v":"mit Einschränkung"}]
[50001689,"AFORE","AF20K-TH",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H32,1)=\"J\",LEFT(H32,2),LEFT(H32,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H32,1)=\"J\",RIGHT(H32,LEN(H32)-4),RIGHT(H32,LEN(H32)-6)),\"\"))","v":"mit Einschränkung"}]
[50001690,"AFORE","AF25K-TH",25,27.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H33,1)=\"J\",LEFT(H33,2),LEFT(H33,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H33,1)=\"J\",RIGHT(H33,LEN(H33)-4),RIGHT(H33,LEN(H33)-6)),\"\"))","v":"mit Einschränkung"}]
[50001691,"AFORE","AF30K-TH",30,33,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-09","Martin Bertsch","2024-04-09","Protocol_Version: 2.32 HMI: 1.40 Main_DSP: 1.56 Vice_DSP: 1.01",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6162741.50","2023-08-01",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H34,1)=\"J\",LEFT(H34,2),LEFT(H34,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H34,1)=\"J\",RIGHT(H34,LEN(H34)-4),RIGHT(H34,LEN(H34)-6)),\"\"))","v":"mit Einschränkung"}]
[50000046,"Alpha ESS","SMILE-T10-HV-INV",10,10,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2024-01-12","V0.B8 EMS-Firmware-Version V0.00.65V",null,null,null,null,null,null,"Vorhanden","Martin Bertsch (OE)",null,null,"nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H35,1)=\"J\",LEFT(H35,2),LEFT(H35,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H35,1)=\"J\",RIGHT(H35,LEN(H35)-4),RIGHT(H35,LEN(H35)-6)),\"\"))","v":"mit Einschränkung"}]
[50000050,"ANKER","A-SPE",0.5,0.5,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-10-17","Martin Bertsch","2023-10-17",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"ZEK-ESH-P21011140-R3","2023-06-20","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H36,1)=\"J\",LEFT(H36,2),LEFT(H36,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H36,1)=\"J\",RIGHT(H36,LEN(H36)-4),RIGHT(H36,LEN(H36)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000051,"ANKER","A5142",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-10-17","Martin Bertsch","2023-10-17",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"ZEK-ESH-P21011140-R3","2023-06-20","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H37,1)=\"J\",LEFT(H37,2),LEFT(H37,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H37,1)=\"J\",RIGHT(H37,LEN(H37)-4),RIGHT(H37,LEN(H37)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000052,"ANKER","A5143",0.79900000000000004,0.79900000000000004,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-10-17","Martin Bertsch","2023-10-17",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"ZEK-ESH-P21011140-R3","2023-06-20","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H38,1)=\"J\",LEFT(H38,2),LEFT(H38,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H38,1)=\"J\",RIGHT(H38,LEN(H38)-4),RIGHT(H38,LEN(H38)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002109,"ANKER","A17C1",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"SUEE240400004251","2024-04-09","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H39,1)=\"J\",LEFT(H39,2),LEFT(H39,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H39,1)=\"J\",RIGHT(H39,LEN(H39)-4),RIGHT(H39,LEN(H39)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002110,"ANKER","A17C3",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"SUEE240400004251","2024-04-09","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H40,1)=\"J\",LEFT(H40,2),LEFT(H40,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H40,1)=\"J\",RIGHT(H40,LEN(H40)-4),RIGHT(H40,LEN(H40)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000053,"APSystems","DS3-L-SPE",0.5,0.5,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2022-07-07",null,"2022-07-07",null,null,null,null,null,null,null,"VDE4105/4110","Martin Bertsch (OE)",null,null,"Vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H41,1)=\"J\",LEFT(H41,2),LEFT(H41,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H41,1)=\"J\",RIGHT(H41,LEN(H41)-4),RIGHT(H41,LEN(H41)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000054,"APSystems","EZ1-SPE",0.5,0.5,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-05-08","Martin Bertsch","2023-05-08",null,null,null,null,null,null,null,"VDE4105/4110","Martin Bertsch (OE)","ZEK-ESH-P21011140-R3","2023-05-04","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H42,1)=\"J\",LEFT(H42,2),LEFT(H42,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H42,1)=\"J\",RIGHT(H42,LEN(H42)-4),RIGHT(H42,LEN(H42)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000055,"APSystems","DS3-S",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2022-07-08",null,"2022-07-08",null,null,null,null,null,null,null,"VDE4105/4110","Martin Bertsch (OE)",null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H43,1)=\"J\",LEFT(H43,2),LEFT(H43,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H43,1)=\"J\",RIGHT(H43,LEN(H43)-4),RIGHT(H43,LEN(H43)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000056,"APSystems","EZ1-S",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-05-08","Martin Bertsch","2023-05-08",null,null,null,null,null,null,null,"VDE4105/4110","Martin Bertsch (OE)","ZEK-ESH-P21011140-R3","2023-05-04","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H44,1)=\"J\",LEFT(H44,2),LEFT(H44,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H44,1)=\"J\",RIGHT(H44,LEN(H44)-4),RIGHT(H44,LEN(H44)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000057,"APSystems","YC 600 ",null,0.6,1,"PV-Wechselrichter","Nein","2022-07-08",null,null,null,null,null,null,"Nein","Nein","Nein","nicht vorhanden","Martin Bertsch (OE)",null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H45,1)=\"J\",LEFT(H45,2),LEFT(H45,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H45,1)=\"J\",RIGHT(H45,LEN(H45)-4),RIGHT(H45,LEN(H45)-6)),\"\"))","v":""}]
[50000058,"APSystems","DS3-L",0.73,0.73,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2022-07-07",null,"2022-07-07",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110","Martin Bertsch (OE)",null,null,"Vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H46,1)=\"J\",LEFT(H46,2),LEFT(H46,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H46,1)=\"J\",RIGHT(H46,LEN(H46)-4),RIGHT(H46,LEN(H46)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000059,"APSystems","DS3-M",0.79900000000000004,0.79900000000000004,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-05-26","Martin Bertsch","2022-10-18",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110","Martin Bertsch (OE)",null,null,"nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H47,1)=\"J\",LEFT(H47,2),LEFT(H47,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H47,1)=\"J\",RIGHT(H47,LEN(H47)-4),RIGHT(H47,LEN(H47)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000060,"APSystems","EZ1-M",0.79900000000000004,0.79900000000000004,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-05-08","Martin Bertsch","2023-05-08",null,null,null,null,null,null,null,"VDE4105/4110","Martin Bertsch (OE)","ZEK-ESH-P21011140-R3","2023-05-04","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H48,1)=\"J\",LEFT(H48,2),LEFT(H48,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H48,1)=\"J\",RIGHT(H48,LEN(H48)-4),RIGHT(H48,LEN(H48)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000061,"APSystems","DS3",0.88,0.88,1,"PV-Wechselrichter","Nein","2022-07-07",null,null,null,null,null,null,"Nein","Nein","Nein","nicht vorhanden","Martin Bertsch (OE)",null,null,"Vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H49,1)=\"J\",LEFT(H49,2),LEFT(H49,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H49,1)=\"J\",RIGHT(H49,LEN(H49)-4),RIGHT(H49,LEN(H49)-6)),\"\"))","v":""}]
[50000062,"APSystems","DS3-H",0.96,0.96,1,"PV-Wechselrichter","Nein","2022-07-07",null,null,null,null,null,null,"Nein","Nein","Nein","nicht vorhanden","Martin Bertsch (OE)",null,null,"Vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H50,1)=\"J\",LEFT(H50,2),LEFT(H50,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H50,1)=\"J\",RIGHT(H50,LEN(H50)-4),RIGHT(H50,LEN(H50)-6)),\"\"))","v":""}]
[50000063,"APSystems","YC 1000"," ",1.1299999999999999,3,"PV-Wechselrichter","Nein","2022-07-08",null,null,null,null,null," ","Nein","Nein","Nein","nicht vorhanden","Martin Bertsch (OE)"," "," ","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H51,1)=\"J\",LEFT(H51,2),LEFT(H51,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H51,1)=\"J\",RIGHT(H51,LEN(H51)-4),RIGHT(H51,LEN(H51)-6)),\"\"))","v":""}]
[50000064,"APSystems","ELS-3K",3.68,3.68,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage","2023-03-08","Martin Bertsch","2022-11-30",null,null,null,null,null,null,null,"OK","Roland Bründlinger","6095762.50V1.1","2023-02-17",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H52,1)=\"J\",LEFT(H52,2),LEFT(H52,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H52,1)=\"J\",RIGHT(H52,LEN(H52)-4),RIGHT(H52,LEN(H52)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001909,"ARKCHU","ARK-4KTL-HT",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","6173945.50","2023-11-24",null,"OK",null,null,null,null,"ident zu SUNWAYS",null,null,null,null,{"$f":"IF(LEFT(H53,1)=\"J\",LEFT(H53,2),LEFT(H53,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H53,1)=\"J\",RIGHT(H53,LEN(H53)-4),RIGHT(H53,LEN(H53)-6)),\"\"))","v":""}]
[50002054,"ARKCHU","ARK-4KTL-HT-13",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6173945.50","2023-11-24",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H54,1)=\"J\",LEFT(H54,2),LEFT(H54,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H54,1)=\"J\",RIGHT(H54,LEN(H54)-4),RIGHT(H54,LEN(H54)-6)),\"\"))","v":""}]
[50001910,"ARKCHU","ARK-5KTL-HT",5,5.5,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","6173945.50","2023-11-24",null,"OK",null,null,null,null,"ident zu SUNWAYS",null,null,null,null,{"$f":"IF(LEFT(H55,1)=\"J\",LEFT(H55,2),LEFT(H55,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H55,1)=\"J\",RIGHT(H55,LEN(H55)-4),RIGHT(H55,LEN(H55)-6)),\"\"))","v":""}]
[50002055,"ARKCHU","ARK-5KTL-HT-13",5,5.5,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6173945.50","2023-11-24",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H56,1)=\"J\",LEFT(H56,2),LEFT(H56,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H56,1)=\"J\",RIGHT(H56,LEN(H56)-4),RIGHT(H56,LEN(H56)-6)),\"\"))","v":""}]
[50001911,"ARKCHU","ARK-6KTL-HT",6,6.6,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","6173945.50","2023-11-24",null,"OK",null,null,null,null,"ident zu SUNWAYS",null,null,null,null,{"$f":"IF(LEFT(H57,1)=\"J\",LEFT(H57,2),LEFT(H57,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H57,1)=\"J\",RIGHT(H57,LEN(H57)-4),RIGHT(H57,LEN(H57)-6)),\"\"))","v":""}]
[50002056,"ARKCHU","ARK-6KTL-HT-13 ",6,6.6,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6173945.50","2023-11-24",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H58,1)=\"J\",LEFT(H58,2),LEFT(H58,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H58,1)=\"J\",RIGHT(H58,LEN(H58)-4),RIGHT(H58,LEN(H58)-6)),\"\"))","v":""}]
[50001912,"ARKCHU","ARK-8KTL-HT",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","6173945.50","2023-11-24",null,"OK",null,null,null,null,"ident zu SUNWAYS",null,null,null,null,{"$f":"IF(LEFT(H59,1)=\"J\",LEFT(H59,2),LEFT(H59,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H59,1)=\"J\",RIGHT(H59,LEN(H59)-4),RIGHT(H59,LEN(H59)-6)),\"\"))","v":""}]
[50002057,"ARKCHU","ARK-8KTL-HT-13",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6173945.50","2023-11-24",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H60,1)=\"J\",LEFT(H60,2),LEFT(H60,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H60,1)=\"J\",RIGHT(H60,LEN(H60)-4),RIGHT(H60,LEN(H60)-6)),\"\"))","v":""}]
[50001913,"ARKCHU","ARK-10KTL-HT",10,11,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","6173945.50","2023-11-24",null,"OK",null,null,null,null,"ident zu SUNWAYS",null,null,null,null,{"$f":"IF(LEFT(H61,1)=\"J\",LEFT(H61,2),LEFT(H61,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H61,1)=\"J\",RIGHT(H61,LEN(H61)-4),RIGHT(H61,LEN(H61)-6)),\"\"))","v":""}]
[50002058,"ARKCHU","ARK-10KTL-HT-13",10,11,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6173945.50","2023-11-24",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H62,1)=\"J\",LEFT(H62,2),LEFT(H62,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H62,1)=\"J\",RIGHT(H62,LEN(H62)-4),RIGHT(H62,LEN(H62)-6)),\"\"))","v":""}]
[50001914,"ARKCHU","ARK-12KTL-HT",12,13.2,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","6173945.50","2023-11-24",null,"OK",null,null,null,null,"ident zu SUNWAYS",null,null,null,null,{"$f":"IF(LEFT(H63,1)=\"J\",LEFT(H63,2),LEFT(H63,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H63,1)=\"J\",RIGHT(H63,LEN(H63)-4),RIGHT(H63,LEN(H63)-6)),\"\"))","v":""}]
[50002059,"ARKCHU","ARK-12KTL-HT-13",12,13.2,3,"Hybrid-Wechselrichter","Ja","2024-01-08","Martin Bertsch","2024-01-08","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6173945.50","2023-11-24",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H64,1)=\"J\",LEFT(H64,2),LEFT(H64,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H64,1)=\"J\",RIGHT(H64,LEN(H64)-4),RIGHT(H64,LEN(H64)-6)),\"\"))","v":""}]
[50000065,"a-TroniX","Hybridpower 4kW 3ph",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Nein","2023-05-08","Martin Bertsch",null,null,null,null,"ident zu SUNWAYS; Fehlverhalten des Geräts","Ja","Nein","Nein","OK","Martin Bertsch (OE)","6134610.50V1.1","2023-04-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H65,1)=\"J\",LEFT(H65,2),LEFT(H65,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H65,1)=\"J\",RIGHT(H65,LEN(H65)-4),RIGHT(H65,LEN(H65)-6)),\"\"))","v":""}]
[50002060,"a-Tronix","AX5.0kW-3ph",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2024-01-17","1.96 (Master)",null,null,"ident zu FOXESS","Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H66,1)=\"J\",LEFT(H66,2),LEFT(H66,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H66,1)=\"J\",RIGHT(H66,LEN(H66)-4),RIGHT(H66,LEN(H66)-6)),\"\"))","v":"mit Einschränkung"}]
[50000066,"a-TroniX","Hybridpower 5kW 3ph",5,5.5,3,"Hybrid-Wechselrichter","Nein","2023-05-08","Martin Bertsch",null,null,null,null,"ident zu SUNWAYS; Fehlverhalten des Geräts","Ja","Nein","Nein","OK","Martin Bertsch (OE)","6134610.50V1.1","2023-04-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H67,1)=\"J\",LEFT(H67,2),LEFT(H67,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H67,1)=\"J\",RIGHT(H67,LEN(H67)-4),RIGHT(H67,LEN(H67)-6)),\"\"))","v":""}]
[50002061,"a-Tronix","AX6.0kW-3ph",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2024-01-17","1.96 (Master)",null,null,"ident zu FOXESS","Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H68,1)=\"J\",LEFT(H68,2),LEFT(H68,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H68,1)=\"J\",RIGHT(H68,LEN(H68)-4),RIGHT(H68,LEN(H68)-6)),\"\"))","v":"mit Einschränkung"}]
[50000067,"a-TroniX","Hybridpower 6kW 3ph",6,6.6,3,"Hybrid-Wechselrichter","Nein","2023-05-08","Martin Bertsch",null,null,null,null,"ident zu SUNWAYS; Fehlverhalten des Geräts","Ja","Nein","Nein","OK","Martin Bertsch (OE)","6134610.50V1.1","2023-04-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H69,1)=\"J\",LEFT(H69,2),LEFT(H69,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H69,1)=\"J\",RIGHT(H69,LEN(H69)-4),RIGHT(H69,LEN(H69)-6)),\"\"))","v":""}]
[50002062,"a-Tronix","AX8.0kW-3ph",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2024-01-17","1.96 (Master)",null,null,"ident zu FOXESS","Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H70,1)=\"J\",LEFT(H70,2),LEFT(H70,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H70,1)=\"J\",RIGHT(H70,LEN(H70)-4),RIGHT(H70,LEN(H70)-6)),\"\"))","v":"mit Einschränkung"}]
[50000068,"a-TroniX","Hybridpower 8kW 3ph",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein","2023-05-08","Martin Bertsch",null,null,null,null,"ident zu SUNWAYS; Fehlverhalten des Geräts","Ja","Nein","Nein","OK","Martin Bertsch (OE)","6134610.50V1.1","2023-04-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H71,1)=\"J\",LEFT(H71,2),LEFT(H71,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H71,1)=\"J\",RIGHT(H71,LEN(H71)-4),RIGHT(H71,LEN(H71)-6)),\"\"))","v":""}]
[50002063,"a-Tronix","AX10.0kW-3ph",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2024-01-17","1.96 (Master)",null,null,"ident zu FOXESS","Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H72,1)=\"J\",LEFT(H72,2),LEFT(H72,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H72,1)=\"J\",RIGHT(H72,LEN(H72)-4),RIGHT(H72,LEN(H72)-6)),\"\"))","v":"mit Einschränkung"}]
[50000069,"a-TroniX","Hybridpower 10kW 3ph",10,11,3,"Hybrid-Wechselrichter","Nein","2023-05-08","Martin Bertsch",null,null,null,null,"ident zu SUNWAYS; Fehlverhalten des Geräts","Ja","Nein","Nein","OK","Martin Bertsch (OE)","6134610.50V1.1","2023-04-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H73,1)=\"J\",LEFT(H73,2),LEFT(H73,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H73,1)=\"J\",RIGHT(H73,LEN(H73)-4),RIGHT(H73,LEN(H73)-6)),\"\"))","v":""}]
[50002064,"a-Tronix","AX12.0kW-3ph",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2024-01-17","1.96 (Master)",null,null,"ident zu FOXESS","Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H74,1)=\"J\",LEFT(H74,2),LEFT(H74,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H74,1)=\"J\",RIGHT(H74,LEN(H74)-4),RIGHT(H74,LEN(H74)-6)),\"\"))","v":"mit Einschränkung"}]
[50000070,"a-TroniX","Hybridpower 12kW 3ph",12,13.2,3,"Hybrid-Wechselrichter","Nein","2023-05-08","Martin Bertsch",null,null,null,null,"ident zu SUNWAYS; Fehlverhalten des Geräts","Ja","Nein","Nein","OK","Martin Bertsch (OE)","6134610.50V1.1","2023-04-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H75,1)=\"J\",LEFT(H75,2),LEFT(H75,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H75,1)=\"J\",RIGHT(H75,LEN(H75)-4),RIGHT(H75,LEN(H75)-6)),\"\"))","v":""}]
[50001975,"AUSTA","AU-1P6002G",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2023-12-04","Martin Bertsch","2023-12-04","FW 0x9200 ",null,null,null,"Nein","Nein","Nein","OK","Michael Tippmann","64.290.20.30267.03","2022-01-10","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H76,1)=\"J\",LEFT(H76,2),LEFT(H76,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H76,1)=\"J\",RIGHT(H76,LEN(H76)-4),RIGHT(H76,LEN(H76)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50001976,"AUSTA","AU-1P8002G",0.75,0.75,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2023-12-04","Martin Bertsch","2023-12-04","FW 0x9200 ",null,null,null,"Nein","Nein","Nein","OK","Michael Tippmann","64.290.20.30267.03","2022-01-10","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H77,1)=\"J\",LEFT(H77,2),LEFT(H77,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H77,1)=\"J\",RIGHT(H77,LEN(H77)-4),RIGHT(H77,LEN(H77)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50000071,"batterX","batterX h10 ",10,10,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2024-03-12","Martin Bertsch",null,null,null,"2023-12-31","Frist wurde um 1 Monat verlängert; Testgerät wurde geliefert","Ja","Ja",null,"OK","Moustafa Mohamed (Netz NÖ)","21TH0361-OVE-directive R25_0","2021-05-21","nicht vorhanden","nicht vorhanden",null,null,null,null,"Hybridwechselrichter 3~ - NETZUMSCHALTBOX - KONFORM - TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H78,1)=\"J\",LEFT(H78,2),LEFT(H78,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H78,1)=\"J\",RIGHT(H78,LEN(H78)-4),RIGHT(H78,LEN(H78)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000072,"BLUESUN","BSE6KH3",6,6.6,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-31",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein",null,"Vorhanden",null,"64.290.23.30588.01","2023-04-20","nicht vorhanden","OK",null,null,null,null,"ident zu Megarevo",null,null,null,null,{"$f":"IF(LEFT(H79,1)=\"J\",LEFT(H79,2),LEFT(H79,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H79,1)=\"J\",RIGHT(H79,LEN(H79)-4),RIGHT(H79,LEN(H79)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000073,"BLUESUN","BSE8KH3",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-31",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein",null,"Vorhanden",null,"64.290.23.30588.01","2023-04-20","nicht vorhanden","OK",null,null,null,null,"ident zu Megarevo",null,null,null,null,{"$f":"IF(LEFT(H80,1)=\"J\",LEFT(H80,2),LEFT(H80,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H80,1)=\"J\",RIGHT(H80,LEN(H80)-4),RIGHT(H80,LEN(H80)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000074,"BLUESUN","BSE10KH3",10,11,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-31",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein",null,"Vorhanden",null,"64.290.23.30588.01","2023-04-20","nicht vorhanden","OK",null,null,null,null,"ident zu Megarevo",null,null,null,null,{"$f":"IF(LEFT(H81,1)=\"J\",LEFT(H81,2),LEFT(H81,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H81,1)=\"J\",RIGHT(H81,LEN(H81)-4),RIGHT(H81,LEN(H81)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000075,"BLUESUN","BSE12KH3",12,13.2,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-31",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein",null,"Vorhanden",null,"64.290.23.30588.01","2023-04-20","nicht vorhanden","OK",null,null,null,null,"ident zu Megarevo",null,null,null,null,{"$f":"IF(LEFT(H82,1)=\"J\",LEFT(H82,2),LEFT(H82,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H82,1)=\"J\",RIGHT(H82,LEN(H82)-4),RIGHT(H82,LEN(H82)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000076,"BLUESUN","BSE15KH3",15,16.5,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-31",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein",null,"Vorhanden",null,"64.290.23.30588.01","2023-04-20","nicht vorhanden","OK",null,null,null,null,"ident zu Megarevo",null,null,null,null,{"$f":"IF(LEFT(H83,1)=\"J\",LEFT(H83,2),LEFT(H83,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H83,1)=\"J\",RIGHT(H83,LEN(H83)-4),RIGHT(H83,LEN(H83)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001881,"BLUESUN","BSM25K-B4",25,27.5,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H84,1)=\"J\",LEFT(H84,2),LEFT(H84,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H84,1)=\"J\",RIGHT(H84,LEN(H84)-4),RIGHT(H84,LEN(H84)-6)),\"\"))","v":"In Prüfung"}]
[50001882,"BLUESUN","BSM25K-B5",25,27.5,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H85,1)=\"J\",LEFT(H85,2),LEFT(H85,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H85,1)=\"J\",RIGHT(H85,LEN(H85)-4),RIGHT(H85,LEN(H85)-6)),\"\"))","v":"In Prüfung"}]
[50001883,"BLUESUN","BSM25K-B6",25,27.5,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H86,1)=\"J\",LEFT(H86,2),LEFT(H86,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H86,1)=\"J\",RIGHT(H86,LEN(H86)-4),RIGHT(H86,LEN(H86)-6)),\"\"))","v":"In Prüfung"}]
[50001884,"BLUESUN","BSM25K-B7",25,27.5,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H87,1)=\"J\",LEFT(H87,2),LEFT(H87,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H87,1)=\"J\",RIGHT(H87,LEN(H87)-4),RIGHT(H87,LEN(H87)-6)),\"\"))","v":"In Prüfung"}]
[50001886,"BLUESUN","BSM30K-B",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H88,1)=\"J\",LEFT(H88,2),LEFT(H88,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H88,1)=\"J\",RIGHT(H88,LEN(H88)-4),RIGHT(H88,LEN(H88)-6)),\"\"))","v":"In Prüfung"}]
[50001885,"BLUESUN","BSM30K-B1",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H89,1)=\"J\",LEFT(H89,2),LEFT(H89,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H89,1)=\"J\",RIGHT(H89,LEN(H89)-4),RIGHT(H89,LEN(H89)-6)),\"\"))","v":"In Prüfung"}]
[50001887,"BLUESUN","BSM30K-B2",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H90,1)=\"J\",LEFT(H90,2),LEFT(H90,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H90,1)=\"J\",RIGHT(H90,LEN(H90)-4),RIGHT(H90,LEN(H90)-6)),\"\"))","v":"In Prüfung"}]
[50001888,"BLUESUN","BSM30K-B3",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H91,1)=\"J\",LEFT(H91,2),LEFT(H91,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H91,1)=\"J\",RIGHT(H91,LEN(H91)-4),RIGHT(H91,LEN(H91)-6)),\"\"))","v":"In Prüfung"}]
[50001889,"BLUESUN","BSM30K-B4",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H92,1)=\"J\",LEFT(H92,2),LEFT(H92,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H92,1)=\"J\",RIGHT(H92,LEN(H92)-4),RIGHT(H92,LEN(H92)-6)),\"\"))","v":"In Prüfung"}]
[50001890,"BLUESUN","BSM30K-B5",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H93,1)=\"J\",LEFT(H93,2),LEFT(H93,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H93,1)=\"J\",RIGHT(H93,LEN(H93)-4),RIGHT(H93,LEN(H93)-6)),\"\"))","v":"In Prüfung"}]
[50001892,"BLUESUN","BSM33K-B",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H94,1)=\"J\",LEFT(H94,2),LEFT(H94,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H94,1)=\"J\",RIGHT(H94,LEN(H94)-4),RIGHT(H94,LEN(H94)-6)),\"\"))","v":"In Prüfung"}]
[50001891,"BLUESUN","BSM33K-B1",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H95,1)=\"J\",LEFT(H95,2),LEFT(H95,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H95,1)=\"J\",RIGHT(H95,LEN(H95)-4),RIGHT(H95,LEN(H95)-6)),\"\"))","v":"In Prüfung"}]
[50001893,"BLUESUN","BSM33K-B2",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H96,1)=\"J\",LEFT(H96,2),LEFT(H96,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H96,1)=\"J\",RIGHT(H96,LEN(H96)-4),RIGHT(H96,LEN(H96)-6)),\"\"))","v":"In Prüfung"}]
[50001894,"BLUESUN","BSM33K-B3",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H97,1)=\"J\",LEFT(H97,2),LEFT(H97,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H97,1)=\"J\",RIGHT(H97,LEN(H97)-4),RIGHT(H97,LEN(H97)-6)),\"\"))","v":"In Prüfung"}]
[50001895,"BLUESUN","BSM33K-B4",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H98,1)=\"J\",LEFT(H98,2),LEFT(H98,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H98,1)=\"J\",RIGHT(H98,LEN(H98)-4),RIGHT(H98,LEN(H98)-6)),\"\"))","v":"In Prüfung"}]
[50001896,"BLUESUN","BSM33K-B5",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H99,1)=\"J\",LEFT(H99,2),LEFT(H99,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H99,1)=\"J\",RIGHT(H99,LEN(H99)-4),RIGHT(H99,LEN(H99)-6)),\"\"))","v":"In Prüfung"}]
[50001898,"BLUESUN","BSM36K-B",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H100,1)=\"J\",LEFT(H100,2),LEFT(H100,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H100,1)=\"J\",RIGHT(H100,LEN(H100)-4),RIGHT(H100,LEN(H100)-6)),\"\"))","v":"In Prüfung"}]
[50001897,"BLUESUN","BSM36K-B1",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H101,1)=\"J\",LEFT(H101,2),LEFT(H101,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H101,1)=\"J\",RIGHT(H101,LEN(H101)-4),RIGHT(H101,LEN(H101)-6)),\"\"))","v":"In Prüfung"}]
[50001899,"BLUESUN","BSM36K-B2",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H102,1)=\"J\",LEFT(H102,2),LEFT(H102,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H102,1)=\"J\",RIGHT(H102,LEN(H102)-4),RIGHT(H102,LEN(H102)-6)),\"\"))","v":"In Prüfung"}]
[50001900,"BLUESUN","BSM36K-B3",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H103,1)=\"J\",LEFT(H103,2),LEFT(H103,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H103,1)=\"J\",RIGHT(H103,LEN(H103)-4),RIGHT(H103,LEN(H103)-6)),\"\"))","v":"In Prüfung"}]
[50001901,"BLUESUN","BSM36K-B4",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H104,1)=\"J\",LEFT(H104,2),LEFT(H104,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H104,1)=\"J\",RIGHT(H104,LEN(H104)-4),RIGHT(H104,LEN(H104)-6)),\"\"))","v":"In Prüfung"}]
[50001902,"BLUESUN","BSM36K-B5",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H105,1)=\"J\",LEFT(H105,2),LEFT(H105,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H105,1)=\"J\",RIGHT(H105,LEN(H105)-4),RIGHT(H105,LEN(H105)-6)),\"\"))","v":"In Prüfung"}]
[50001904,"BLUESUN","BSM40K-B",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H106,1)=\"J\",LEFT(H106,2),LEFT(H106,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H106,1)=\"J\",RIGHT(H106,LEN(H106)-4),RIGHT(H106,LEN(H106)-6)),\"\"))","v":"In Prüfung"}]
[50001903,"BLUESUN","BSM40K-B1",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H107,1)=\"J\",LEFT(H107,2),LEFT(H107,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H107,1)=\"J\",RIGHT(H107,LEN(H107)-4),RIGHT(H107,LEN(H107)-6)),\"\"))","v":"In Prüfung"}]
[50001905,"BLUESUN","BSM40K-B2",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H108,1)=\"J\",LEFT(H108,2),LEFT(H108,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H108,1)=\"J\",RIGHT(H108,LEN(H108)-4),RIGHT(H108,LEN(H108)-6)),\"\"))","v":"In Prüfung"}]
[50001906,"BLUESUN","BSM40K-B3",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H109,1)=\"J\",LEFT(H109,2),LEFT(H109,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H109,1)=\"J\",RIGHT(H109,LEN(H109)-4),RIGHT(H109,LEN(H109)-6)),\"\"))","v":"In Prüfung"}]
[50001907,"BLUESUN","BSM40K-B4",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H110,1)=\"J\",LEFT(H110,2),LEFT(H110,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H110,1)=\"J\",RIGHT(H110,LEN(H110)-4),RIGHT(H110,LEN(H110)-6)),\"\"))","v":"In Prüfung"}]
[50001908,"BLUESUN","BSM40K-B5",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-10-10","Martin Bertsch",null,null,null,null,"OEM Gerät befindet sich gerade beim AIT. Schwere Fehler.","Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVP05010/23B-01","2023-08-11","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H111,1)=\"J\",LEFT(H111,2),LEFT(H111,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H111,1)=\"J\",RIGHT(H111,LEN(H111)-4),RIGHT(H111,LEN(H111)-6)),\"\"))","v":"In Prüfung"}]
[50001880,"BLUETTI","EP600",6,6,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-07-18","Martin Bertsch",null,null,null,null,null,"Ja","Ja","Ja","Vorhanden",null,"230216054GZU-001","2023-05-24","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H112,1)=\"J\",LEFT(H112,2),LEFT(H112,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H112,1)=\"J\",RIGHT(H112,LEN(H112)-4),RIGHT(H112,LEN(H112)-6)),\"\"))","v":"In Prüfung"}]
[50000078,"BOSSWERK","BW-MI300",0.3,0.3,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,"2021-10-21",null,null,null,null,"Nein","Nein",null,"VDE4105/4110",null,null,null,"Vorhanden",null,null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H113,1)=\"J\",LEFT(H113,2),LEFT(H113,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H113,1)=\"J\",RIGHT(H113,LEN(H113)-4),RIGHT(H113,LEN(H113)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000079,"BOSSWERK","BW-MI500",0.5,0.5,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,null,null,null,null,null,null,null,null,"VDE4105/4110",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H114,1)=\"J\",LEFT(H114,2),LEFT(H114,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H114,1)=\"J\",RIGHT(H114,LEN(H114)-4),RIGHT(H114,LEN(H114)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000080,"BOSSWERK","BW-MI600",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,"2021-10-21",null,null,null,null,"Nein","Nein",null,"VDE4105/4110",null,null,null,"Vorhanden",null,null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H115,1)=\"J\",LEFT(H115,2),LEFT(H115,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H115,1)=\"J\",RIGHT(H115,LEN(H115)-4),RIGHT(H115,LEN(H115)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000081,"BOSSWERK","BW-MI800",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,null,null,null,null,null,null,null,null,"VDE4105/4110",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H116,1)=\"J\",LEFT(H116,2),LEFT(H116,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H116,1)=\"J\",RIGHT(H116,LEN(H116)-4),RIGHT(H116,LEN(H116)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002291,"CESC","Mars 5000 HVT",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2024-06-17","V1.05",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CMPM-ESH_P23101015","2024-06-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H117,1)=\"J\",LEFT(H117,2),LEFT(H117,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H117,1)=\"J\",RIGHT(H117,LEN(H117)-4),RIGHT(H117,LEN(H117)-6)),\"\"))","v":"mit Einschränkung"}]
[50002292,"CESC","Mars 6000 HVT",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2024-06-17","V1.05",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CMPM-ESH_P23101015","2024-06-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H118,1)=\"J\",LEFT(H118,2),LEFT(H118,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H118,1)=\"J\",RIGHT(H118,LEN(H118)-4),RIGHT(H118,LEN(H118)-6)),\"\"))","v":"mit Einschränkung"}]
[50002293,"CESC","Mars 8000 HVT",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2024-06-17","V1.05",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CMPM-ESH_P23101015","2024-06-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H119,1)=\"J\",LEFT(H119,2),LEFT(H119,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H119,1)=\"J\",RIGHT(H119,LEN(H119)-4),RIGHT(H119,LEN(H119)-6)),\"\"))","v":"mit Einschränkung"}]
[50002294,"CESC","Mars 10000 HVT",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2024-06-17","V1.05",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CMPM-ESH_P23101015","2024-06-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H120,1)=\"J\",LEFT(H120,2),LEFT(H120,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H120,1)=\"J\",RIGHT(H120,LEN(H120)-4),RIGHT(H120,LEN(H120)-6)),\"\"))","v":"mit Einschränkung"}]
[50000085,"Chint","CPS SCA1KTL-S/EU",1,1.1000000000000001,1,"PV-Wechselrichter","Nein","2022-09-13","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H121,1)=\"J\",LEFT(H121,2),LEFT(H121,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H121,1)=\"J\",RIGHT(H121,LEN(H121)-4),RIGHT(H121,LEN(H121)-6)),\"\"))","v":""}]
[50000086,"Chint","CPS SCA2KTL-S/EU",2,2.2000000000000002,1,"PV-Wechselrichter","Nein","2022-09-14","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H122,1)=\"J\",LEFT(H122,2),LEFT(H122,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H122,1)=\"J\",RIGHT(H122,LEN(H122)-4),RIGHT(H122,LEN(H122)-6)),\"\"))","v":""}]
[50000087,"Chint","CPS SCA3KTL-S/EU",3,3.3,1,"PV-Wechselrichter","Nein","2022-09-15","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H123,1)=\"J\",LEFT(H123,2),LEFT(H123,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H123,1)=\"J\",RIGHT(H123,LEN(H123)-4),RIGHT(H123,LEN(H123)-6)),\"\"))","v":""}]
[50000088,"Chint","CPS SCA3KTL-SM/EU",3,3.3,1,"PV-Wechselrichter","Nein","2022-09-16","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H124,1)=\"J\",LEFT(H124,2),LEFT(H124,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H124,1)=\"J\",RIGHT(H124,LEN(H124)-4),RIGHT(H124,LEN(H124)-6)),\"\"))","v":""}]
[50000089,"Chint","CPS SCA4KTL-SM/EU",4,4.4000000000000004,1,"PV-Wechselrichter","Nein","2022-09-17","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H125,1)=\"J\",LEFT(H125,2),LEFT(H125,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H125,1)=\"J\",RIGHT(H125,LEN(H125)-4),RIGHT(H125,LEN(H125)-6)),\"\"))","v":""}]
[50000090,"Chint","CPS SCA4.6KTL-SM/EU",4.5999999999999996,4.5999999999999996,1,"PV-Wechselrichter","Nein","2022-09-18","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H126,1)=\"J\",LEFT(H126,2),LEFT(H126,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H126,1)=\"J\",RIGHT(H126,LEN(H126)-4),RIGHT(H126,LEN(H126)-6)),\"\"))","v":""}]
[50000091,"Chint","CPS SCA6KTL-T/EU",6,6.6,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2023-10-09",null,"2024-03-13","2024-03-13","schwere Fehler","Nein",null,"Nein","Vorhanden","Martin Bertsch (OE)","PVAT2212WDG0040-1-R1","2023-07-14","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H127,1)=\"J\",LEFT(H127,2),LEFT(H127,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H127,1)=\"J\",RIGHT(H127,LEN(H127)-4),RIGHT(H127,LEN(H127)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000092,"Chint","CPS SCA8KTL-T/EU",8,8.8000000000000007,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2023-10-09",null,"2024-03-13","2024-03-13","schwere Fehler","Nein",null,"Nein","Vorhanden","Martin Bertsch (OE)","PVAT2212WDG0040-1-R1","2023-07-14","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H128,1)=\"J\",LEFT(H128,2),LEFT(H128,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H128,1)=\"J\",RIGHT(H128,LEN(H128)-4),RIGHT(H128,LEN(H128)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000093,"Chint","CPS SCA10KTL-T/EU",10,11,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2023-10-09",null,"2024-03-13","2024-03-13","schwere Fehler","Nein",null,"Nein","Vorhanden","Martin Bertsch (OE)","PVAT2212WDG0040-1-R1","2023-07-14","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H129,1)=\"J\",LEFT(H129,2),LEFT(H129,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H129,1)=\"J\",RIGHT(H129,LEN(H129)-4),RIGHT(H129,LEN(H129)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000094,"Chint","CPS SCA12KTL-T/EU",12,13.2,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2023-10-09",null,"2024-03-13","2024-03-13","schwere Fehler","Nein",null,"Nein","Vorhanden","Martin Bertsch (OE)","PVAT2212WDG0040-1-R1","2023-07-14","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H130,1)=\"J\",LEFT(H130,2),LEFT(H130,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H130,1)=\"J\",RIGHT(H130,LEN(H130)-4),RIGHT(H130,LEN(H130)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000095,"Chint","CPS SCA15KTL-T/EU",15,16.5,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2023-10-09",null,"2024-03-13","2024-03-13","schwere Fehler","Nein",null,"Nein","Vorhanden","Martin Bertsch (OE)","PVAT2212WDG0040-1-R1","2023-07-14","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H131,1)=\"J\",LEFT(H131,2),LEFT(H131,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H131,1)=\"J\",RIGHT(H131,LEN(H131)-4),RIGHT(H131,LEN(H131)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000096,"Chint","CPS SCA17KTL-T/EU",17,18.7,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2022-11-30",null,"2024-03-13","2024-03-13","schwere Fehler",null,null,null,"nicht OK","Roland Bründlinger","PVAT2210WDG0050-1","2022-10-31","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H132,1)=\"J\",LEFT(H132,2),LEFT(H132,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H132,1)=\"J\",RIGHT(H132,LEN(H132)-4),RIGHT(H132,LEN(H132)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000097,"Chint","CPS SCA20KTL-T/EU",20,22,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2022-11-30",null,"2024-03-13","2024-03-13","schwere Fehler",null,null,null,"nicht OK","Roland Bründlinger","PVAT2210WDG0050-1","2022-10-31","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H133,1)=\"J\",LEFT(H133,2),LEFT(H133,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H133,1)=\"J\",RIGHT(H133,LEN(H133)-4),RIGHT(H133,LEN(H133)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000098,"Chint","CPS SCA22KTL-T/EU",22,24.2,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2022-11-30",null,"2024-03-13","2024-03-13","schwere Fehler",null,null,null,"nicht OK","Roland Bründlinger","PVAT2210WDG0050-1","2022-10-31","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H134,1)=\"J\",LEFT(H134,2),LEFT(H134,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H134,1)=\"J\",RIGHT(H134,LEN(H134)-4),RIGHT(H134,LEN(H134)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000099,"Chint","CPS SCA25KTL-T/EU",25,27.5,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2022-11-30",null,"2024-03-13","2024-03-13","schwere Fehler",null,null,null,"nicht OK","Roland Bründlinger","PVAT2210WDG0050-1","2022-10-31","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H135,1)=\"J\",LEFT(H135,2),LEFT(H135,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H135,1)=\"J\",RIGHT(H135,LEN(H135)-4),RIGHT(H135,LEN(H135)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000100,"Chint","CPS SCA28KTL-T/EU",28,30.8,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2022-11-30",null,"2024-03-13","2024-03-13","schwere Fehler",null,null,null,"nicht OK","Roland Bründlinger","PVAT2210WDG0050-1","2022-10-31","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H136,1)=\"J\",LEFT(H136,2),LEFT(H136,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H136,1)=\"J\",RIGHT(H136,LEN(H136)-4),RIGHT(H136,LEN(H136)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000101,"Chint","CPS SCA30KTL-T1/EU",30,33,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2022-11-30",null,"2024-03-13","2024-03-13","schwere Fehler",null,null,null,"nicht OK","Roland Bründlinger","PVAT2210WDG0050-1","2022-10-31","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H137,1)=\"J\",LEFT(H137,2),LEFT(H137,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H137,1)=\"J\",RIGHT(H137,LEN(H137)-4),RIGHT(H137,LEN(H137)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000102,"Chint","CPS SCA50KTL-T/EU",50,55,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2022-11-30",null,"2024-03-13","2024-03-13","schwere Fehler",null,null,null,"OK","Roland Bründlinger","PVAT2209WDG0118-1-R1","2023-05-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H138,1)=\"J\",LEFT(H138,2),LEFT(H138,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H138,1)=\"J\",RIGHT(H138,LEN(H138)-4),RIGHT(H138,LEN(H138)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000103,"Chint","CPS SCA60KTL-T/EU",60,66,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-03-13","Martin Bertsch","2022-11-30",null,"2024-03-13","2024-03-13","schwere Fehler",null,null,null,"OK","Roland Bründlinger","PVAT2209WDG0118-1-R1","2023-05-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H139,1)=\"J\",LEFT(H139,2),LEFT(H139,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H139,1)=\"J\",RIGHT(H139,LEN(H139)-4),RIGHT(H139,LEN(H139)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000104,"CHISAGE","CE-3P5K1G-LE-EU",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2024-04-23","FW Ver 1150. Nach Update Werksreset durchführen und Ländereinstellungen neu setzen.",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","ASUE-ESH-P23020559","2023-02-14","nicht vorhanden","OK",null,null,null,null,"ident zu DEYE",null,null,null,null,{"$f":"IF(LEFT(H140,1)=\"J\",LEFT(H140,2),LEFT(H140,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H140,1)=\"J\",RIGHT(H140,LEN(H140)-4),RIGHT(H140,LEN(H140)-6)),\"\"))","v":"mit Einschränkung"}]
[50000105,"CHISAGE","CE-3P6K1G-LE-EU",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2024-04-23","FW Ver 1150. Nach Update Werksreset durchführen und Ländereinstellungen neu setzen.",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","ASUE-ESH-P23020559","2023-02-14","nicht vorhanden","OK",null,null,null,null,"ident zu DEYE",null,null,null,null,{"$f":"IF(LEFT(H141,1)=\"J\",LEFT(H141,2),LEFT(H141,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H141,1)=\"J\",RIGHT(H141,LEN(H141)-4),RIGHT(H141,LEN(H141)-6)),\"\"))","v":"mit Einschränkung"}]
[50000106,"CHISAGE","CE-3P8K1G-LE-EU",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2024-04-23","FW Ver 1150. Nach Update Werksreset durchführen und Ländereinstellungen neu setzen.",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","ASUE-ESH-P23020559","2023-02-14","nicht vorhanden","OK",null,null,null,null,"ident zu DEYE",null,null,null,null,{"$f":"IF(LEFT(H142,1)=\"J\",LEFT(H142,2),LEFT(H142,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H142,1)=\"J\",RIGHT(H142,LEN(H142)-4),RIGHT(H142,LEN(H142)-6)),\"\"))","v":"mit Einschränkung"}]
[50000107,"CHISAGE","CE-3P10K1G-LE-EU",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2024-04-23","FW Ver 1150. Nach Update Werksreset durchführen und Ländereinstellungen neu setzen.",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","ASUE-ESH-P23020559","2023-02-14","nicht vorhanden","OK",null,null,null,null,"ident zu DEYE",null,null,null,null,{"$f":"IF(LEFT(H143,1)=\"J\",LEFT(H143,2),LEFT(H143,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H143,1)=\"J\",RIGHT(H143,LEN(H143)-4),RIGHT(H143,LEN(H143)-6)),\"\"))","v":"mit Einschränkung"}]
[50000108,"CHISAGE","CE-3P12K1G-LE-EU",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2024-04-23","FW Ver 1150. Nach Update Werksreset durchführen und Ländereinstellungen neu setzen.",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","ASUE-ESH-P23020559","2023-02-14","nicht vorhanden","OK",null,null,null,null,"ident zu DEYE",null,null,null,null,{"$f":"IF(LEFT(H144,1)=\"J\",LEFT(H144,2),LEFT(H144,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H144,1)=\"J\",RIGHT(H144,LEN(H144)-4),RIGHT(H144,LEN(H144)-6)),\"\"))","v":"mit Einschränkung"}]
[50000109,"CRAFTSTROM","Hedy",0.3,0.3,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-05-26","Martin Bertsch","2023-05-26",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"230300276SHA-001","2023-03-21","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H145,1)=\"J\",LEFT(H145,2),LEFT(H145,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H145,1)=\"J\",RIGHT(H145,LEN(H145)-4),RIGHT(H145,LEN(H145)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000110,"DAH Solar","DHN-SU600D-G0",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2024-06-17","Martin Bertsch","2024-06-17","DHN-SU1K5T-G0-SW V1.0 DSP date version HAB85XAaV101A240521 Gateway version 3.0.2",null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","230421BWA078-EG-AT-001-R1","2023-07-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H146,1)=\"J\",LEFT(H146,2),LEFT(H146,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H146,1)=\"J\",RIGHT(H146,LEN(H146)-4),RIGHT(H146,LEN(H146)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50000111,"DAH Solar","DHN-SU800D-G0",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2024-03-13","Martin Bertsch","2024-06-17","DHN-SU1K5T-G0-SW V1.0 DSP date version HAB85XAaV101A240521 Gateway version 3.0.2",null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","230421BWA078-EG-AT-001-R1","2023-07-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H147,1)=\"J\",LEFT(H147,2),LEFT(H147,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H147,1)=\"J\",RIGHT(H147,LEN(H147)-4),RIGHT(H147,LEN(H147)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50000112,"DAH Solar","DHN-SU920D-G0",0.92,0.92,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2024-03-13","Martin Bertsch","2024-06-17","DHN-SU1K5T-G0-SW V1.0 DSP date version HAB85XAaV101A240521 Gateway version 3.0.2",null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","230421BWA078-EG-AT-001-R1","2023-07-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H148,1)=\"J\",LEFT(H148,2),LEFT(H148,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H148,1)=\"J\",RIGHT(H148,LEN(H148)-4),RIGHT(H148,LEN(H148)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50000113,"DAH Solar","DHN-SU1K5T-G0",1.5,1.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2024-03-13","Martin Bertsch","2024-06-17","DHN-SU1K5T-G0-SW V1.0 DSP date version HAB85XAaV101A240521 Gateway version 3.0.2",null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","230421BWA078-EG-AT-001-R1","2023-07-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H149,1)=\"J\",LEFT(H149,2),LEFT(H149,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H149,1)=\"J\",RIGHT(H149,LEN(H149)-4),RIGHT(H149,LEN(H149)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50000114,"DELIOS","DLX 1000 HV",10,10,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-07-27",null,"2024-09-30",null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","IT23I6Z8 001","2023-03-30","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H150,1)=\"J\",LEFT(H150,2),LEFT(H150,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H150,1)=\"J\",RIGHT(H150,LEN(H150)-4),RIGHT(H150,LEN(H150)-6)),\"\"))","v":"befristet"}]
[50000115,"Delta Energy","H2.5 FLEX"," ",2.5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null," ",null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H151,1)=\"J\",LEFT(H151,2),LEFT(H151,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H151,1)=\"J\",RIGHT(H151,LEN(H151)-4),RIGHT(H151,LEN(H151)-6)),\"\"))","v":""}]
[50000116,"Delta Energy","H3A FLEX ",null,3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H152,1)=\"J\",LEFT(H152,2),LEFT(H152,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H152,1)=\"J\",RIGHT(H152,LEN(H152)-4),RIGHT(H152,LEN(H152)-6)),\"\"))","v":""}]
[50000117,"Delta Energy","H4A FLEX"," ",4,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null," ",null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H153,1)=\"J\",LEFT(H153,2),LEFT(H153,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H153,1)=\"J\",RIGHT(H153,LEN(H153)-4),RIGHT(H153,LEN(H153)-6)),\"\"))","v":""}]
[50000118,"Delta Energy","H5A FLEX"," ",5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null," ",null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H154,1)=\"J\",LEFT(H154,2),LEFT(H154,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H154,1)=\"J\",RIGHT(H154,LEN(H154)-4),RIGHT(H154,LEN(H154)-6)),\"\"))","v":""}]
[50000119,"Delta Energy","RPI M6A ",null,6,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H155,1)=\"J\",LEFT(H155,2),LEFT(H155,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H155,1)=\"J\",RIGHT(H155,LEN(H155)-4),RIGHT(H155,LEN(H155)-6)),\"\"))","v":""}]
[50000120,"Delta Energy","RPI M8A ",null,8,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H156,1)=\"J\",LEFT(H156,2),LEFT(H156,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H156,1)=\"J\",RIGHT(H156,LEN(H156)-4),RIGHT(H156,LEN(H156)-6)),\"\"))","v":""}]
[50000121,"Delta Energy","RPI M10A ",null,10,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H157,1)=\"J\",LEFT(H157,2),LEFT(H157,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H157,1)=\"J\",RIGHT(H157,LEN(H157)-4),RIGHT(H157,LEN(H157)-6)),\"\"))","v":""}]
[50000122,"Delta Energy","M15A FLEX "," ",15,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null," ",null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H158,1)=\"J\",LEFT(H158,2),LEFT(H158,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H158,1)=\"J\",RIGHT(H158,LEN(H158)-4),RIGHT(H158,LEN(H158)-6)),\"\"))","v":""}]
[50000123,"Delta Energy","RPI M15A ",null,15,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H159,1)=\"J\",LEFT(H159,2),LEFT(H159,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H159,1)=\"J\",RIGHT(H159,LEN(H159)-4),RIGHT(H159,LEN(H159)-6)),\"\"))","v":""}]
[50000124,"Delta Energy","M20A FLEX"," ",20,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null," ",null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H160,1)=\"J\",LEFT(H160,2),LEFT(H160,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H160,1)=\"J\",RIGHT(H160,LEN(H160)-4),RIGHT(H160,LEN(H160)-6)),\"\"))","v":""}]
[50000125,"Delta Energy","RPI M20A ",null,20,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H161,1)=\"J\",LEFT(H161,2),LEFT(H161,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H161,1)=\"J\",RIGHT(H161,LEN(H161)-4),RIGHT(H161,LEN(H161)-6)),\"\"))","v":""}]
[50000126,"Delta Energy","M30A FLEX"," ",30,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null," ",null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H162,1)=\"J\",LEFT(H162,2),LEFT(H162,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H162,1)=\"J\",RIGHT(H162,LEN(H162)-4),RIGHT(H162,LEN(H162)-6)),\"\"))","v":""}]
[50000127,"Delta Energy","RPI M30A ",null,30,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H163,1)=\"J\",LEFT(H163,2),LEFT(H163,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H163,1)=\"J\",RIGHT(H163,LEN(H163)-4),RIGHT(H163,LEN(H163)-6)),\"\"))","v":""}]
[50000128,"Delta Energy","M50A FLEX"," ",50,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null," ",null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H164,1)=\"J\",LEFT(H164,2),LEFT(H164,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H164,1)=\"J\",RIGHT(H164,LEN(H164)-4),RIGHT(H164,LEN(H164)-6)),\"\"))","v":""}]
[50000129,"Delta Energy","RPI M50A ",null,50,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H165,1)=\"J\",LEFT(H165,2),LEFT(H165,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H165,1)=\"J\",RIGHT(H165,LEN(H165)-4),RIGHT(H165,LEN(H165)-6)),\"\"))","v":""}]
[50000130,"Delta Energy","M70A FLEX"," ",70,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null," ",null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H166,1)=\"J\",LEFT(H166,2),LEFT(H166,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H166,1)=\"J\",RIGHT(H166,LEN(H166)-4),RIGHT(H166,LEN(H166)-6)),\"\"))","v":""}]
[50000131,"Delta Energy","M88H ",null,73,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H167,1)=\"J\",LEFT(H167,2),LEFT(H167,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H167,1)=\"J\",RIGHT(H167,LEN(H167)-4),RIGHT(H167,LEN(H167)-6)),\"\"))","v":""}]
[50000132,"Deye","SUN300G3-EU-230 mit SUN-MI-RELAY-01",0.3,0.3,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein",null,"Nein","VDE4105",null,"ASUE-ESH-P23080069","2023-08-11","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H168,1)=\"J\",LEFT(H168,2),LEFT(H168,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H168,1)=\"J\",RIGHT(H168,LEN(H168)-4),RIGHT(H168,LEN(H168)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000133,"Deye","SUN500G3-EU-230 mit SUN-MI-RELAY-01",0.5,0.5,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein",null,"Nein","VDE4105",null,"ASUE-ESH-P23080069","2023-08-11","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H169,1)=\"J\",LEFT(H169,2),LEFT(H169,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H169,1)=\"J\",RIGHT(H169,LEN(H169)-4),RIGHT(H169,LEN(H169)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000134,"Deye","SUN600G3-EU-230 mit SUN-MI-RELAY-01",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein",null,"Nein","VDE4105",null,"2306A0879SHA-003","2023-07-27","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H170,1)=\"J\",LEFT(H170,2),LEFT(H170,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H170,1)=\"J\",RIGHT(H170,LEN(H170)-4),RIGHT(H170,LEN(H170)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000135,"Deye","SUN-M60G3-EU-Q0 (mit integrierten NA-Schutz)",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,null,null,null,"VDE4105/4110",null,"CN23TLUP 001","2023-07-28","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H171,1)=\"J\",LEFT(H171,2),LEFT(H171,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H171,1)=\"J\",RIGHT(H171,LEN(H171)-4),RIGHT(H171,LEN(H171)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001962,"Deye","SUN-M60G4-EU-Q0",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-11-05","Martin Bertsch","2023-11-05",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"2309A0184SHA-001","2023-09-19","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H172,1)=\"J\",LEFT(H172,2),LEFT(H172,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H172,1)=\"J\",RIGHT(H172,LEN(H172)-4),RIGHT(H172,LEN(H172)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000136,"Deye","SUN800G3-EU-230 mit SUN-MI-RELAY-01",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein",null,"Nein","VDE4105",null,"2306A0879SHA-003","2023-07-27","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H173,1)=\"J\",LEFT(H173,2),LEFT(H173,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H173,1)=\"J\",RIGHT(H173,LEN(H173)-4),RIGHT(H173,LEN(H173)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000137,"Deye","SUN-M80G3-EU-Q0 (mit integrierten NA-Schutz)",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,null,null,null,"VDE4105/4110",null,"CN23TLUP 001","2023-07-28","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H174,1)=\"J\",LEFT(H174,2),LEFT(H174,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H174,1)=\"J\",RIGHT(H174,LEN(H174)-4),RIGHT(H174,LEN(H174)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001963,"Deye","SUN-M80G4-EU-Q0",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-11-05","Martin Bertsch","2023-11-05",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"2309A0184SHA-001","2023-09-19","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H175,1)=\"J\",LEFT(H175,2),LEFT(H175,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H175,1)=\"J\",RIGHT(H175,LEN(H175)-4),RIGHT(H175,LEN(H175)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001964,"Deye","SUN-M100G4-EU-Q0",1,1,1,"PV-Wechselrichter","Nein","2023-11-05","Martin Bertsch","2023-11-05",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"2309A0184SHA-001","2023-09-19","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H176,1)=\"J\",LEFT(H176,2),LEFT(H176,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H176,1)=\"J\",RIGHT(H176,LEN(H176)-4),RIGHT(H176,LEN(H176)-6)),\"\"))","v":""}]
[50000138,"Deye","SUN1300G3-EU-230-Q1",1.3,1.3,1,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,null,null,null,"Vorhanden",null,"ASUE-ESH-P22110233","2022-12-14",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H177,1)=\"J\",LEFT(H177,2),LEFT(H177,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H177,1)=\"J\",RIGHT(H177,LEN(H177)-4),RIGHT(H177,LEN(H177)-6)),\"\"))","v":""}]
[50000139,"Deye","SUN1600G3-EU-230-Q1",1.6,1.6,1,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,null,null,null,"Vorhanden",null,"ASUE-ESH-P22110233","2022-12-14",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H178,1)=\"J\",LEFT(H178,2),LEFT(H178,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H178,1)=\"J\",RIGHT(H178,LEN(H178)-4),RIGHT(H178,LEN(H178)-6)),\"\"))","v":""}]
[50000140,"Deye","SUN1800G3-EU-230-Q1",1.8,1.8,1,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,null,null,null,"Vorhanden",null,"ASUE-ESH-P22110233","2022-12-14",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H179,1)=\"J\",LEFT(H179,2),LEFT(H179,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H179,1)=\"J\",RIGHT(H179,LEN(H179)-4),RIGHT(H179,LEN(H179)-6)),\"\"))","v":""}]
[50000141,"Deye","SUN2000G3-EU-230-Q1",2,2,1,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,null,null,null,"Vorhanden",null,"ASUE-ESH-P22110233","2022-12-14",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H180,1)=\"J\",LEFT(H180,2),LEFT(H180,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H180,1)=\"J\",RIGHT(H180,LEN(H180)-4),RIGHT(H180,LEN(H180)-6)),\"\"))","v":""}]
[50000142,"Deye","SUN-6K-SG04LP3-EU",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-03-21","Martin Bertsch","2024-03-21","FW Ver 1150. Nach Update Werksreset durchführen und Ländereinstellungen neu setzen.",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","CDAN-ESH-P21110559-R1","2022-07-18","Vorhanden","OK","OK",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H181,1)=\"J\",LEFT(H181,2),LEFT(H181,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H181,1)=\"J\",RIGHT(H181,LEN(H181)-4),RIGHT(H181,LEN(H181)-6)),\"\"))","v":"mit Einschränkung"}]
[50000143,"Deye","SUN-8K-SG04LP3-EU",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-03-21","Martin Bertsch","2024-03-21","FW Ver 1150. Nach Update Werksreset durchführen und Ländereinstellungen neu setzen.",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","CDAN-ESH-P21110559-R1","2022-07-18","Vorhanden","OK","OK",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H182,1)=\"J\",LEFT(H182,2),LEFT(H182,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H182,1)=\"J\",RIGHT(H182,LEN(H182)-4),RIGHT(H182,LEN(H182)-6)),\"\"))","v":"mit Einschränkung"}]
[50000144,"Deye","SUN-10K-SG04LP3-EU",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-03-21","Martin Bertsch","2024-03-21","FW Ver 1150. Nach Update Werksreset durchführen und Ländereinstellungen neu setzen.",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","CDAN-ESH-P21110559-R1","2022-07-18","Vorhanden","OK","OK",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H183,1)=\"J\",LEFT(H183,2),LEFT(H183,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H183,1)=\"J\",RIGHT(H183,LEN(H183)-4),RIGHT(H183,LEN(H183)-6)),\"\"))","v":"mit Einschränkung"}]
[50000145,"Deye","SUN-12K-SG04LP3-EU",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-03-21","Martin Bertsch","2024-03-21","FW Ver 1150. Nach Update Werksreset durchführen und Ländereinstellungen neu setzen.",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","CDAN-ESH-P21110559-R1","2022-07-18","Vorhanden","OK","OK",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H184,1)=\"J\",LEFT(H184,2),LEFT(H184,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H184,1)=\"J\",RIGHT(H184,LEN(H184)-4),RIGHT(H184,LEN(H184)-6)),\"\"))","v":"mit Einschränkung"}]
[50000146,"Deye","SUN-70K-G03",70,77,3,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN227MEP 001","2022-11-17",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H185,1)=\"J\",LEFT(H185,2),LEFT(H185,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H185,1)=\"J\",RIGHT(H185,LEN(H185)-4),RIGHT(H185,LEN(H185)-6)),\"\"))","v":""}]
[50000147,"Deye","SUN-75K-G03",75,82.5,3,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN227MEP 001","2022-11-17",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H186,1)=\"J\",LEFT(H186,2),LEFT(H186,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H186,1)=\"J\",RIGHT(H186,LEN(H186)-4),RIGHT(H186,LEN(H186)-6)),\"\"))","v":""}]
[50000148,"Deye","SUN-80K-G03",80,88,3,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN227MEP 001","2022-11-17",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H187,1)=\"J\",LEFT(H187,2),LEFT(H187,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H187,1)=\"J\",RIGHT(H187,LEN(H187)-4),RIGHT(H187,LEN(H187)-6)),\"\"))","v":""}]
[50000149,"Deye","SUN-90K-G03",90,99,3,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN227MEP 001","2022-11-17",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H188,1)=\"J\",LEFT(H188,2),LEFT(H188,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H188,1)=\"J\",RIGHT(H188,LEN(H188)-4),RIGHT(H188,LEN(H188)-6)),\"\"))","v":""}]
[50000150,"Deye","SUN-100K-G03",100,110,3,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN227MEP 001","2022-11-17",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H189,1)=\"J\",LEFT(H189,2),LEFT(H189,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H189,1)=\"J\",RIGHT(H189,LEN(H189)-4),RIGHT(H189,LEN(H189)-6)),\"\"))","v":""}]
[50000151,"Deye","SUN-110K-G03",110,121,3,"PV-Wechselrichter","Nein","2024-04-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN227MEP 001","2022-11-17",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H190,1)=\"J\",LEFT(H190,2),LEFT(H190,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H190,1)=\"J\",RIGHT(H190,LEN(H190)-4),RIGHT(H190,LEN(H190)-6)),\"\"))","v":""}]
[50000152,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-295"," ",0.29499999999999998,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H191,1)=\"J\",LEFT(H191,2),LEFT(H191,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H191,1)=\"J\",RIGHT(H191,LEN(H191)-4),RIGHT(H191,LEN(H191)-6)),\"\"))","v":""}]
[50000153,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-300"," ",0.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H192,1)=\"J\",LEFT(H192,2),LEFT(H192,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H192,1)=\"J\",RIGHT(H192,LEN(H192)-4),RIGHT(H192,LEN(H192)-6)),\"\"))","v":""}]
[50000154,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-350"," ",0.35,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H193,1)=\"J\",LEFT(H193,2),LEFT(H193,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H193,1)=\"J\",RIGHT(H193,LEN(H193)-4),RIGHT(H193,LEN(H193)-6)),\"\"))","v":""}]
[50000155,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-600 ",null,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-04-19","Martin Bertsch","2023-04-19",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"220907STA099-EG-DE-001","2022-12-29","nicht vorhanden","nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H194,1)=\"J\",LEFT(H194,2),LEFT(H194,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H194,1)=\"J\",RIGHT(H194,LEN(H194)-4),RIGHT(H194,LEN(H194)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000156,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-700"," ",0.7,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-04-19","Martin Bertsch","2023-04-19",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"220907STA099-EG-DE-001","2022-12-29","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H195,1)=\"J\",LEFT(H195,2),LEFT(H195,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H195,1)=\"J\",RIGHT(H195,LEN(H195)-4),RIGHT(H195,LEN(H195)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000157,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-800",null,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-04-19","Martin Bertsch","2023-04-19",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"220907STA099-EG-DE-001","2022-12-29","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H196,1)=\"J\",LEFT(H196,2),LEFT(H196,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H196,1)=\"J\",RIGHT(H196,LEN(H196)-4),RIGHT(H196,LEN(H196)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000158,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-1200"," ",1.2,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H197,1)=\"J\",LEFT(H197,2),LEFT(H197,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H197,1)=\"J\",RIGHT(H197,LEN(H197)-4),RIGHT(H197,LEN(H197)-6)),\"\"))","v":""}]
[50000159,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-1400"," ",1.4,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H198,1)=\"J\",LEFT(H198,2),LEFT(H198,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H198,1)=\"J\",RIGHT(H198,LEN(H198)-4),RIGHT(H198,LEN(H198)-6)),\"\"))","v":""}]
[50000160,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-1600"," ",1.6,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H199,1)=\"J\",LEFT(H199,2),LEFT(H199,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H199,1)=\"J\",RIGHT(H199,LEN(H199)-4),RIGHT(H199,LEN(H199)-6)),\"\"))","v":""}]
[50000161,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-2000"," ",2,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H200,1)=\"J\",LEFT(H200,2),LEFT(H200,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H200,1)=\"J\",RIGHT(H200,LEN(H200)-4),RIGHT(H200,LEN(H200)-6)),\"\"))","v":""}]
[50000162,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-2400"," ",2.4,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H201,1)=\"J\",LEFT(H201,2),LEFT(H201,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H201,1)=\"J\",RIGHT(H201,LEN(H201)-4),RIGHT(H201,LEN(H201)-6)),\"\"))","v":""}]
[50000163,"Dongguan KaiDeng Energy Technology Co., Ltd.","WVC-2800"," ",2.8,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H202,1)=\"J\",LEFT(H202,2),LEFT(H202,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H202,1)=\"J\",RIGHT(H202,LEN(H202)-4),RIGHT(H202,LEN(H202)-6)),\"\"))","v":""}]
[50002111,"Dream Maker","PCS-3-4KW-25A-1",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H203,1)=\"J\",LEFT(H203,2),LEFT(H203,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H203,1)=\"J\",RIGHT(H203,LEN(H203)-4),RIGHT(H203,LEN(H203)-6)),\"\"))","v":"mit Einschränkung"}]
[50002112,"Dream Maker","PCS-3-5KW-25A-1",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H204,1)=\"J\",LEFT(H204,2),LEFT(H204,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H204,1)=\"J\",RIGHT(H204,LEN(H204)-4),RIGHT(H204,LEN(H204)-6)),\"\"))","v":"mit Einschränkung"}]
[50002113,"Dream Maker","PCS-3-6KW-25A-1",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H205,1)=\"J\",LEFT(H205,2),LEFT(H205,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H205,1)=\"J\",RIGHT(H205,LEN(H205)-4),RIGHT(H205,LEN(H205)-6)),\"\"))","v":"mit Einschränkung"}]
[50002114,"Dream Maker","PCS-3-8KW-25A-1",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H206,1)=\"J\",LEFT(H206,2),LEFT(H206,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H206,1)=\"J\",RIGHT(H206,LEN(H206)-4),RIGHT(H206,LEN(H206)-6)),\"\"))","v":"mit Einschränkung"}]
[50002115,"Dream Maker","PCS-3-10KW-25A-1",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H207,1)=\"J\",LEFT(H207,2),LEFT(H207,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H207,1)=\"J\",RIGHT(H207,LEN(H207)-4),RIGHT(H207,LEN(H207)-6)),\"\"))","v":"mit Einschränkung"}]
[50002116,"Dream Maker","PCS-3-10KW-40A-1",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H208,1)=\"J\",LEFT(H208,2),LEFT(H208,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H208,1)=\"J\",RIGHT(H208,LEN(H208)-4),RIGHT(H208,LEN(H208)-6)),\"\"))","v":"mit Einschränkung"}]
[50002117,"Dream Maker","PCS-3-12KW-25A-1",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H209,1)=\"J\",LEFT(H209,2),LEFT(H209,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H209,1)=\"J\",RIGHT(H209,LEN(H209)-4),RIGHT(H209,LEN(H209)-6)),\"\"))","v":"mit Einschränkung"}]
[50002118,"Dream Maker","PCS-3-12KW-40A-1",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H210,1)=\"J\",LEFT(H210,2),LEFT(H210,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H210,1)=\"J\",RIGHT(H210,LEN(H210)-4),RIGHT(H210,LEN(H210)-6)),\"\"))","v":"mit Einschränkung"}]
[50002119,"Dream Maker","PCS-3-15KW-40A-1",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H211,1)=\"J\",LEFT(H211,2),LEFT(H211,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H211,1)=\"J\",RIGHT(H211,LEN(H211)-4),RIGHT(H211,LEN(H211)-6)),\"\"))","v":"mit Einschränkung"}]
[50002120,"Dream Maker","PCS-3-20KW-40A-1",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2024-04-15","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC24031903001-EG-AT-001","2024-04-03","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H212,1)=\"J\",LEFT(H212,2),LEFT(H212,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H212,1)=\"J\",RIGHT(H212,LEN(H212)-4),RIGHT(H212,LEN(H212)-6)),\"\"))","v":"mit Einschränkung"}]
[50002027,"E3/DC","S10 SE",8,8,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-08","Christian Elbs","2024-02-09",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"22TH0431-OVE-directive R25_1","2023-08-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H213,1)=\"J\",LEFT(H213,2),LEFT(H213,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H213,1)=\"J\",RIGHT(H213,LEN(H213)-4),RIGHT(H213,LEN(H213)-6)),\"\"))","v":"befristet"}]
[50000168,"E3/DC","S10 E",12,13.8,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-24",null,null,null,null,"Ja","Nein",null,"OK","Christian Elbs","12KFS081-02_2","2021-10-14","nicht vorhanden","OK",null,"Vorhanden","2021-11-24",null,"Batteriespeicher 3~ - DC gekuppelt KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H214,1)=\"J\",LEFT(H214,2),LEFT(H214,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H214,1)=\"J\",RIGHT(H214,LEN(H214)-4),RIGHT(H214,LEN(H214)-6)),\"\"))","v":""}]
[50000169,"E3/DC","S10 E Compact",12,13.8,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-24",null,null,null,null,"Ja","Nein",null,"OK","Christian Elbs","20PP379-02_1","2021-10-14","nicht vorhanden","OK",null,"Vorhanden","2021-11-24",null,null,null,null,null,null,{"$f":"IF(LEFT(H215,1)=\"J\",LEFT(H215,2),LEFT(H215,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H215,1)=\"J\",RIGHT(H215,LEN(H215)-4),RIGHT(H215,LEN(H215)-6)),\"\"))","v":""}]
[50000171,"E3/DC","S10 E Pro",12,13.8,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-24",null,null,null,null,"Ja","Nein",null,"OK","Christian Elbs","19PP130-02_6","2021-10-14","nicht vorhanden","OK",null,"Vorhanden","2021-11-24",null,"Hybridstromrichter 3~ KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H216,1)=\"J\",LEFT(H216,2),LEFT(H216,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H216,1)=\"J\",RIGHT(H216,LEN(H216)-4),RIGHT(H216,LEN(H216)-6)),\"\"))","v":""}]
[50000172,"E3/DC","S10 X",12,13.8,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-24",null,null,null,null,"Ja","Nein",null,"OK","Christian Elbs","19PP130-02_6","2021-10-14","nicht vorhanden","OK",null,"Vorhanden","2021-11-24",null,"Hybridstromrichter 3~ KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H217,1)=\"J\",LEFT(H217,2),LEFT(H217,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H217,1)=\"J\",RIGHT(H217,LEN(H217)-4),RIGHT(H217,LEN(H217)-6)),\"\"))","v":""}]
[50002025,"E3/DC","S10 X PRO",12,13.8,3,"Hybrid-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Ja","Nein",null,"OK","Christian Elbs","19PP130-02_6","2023-07-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H218,1)=\"J\",LEFT(H218,2),LEFT(H218,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H218,1)=\"J\",RIGHT(H218,LEN(H218)-4),RIGHT(H218,LEN(H218)-6)),\"\"))","v":""}]
[50000174,"E3/DC","SWR12P3",12,13.8,3,"PV-Wechselrichter","Ja",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht OK","Roland Bründlinger","18PP160-09_0","2021-12-10","nicht vorhanden","OK",null,"Vorhanden","2021-11-24",null,null,null,null,null,null,{"$f":"IF(LEFT(H219,1)=\"J\",LEFT(H219,2),LEFT(H219,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H219,1)=\"J\",RIGHT(H219,LEN(H219)-4),RIGHT(H219,LEN(H219)-6)),\"\"))","v":""}]
[50002026,"E3/DC","S20 X PRO",30,33.299999999999997,3,"Hybrid-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"21PP589-05_0","2023-07-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H220,1)=\"J\",LEFT(H220,2),LEFT(H220,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H220,1)=\"J\",RIGHT(H220,LEN(H220)-4),RIGHT(H220,LEN(H220)-6)),\"\"))","v":""}]
[50000175,"EATON","xStorage Compact 20kW",20,20,3,"AC-Batteriewechselrichter","Nein - In Prüfung","2023-07-26","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden","Martin Bertsch (OE)","21TH0210-OVE-directive R25_0","2023-04-17","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H221,1)=\"J\",LEFT(H221,2),LEFT(H221,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H221,1)=\"J\",RIGHT(H221,LEN(H221)-4),RIGHT(H221,LEN(H221)-6)),\"\"))","v":"In Prüfung"}]
[50000176,"EATON","xStorage Compact 30kW",30,30,3,"AC-Batteriewechselrichter","Nein - In Prüfung","2023-07-26","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden","Martin Bertsch (OE)","21TH0210-OVE-directive R25_0","2023-04-17","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H222,1)=\"J\",LEFT(H222,2),LEFT(H222,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H222,1)=\"J\",RIGHT(H222,LEN(H222)-4),RIGHT(H222,LEN(H222)-6)),\"\"))","v":"In Prüfung"}]
[50000177,"EATON","xStorage Compact 40kW",40,40,3,"AC-Batteriewechselrichter","Nein - In Prüfung","2023-07-26","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden","Martin Bertsch (OE)","21TH0210-OVE-directive R25_0","2023-04-17","nicht vorhanden","Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H223,1)=\"J\",LEFT(H223,2),LEFT(H223,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H223,1)=\"J\",RIGHT(H223,LEN(H223)-4),RIGHT(H223,LEN(H223)-6)),\"\"))","v":"In Prüfung"}]
[50000178,"ecocoach AG","ecoBatterySystemT",25,25,3,"AC-Batteriewechselrichter","Ja","2023-10-25","Martin Bertsch","2023-08-29",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","19TH0414-OVE-directive R25_4","2023-10-16",null,"OK",null,null,null,null,"beinhaltet TRUMPF TruConvert AC 3025",null,null,null,null,{"$f":"IF(LEFT(H224,1)=\"J\",LEFT(H224,2),LEFT(H224,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H224,1)=\"J\",RIGHT(H224,LEN(H224)-4),RIGHT(H224,LEN(H224)-6)),\"\"))","v":""}]
[50000179,"ECOFLOW","EFWN511B",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2023-12-05","Martin Bertsch","2023-09-06","FW V1.0.0.155",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","4905636.51","2023-08-30","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H225,1)=\"J\",LEFT(H225,2),LEFT(H225,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H225,1)=\"J\",RIGHT(H225,LEN(H225)-4),RIGHT(H225,LEN(H225)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50000180,"ECOFLOW","EFWN511",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2023-12-05","Martin Bertsch","2023-09-06","FW V1.0.0.155",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","4905636.51","2023-08-30","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H226,1)=\"J\",LEFT(H226,2),LEFT(H226,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H226,1)=\"J\",RIGHT(H226,LEN(H226)-4),RIGHT(H226,LEN(H226)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50001987,"ECOFLOW","EF HD-P3-6K0-S1",6,6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-02","Martin Bertsch","2024-01-02","VW 1.0.0.1",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230299RECO01-E1","2023-08-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H227,1)=\"J\",LEFT(H227,2),LEFT(H227,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H227,1)=\"J\",RIGHT(H227,LEN(H227)-4),RIGHT(H227,LEN(H227)-6)),\"\"))","v":"mit Einschränkung"}]
[50001988,"ECOFLOW","EF HD-P3-8K0-S1",8,8,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-02","Martin Bertsch","2024-01-02","VW 1.0.0.1",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230299RECO01-E1","2023-08-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H228,1)=\"J\",LEFT(H228,2),LEFT(H228,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H228,1)=\"J\",RIGHT(H228,LEN(H228)-4),RIGHT(H228,LEN(H228)-6)),\"\"))","v":"mit Einschränkung"}]
[50001989,"ECOFLOW","EF HD-P3-10K-S1",10,10,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-02","Martin Bertsch","2024-01-02","VW 1.0.0.1",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230299RECO01-E1","2023-08-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H229,1)=\"J\",LEFT(H229,2),LEFT(H229,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H229,1)=\"J\",RIGHT(H229,LEN(H229)-4),RIGHT(H229,LEN(H229)-6)),\"\"))","v":"mit Einschränkung"}]
[50002201,"ECOFLOW","EF HD-P3-12K-S1",12,12,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2024-05-13","VW 1.0.0.1",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230299RECO01-E1-1","2024-03-22","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H230,1)=\"J\",LEFT(H230,2),LEFT(H230,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H230,1)=\"J\",RIGHT(H230,LEN(H230)-4),RIGHT(H230,LEN(H230)-6)),\"\"))","v":"mit Einschränkung"}]
[50000201,"Enphase Energy","IQ7-60-2-INT mit Q-RELAY-1P-INT",0.24,0.25,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-12-19","Martin Bertsch","2023-01-30",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","P2021072021_F","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig",null,null,null,null,{"$f":"IF(LEFT(H231,1)=\"J\",LEFT(H231,2),LEFT(H231,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H231,1)=\"J\",RIGHT(H231,LEN(H231)-4),RIGHT(H231,LEN(H231)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000202,"Enphase Energy","IQ7-60-2-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.24,0.25,3,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-12-19","Martin Bertsch","2023-01-30",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","P2021072021_F","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig; Q-Relay nicht als externer NA-Schutz zulässig",null,null,null,null,{"$f":"IF(LEFT(H232,1)=\"J\",LEFT(H232,2),LEFT(H232,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H232,1)=\"J\",RIGHT(H232,LEN(H232)-4),RIGHT(H232,LEN(H232)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000203,"Enphase Energy","IQ7PLUS-72-2-INT mit Q-RELAY-1P-INT",0.28999999999999998,0.29499999999999998,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-12-19","Martin Bertsch","2023-01-30",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","P2021072021_F","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig",null,null,null,null,{"$f":"IF(LEFT(H233,1)=\"J\",LEFT(H233,2),LEFT(H233,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H233,1)=\"J\",RIGHT(H233,LEN(H233)-4),RIGHT(H233,LEN(H233)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000204,"Enphase Energy","IQ7PLUS-72-2-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.28999999999999998,0.29499999999999998,3,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-12-19","Martin Bertsch","2023-01-30",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","P2021072021_F","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig; Q-Relay nicht als externer NA-Schutz zulässig",null,null,null,null,{"$f":"IF(LEFT(H234,1)=\"J\",LEFT(H234,2),LEFT(H234,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H234,1)=\"J\",RIGHT(H234,LEN(H234)-4),RIGHT(H234,LEN(H234)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000205,"Enphase Energy","IQ7X-96-2-INT mit Q-RELAY-1P-INT",0.315,0.32,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-12-19","Martin Bertsch","2023-01-30",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","P2021072021_F","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig",null,null,null,null,{"$f":"IF(LEFT(H235,1)=\"J\",LEFT(H235,2),LEFT(H235,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H235,1)=\"J\",RIGHT(H235,LEN(H235)-4),RIGHT(H235,LEN(H235)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000206,"Enphase Energy","IQ7X-96-2-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.315,0.32,3,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-12-19","Martin Bertsch","2023-01-30",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","P2021072021_F","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig; Q-Relay nicht als externer NA-Schutz zulässig",null,null,null,null,{"$f":"IF(LEFT(H236,1)=\"J\",LEFT(H236,2),LEFT(H236,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H236,1)=\"J\",RIGHT(H236,LEN(H236)-4),RIGHT(H236,LEN(H236)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001990,"Enphase Energy","IQ8MC-72-M-ACM-INT mit Q-RELAY-1P-INT",0.32500000000000001,0.33,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H237,1)=\"J\",LEFT(H237,2),LEFT(H237,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H237,1)=\"J\",RIGHT(H237,LEN(H237)-4),RIGHT(H237,LEN(H237)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001991,"Enphase Energy","IQ8MC-72-M-ACM-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.32500000000000001,0.33,3,"PV-Wechselrichter","Ja","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H238,1)=\"J\",LEFT(H238,2),LEFT(H238,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H238,1)=\"J\",RIGHT(H238,LEN(H238)-4),RIGHT(H238,LEN(H238)-6)),\"\"))","v":""}]
[50001992,"Enphase Energy","IQ8MC-72-M-ACM-INT-NM mit Q-RELAY-1P-INT",0.32500000000000001,0.33,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H239,1)=\"J\",LEFT(H239,2),LEFT(H239,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H239,1)=\"J\",RIGHT(H239,LEN(H239)-4),RIGHT(H239,LEN(H239)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001993,"Enphase Energy","IQ8MC-72-M-ACM-INT-NM mit Q-RELAY-3P-INT und ENV-S-EM-230",0.32500000000000001,0.33,3,"PV-Wechselrichter","Ja","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H240,1)=\"J\",LEFT(H240,2),LEFT(H240,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H240,1)=\"J\",RIGHT(H240,LEN(H240)-4),RIGHT(H240,LEN(H240)-6)),\"\"))","v":""}]
[50001994,"Enphase Energy","IQ8MC-72-M-ACM-INT-RMA mit Q-RELAY-1P-INT",0.32500000000000001,0.33,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H241,1)=\"J\",LEFT(H241,2),LEFT(H241,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H241,1)=\"J\",RIGHT(H241,LEN(H241)-4),RIGHT(H241,LEN(H241)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001995,"Enphase Energy","IQ8MC-72-M-ACM-INT-RMA mit Q-RELAY-3P-INT und ENV-S-EM-230",0.32500000000000001,0.33,3,"PV-Wechselrichter","Ja","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H242,1)=\"J\",LEFT(H242,2),LEFT(H242,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H242,1)=\"J\",RIGHT(H242,LEN(H242)-4),RIGHT(H242,LEN(H242)-6)),\"\"))","v":""}]
[50000207,"Enphase Energy","IQ8MC-72-M-INT mit Q-RELAY-1P-INT",0.32500000000000001,0.33,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-19","Martin Bertsch","2023-08-10",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H243,1)=\"J\",LEFT(H243,2),LEFT(H243,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H243,1)=\"J\",RIGHT(H243,LEN(H243)-4),RIGHT(H243,LEN(H243)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000208,"Enphase Energy","IQ8MC-72-M-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.32500000000000001,0.33,3,"PV-Wechselrichter","Ja","2024-03-19","Martin Bertsch","2023-08-10",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H244,1)=\"J\",LEFT(H244,2),LEFT(H244,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H244,1)=\"J\",RIGHT(H244,LEN(H244)-4),RIGHT(H244,LEN(H244)-6)),\"\"))","v":""}]
[50000209,"Enphase Energy","IQ7A-72-INT mit Q-RELAY-1P-INT",0.34899999999999998,0.36599999999999999,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-12-19","Martin Bertsch","2023-01-30",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","P2021072021_F","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig",null,null,null,null,{"$f":"IF(LEFT(H245,1)=\"J\",LEFT(H245,2),LEFT(H245,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H245,1)=\"J\",RIGHT(H245,LEN(H245)-4),RIGHT(H245,LEN(H245)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000210,"Enphase Energy","IQ7A-72-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.34899999999999998,0.36599999999999999,3,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-12-19","Martin Bertsch","2023-01-30",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","P2021072021_F","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig; Q-Relay nicht als externer NA-Schutz zulässig",null,null,null,null,{"$f":"IF(LEFT(H246,1)=\"J\",LEFT(H246,2),LEFT(H246,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H246,1)=\"J\",RIGHT(H246,LEN(H246)-4),RIGHT(H246,LEN(H246)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001996,"Enphase Energy","IQ8AC-72-M-ACM-INT mit Q-RELAY-1P-INT",0.36,0.36599999999999999,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H247,1)=\"J\",LEFT(H247,2),LEFT(H247,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H247,1)=\"J\",RIGHT(H247,LEN(H247)-4),RIGHT(H247,LEN(H247)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001997,"Enphase Energy","IQ8AC-72-M-ACM-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.36,0.36599999999999999,3,"PV-Wechselrichter","Ja","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H248,1)=\"J\",LEFT(H248,2),LEFT(H248,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H248,1)=\"J\",RIGHT(H248,LEN(H248)-4),RIGHT(H248,LEN(H248)-6)),\"\"))","v":""}]
[50001998,"Enphase Energy","IQ8AC-72-M-ACM-INT-NM mit Q-RELAY-1P-INT",0.36,0.36599999999999999,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H249,1)=\"J\",LEFT(H249,2),LEFT(H249,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H249,1)=\"J\",RIGHT(H249,LEN(H249)-4),RIGHT(H249,LEN(H249)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001999,"Enphase Energy","IQ8AC-72-M-ACM-INT-NM mit Q-RELAY-3P-INT und ENV-S-EM-230",0.36,0.36599999999999999,3,"PV-Wechselrichter","Ja","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H250,1)=\"J\",LEFT(H250,2),LEFT(H250,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H250,1)=\"J\",RIGHT(H250,LEN(H250)-4),RIGHT(H250,LEN(H250)-6)),\"\"))","v":""}]
[50002000,"Enphase Energy","IQ8AC-72-M-ACM-INT-RMA mit Q-RELAY-1P-INT",0.36,0.36599999999999999,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H251,1)=\"J\",LEFT(H251,2),LEFT(H251,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H251,1)=\"J\",RIGHT(H251,LEN(H251)-4),RIGHT(H251,LEN(H251)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002001,"Enphase Energy","IQ8AC-72-M-ACM-INT-RMA mit Q-RELAY-3P-INT und ENV-S-EM-230",0.36,0.36599999999999999,3,"PV-Wechselrichter","Ja","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H252,1)=\"J\",LEFT(H252,2),LEFT(H252,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H252,1)=\"J\",RIGHT(H252,LEN(H252)-4),RIGHT(H252,LEN(H252)-6)),\"\"))","v":""}]
[50000211,"Enphase Energy","IQ8AC-72-M-INT mit Q-RELAY-1P-INT",0.36,0.36599999999999999,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-19","Martin Bertsch","2023-08-10",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H253,1)=\"J\",LEFT(H253,2),LEFT(H253,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H253,1)=\"J\",RIGHT(H253,LEN(H253)-4),RIGHT(H253,LEN(H253)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000212,"Enphase Energy","IQ8AC-72-M-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.36,0.36599999999999999,3,"PV-Wechselrichter","Ja","2024-03-19","Martin Bertsch","2023-08-10",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H254,1)=\"J\",LEFT(H254,2),LEFT(H254,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H254,1)=\"J\",RIGHT(H254,LEN(H254)-4),RIGHT(H254,LEN(H254)-6)),\"\"))","v":""}]
[50002002,"Enphase Energy","IQ8HC-72-M-ACM-INT mit Q-RELAY-1P-INT",0.38,0.38400000000000001,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H255,1)=\"J\",LEFT(H255,2),LEFT(H255,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H255,1)=\"J\",RIGHT(H255,LEN(H255)-4),RIGHT(H255,LEN(H255)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002003,"Enphase Energy","IQ8HC-72-M-ACM-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.38,0.38400000000000001,3,"PV-Wechselrichter","Ja","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H256,1)=\"J\",LEFT(H256,2),LEFT(H256,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H256,1)=\"J\",RIGHT(H256,LEN(H256)-4),RIGHT(H256,LEN(H256)-6)),\"\"))","v":""}]
[50002004,"Enphase Energy","IQ8HC-72-M-ACM-INT-RMA mit Q-RELAY-1P-INT",0.38,0.38400000000000001,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H257,1)=\"J\",LEFT(H257,2),LEFT(H257,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H257,1)=\"J\",RIGHT(H257,LEN(H257)-4),RIGHT(H257,LEN(H257)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002005,"Enphase Energy","IQ8HC-72-M-ACM-INT-RMA mit Q-RELAY-3P-INT und ENV-S-EM-230",0.38,0.38400000000000001,3,"PV-Wechselrichter","Ja","2024-01-02","Martin Bertsch","2024-01-02",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H258,1)=\"J\",LEFT(H258,2),LEFT(H258,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H258,1)=\"J\",RIGHT(H258,LEN(H258)-4),RIGHT(H258,LEN(H258)-6)),\"\"))","v":""}]
[50000213,"Enphase Energy","IQ8HC-72-M-INT mit Q-RELAY-1P-INT",0.38,0.38400000000000001,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-19","Martin Bertsch","2023-08-10",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H259,1)=\"J\",LEFT(H259,2),LEFT(H259,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H259,1)=\"J\",RIGHT(H259,LEN(H259)-4),RIGHT(H259,LEN(H259)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000214,"Enphase Energy","IQ8HC-72-M-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.38,0.38400000000000001,3,"PV-Wechselrichter","Ja","2024-03-19","Martin Bertsch","2023-08-10",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2022103101_A","2023-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H260,1)=\"J\",LEFT(H260,2),LEFT(H260,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H260,1)=\"J\",RIGHT(H260,LEN(H260)-4),RIGHT(H260,LEN(H260)-6)),\"\"))","v":""}]
[50002093,"Enphase Energy","IQ8X-80-M-INT mit Q-RELAY-1P-INT",0.38,0.38400000000000001,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2024-03-14",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2024020201_A","2024-03-11","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H261,1)=\"J\",LEFT(H261,2),LEFT(H261,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H261,1)=\"J\",RIGHT(H261,LEN(H261)-4),RIGHT(H261,LEN(H261)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002094,"Enphase Energy","IQ8X-80-M-INT mit Q-RELAY-3P-INT und ENV-S-EM-230",0.38,0.38400000000000001,3,"PV-Wechselrichter","Ja","2024-03-14","Martin Bertsch","2024-03-14",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","P2024020201_A","2024-03-11","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H262,1)=\"J\",LEFT(H262,2),LEFT(H262,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H262,1)=\"J\",RIGHT(H262,LEN(H262)-4),RIGHT(H262,LEN(H262)-6)),\"\"))","v":""}]
[50000215,"Enphase Energy","B03-T01-INT00-1-2 mit Q-RELAY-1P-INT",1.28,1.28,1,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-10","Martin Bertsch","2023-01-30",null,null,null,"Prüfbericht ok, warten auf Testgerät",null,null,null,"OK","Roland Bründlinger","P2021062201_G","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig",null,null,null,null,{"$f":"IF(LEFT(H263,1)=\"J\",LEFT(H263,2),LEFT(H263,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H263,1)=\"J\",RIGHT(H263,LEN(H263)-4),RIGHT(H263,LEN(H263)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000216,"Enphase Energy","B03-T01-INT00-1-2 mit Q-RELAY-3P-INT und ENV-S-EM-230",1.28,1.28,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-10","Martin Bertsch","2023-01-30",null,null,null,"Prüfbericht ok, warten auf Testgerät",null,null,null,"OK","Roland Bründlinger","P2021062201_G","2023-01-20","nicht vorhanden","OK",null,null,null,null,"Modul-Wechserichter mit Zentrale und Unsymmetrieüberwachung; unbegrenzt zulässig; Q-Relay nicht als externer NA-Schutz zulässig",null,null,null,null,{"$f":"IF(LEFT(H264,1)=\"J\",LEFT(H264,2),LEFT(H264,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H264,1)=\"J\",RIGHT(H264,LEN(H264)-4),RIGHT(H264,LEN(H264)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000217,"Envertech","EVT 300 ",0.3,0.3,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","Vorhanden","OK",null,null,null,null,"Modul-Wechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H265,1)=\"J\",LEFT(H265,2),LEFT(H265,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H265,1)=\"J\",RIGHT(H265,LEN(H265)-4),RIGHT(H265,LEN(H265)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000218,"Envertech","EVT 360 ",0.36,0.36,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","Vorhanden","OK",null,null,null,null,"Modul-Wechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H266,1)=\"J\",LEFT(H266,2),LEFT(H266,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H266,1)=\"J\",RIGHT(H266,LEN(H266)-4),RIGHT(H266,LEN(H266)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001848,"Envertech","EVT 400",0.4,0.4,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2023-09-25","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger",60436007003,"2023-07-28","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H267,1)=\"J\",LEFT(H267,2),LEFT(H267,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H267,1)=\"J\",RIGHT(H267,LEN(H267)-4),RIGHT(H267,LEN(H267)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000219,"Envertech","EVT 560 ",0.56000000000000005,0.56000000000000005,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","Vorhanden","OK",null,null,null,null,"Modul-Wechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H268,1)=\"J\",LEFT(H268,2),LEFT(H268,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H268,1)=\"J\",RIGHT(H268,LEN(H268)-4),RIGHT(H268,LEN(H268)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000220,"Envertech","EVT 600",0.6,0.6,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","Vorhanden","OK",null,null,null,null,"Modul-Wechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H269,1)=\"J\",LEFT(H269,2),LEFT(H269,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H269,1)=\"J\",RIGHT(H269,LEN(H269)-4),RIGHT(H269,LEN(H269)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000221,"Envertech","EVT 660",0.66,0.66,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","Vorhanden","OK",null,null,null,null,"Modul-Wechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H270,1)=\"J\",LEFT(H270,2),LEFT(H270,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H270,1)=\"J\",RIGHT(H270,LEN(H270)-4),RIGHT(H270,LEN(H270)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000222,"Envertech","EVT 720 ",0.72,0.72,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","Vorhanden","OK",null,null,null,null,"Modul-Wechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H271,1)=\"J\",LEFT(H271,2),LEFT(H271,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H271,1)=\"J\",RIGHT(H271,LEN(H271)-4),RIGHT(H271,LEN(H271)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000223,"Envertech","EVT 800 ",0.8,0.8,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","Vorhanden","OK",null,null,null,null,"Modul-Wechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H272,1)=\"J\",LEFT(H272,2),LEFT(H272,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H272,1)=\"J\",RIGHT(H272,LEN(H272)-4),RIGHT(H272,LEN(H272)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000224,"Envertech","EVT 1200 ",1.2,1.2,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3~ bis Sum. Sn 11,04 kVA - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H273,1)=\"J\",LEFT(H273,2),LEFT(H273,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H273,1)=\"J\",RIGHT(H273,LEN(H273)-4),RIGHT(H273,LEN(H273)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000225,"Envertech","EVT 1400 ",1.4,1.4,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3~ bis Sum. Sn 11,04 kVA - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H274,1)=\"J\",LEFT(H274,2),LEFT(H274,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H274,1)=\"J\",RIGHT(H274,LEN(H274)-4),RIGHT(H274,LEN(H274)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000226,"Envertech","EVT 1500 ",1.5,1.5,1,"PV-Wechselrichter","Nein - Befristung abgelaufen","2024-06-13","Martin Bertsch","2022-10-17","diverse Fehler bei Überprüfung durch AIT festgestellt.","2024-06-30",null,null,"Nein","Nein",null,"OK","Roland Bründlinger","60436007 002","2023-04-12","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3~ bis Sum. Sn 11,04 kVA - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H275,1)=\"J\",LEFT(H275,2),LEFT(H275,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H275,1)=\"J\",RIGHT(H275,LEN(H275)-4),RIGHT(H275,LEN(H275)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001847,"EPOCH","ESI-6KW-H3",6,6.6,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.23.30607.01","2023-04-25",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H276,1)=\"J\",LEFT(H276,2),LEFT(H276,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H276,1)=\"J\",RIGHT(H276,LEN(H276)-4),RIGHT(H276,LEN(H276)-6)),\"\"))","v":"In Prüfung"}]
[50001748,"EPOCH","ESI-8KW-H3",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.23.30607.01","2023-04-25",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H277,1)=\"J\",LEFT(H277,2),LEFT(H277,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H277,1)=\"J\",RIGHT(H277,LEN(H277)-4),RIGHT(H277,LEN(H277)-6)),\"\"))","v":"In Prüfung"}]
[50001751,"EPOCH","ESI-10KW-H3",10,11,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.23.30607.01","2023-04-25",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H278,1)=\"J\",LEFT(H278,2),LEFT(H278,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H278,1)=\"J\",RIGHT(H278,LEN(H278)-4),RIGHT(H278,LEN(H278)-6)),\"\"))","v":"In Prüfung"}]
[50001752,"EPOCH","ESI-12KW-H3",12,13.2,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.23.30607.01","2023-04-25",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H279,1)=\"J\",LEFT(H279,2),LEFT(H279,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H279,1)=\"J\",RIGHT(H279,LEN(H279)-4),RIGHT(H279,LEN(H279)-6)),\"\"))","v":"In Prüfung"}]
[50001753,"EPOCH","ESI-15KW-H3",15,16.5,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.23.30607.01","2023-04-25",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H280,1)=\"J\",LEFT(H280,2),LEFT(H280,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H280,1)=\"J\",RIGHT(H280,LEN(H280)-4),RIGHT(H280,LEN(H280)-6)),\"\"))","v":"In Prüfung"}]
[50000234,"Fenecon","FENECON Home 10 (FHI-10-DAH)",10,11,3,"Hybrid-Wechselrichter","Ja","2023-10-25","Martin Bertsch","2022-10-13","(DSP 9, ARM 23)",null,null,null,"Ja","Nein","Ja","Vorhanden",null,"50314995 006",null,null,"OK",null,null,null,null,"Goodwe Hypridwechselrichter gebrandet",null,null,null,null,{"$f":"IF(LEFT(H281,1)=\"J\",LEFT(H281,2),LEFT(H281,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H281,1)=\"J\",RIGHT(H281,LEN(H281)-4),RIGHT(H281,LEN(H281)-6)),\"\"))","v":""}]
[50000235,"Fenecon","FENECON Home 10 (FHI-10-DAH-16A)",10,11,3,"Hybrid-Wechselrichter","Ja","2023-10-25","Martin Bertsch","2023-03-17","(DSP 9, ARM 23)",null,null,null,"Ja","Nein","Ja","Vorhanden",null,"50314995 006",null,null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H282,1)=\"J\",LEFT(H282,2),LEFT(H282,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H282,1)=\"J\",RIGHT(H282,LEN(H282)-4),RIGHT(H282,LEN(H282)-6)),\"\"))","v":""}]
[50001916,"Fenecon","FENECON Home 20 (FHI-20-DAH)",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-23","Martin Bertsch","2024-01-23","FW: 060608",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN23NT8A 001 ","2023-03-28","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H283,1)=\"J\",LEFT(H283,2),LEFT(H283,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H283,1)=\"J\",RIGHT(H283,LEN(H283)-4),RIGHT(H283,LEN(H283)-6)),\"\"))","v":"mit Einschränkung"}]
[50001920,"Fenecon","FENECON Home 30 (FHI-29,9-DAH)",29.9,29.9,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-23","Martin Bertsch","2024-01-23","FW: 060608",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN23NT8A 001 ","2023-03-28","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H284,1)=\"J\",LEFT(H284,2),LEFT(H284,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H284,1)=\"J\",RIGHT(H284,LEN(H284)-4),RIGHT(H284,LEN(H284)-6)),\"\"))","v":"mit Einschränkung"}]
[50000236,"Fenecon","Commercial 30"," ",30,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2022-06-22",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H285,1)=\"J\",LEFT(H285,2),LEFT(H285,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H285,1)=\"J\",RIGHT(H285,LEN(H285)-4),RIGHT(H285,LEN(H285)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000237,"Fenecon","Commercial 50"," ",50,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2022-06-22",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H286,1)=\"J\",LEFT(H286,2),LEFT(H286,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H286,1)=\"J\",RIGHT(H286,LEN(H286)-4),RIGHT(H286,LEN(H286)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000238,"Fenecon","Industrial 88 ",null,88,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H287,1)=\"J\",LEFT(H287,2),LEFT(H287,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H287,1)=\"J\",RIGHT(H287,LEN(H287)-4),RIGHT(H287,LEN(H287)-6)),\"\"))","v":""}]
[50000239,"Fenecon","Industrial 92"," ",92,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H288,1)=\"J\",LEFT(H288,2),LEFT(H288,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H288,1)=\"J\",RIGHT(H288,LEN(H288)-4),RIGHT(H288,LEN(H288)-6)),\"\"))","v":""}]
[50001919,"FOXESS","AC3-5.0-E",5,5.5,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H289,1)=\"J\",LEFT(H289,2),LEFT(H289,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H289,1)=\"J\",RIGHT(H289,LEN(H289)-4),RIGHT(H289,LEN(H289)-6)),\"\"))","v":"mit Einschränkung"}]
[50000241,"FOXESS","H3-5.0-E",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H290,1)=\"J\",LEFT(H290,2),LEFT(H290,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H290,1)=\"J\",RIGHT(H290,LEN(H290)-4),RIGHT(H290,LEN(H290)-6)),\"\"))","v":"mit Einschränkung"}]
[50000242,"FOXESS","AC3-6.0-E",6,6.6,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H291,1)=\"J\",LEFT(H291,2),LEFT(H291,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H291,1)=\"J\",RIGHT(H291,LEN(H291)-4),RIGHT(H291,LEN(H291)-6)),\"\"))","v":"mit Einschränkung"}]
[50000243,"FOXESS","H3-6.0-E",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H292,1)=\"J\",LEFT(H292,2),LEFT(H292,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H292,1)=\"J\",RIGHT(H292,LEN(H292)-4),RIGHT(H292,LEN(H292)-6)),\"\"))","v":"mit Einschränkung"}]
[50000244,"FOXESS","AC3-8.0-E",8,8.8000000000000007,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H293,1)=\"J\",LEFT(H293,2),LEFT(H293,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H293,1)=\"J\",RIGHT(H293,LEN(H293)-4),RIGHT(H293,LEN(H293)-6)),\"\"))","v":"mit Einschränkung"}]
[50000245,"FOXESS","H3-8.0-E",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H294,1)=\"J\",LEFT(H294,2),LEFT(H294,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H294,1)=\"J\",RIGHT(H294,LEN(H294)-4),RIGHT(H294,LEN(H294)-6)),\"\"))","v":"mit Einschränkung"}]
[50000246,"FOXESS","AC3-10.0-E",10,11,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H295,1)=\"J\",LEFT(H295,2),LEFT(H295,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H295,1)=\"J\",RIGHT(H295,LEN(H295)-4),RIGHT(H295,LEN(H295)-6)),\"\"))","v":"mit Einschränkung"}]
[50002250,"FOXESS","AC3-Pro-10.0",10,11,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H296,1)=\"J\",LEFT(H296,2),LEFT(H296,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H296,1)=\"J\",RIGHT(H296,LEN(H296)-4),RIGHT(H296,LEN(H296)-6)),\"\"))","v":"befristet"}]
[50000247,"FOXESS","H3-10.0-E",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H297,1)=\"J\",LEFT(H297,2),LEFT(H297,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H297,1)=\"J\",RIGHT(H297,LEN(H297)-4),RIGHT(H297,LEN(H297)-6)),\"\"))","v":"mit Einschränkung"}]
[50002241,"FOXESS","H3-Pro-10.0",10,11,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H298,1)=\"J\",LEFT(H298,2),LEFT(H298,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H298,1)=\"J\",RIGHT(H298,LEN(H298)-4),RIGHT(H298,LEN(H298)-6)),\"\"))","v":"befristet"}]
[50000248,"FOXESS","AC3-12.0-E",12,13.2,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H299,1)=\"J\",LEFT(H299,2),LEFT(H299,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H299,1)=\"J\",RIGHT(H299,LEN(H299)-4),RIGHT(H299,LEN(H299)-6)),\"\"))","v":"mit Einschränkung"}]
[50002251,"FOXESS","AC3-Pro-12.0",12,13.2,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H300,1)=\"J\",LEFT(H300,2),LEFT(H300,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H300,1)=\"J\",RIGHT(H300,LEN(H300)-4),RIGHT(H300,LEN(H300)-6)),\"\"))","v":"befristet"}]
[50000249,"FOXESS","H3-12.0-E",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H301,1)=\"J\",LEFT(H301,2),LEFT(H301,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H301,1)=\"J\",RIGHT(H301,LEN(H301)-4),RIGHT(H301,LEN(H301)-6)),\"\"))","v":"mit Einschränkung"}]
[50002242,"FOXESS","H3-Pro-12.0",12,13.2,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H302,1)=\"J\",LEFT(H302,2),LEFT(H302,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H302,1)=\"J\",RIGHT(H302,LEN(H302)-4),RIGHT(H302,LEN(H302)-6)),\"\"))","v":"befristet"}]
[50002252,"FOXESS","AC3-Pro-15.0",15,16.5,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H303,1)=\"J\",LEFT(H303,2),LEFT(H303,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H303,1)=\"J\",RIGHT(H303,LEN(H303)-4),RIGHT(H303,LEN(H303)-6)),\"\"))","v":"befristet"}]
[50002243,"FOXESS","H3-Pro-15.0",15,16.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H304,1)=\"J\",LEFT(H304,2),LEFT(H304,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H304,1)=\"J\",RIGHT(H304,LEN(H304)-4),RIGHT(H304,LEN(H304)-6)),\"\"))","v":"befristet"}]
[50001969,"FOXESS","T15-G3",15,16.5,3,"PV-Wechselrichter","Nein","2023-11-06","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CGDY-ESH-P23071093-1","2023-10-20",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H305,1)=\"J\",LEFT(H305,2),LEFT(H305,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H305,1)=\"J\",RIGHT(H305,LEN(H305)-4),RIGHT(H305,LEN(H305)-6)),\"\"))","v":""}]
[50001968,"FOXESS","T17-G3",17,18.7,3,"PV-Wechselrichter","Nein","2023-11-06","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CGDY-ESH-P23071093-1","2023-10-20",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H306,1)=\"J\",LEFT(H306,2),LEFT(H306,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H306,1)=\"J\",RIGHT(H306,LEN(H306)-4),RIGHT(H306,LEN(H306)-6)),\"\"))","v":""}]
[50002253,"FOXESS","AC3-Pro-20.0",20,22,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H307,1)=\"J\",LEFT(H307,2),LEFT(H307,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H307,1)=\"J\",RIGHT(H307,LEN(H307)-4),RIGHT(H307,LEN(H307)-6)),\"\"))","v":"befristet"}]
[50002244,"FOXESS","H3-Pro-20.0",20,22,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H308,1)=\"J\",LEFT(H308,2),LEFT(H308,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H308,1)=\"J\",RIGHT(H308,LEN(H308)-4),RIGHT(H308,LEN(H308)-6)),\"\"))","v":"befristet"}]
[50001967,"FOXESS","T20-G3",20,22,3,"PV-Wechselrichter","Nein","2023-11-06","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CGDY-ESH-P23071093-1","2023-10-20",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H309,1)=\"J\",LEFT(H309,2),LEFT(H309,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H309,1)=\"J\",RIGHT(H309,LEN(H309)-4),RIGHT(H309,LEN(H309)-6)),\"\"))","v":""}]
[50002254,"FOXESS","AC3-Pro-22.0",22,24.2,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H310,1)=\"J\",LEFT(H310,2),LEFT(H310,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H310,1)=\"J\",RIGHT(H310,LEN(H310)-4),RIGHT(H310,LEN(H310)-6)),\"\"))","v":"befristet"}]
[50002245,"FOXESS","H3-Pro-22.0",22,24.2,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H311,1)=\"J\",LEFT(H311,2),LEFT(H311,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H311,1)=\"J\",RIGHT(H311,LEN(H311)-4),RIGHT(H311,LEN(H311)-6)),\"\"))","v":"befristet"}]
[50002255,"FOXESS","AC3-Pro-24.9",24.9,24.9,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H312,1)=\"J\",LEFT(H312,2),LEFT(H312,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H312,1)=\"J\",RIGHT(H312,LEN(H312)-4),RIGHT(H312,LEN(H312)-6)),\"\"))","v":"befristet"}]
[50002246,"FOXESS","H3-Pro-24.9",24.9,24.9,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H313,1)=\"J\",LEFT(H313,2),LEFT(H313,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H313,1)=\"J\",RIGHT(H313,LEN(H313)-4),RIGHT(H313,LEN(H313)-6)),\"\"))","v":"befristet"}]
[50001966,"FOXESS","T23-G3",23,25.3,3,"PV-Wechselrichter","Nein","2023-11-06","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CGDY-ESH-P23071093-1","2023-10-20",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H314,1)=\"J\",LEFT(H314,2),LEFT(H314,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H314,1)=\"J\",RIGHT(H314,LEN(H314)-4),RIGHT(H314,LEN(H314)-6)),\"\"))","v":""}]
[50002256,"FOXESS","AC3-Pro-25.0",25,27.5,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H315,1)=\"J\",LEFT(H315,2),LEFT(H315,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H315,1)=\"J\",RIGHT(H315,LEN(H315)-4),RIGHT(H315,LEN(H315)-6)),\"\"))","v":"befristet"}]
[50002247,"FOXESS","H3-Pro-25.0",25,27.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H316,1)=\"J\",LEFT(H316,2),LEFT(H316,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H316,1)=\"J\",RIGHT(H316,LEN(H316)-4),RIGHT(H316,LEN(H316)-6)),\"\"))","v":"befristet"}]
[50001965,"FOXESS","T25-G3",25,27.5,3,"PV-Wechselrichter","Nein","2023-11-06","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CGDY-ESH-P23071093-1","2023-10-20",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H317,1)=\"J\",LEFT(H317,2),LEFT(H317,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H317,1)=\"J\",RIGHT(H317,LEN(H317)-4),RIGHT(H317,LEN(H317)-6)),\"\"))","v":""}]
[50002257,"FOXESS","AC3-Pro-29.9",29.9,29.9,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H318,1)=\"J\",LEFT(H318,2),LEFT(H318,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H318,1)=\"J\",RIGHT(H318,LEN(H318)-4),RIGHT(H318,LEN(H318)-6)),\"\"))","v":"befristet"}]
[50002248,"FOXESS","H3-Pro-29.9",29.9,29.9,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H319,1)=\"J\",LEFT(H319,2),LEFT(H319,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H319,1)=\"J\",RIGHT(H319,LEN(H319)-4),RIGHT(H319,LEN(H319)-6)),\"\"))","v":"befristet"}]
[50002258,"FOXESS","AC3-Pro-30.0",30,33,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H320,1)=\"J\",LEFT(H320,2),LEFT(H320,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H320,1)=\"J\",RIGHT(H320,LEN(H320)-4),RIGHT(H320,LEN(H320)-6)),\"\"))","v":"befristet"}]
[50002249,"FOXESS","H3-Pro-30.0",30,33,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-08-31",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24V21V 001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H321,1)=\"J\",LEFT(H321,2),LEFT(H321,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H321,1)=\"J\",RIGHT(H321,LEN(H321)-4),RIGHT(H321,LEN(H321)-6)),\"\"))","v":"befristet"}]
[50000250,"FOXESS","R75",75,82.5,3,"PV-Wechselrichter","Nein","2023-06-04","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23FYQN 001","2023-05-15",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H322,1)=\"J\",LEFT(H322,2),LEFT(H322,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H322,1)=\"J\",RIGHT(H322,LEN(H322)-4),RIGHT(H322,LEN(H322)-6)),\"\"))","v":""}]
[50000251,"FOXESS","R100",100,110,3,"PV-Wechselrichter","Nein","2023-06-04","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23FYQN 001","2023-05-15",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H323,1)=\"J\",LEFT(H323,2),LEFT(H323,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H323,1)=\"J\",RIGHT(H323,LEN(H323)-4),RIGHT(H323,LEN(H323)-6)),\"\"))","v":""}]
[50000252,"FOXESS","R110",110,121,3,"PV-Wechselrichter","Nein","2023-06-04","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23FYQN 001","2023-05-15",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H324,1)=\"J\",LEFT(H324,2),LEFT(H324,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H324,1)=\"J\",RIGHT(H324,LEN(H324)-4),RIGHT(H324,LEN(H324)-6)),\"\"))","v":""}]
[50000253,"Fronius","PRIMO 3.0-1 ",3,3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H325,1)=\"J\",LEFT(H325,2),LEFT(H325,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H325,1)=\"J\",RIGHT(H325,LEN(H325)-4),RIGHT(H325,LEN(H325)-6)),\"\"))","v":""}]
[50000254,"Fronius","PRIMO GEN24 3.0 PLUS",3,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,"Elbs: Noch kein Prüfbericht vorhanden","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~","F","F",null,null,{"$f":"IF(LEFT(H326,1)=\"J\",LEFT(H326,2),LEFT(H326,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H326,1)=\"J\",RIGHT(H326,LEN(H326)-4),RIGHT(H326,LEN(H326)-6)),\"\"))","v":""}]
[50000255,"Fronius","Symo 3.0-3-M ",3,3,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H327,1)=\"J\",LEFT(H327,2),LEFT(H327,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H327,1)=\"J\",RIGHT(H327,LEN(H327)-4),RIGHT(H327,LEN(H327)-6)),\"\"))","v":""}]
[50000256,"Fronius","Symo 3.0-3-S",3,3,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H328,1)=\"J\",LEFT(H328,2),LEFT(H328,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H328,1)=\"J\",RIGHT(H328,LEN(H328)-4),RIGHT(H328,LEN(H328)-6)),\"\"))","v":""}]
[50001841,"Fronius","Symo GEN24 3.0",3,3,3,"Hybrid-Wechselrichter","Ja","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","SGP-17698_01_R1","2020-05-04",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H329,1)=\"J\",LEFT(H329,2),LEFT(H329,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H329,1)=\"J\",RIGHT(H329,LEN(H329)-4),RIGHT(H329,LEN(H329)-6)),\"\"))","v":""}]
[50000257,"Fronius","Symo GEN24 3.0 PLUS",3,3,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","SGP-17698_01_R1","2020-05-04",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H330,1)=\"J\",LEFT(H330,2),LEFT(H330,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H330,1)=\"J\",RIGHT(H330,LEN(H330)-4),RIGHT(H330,LEN(H330)-6)),\"\"))","v":""}]
[50000258,"Fronius","Symo Hybrid 3.0-3-S ",3,3,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0446-OVE-directive R25_2","2021-03-09",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - ggf. NETZUMSCHALTBOX - KONFORM TOR ERZ A + R25","F","F",null,null,{"$f":"IF(LEFT(H331,1)=\"J\",LEFT(H331,2),LEFT(H331,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H331,1)=\"J\",RIGHT(H331,LEN(H331)-4),RIGHT(H331,LEN(H331)-6)),\"\"))","v":""}]
[50000259,"Fronius","PRIMO 3.5-1 ",3.5,3.5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H332,1)=\"J\",LEFT(H332,2),LEFT(H332,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H332,1)=\"J\",RIGHT(H332,LEN(H332)-4),RIGHT(H332,LEN(H332)-6)),\"\"))","v":""}]
[50000260,"Fronius","PRIMO 3.6-1 ",3.68,3.68,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H333,1)=\"J\",LEFT(H333,2),LEFT(H333,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H333,1)=\"J\",RIGHT(H333,LEN(H333)-4),RIGHT(H333,LEN(H333)-6)),\"\"))","v":""}]
[50000261,"Fronius","PRIMO GEN24 3.6 PLUS",3.68,3.68,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,"Elbs: Noch kein Prüfbericht vorhanden","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~","F","F",null,null,{"$f":"IF(LEFT(H334,1)=\"J\",LEFT(H334,2),LEFT(H334,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H334,1)=\"J\",RIGHT(H334,LEN(H334)-4),RIGHT(H334,LEN(H334)-6)),\"\"))","v":""}]
[50000262,"Fronius","Symo 3.7-3-M ",3.7,3.7,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H335,1)=\"J\",LEFT(H335,2),LEFT(H335,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H335,1)=\"J\",RIGHT(H335,LEN(H335)-4),RIGHT(H335,LEN(H335)-6)),\"\"))","v":""}]
[50000263,"Fronius","Symo 3.7-3-S",3.7,3.7,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H336,1)=\"J\",LEFT(H336,2),LEFT(H336,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H336,1)=\"J\",RIGHT(H336,LEN(H336)-4),RIGHT(H336,LEN(H336)-6)),\"\"))","v":""}]
[50000264,"Fronius","PRIMO 4.0-1 ",4,4,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H337,1)=\"J\",LEFT(H337,2),LEFT(H337,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H337,1)=\"J\",RIGHT(H337,LEN(H337)-4),RIGHT(H337,LEN(H337)-6)),\"\"))","v":""}]
[50000265,"Fronius","PRIMO GEN24 4.0 PLUS",4,4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,"Elbs: Noch kein Prüfbericht vorhanden","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~","F","F",null,null,{"$f":"IF(LEFT(H338,1)=\"J\",LEFT(H338,2),LEFT(H338,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H338,1)=\"J\",RIGHT(H338,LEN(H338)-4),RIGHT(H338,LEN(H338)-6)),\"\"))","v":""}]
[50001842,"Fronius","Symo GEN24 4.0",4,4,3,"Hybrid-Wechselrichter","Ja","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","SGP-17698_01_R1","2020-05-04",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H339,1)=\"J\",LEFT(H339,2),LEFT(H339,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H339,1)=\"J\",RIGHT(H339,LEN(H339)-4),RIGHT(H339,LEN(H339)-6)),\"\"))","v":""}]
[50000266,"Fronius","Symo GEN24 4.0 PLUS",4,4,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","SGP-17698_01_R1","2020-05-04",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H340,1)=\"J\",LEFT(H340,2),LEFT(H340,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H340,1)=\"J\",RIGHT(H340,LEN(H340)-4),RIGHT(H340,LEN(H340)-6)),\"\"))","v":""}]
[50000267,"Fronius","Symo Hybrid 4.0-3-S ",4,4,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0446-OVE-directive R25_2","2021-03-09",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - ggf. NETZUMSCHALTBOX - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H341,1)=\"J\",LEFT(H341,2),LEFT(H341,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H341,1)=\"J\",RIGHT(H341,LEN(H341)-4),RIGHT(H341,LEN(H341)-6)),\"\"))","v":""}]
[50000268,"Fronius","Symo 4.5-3-M ",4.5,4.5,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H342,1)=\"J\",LEFT(H342,2),LEFT(H342,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H342,1)=\"J\",RIGHT(H342,LEN(H342)-4),RIGHT(H342,LEN(H342)-6)),\"\"))","v":""}]
[50000269,"Fronius","Symo 4.5-3-S ",4.5,4.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H343,1)=\"J\",LEFT(H343,2),LEFT(H343,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H343,1)=\"J\",RIGHT(H343,LEN(H343)-4),RIGHT(H343,LEN(H343)-6)),\"\"))","v":""}]
[50000270,"Fronius","PRIMO 4.6-1 ",4.5999999999999996,4.5999999999999996,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H344,1)=\"J\",LEFT(H344,2),LEFT(H344,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H344,1)=\"J\",RIGHT(H344,LEN(H344)-4),RIGHT(H344,LEN(H344)-6)),\"\"))","v":""}]
[50000271,"Fronius","PRIMO 5.0-1 AUS",4.5999999999999996,4.5999999999999996,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H345,1)=\"J\",LEFT(H345,2),LEFT(H345,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H345,1)=\"J\",RIGHT(H345,LEN(H345)-4),RIGHT(H345,LEN(H345)-6)),\"\"))","v":""}]
[50000272,"Fronius","PRIMO GEN24 4.6 PLUS",4.5999999999999996,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H346,1)=\"J\",LEFT(H346,2),LEFT(H346,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H346,1)=\"J\",RIGHT(H346,LEN(H346)-4),RIGHT(H346,LEN(H346)-6)),\"\"))","v":""}]
[50000273,"Fronius","PRIMO 5.0-1 ",5,5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H347,1)=\"J\",LEFT(H347,2),LEFT(H347,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H347,1)=\"J\",RIGHT(H347,LEN(H347)-4),RIGHT(H347,LEN(H347)-6)),\"\"))","v":""}]
[50000274,"Fronius","PRIMO GEN24 5.0 PLUS",5,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H348,1)=\"J\",LEFT(H348,2),LEFT(H348,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H348,1)=\"J\",RIGHT(H348,LEN(H348)-4),RIGHT(H348,LEN(H348)-6)),\"\"))","v":""}]
[50000275,"Fronius","Symo 5.0-3-M ",5,5,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H349,1)=\"J\",LEFT(H349,2),LEFT(H349,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H349,1)=\"J\",RIGHT(H349,LEN(H349)-4),RIGHT(H349,LEN(H349)-6)),\"\"))","v":""}]
[50001843,"Fronius","Symo GEN24 5.0",5,5,3,"Hybrid-Wechselrichter","Ja","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","SGP-17698_01_R1","2020-05-04",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H350,1)=\"J\",LEFT(H350,2),LEFT(H350,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H350,1)=\"J\",RIGHT(H350,LEN(H350)-4),RIGHT(H350,LEN(H350)-6)),\"\"))","v":""}]
[50000276,"Fronius","Symo GEN24 5.0 PLUS",5,5,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","SGP-17698_01_R1","2020-05-04",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H351,1)=\"J\",LEFT(H351,2),LEFT(H351,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H351,1)=\"J\",RIGHT(H351,LEN(H351)-4),RIGHT(H351,LEN(H351)-6)),\"\"))","v":""}]
[50000277,"Fronius","Symo Hybrid 5.0-3-S ",5,5,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0446-OVE-directive R25_2","2021-03-09",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - ggf. NETZUMSCHALTBOX - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H352,1)=\"J\",LEFT(H352,2),LEFT(H352,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H352,1)=\"J\",RIGHT(H352,LEN(H352)-4),RIGHT(H352,LEN(H352)-6)),\"\"))","v":""}]
[50000278,"Fronius","Symo 5.5-3-M ",5.5,5.5,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H353,1)=\"J\",LEFT(H353,2),LEFT(H353,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H353,1)=\"J\",RIGHT(H353,LEN(H353)-4),RIGHT(H353,LEN(H353)-6)),\"\"))","v":""}]
[50000279,"Fronius","PRIMO 6.0-1 ",6,6,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H354,1)=\"J\",LEFT(H354,2),LEFT(H354,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H354,1)=\"J\",RIGHT(H354,LEN(H354)-4),RIGHT(H354,LEN(H354)-6)),\"\"))","v":""}]
[50000280,"Fronius","PRIMO GEN24 6.0 PLUS",6,6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H355,1)=\"J\",LEFT(H355,2),LEFT(H355,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H355,1)=\"J\",RIGHT(H355,LEN(H355)-4),RIGHT(H355,LEN(H355)-6)),\"\"))","v":""}]
[50000281,"Fronius","Symo 6.0-3-M ",6,6,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H356,1)=\"J\",LEFT(H356,2),LEFT(H356,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H356,1)=\"J\",RIGHT(H356,LEN(H356)-4),RIGHT(H356,LEN(H356)-6)),\"\"))","v":""}]
[50001836,"Fronius","Symo GEN24 6.0",6,6,3,"Hybrid-Wechselrichter","Ja","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H357,1)=\"J\",LEFT(H357,2),LEFT(H357,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H357,1)=\"J\",RIGHT(H357,LEN(H357)-4),RIGHT(H357,LEN(H357)-6)),\"\"))","v":""}]
[50000282,"Fronius","Symo GEN24 6.0 PLUS",6,6,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H358,1)=\"J\",LEFT(H358,2),LEFT(H358,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H358,1)=\"J\",RIGHT(H358,LEN(H358)-4),RIGHT(H358,LEN(H358)-6)),\"\"))","v":""}]
[50000283,"Fronius","Symo GEN24 6.0 Plus SC",6,6,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H359,1)=\"J\",LEFT(H359,2),LEFT(H359,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H359,1)=\"J\",RIGHT(H359,LEN(H359)-4),RIGHT(H359,LEN(H359)-6)),\"\"))","v":""}]
[50000284,"Fronius","Symo GEN24 6.0 SC",6,6,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H360,1)=\"J\",LEFT(H360,2),LEFT(H360,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H360,1)=\"J\",RIGHT(H360,LEN(H360)-4),RIGHT(H360,LEN(H360)-6)),\"\"))","v":""}]
[50000285,"Fronius","Symo 6.7-3-M ",6.7,6.7,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H361,1)=\"J\",LEFT(H361,2),LEFT(H361,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H361,1)=\"J\",RIGHT(H361,LEN(H361)-4),RIGHT(H361,LEN(H361)-6)),\"\"))","v":""}]
[50000286,"Fronius","Symo 7.0-3-M ",7,7,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H362,1)=\"J\",LEFT(H362,2),LEFT(H362,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H362,1)=\"J\",RIGHT(H362,LEN(H362)-4),RIGHT(H362,LEN(H362)-6)),\"\"))","v":""}]
[50001837,"Fronius","Symo GEN24 7.0",7,7,3,"Hybrid-Wechselrichter","Ja","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H363,1)=\"J\",LEFT(H363,2),LEFT(H363,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H363,1)=\"J\",RIGHT(H363,LEN(H363)-4),RIGHT(H363,LEN(H363)-6)),\"\"))","v":""}]
[50000287,"Fronius","Symo GEN24 7.0 PLUS",7,7,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H364,1)=\"J\",LEFT(H364,2),LEFT(H364,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H364,1)=\"J\",RIGHT(H364,LEN(H364)-4),RIGHT(H364,LEN(H364)-6)),\"\"))","v":""}]
[50000288,"Fronius","Symo GEN24 7.0 Plus SC",7,7,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H365,1)=\"J\",LEFT(H365,2),LEFT(H365,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H365,1)=\"J\",RIGHT(H365,LEN(H365)-4),RIGHT(H365,LEN(H365)-6)),\"\"))","v":""}]
[50000289,"Fronius","Symo GEN24 7.0 SC",7,7,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H366,1)=\"J\",LEFT(H366,2),LEFT(H366,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H366,1)=\"J\",RIGHT(H366,LEN(H366)-4),RIGHT(H366,LEN(H366)-6)),\"\"))","v":""}]
[50000290,"Fronius","Symo 8.0-3-M ",8,8,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H367,1)=\"J\",LEFT(H367,2),LEFT(H367,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H367,1)=\"J\",RIGHT(H367,LEN(H367)-4),RIGHT(H367,LEN(H367)-6)),\"\"))","v":""}]
[50001838,"Fronius","Symo GEN24 8.0",8,8,3,"Hybrid-Wechselrichter","Ja","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H368,1)=\"J\",LEFT(H368,2),LEFT(H368,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H368,1)=\"J\",RIGHT(H368,LEN(H368)-4),RIGHT(H368,LEN(H368)-6)),\"\"))","v":""}]
[50000291,"Fronius","Symo GEN24 8.0 PLUS",8,8,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H369,1)=\"J\",LEFT(H369,2),LEFT(H369,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H369,1)=\"J\",RIGHT(H369,LEN(H369)-4),RIGHT(H369,LEN(H369)-6)),\"\"))","v":""}]
[50000292,"Fronius","Symo GEN24 8.0 Plus SC",8,8,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H370,1)=\"J\",LEFT(H370,2),LEFT(H370,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H370,1)=\"J\",RIGHT(H370,LEN(H370)-4),RIGHT(H370,LEN(H370)-6)),\"\"))","v":""}]
[50000293,"Fronius","Symo GEN24 8.0 SC",8,8,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H371,1)=\"J\",LEFT(H371,2),LEFT(H371,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H371,1)=\"J\",RIGHT(H371,LEN(H371)-4),RIGHT(H371,LEN(H371)-6)),\"\"))","v":""}]
[50000294,"Fronius","PRIMO 8.2-1 ",8.1999999999999993,8.1999999999999993,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H372,1)=\"J\",LEFT(H372,2),LEFT(H372,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H372,1)=\"J\",RIGHT(H372,LEN(H372)-4),RIGHT(H372,LEN(H372)-6)),\"\"))","v":""}]
[50000295,"Fronius","Symo 8.2-3-M ",8.1999999999999993,8.1999999999999993,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0406-OVE-directive R25_2","2021-06-16","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H373,1)=\"J\",LEFT(H373,2),LEFT(H373,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H373,1)=\"J\",RIGHT(H373,LEN(H373)-4),RIGHT(H373,LEN(H373)-6)),\"\"))","v":""}]
[50001839,"Fronius","Symo GEN24 9.0",9,9,3,"Hybrid-Wechselrichter","Ja","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H374,1)=\"J\",LEFT(H374,2),LEFT(H374,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H374,1)=\"J\",RIGHT(H374,LEN(H374)-4),RIGHT(H374,LEN(H374)-6)),\"\"))","v":""}]
[50000296,"Fronius","Symo GEN24 9.0 PLUS",9,9,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H375,1)=\"J\",LEFT(H375,2),LEFT(H375,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H375,1)=\"J\",RIGHT(H375,LEN(H375)-4),RIGHT(H375,LEN(H375)-6)),\"\"))","v":""}]
[50000297,"Fronius","Symo GEN24 9.0 Plus SC",9,9,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H376,1)=\"J\",LEFT(H376,2),LEFT(H376,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H376,1)=\"J\",RIGHT(H376,LEN(H376)-4),RIGHT(H376,LEN(H376)-6)),\"\"))","v":""}]
[50000298,"Fronius","Symo GEN24 9.0 SC",9,9,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H377,1)=\"J\",LEFT(H377,2),LEFT(H377,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H377,1)=\"J\",RIGHT(H377,LEN(H377)-4),RIGHT(H377,LEN(H377)-6)),\"\"))","v":""}]
[50000299,"Fronius","Fronius Symo Advanced 10.0-3-M",10,10,3,"PV-Wechselrichter","Ja","2023-05-15","Martin Bertsch","2023-04-19",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","21TH0549-OVE-directive R25_1","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H378,1)=\"J\",LEFT(H378,2),LEFT(H378,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H378,1)=\"J\",RIGHT(H378,LEN(H378)-4),RIGHT(H378,LEN(H378)-6)),\"\"))","v":""}]
[50000300,"Fronius","Symo 10.0-3-M ",10,10,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0407-OVE-directive R25_2","2021-06-16","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H379,1)=\"J\",LEFT(H379,2),LEFT(H379,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H379,1)=\"J\",RIGHT(H379,LEN(H379)-4),RIGHT(H379,LEN(H379)-6)),\"\"))","v":""}]
[50000301,"Fronius","Symo 10.0-3-M Light",10,10,3,"PV-Wechselrichter","Ja","2022-07-18",null,"2022-07-18",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0407-OVE-directive R25_2","2021-06-16",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H380,1)=\"J\",LEFT(H380,2),LEFT(H380,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H380,1)=\"J\",RIGHT(H380,LEN(H380)-4),RIGHT(H380,LEN(H380)-6)),\"\"))","v":""}]
[50001840,"Fronius","Symo GEN24 10.0",10,10,3,"Hybrid-Wechselrichter","Ja","2023-09-25","Martin Bertsch","2023-09-25",null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H381,1)=\"J\",LEFT(H381,2),LEFT(H381,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H381,1)=\"J\",RIGHT(H381,LEN(H381)-4),RIGHT(H381,LEN(H381)-6)),\"\"))","v":""}]
[50000302,"Fronius","Symo GEN24 10.0 PLUS",10,10,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","19TH0445-OVE-directive R25_1","2020-05-13",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H382,1)=\"J\",LEFT(H382,2),LEFT(H382,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H382,1)=\"J\",RIGHT(H382,LEN(H382)-4),RIGHT(H382,LEN(H382)-6)),\"\"))","v":""}]
[50001835,"Fronius","Symo GEN24 10.0 Plus SC",10,10,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H383,1)=\"J\",LEFT(H383,2),LEFT(H383,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H383,1)=\"J\",RIGHT(H383,LEN(H383)-4),RIGHT(H383,LEN(H383)-6)),\"\"))","v":""}]
[50000304,"Fronius","Symo GEN24 10.0 SC",10,10,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H384,1)=\"J\",LEFT(H384,2),LEFT(H384,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H384,1)=\"J\",RIGHT(H384,LEN(H384)-4),RIGHT(H384,LEN(H384)-6)),\"\"))","v":""}]
[50000305,"Fronius","Symo GEN24 11.0 Plus SC",11,11,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H385,1)=\"J\",LEFT(H385,2),LEFT(H385,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H385,1)=\"J\",RIGHT(H385,LEN(H385)-4),RIGHT(H385,LEN(H385)-6)),\"\"))","v":""}]
[50000306,"Fronius","Symo GEN24 11.0 SC",11,11,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H386,1)=\"J\",LEFT(H386,2),LEFT(H386,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H386,1)=\"J\",RIGHT(H386,LEN(H386)-4),RIGHT(H386,LEN(H386)-6)),\"\"))","v":""}]
[50000307,"Fronius","Symo GEN24 12.0 Plus SC",12,12,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H387,1)=\"J\",LEFT(H387,2),LEFT(H387,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H387,1)=\"J\",RIGHT(H387,LEN(H387)-4),RIGHT(H387,LEN(H387)-6)),\"\"))","v":""}]
[50000308,"Fronius","Symo GEN24 12.0 SC",12,12,3,"Hybrid-Wechselrichter","Ja","2023-08-17","Martin Bertsch","2023-08-17",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","SGP-23837_01_R1","2023-06-02","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H388,1)=\"J\",LEFT(H388,2),LEFT(H388,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H388,1)=\"J\",RIGHT(H388,LEN(H388)-4),RIGHT(H388,LEN(H388)-6)),\"\"))","v":""}]
[50000309,"Fronius","Fronius Symo Advanced 12.5-3-M",12.5,12.5,3,"PV-Wechselrichter","Ja","2023-05-15","Martin Bertsch","2023-04-19",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","21TH0549-OVE-directive R25_1","2023-05-12","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H389,1)=\"J\",LEFT(H389,2),LEFT(H389,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H389,1)=\"J\",RIGHT(H389,LEN(H389)-4),RIGHT(H389,LEN(H389)-6)),\"\"))","v":""}]
[50000310,"Fronius","Symo 12.5-3-M ",12.5,12.5,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0407-OVE-directive R25_2","2021-06-16","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H390,1)=\"J\",LEFT(H390,2),LEFT(H390,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H390,1)=\"J\",RIGHT(H390,LEN(H390)-4),RIGHT(H390,LEN(H390)-6)),\"\"))","v":""}]
[50000311,"Fronius","Fronius Symo Advanced 15.0-3-M",15,15,3,"PV-Wechselrichter","Ja","2023-05-15","Martin Bertsch","2023-04-19",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","21TH0549-OVE-directive R25_1","2023-05-12","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H391,1)=\"J\",LEFT(H391,2),LEFT(H391,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H391,1)=\"J\",RIGHT(H391,LEN(H391)-4),RIGHT(H391,LEN(H391)-6)),\"\"))","v":""}]
[50000312,"Fronius","Symo 15.0-3-M ",15,15,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0407-OVE-directive R25_2","2021-06-16","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H392,1)=\"J\",LEFT(H392,2),LEFT(H392,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H392,1)=\"J\",RIGHT(H392,LEN(H392)-4),RIGHT(H392,LEN(H392)-6)),\"\"))","v":""}]
[50000313,"Fronius","Fronius Symo Advanced 17.5-3-M",17.5,17.5,3,"PV-Wechselrichter","Ja","2023-05-15","Martin Bertsch","2023-04-19",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","21TH0549-OVE-directive R25_1","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H393,1)=\"J\",LEFT(H393,2),LEFT(H393,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H393,1)=\"J\",RIGHT(H393,LEN(H393)-4),RIGHT(H393,LEN(H393)-6)),\"\"))","v":""}]
[50000314,"Fronius","Symo 17.5-3-M ",17.5,17.5,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0407-OVE-directive R25_2","2021-06-16","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H394,1)=\"J\",LEFT(H394,2),LEFT(H394,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H394,1)=\"J\",RIGHT(H394,LEN(H394)-4),RIGHT(H394,LEN(H394)-6)),\"\"))","v":""}]
[50000315,"Fronius","Fronius Symo Advanced 20.0-3-M",20,20,3,"PV-Wechselrichter","Ja","2023-05-15","Martin Bertsch","2023-04-19",null,null,null,null,"Nein",null,"Nein","OK","Roland Bründlinger","21TH0549-OVE-directive R25_1","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H395,1)=\"J\",LEFT(H395,2),LEFT(H395,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H395,1)=\"J\",RIGHT(H395,LEN(H395)-4),RIGHT(H395,LEN(H395)-6)),\"\"))","v":""}]
[50000316,"Fronius","Symo 20.0-3-M ",20,20,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","19TH0407-OVE-directive R25_2","2021-06-16","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H396,1)=\"J\",LEFT(H396,2),LEFT(H396,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H396,1)=\"J\",RIGHT(H396,LEN(H396)-4),RIGHT(H396,LEN(H396)-6)),\"\"))","v":""}]
[50000317,"Fronius","Eco 25.0-3-S ",25,25,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","15TH0304-OVE-directive R25_1","2021-02-22","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H397,1)=\"J\",LEFT(H397,2),LEFT(H397,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H397,1)=\"J\",RIGHT(H397,LEN(H397)-4),RIGHT(H397,LEN(H397)-6)),\"\"))","v":""}]
[50002080,"Fronius","Verto 25.0",25,25,3,"PV-Wechselrichter","Ja","2024-02-01","Martin Bertsch","2024-02-01",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"SGP-23792_02_R2","2023-11-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H398,1)=\"J\",LEFT(H398,2),LEFT(H398,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H398,1)=\"J\",RIGHT(H398,LEN(H398)-4),RIGHT(H398,LEN(H398)-6)),\"\"))","v":""}]
[50000318,"Fronius","Eco 27.0-3-S ",27,27,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","15TH0304-OVE-directive R25_1","2021-02-22","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H399,1)=\"J\",LEFT(H399,2),LEFT(H399,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H399,1)=\"J\",RIGHT(H399,LEN(H399)-4),RIGHT(H399,LEN(H399)-6)),\"\"))","v":""}]
[50002081,"Fronius","Verto 27.0",27,27,3,"PV-Wechselrichter","Ja","2024-02-01","Martin Bertsch","2024-02-01",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"SGP-23792_02_R2","2023-11-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H400,1)=\"J\",LEFT(H400,2),LEFT(H400,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H400,1)=\"J\",RIGHT(H400,LEN(H400)-4),RIGHT(H400,LEN(H400)-6)),\"\"))","v":""}]
[50002082,"Fronius","Verto 30.0",30,30,3,"PV-Wechselrichter","Ja","2024-02-01","Martin Bertsch","2024-02-01",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"SGP-23792_02_R2","2023-11-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H401,1)=\"J\",LEFT(H401,2),LEFT(H401,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H401,1)=\"J\",RIGHT(H401,LEN(H401)-4),RIGHT(H401,LEN(H401)-6)),\"\"))","v":""}]
[50002083,"Fronius","Verto 33.3",33.299999999999997,33.299999999999997,3,"PV-Wechselrichter","Ja","2024-02-01","Martin Bertsch","2024-02-01",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"SGP-23792_02_R2","2023-11-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H402,1)=\"J\",LEFT(H402,2),LEFT(H402,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H402,1)=\"J\",RIGHT(H402,LEN(H402)-4),RIGHT(H402,LEN(H402)-6)),\"\"))","v":""}]
[50000319,"Fronius","TAURO 50-3 ",50,50,3,"PV-Wechselrichter","Ja",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"SGP-18697_02_R1 ","2021-01-11",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H403,1)=\"J\",LEFT(H403,2),LEFT(H403,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H403,1)=\"J\",RIGHT(H403,LEN(H403)-4),RIGHT(H403,LEN(H403)-6)),\"\"))","v":""}]
[50000320,"Fronius","TAURO ECO 50-3",50,50,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"SGP-18697_02_R1","2021-01-11",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H404,1)=\"J\",LEFT(H404,2),LEFT(H404,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H404,1)=\"J\",RIGHT(H404,LEN(H404)-4),RIGHT(H404,LEN(H404)-6)),\"\"))","v":""}]
[50000321,"Fronius","TAURO ECO 99-3 ",null,99.9,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"SGP-18697_01_R1","2021-01-11",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H405,1)=\"J\",LEFT(H405,2),LEFT(H405,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H405,1)=\"J\",RIGHT(H405,LEN(H405)-4),RIGHT(H405,LEN(H405)-6)),\"\"))","v":""}]
[50000322,"Fronius","TAURO ECO 100-3",100,100,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"SGP-18697_01_R1","2021-01-11",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H406,1)=\"J\",LEFT(H406,2),LEFT(H406,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H406,1)=\"J\",RIGHT(H406,LEN(H406)-4),RIGHT(H406,LEN(H406)-6)),\"\"))","v":""}]
[50000325,"FSP Solar Power","FSP Power manager 10kW ",null,10,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-12-05","Martin Bertsch","2021-05-06",null,null,"2023-12-05",null,"Ja","Ja","Nein","OK","Martin Bertsch (OE)","PVAT2101WDG0266-R2","2023-05-10","nicht vorhanden","OK",null,null,null,null,"Hybridstromrichter 3~ - ggf. NETZUMSCHALTBOX - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H407,1)=\"J\",LEFT(H407,2),LEFT(H407,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H407,1)=\"J\",RIGHT(H407,LEN(H407)-4),RIGHT(H407,LEN(H407)-6)),\"\"))","v":"In Prüfung"}]
[50000326,"FSP Solar Power","FSP103PV-230TH-48 ",null,10,3,"Hybrid-Wechselrichter","Nein","2022-11-16","Martin Bertsch","2021-05-06",null,null,"2022-10-21",null,"Ja","Ja","Nein","nicht OK","Martin Bertsch (OE)","PVAT2101WDG0266-R1","2021-02-20",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - ggf. NETZUMSCHALTBOX - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H408,1)=\"J\",LEFT(H408,2),LEFT(H408,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H408,1)=\"J\",RIGHT(H408,LEN(H408)-4),RIGHT(H408,LEN(H408)-6)),\"\"))","v":""}]
[50000327,"FSP Solar Power","FSP PowerManager-Hybrid 15kW"," ",15,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-12-05","Martin Bertsch","2022-10-24",null,null,"2023-12-05","Prüfbericht Fehlerhaft","ja","ja",null,"nicht OK","Dominik Schuller/RB","210500330TPE-001","2021-08-31",null,null,null,null,null,null,"Hybridstromrichter 3~ - ggf. NETZUMSCHALTBOX - KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H409,1)=\"J\",LEFT(H409,2),LEFT(H409,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H409,1)=\"J\",RIGHT(H409,LEN(H409)-4),RIGHT(H409,LEN(H409)-6)),\"\"))","v":"In Prüfung"}]
[50002239,"Ginlong Technologies","S6-GR1P0.6K-UM",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-20","Martin Bertsch","2024-05-20",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"CN24U7UT 001","2024-01-19","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H410,1)=\"J\",LEFT(H410,2),LEFT(H410,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H410,1)=\"J\",RIGHT(H410,LEN(H410)-4),RIGHT(H410,LEN(H410)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000328,"Ginlong Technologies","S6-GR1P0.7K-M",0.7,0.77,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H411,1)=\"J\",LEFT(H411,2),LEFT(H411,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H411,1)=\"J\",RIGHT(H411,LEN(H411)-4),RIGHT(H411,LEN(H411)-6)),\"\"))","v":""}]
[50002240,"Ginlong Technologies","S6-GR1P0.8K-UM",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-20","Martin Bertsch","2024-05-20",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"CN24U7UT 001","2024-01-19","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H412,1)=\"J\",LEFT(H412,2),LEFT(H412,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H412,1)=\"J\",RIGHT(H412,LEN(H412)-4),RIGHT(H412,LEN(H412)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000329,"Ginlong Technologies","S6-GR1P1K-M",1,1.1000000000000001,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H413,1)=\"J\",LEFT(H413,2),LEFT(H413,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H413,1)=\"J\",RIGHT(H413,LEN(H413)-4),RIGHT(H413,LEN(H413)-6)),\"\"))","v":""}]
[50000330,"Ginlong Technologies","S6-GR1P1.5K-M",1.5,1.65,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,"gem. Diskussion am 16062021 mit VDE und Parametrieranleitung (TOR-Setting) zugelassen",null,{"$f":"IF(LEFT(H414,1)=\"J\",LEFT(H414,2),LEFT(H414,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H414,1)=\"J\",RIGHT(H414,LEN(H414)-4),RIGHT(H414,LEN(H414)-6)),\"\"))","v":""}]
[50000331,"Ginlong Technologies","S6-GR1P2K-M",2,2.2000000000000002,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H415,1)=\"J\",LEFT(H415,2),LEFT(H415,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H415,1)=\"J\",RIGHT(H415,LEN(H415)-4),RIGHT(H415,LEN(H415)-6)),\"\"))","v":""}]
[50000332,"Ginlong Technologies","S6-GR1P2.5K-M",2.5,2.75,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H416,1)=\"J\",LEFT(H416,2),LEFT(H416,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H416,1)=\"J\",RIGHT(H416,LEN(H416)-4),RIGHT(H416,LEN(H416)-6)),\"\"))","v":""}]
[50000333,"Ginlong Technologies","S6-GR1P2.5K",2.5,2.8,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H417,1)=\"J\",LEFT(H417,2),LEFT(H417,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H417,1)=\"J\",RIGHT(H417,LEN(H417)-4),RIGHT(H417,LEN(H417)-6)),\"\"))","v":""}]
[50000334,"Ginlong Technologies","RAI-3K-48ES-5G",3,3.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H418,1)=\"J\",LEFT(H418,2),LEFT(H418,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H418,1)=\"J\",RIGHT(H418,LEN(H418)-4),RIGHT(H418,LEN(H418)-6)),\"\"))","v":""}]
[50000335,"Ginlong Technologies","RHI-3K-48ES-5G",3,3.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H419,1)=\"J\",LEFT(H419,2),LEFT(H419,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H419,1)=\"J\",RIGHT(H419,LEN(H419)-4),RIGHT(H419,LEN(H419)-6)),\"\"))","v":""}]
[50000336,"Ginlong Technologies","S5-EH1P3K-L",3,3.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H420,1)=\"J\",LEFT(H420,2),LEFT(H420,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H420,1)=\"J\",RIGHT(H420,LEN(H420)-4),RIGHT(H420,LEN(H420)-6)),\"\"))","v":""}]
[50000337,"Ginlong Technologies","S5-EH1P3K-L-UN",3,3.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H421,1)=\"J\",LEFT(H421,2),LEFT(H421,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H421,1)=\"J\",RIGHT(H421,LEN(H421)-4),RIGHT(H421,LEN(H421)-6)),\"\"))","v":""}]
[50000338,"Ginlong Technologies","S5-EH1P3K-L-UN-EX",3,3.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H422,1)=\"J\",LEFT(H422,2),LEFT(H422,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H422,1)=\"J\",RIGHT(H422,LEN(H422)-4),RIGHT(H422,LEN(H422)-6)),\"\"))","v":""}]
[50000339,"Ginlong Technologies","S5-GR3P3K",3,3.3,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,"gem. Diskussion am 16062021 mit VDE und Parametrieranleitung (TOR-Setting) zugelassen",null,{"$f":"IF(LEFT(H423,1)=\"J\",LEFT(H423,2),LEFT(H423,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H423,1)=\"J\",RIGHT(H423,LEN(H423)-4),RIGHT(H423,LEN(H423)-6)),\"\"))","v":""}]
[50000340,"Ginlong Technologies","S6-GR1P3K",3,3.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H424,1)=\"J\",LEFT(H424,2),LEFT(H424,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H424,1)=\"J\",RIGHT(H424,LEN(H424)-4),RIGHT(H424,LEN(H424)-6)),\"\"))","v":""}]
[50000341,"Ginlong Technologies","S6-GR1P3K-M",3,3.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H425,1)=\"J\",LEFT(H425,2),LEFT(H425,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H425,1)=\"J\",RIGHT(H425,LEN(H425)-4),RIGHT(H425,LEN(H425)-6)),\"\"))","v":""}]
[50000342,"Ginlong Technologies","S6-GR1P3.6K-M",3.6,3.6,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H426,1)=\"J\",LEFT(H426,2),LEFT(H426,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H426,1)=\"J\",RIGHT(H426,LEN(H426)-4),RIGHT(H426,LEN(H426)-6)),\"\"))","v":""}]
[50000343,"Ginlong Technologies","RHI-3.6K-48ES-5G",3.6,4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H427,1)=\"J\",LEFT(H427,2),LEFT(H427,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H427,1)=\"J\",RIGHT(H427,LEN(H427)-4),RIGHT(H427,LEN(H427)-6)),\"\"))","v":""}]
[50000344,"Ginlong Technologies","S5-EH1P3.6K-L",3.6,4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H428,1)=\"J\",LEFT(H428,2),LEFT(H428,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H428,1)=\"J\",RIGHT(H428,LEN(H428)-4),RIGHT(H428,LEN(H428)-6)),\"\"))","v":""}]
[50000345,"Ginlong Technologies","S5-EH1P3.6K-L-UN",3.6,4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H429,1)=\"J\",LEFT(H429,2),LEFT(H429,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H429,1)=\"J\",RIGHT(H429,LEN(H429)-4),RIGHT(H429,LEN(H429)-6)),\"\"))","v":""}]
[50000346,"Ginlong Technologies","S5-EH1P3.6K-L-UN-EX",3.6,4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H430,1)=\"J\",LEFT(H430,2),LEFT(H430,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H430,1)=\"J\",RIGHT(H430,LEN(H430)-4),RIGHT(H430,LEN(H430)-6)),\"\"))","v":""}]
[50000347,"Ginlong Technologies","S5-EO1P4K-48",4,4,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H431,1)=\"J\",LEFT(H431,2),LEFT(H431,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H431,1)=\"J\",RIGHT(H431,LEN(H431)-4),RIGHT(H431,LEN(H431)-6)),\"\"))","v":""}]
[50000348,"Ginlong Technologies","S5-EO1P4K-48-P",4,4,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H432,1)=\"J\",LEFT(H432,2),LEFT(H432,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H432,1)=\"J\",RIGHT(H432,LEN(H432)-4),RIGHT(H432,LEN(H432)-6)),\"\"))","v":""}]
[50000349,"Ginlong Technologies","S6-GR1P3.6K",3.6,4,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H433,1)=\"J\",LEFT(H433,2),LEFT(H433,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H433,1)=\"J\",RIGHT(H433,LEN(H433)-4),RIGHT(H433,LEN(H433)-6)),\"\"))","v":""}]
[50000350,"Ginlong Technologies","S5-GR3P4K",4,4.4000000000000004,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H434,1)=\"J\",LEFT(H434,2),LEFT(H434,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H434,1)=\"J\",RIGHT(H434,LEN(H434)-4),RIGHT(H434,LEN(H434)-6)),\"\"))","v":""}]
[50000351,"Ginlong Technologies","S6-GR1P4K",4,4.4000000000000004,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H435,1)=\"J\",LEFT(H435,2),LEFT(H435,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H435,1)=\"J\",RIGHT(H435,LEN(H435)-4),RIGHT(H435,LEN(H435)-6)),\"\"))","v":""}]
[50000352,"Ginlong Technologies","RHI-4.6K-48ES-5G",4.5999999999999996,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H436,1)=\"J\",LEFT(H436,2),LEFT(H436,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H436,1)=\"J\",RIGHT(H436,LEN(H436)-4),RIGHT(H436,LEN(H436)-6)),\"\"))","v":""}]
[50000353,"Ginlong Technologies","S5-EH1P4.6K-L",4.5999999999999996,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H437,1)=\"J\",LEFT(H437,2),LEFT(H437,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H437,1)=\"J\",RIGHT(H437,LEN(H437)-4),RIGHT(H437,LEN(H437)-6)),\"\"))","v":""}]
[50000354,"Ginlong Technologies","S5-EH1P4.6K-L-UN",4.5999999999999996,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H438,1)=\"J\",LEFT(H438,2),LEFT(H438,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H438,1)=\"J\",RIGHT(H438,LEN(H438)-4),RIGHT(H438,LEN(H438)-6)),\"\"))","v":""}]
[50000355,"Ginlong Technologies","S5-EH1P4.6K-L-UN-EX",4.5999999999999996,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H439,1)=\"J\",LEFT(H439,2),LEFT(H439,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H439,1)=\"J\",RIGHT(H439,LEN(H439)-4),RIGHT(H439,LEN(H439)-6)),\"\"))","v":""}]
[50000356,"Ginlong Technologies","RHI-3P5K-HVES-5G",null,5,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Ja",null,"nicht vorhanden",null,null,null,null,"OK","TOR-Einstellung vorhanden",null,null,null,"Batteriespeicher 3~ - DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H440,1)=\"J\",LEFT(H440,2),LEFT(H440,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H440,1)=\"J\",RIGHT(H440,LEN(H440)-4),RIGHT(H440,LEN(H440)-6)),\"\"))","v":""}]
[50000357,"Ginlong Technologies","S5-EO1P5K-48",5,5,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H441,1)=\"J\",LEFT(H441,2),LEFT(H441,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H441,1)=\"J\",RIGHT(H441,LEN(H441)-4),RIGHT(H441,LEN(H441)-6)),\"\"))","v":""}]
[50000358,"Ginlong Technologies","S5-EO1P5K-48-P",5,5,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H442,1)=\"J\",LEFT(H442,2),LEFT(H442,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H442,1)=\"J\",RIGHT(H442,LEN(H442)-4),RIGHT(H442,LEN(H442)-6)),\"\"))","v":""}]
[50000359,"Ginlong Technologies","S6-GR1P4.6K",4.5999999999999996,5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H443,1)=\"J\",LEFT(H443,2),LEFT(H443,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H443,1)=\"J\",RIGHT(H443,LEN(H443)-4),RIGHT(H443,LEN(H443)-6)),\"\"))","v":""}]
[50000360,"Ginlong Technologies","S5-GR3P5K",5,5.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H444,1)=\"J\",LEFT(H444,2),LEFT(H444,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H444,1)=\"J\",RIGHT(H444,LEN(H444)-4),RIGHT(H444,LEN(H444)-6)),\"\"))","v":""}]
[50000361,"Ginlong Technologies","Solis-3P5K-4G",5,5.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H445,1)=\"J\",LEFT(H445,2),LEFT(H445,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H445,1)=\"J\",RIGHT(H445,LEN(H445)-4),RIGHT(H445,LEN(H445)-6)),\"\"))","v":""}]
[50000362,"Ginlong Technologies","RHI-3P6K-HVES-5G",null,6,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Ja",null,"nicht vorhanden",null,null,null,null,"OK","TOR-Einstellung vorhanden",null,null,null,"Batteriespeicher 3~ - DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H446,1)=\"J\",LEFT(H446,2),LEFT(H446,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H446,1)=\"J\",RIGHT(H446,LEN(H446)-4),RIGHT(H446,LEN(H446)-6)),\"\"))","v":""}]
[50000363,"Ginlong Technologies","S5-GR3P6K",6,6.6,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,"gem. Diskussion am 16062021 mit VDE und Parametrieranleitung (TOR-Setting) zugelassen",null,{"$f":"IF(LEFT(H447,1)=\"J\",LEFT(H447,2),LEFT(H447,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H447,1)=\"J\",RIGHT(H447,LEN(H447)-4),RIGHT(H447,LEN(H447)-6)),\"\"))","v":""}]
[50000364,"Ginlong Technologies","Solis-3P6K-4G",6,6.6,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H448,1)=\"J\",LEFT(H448,2),LEFT(H448,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H448,1)=\"J\",RIGHT(H448,LEN(H448)-4),RIGHT(H448,LEN(H448)-6)),\"\"))","v":""}]
[50000365,"Ginlong Technologies","RHI-3P8K-HVES-5G",null,8,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Ja",null,"nicht vorhanden",null,null,null,null,"OK","TOR-Einstellung vorhanden",null,null,null,"Batteriespeicher 3~ - DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H449,1)=\"J\",LEFT(H449,2),LEFT(H449,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H449,1)=\"J\",RIGHT(H449,LEN(H449)-4),RIGHT(H449,LEN(H449)-6)),\"\"))","v":""}]
[50000366,"Ginlong Technologies","S5-GR3P8K",8,8.8000000000000007,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,"gem. Diskussion am 16062021 mit VDE und Parametrieranleitung (TOR-Setting) zugelassen",null,{"$f":"IF(LEFT(H450,1)=\"J\",LEFT(H450,2),LEFT(H450,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H450,1)=\"J\",RIGHT(H450,LEN(H450)-4),RIGHT(H450,LEN(H450)-6)),\"\"))","v":""}]
[50000367,"Ginlong Technologies","Solis-3P8K-4G",8,8.8000000000000007,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H451,1)=\"J\",LEFT(H451,2),LEFT(H451,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H451,1)=\"J\",RIGHT(H451,LEN(H451)-4),RIGHT(H451,LEN(H451)-6)),\"\"))","v":""}]
[50000368,"Ginlong Technologies","S5-GR3P9K",9,9.9,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H452,1)=\"J\",LEFT(H452,2),LEFT(H452,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H452,1)=\"J\",RIGHT(H452,LEN(H452)-4),RIGHT(H452,LEN(H452)-6)),\"\"))","v":""}]
[50000369,"Ginlong Technologies","Solis-3P9K-4G",9,9.9,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H453,1)=\"J\",LEFT(H453,2),LEFT(H453,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H453,1)=\"J\",RIGHT(H453,LEN(H453)-4),RIGHT(H453,LEN(H453)-6)),\"\"))","v":""}]
[50000370,"Ginlong Technologies","RHI-3P10K-HVES-5G",null,10,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Ja",null,"nicht vorhanden",null,null,null,null,"OK","TOR-Einstellung vorhanden",null,null,null,"Batteriespeicher 3~ - DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H454,1)=\"J\",LEFT(H454,2),LEFT(H454,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H454,1)=\"J\",RIGHT(H454,LEN(H454)-4),RIGHT(H454,LEN(H454)-6)),\"\"))","v":""}]
[50000371,"Ginlong Technologies","S5-GR3P10K",10,11,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H455,1)=\"J\",LEFT(H455,2),LEFT(H455,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H455,1)=\"J\",RIGHT(H455,LEN(H455)-4),RIGHT(H455,LEN(H455)-6)),\"\"))","v":""}]
[50000372,"Ginlong Technologies","Solis-3P10K-4G",10,11,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H456,1)=\"J\",LEFT(H456,2),LEFT(H456,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H456,1)=\"J\",RIGHT(H456,LEN(H456)-4),RIGHT(H456,LEN(H456)-6)),\"\"))","v":""}]
[50000373,"Ginlong Technologies","S5-GR3P12K",12,13.2,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H457,1)=\"J\",LEFT(H457,2),LEFT(H457,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H457,1)=\"J\",RIGHT(H457,LEN(H457)-4),RIGHT(H457,LEN(H457)-6)),\"\"))","v":""}]
[50000374,"Ginlong Technologies","Solis-3P12K-4G",12,13.2,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H458,1)=\"J\",LEFT(H458,2),LEFT(H458,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H458,1)=\"J\",RIGHT(H458,LEN(H458)-4),RIGHT(H458,LEN(H458)-6)),\"\"))","v":""}]
[50000375,"Ginlong Technologies","S5-GR3P13K",13,14.3,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H459,1)=\"J\",LEFT(H459,2),LEFT(H459,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H459,1)=\"J\",RIGHT(H459,LEN(H459)-4),RIGHT(H459,LEN(H459)-6)),\"\"))","v":""}]
[50000376,"Ginlong Technologies","S5-GR3P15K",15,16.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H460,1)=\"J\",LEFT(H460,2),LEFT(H460,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H460,1)=\"J\",RIGHT(H460,LEN(H460)-4),RIGHT(H460,LEN(H460)-6)),\"\"))","v":""}]
[50000377,"Ginlong Technologies","Solis-3P15K-4G",15,16.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H461,1)=\"J\",LEFT(H461,2),LEFT(H461,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H461,1)=\"J\",RIGHT(H461,LEN(H461)-4),RIGHT(H461,LEN(H461)-6)),\"\"))","v":""}]
[50000378,"Ginlong Technologies","S5-GR3P17K",17,18.7,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H462,1)=\"J\",LEFT(H462,2),LEFT(H462,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H462,1)=\"J\",RIGHT(H462,LEN(H462)-4),RIGHT(H462,LEN(H462)-6)),\"\"))","v":""}]
[50000379,"Ginlong Technologies","Solis-3P17K-4G",17,18.7,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H463,1)=\"J\",LEFT(H463,2),LEFT(H463,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H463,1)=\"J\",RIGHT(H463,LEN(H463)-4),RIGHT(H463,LEN(H463)-6)),\"\"))","v":""}]
[50000380,"Ginlong Technologies","S5-GR3P20K",20,22,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,"gem. Diskussion am 16062021 mit VDE und Parametrieranleitung (TOR-Setting) zugelassen",null,{"$f":"IF(LEFT(H464,1)=\"J\",LEFT(H464,2),LEFT(H464,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H464,1)=\"J\",RIGHT(H464,LEN(H464)-4),RIGHT(H464,LEN(H464)-6)),\"\"))","v":""}]
[50000381,"Ginlong Technologies","Solis-3P20K-4G",20,22,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H465,1)=\"J\",LEFT(H465,2),LEFT(H465,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H465,1)=\"J\",RIGHT(H465,LEN(H465)-4),RIGHT(H465,LEN(H465)-6)),\"\"))","v":""}]
[50000382,"Ginlong Technologies","S5-GC25K",25,27.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H466,1)=\"J\",LEFT(H466,2),LEFT(H466,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H466,1)=\"J\",RIGHT(H466,LEN(H466)-4),RIGHT(H466,LEN(H466)-6)),\"\"))","v":""}]
[50000383,"Ginlong Technologies","Solis-25K-5G ",null,27.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"OK","TOR-Einstellung vorhanden",null,null,null,"Stringwechselrichter 3~ - nur VDE 4105 + Einstellung und Bestätigung durch Ingenieurbüro","F","F",null,null,{"$f":"IF(LEFT(H467,1)=\"J\",LEFT(H467,2),LEFT(H467,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H467,1)=\"J\",RIGHT(H467,LEN(H467)-4),RIGHT(H467,LEN(H467)-6)),\"\"))","v":""}]
[50000384,"Ginlong Technologies","S5-GC30K",30,33,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H468,1)=\"J\",LEFT(H468,2),LEFT(H468,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H468,1)=\"J\",RIGHT(H468,LEN(H468)-4),RIGHT(H468,LEN(H468)-6)),\"\"))","v":""}]
[50000385,"Ginlong Technologies","Solis-30K-5G ",null,33,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"OK","TOR-Einstellung vorhanden",null,null,null,"Stringwechselrichter 3~ - nur VDE 4105 + Einstellung und Bestätigung durch Ingenieurbüro","F","F",null,null,{"$f":"IF(LEFT(H469,1)=\"J\",LEFT(H469,2),LEFT(H469,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H469,1)=\"J\",RIGHT(H469,LEN(H469)-4),RIGHT(H469,LEN(H469)-6)),\"\"))","v":""}]
[50000386,"Ginlong Technologies","S5-GC33K",33,36.299999999999997,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H470,1)=\"J\",LEFT(H470,2),LEFT(H470,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H470,1)=\"J\",RIGHT(H470,LEN(H470)-4),RIGHT(H470,LEN(H470)-6)),\"\"))","v":""}]
[50000387,"Ginlong Technologies","Solis-33K-5G ",null,36.299999999999997,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"OK","TOR-Einstellung vorhanden",null,null,null,"Stringwechselrichter 3~ - nur VDE 4105 + Einstellung und Bestätigung durch Ingenieurbüro","F","F",null,null,{"$f":"IF(LEFT(H471,1)=\"J\",LEFT(H471,2),LEFT(H471,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H471,1)=\"J\",RIGHT(H471,LEN(H471)-4),RIGHT(H471,LEN(H471)-6)),\"\"))","v":""}]
[50000388,"Ginlong Technologies","S5-GC36K",36,39.6,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H472,1)=\"J\",LEFT(H472,2),LEFT(H472,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H472,1)=\"J\",RIGHT(H472,LEN(H472)-4),RIGHT(H472,LEN(H472)-6)),\"\"))","v":""}]
[50000389,"Ginlong Technologies","Solis-36K-5G ",null,39.6,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"OK","TOR-Einstellung vorhanden",null,null,null,"Stringwechselrichter 3~ - nur VDE 4105 + Einstellung und Bestätigung durch Ingenieurbüro","F","F",null,null,{"$f":"IF(LEFT(H473,1)=\"J\",LEFT(H473,2),LEFT(H473,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H473,1)=\"J\",RIGHT(H473,LEN(H473)-4),RIGHT(H473,LEN(H473)-6)),\"\"))","v":""}]
[50000390,"Ginlong Technologies","S5-GC40K",40,44,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H474,1)=\"J\",LEFT(H474,2),LEFT(H474,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H474,1)=\"J\",RIGHT(H474,LEN(H474)-4),RIGHT(H474,LEN(H474)-6)),\"\"))","v":""}]
[50000391,"Ginlong Technologies","Solis-40K ",null,44,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H475,1)=\"J\",LEFT(H475,2),LEFT(H475,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H475,1)=\"J\",RIGHT(H475,LEN(H475)-4),RIGHT(H475,LEN(H475)-6)),\"\"))","v":""}]
[50000392,"Ginlong Technologies","Solis-40K-5G ",null,44,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"OK","TOR-Einstellung vorhanden",null,null,null,"Stringwechselrichter 3~ - nur VDE 4105 + Einstellung und Bestätigung durch Ingenieurbüro","F","F",null,null,{"$f":"IF(LEFT(H476,1)=\"J\",LEFT(H476,2),LEFT(H476,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H476,1)=\"J\",RIGHT(H476,LEN(H476)-4),RIGHT(H476,LEN(H476)-6)),\"\"))","v":""}]
[50000393,"Ginlong Technologies","Solis-40K-HV-5G",40,44,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H477,1)=\"J\",LEFT(H477,2),LEFT(H477,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H477,1)=\"J\",RIGHT(H477,LEN(H477)-4),RIGHT(H477,LEN(H477)-6)),\"\"))","v":""}]
[50000394,"Ginlong Technologies","Solis-50K ",null,50,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H478,1)=\"J\",LEFT(H478,2),LEFT(H478,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H478,1)=\"J\",RIGHT(H478,LEN(H478)-4),RIGHT(H478,LEN(H478)-6)),\"\"))","v":""}]
[50000395,"Ginlong Technologies","S5-GC50K",50,55,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H479,1)=\"J\",LEFT(H479,2),LEFT(H479,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H479,1)=\"J\",RIGHT(H479,LEN(H479)-4),RIGHT(H479,LEN(H479)-6)),\"\"))","v":""}]
[50000396,"Ginlong Technologies","Solis-50K-HV ",null,55,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H480,1)=\"J\",LEFT(H480,2),LEFT(H480,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H480,1)=\"J\",RIGHT(H480,LEN(H480)-4),RIGHT(H480,LEN(H480)-6)),\"\"))","v":""}]
[50000397,"Ginlong Technologies","Solis-50K-HV-5G",50,55,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H481,1)=\"J\",LEFT(H481,2),LEFT(H481,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H481,1)=\"J\",RIGHT(H481,LEN(H481)-4),RIGHT(H481,LEN(H481)-6)),\"\"))","v":""}]
[50000398,"Ginlong Technologies","S5-GC60K",60,66,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H482,1)=\"J\",LEFT(H482,2),LEFT(H482,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H482,1)=\"J\",RIGHT(H482,LEN(H482)-4),RIGHT(H482,LEN(H482)-6)),\"\"))","v":""}]
[50000399,"Ginlong Technologies","Solis-60K-HV ",null,66,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","F","F",null,null,{"$f":"IF(LEFT(H483,1)=\"J\",LEFT(H483,2),LEFT(H483,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H483,1)=\"J\",RIGHT(H483,LEN(H483)-4),RIGHT(H483,LEN(H483)-6)),\"\"))","v":""}]
[50000400,"Ginlong Technologies","Solis-60K-HV-4G",60,66,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H484,1)=\"J\",LEFT(H484,2),LEFT(H484,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H484,1)=\"J\",RIGHT(H484,LEN(H484)-4),RIGHT(H484,LEN(H484)-6)),\"\"))","v":""}]
[50000401,"Ginlong Technologies","Solis-70K-HV-4G",70,77,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H485,1)=\"J\",LEFT(H485,2),LEFT(H485,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H485,1)=\"J\",RIGHT(H485,LEN(H485)-4),RIGHT(H485,LEN(H485)-6)),\"\"))","v":""}]
[50000402,"Ginlong Technologies","S5-GC80K",88,88,3,"PV-Wechselrichter","Ja",null,null,"2021-08-16","1900-01-30",null,null,null,"Nein","Nein",null,"OK","Markus Radauer","CN21E7K9001","2021-08-16",null,"OK","TOR-Einstellung vorhanden",null,null,null,"Stringwechselrichter 3~ - nur VDE 4105 + Einstellung und Bestätigung durch Ingenieurbüro","F","F",null,null,{"$f":"IF(LEFT(H486,1)=\"J\",LEFT(H486,2),LEFT(H486,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H486,1)=\"J\",RIGHT(H486,LEN(H486)-4),RIGHT(H486,LEN(H486)-6)),\"\"))","v":""}]
[50000403,"Ginlong Technologies","Solis-80K-5G ",88,88,3,"PV-Wechselrichter","Ja",null,null,"2021-08-16","1900-01-30",null,null,null,"Nein","Nein",null,"OK","Markus Radauer","CN21E7K9001","2021-08-16",null,"OK","TOR-Einstellung vorhanden",null,null,null,"Stringwechselrichter 3~ - nur VDE 4105 + Einstellung und Bestätigung durch Ingenieurbüro","F","F",null,null,{"$f":"IF(LEFT(H487,1)=\"J\",LEFT(H487,2),LEFT(H487,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H487,1)=\"J\",RIGHT(H487,LEN(H487)-4),RIGHT(H487,LEN(H487)-6)),\"\"))","v":""}]
[50000404,"Ginlong Technologies","S5-GC100K",110,110,3,"PV-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","CN21E7K9001","2021-08-16",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H488,1)=\"J\",LEFT(H488,2),LEFT(H488,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H488,1)=\"J\",RIGHT(H488,LEN(H488)-4),RIGHT(H488,LEN(H488)-6)),\"\"))","v":""}]
[50000405,"Ginlong Technologies","Solis-100K-5G ",110,110,3,"PV-Wechselrichter","Ja",null,null,"2021-08-16","1900-01-30",null,null,null,"Nein","Nein",null,"OK","Markus Radauer","CN21E7K9001","2021-08-16","Vorhanden","OK","TOR-Einstellung vorhanden",null,null,null,"Stringwechselrichter 3~ - nur VDE 4105 + Einstellung und Bestätigung durch Ingenieurbüro","F","F",null,null,{"$f":"IF(LEFT(H489,1)=\"J\",LEFT(H489,2),LEFT(H489,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H489,1)=\"J\",RIGHT(H489,LEN(H489)-4),RIGHT(H489,LEN(H489)-6)),\"\"))","v":""}]
[50000406,"Ginlong Technologies","S5-GC110K",121,121,3,"PV-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","CN21E7K9001","2021-08-16",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H490,1)=\"J\",LEFT(H490,2),LEFT(H490,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H490,1)=\"J\",RIGHT(H490,LEN(H490)-4),RIGHT(H490,LEN(H490)-6)),\"\"))","v":""}]
[50000407,"Ginlong Technologies","Solis-110K-5G ",121,121,3,"PV-Wechselrichter","Ja",null,null,"2021-08-16","1900-01-30",null,null,null,"Nein","Nein",null,"OK","Markus Radauer","CN21E7K9001","2021-08-16","Vorhanden","OK","TOR-Einstellung vorhanden",null,null,null,"Stringwechselrichter 3~ - nur VDE 4105 + Einstellung und Bestätigung durch Ingenieurbüro","F","F",null,null,{"$f":"IF(LEFT(H491,1)=\"J\",LEFT(H491,2),LEFT(H491,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H491,1)=\"J\",RIGHT(H491,LEN(H491)-4),RIGHT(H491,LEN(H491)-6)),\"\"))","v":""}]
[50000408,"Ginlong Technologies","Solis-215K-EHV-5G-PLUS",null,215,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H492,1)=\"J\",LEFT(H492,2),LEFT(H492,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H492,1)=\"J\",RIGHT(H492,LEN(H492)-4),RIGHT(H492,LEN(H492)-6)),\"\"))","v":""}]
[50000409,"Ginlong Technologies","Solis-255K-EHV-5G",null,255,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H493,1)=\"J\",LEFT(H493,2),LEFT(H493,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H493,1)=\"J\",RIGHT(H493,LEN(H493)-4),RIGHT(H493,LEN(H493)-6)),\"\"))","v":""}]
[50000410,"Ginlong Technologies","Solis-255K-EHV-5GPLUS",null,255,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H494,1)=\"J\",LEFT(H494,2),LEFT(H494,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H494,1)=\"J\",RIGHT(H494,LEN(H494)-4),RIGHT(H494,LEN(H494)-6)),\"\"))","v":""}]
[50001817,"Goodwe","GW700-XS ",0.7,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"VDE4105/4110",null,null,null,null,"nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H495,1)=\"J\",LEFT(H495,2),LEFT(H495,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H495,1)=\"J\",RIGHT(H495,LEN(H495)-4),RIGHT(H495,LEN(H495)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000412,"Goodwe","GW1000-XS ",1,1.1000000000000001,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H496,1)=\"J\",LEFT(H496,2),LEFT(H496,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H496,1)=\"J\",RIGHT(H496,LEN(H496)-4),RIGHT(H496,LEN(H496)-6)),\"\"))","v":""}]
[50000413,"Goodwe","GW1500-XS ",1.5,1.65,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H497,1)=\"J\",LEFT(H497,2),LEFT(H497,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H497,1)=\"J\",RIGHT(H497,LEN(H497)-4),RIGHT(H497,LEN(H497)-6)),\"\"))","v":""}]
[50000414,"Goodwe","GW2000-XS ",2,2.2000000000000002,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H498,1)=\"J\",LEFT(H498,2),LEFT(H498,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H498,1)=\"J\",RIGHT(H498,LEN(H498)-4),RIGHT(H498,LEN(H498)-6)),\"\"))","v":""}]
[50000415,"Goodwe","GW2500-XS ",2.5,2.75,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H499,1)=\"J\",LEFT(H499,2),LEFT(H499,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H499,1)=\"J\",RIGHT(H499,LEN(H499)-4),RIGHT(H499,LEN(H499)-6)),\"\"))","v":""}]
[50000416,"Goodwe","GW3000-XS ",3,3.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H500,1)=\"J\",LEFT(H500,2),LEFT(H500,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H500,1)=\"J\",RIGHT(H500,LEN(H500)-4),RIGHT(H500,LEN(H500)-6)),\"\"))","v":""}]
[50000417,"Goodwe","GW4K-DT ",4,4.4000000000000004,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H501,1)=\"J\",LEFT(H501,2),LEFT(H501,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H501,1)=\"J\",RIGHT(H501,LEN(H501)-4),RIGHT(H501,LEN(H501)-6)),\"\"))","v":"mit Einschränkung"}]
[50000418,"Goodwe","GW5K-BT ",5,5.5,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2022-09-12","FW: 090922",null,null,null,"Ja","Nein","Ja","Vorhanden","Roland Bründlinger","50314995 005","2022-08-01",null,"Vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H502,1)=\"J\",LEFT(H502,2),LEFT(H502,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H502,1)=\"J\",RIGHT(H502,LEN(H502)-4),RIGHT(H502,LEN(H502)-6)),\"\"))","v":"mit Einschränkung"}]
[50000419,"Goodwe","GW5K-DT ",5,5.5,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H503,1)=\"J\",LEFT(H503,2),LEFT(H503,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H503,1)=\"J\",RIGHT(H503,LEN(H503)-4),RIGHT(H503,LEN(H503)-6)),\"\"))","v":"mit Einschränkung"}]
[50000420,"Goodwe","GW5K-ET ",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-09-12","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H504,1)=\"J\",LEFT(H504,2),LEFT(H504,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H504,1)=\"J\",RIGHT(H504,LEN(H504)-4),RIGHT(H504,LEN(H504)-6)),\"\"))","v":"mit Einschränkung"}]
[50000421,"Goodwe","GW5KL-ET (nur Australien)",5,5.5,3,"Hybrid-Wechselrichter","Nein","2022-10-24","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Ja","nicht OK","Roland Bründlinger","50314995 005","2022-08-01",null,"Vorhanden",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H505,1)=\"J\",LEFT(H505,2),LEFT(H505,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H505,1)=\"J\",RIGHT(H505,LEN(H505)-4),RIGHT(H505,LEN(H505)-6)),\"\"))","v":""}]
[50000422,"Goodwe","GW5KN-ET",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-11-28","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H506,1)=\"J\",LEFT(H506,2),LEFT(H506,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H506,1)=\"J\",RIGHT(H506,LEN(H506)-4),RIGHT(H506,LEN(H506)-6)),\"\"))","v":"mit Einschränkung"}]
[50000423,"Goodwe","GW6K-BT ",6,6.6,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2022-09-12","FW: 090922",null,null,null,"Ja","Nein","Ja","Vorhanden","Roland Bründlinger","50314995 005","2022-08-01",null,"Vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H507,1)=\"J\",LEFT(H507,2),LEFT(H507,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H507,1)=\"J\",RIGHT(H507,LEN(H507)-4),RIGHT(H507,LEN(H507)-6)),\"\"))","v":"mit Einschränkung"}]
[50000424,"Goodwe","GW6K-DT ",6,6.6,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H508,1)=\"J\",LEFT(H508,2),LEFT(H508,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H508,1)=\"J\",RIGHT(H508,LEN(H508)-4),RIGHT(H508,LEN(H508)-6)),\"\"))","v":"mit Einschränkung"}]
[50000425,"Goodwe","GW6KL-ET (nur Australien)",6,6.6,3,"Hybrid-Wechselrichter","Nein","2022-10-24","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Ja","nicht OK","Roland Bründlinger","50314995 005","2022-08-01",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H509,1)=\"J\",LEFT(H509,2),LEFT(H509,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H509,1)=\"J\",RIGHT(H509,LEN(H509)-4),RIGHT(H509,LEN(H509)-6)),\"\"))","v":""}]
[50000426,"Goodwe","GW6.5K-ET ",6.5,7.15,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-09-12","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H510,1)=\"J\",LEFT(H510,2),LEFT(H510,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H510,1)=\"J\",RIGHT(H510,LEN(H510)-4),RIGHT(H510,LEN(H510)-6)),\"\"))","v":"mit Einschränkung"}]
[50000427,"Goodwe","GW6.5KN-ET",6.5,7.15,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-11-28","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H511,1)=\"J\",LEFT(H511,2),LEFT(H511,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H511,1)=\"J\",RIGHT(H511,LEN(H511)-4),RIGHT(H511,LEN(H511)-6)),\"\"))","v":"mit Einschränkung"}]
[50000428,"Goodwe","GW8000-SDT-20",8,8.8000000000000007,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-03-22","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein","Nein","Vorhanden",null,"PVP09056/21E-03","2022-04-22","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H512,1)=\"J\",LEFT(H512,2),LEFT(H512,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H512,1)=\"J\",RIGHT(H512,LEN(H512)-4),RIGHT(H512,LEN(H512)-6)),\"\"))","v":"mit Einschränkung"}]
[50000429,"Goodwe","GW8K-BT ",8,8.8000000000000007,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2022-09-12","FW: 090922",null,null,null,"Ja","Nein","Ja","Vorhanden","Roland Bründlinger","50314995 005","2022-08-01",null,"Vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H513,1)=\"J\",LEFT(H513,2),LEFT(H513,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H513,1)=\"J\",RIGHT(H513,LEN(H513)-4),RIGHT(H513,LEN(H513)-6)),\"\"))","v":"mit Einschränkung"}]
[50000430,"Goodwe","GW8K-DT ",8,8.8000000000000007,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H514,1)=\"J\",LEFT(H514,2),LEFT(H514,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H514,1)=\"J\",RIGHT(H514,LEN(H514)-4),RIGHT(H514,LEN(H514)-6)),\"\"))","v":"mit Einschränkung"}]
[50000431,"Goodwe","GW8K-ET ",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-09-12","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H515,1)=\"J\",LEFT(H515,2),LEFT(H515,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H515,1)=\"J\",RIGHT(H515,LEN(H515)-4),RIGHT(H515,LEN(H515)-6)),\"\"))","v":"mit Einschränkung"}]
[50000432,"Goodwe","GW8KL-ET (nur Australien)",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein","2022-10-24","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Ja","nicht OK","Roland Bründlinger","50314995 005","2022-08-01",null,"Vorhanden",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H516,1)=\"J\",LEFT(H516,2),LEFT(H516,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H516,1)=\"J\",RIGHT(H516,LEN(H516)-4),RIGHT(H516,LEN(H516)-6)),\"\"))","v":""}]
[50000433,"Goodwe","GW8KN-ET",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-11-28","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H517,1)=\"J\",LEFT(H517,2),LEFT(H517,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H517,1)=\"J\",RIGHT(H517,LEN(H517)-4),RIGHT(H517,LEN(H517)-6)),\"\"))","v":"mit Einschränkung"}]
[50000434,"Goodwe","GW10KN-DT",10,10,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H518,1)=\"J\",LEFT(H518,2),LEFT(H518,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H518,1)=\"J\",RIGHT(H518,LEN(H518)-4),RIGHT(H518,LEN(H518)-6)),\"\"))","v":""}]
[50000435,"Goodwe","GW10K-BT ",10,11,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2022-09-12","FW: 090922",null,null,null,"Ja","Nein","Ja","Vorhanden","Roland Bründlinger","50314995 005","2022-08-01",null,"Vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H519,1)=\"J\",LEFT(H519,2),LEFT(H519,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H519,1)=\"J\",RIGHT(H519,LEN(H519)-4),RIGHT(H519,LEN(H519)-6)),\"\"))","v":"mit Einschränkung"}]
[50000436,"Goodwe","GW10K-ET ",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-09-12","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H520,1)=\"J\",LEFT(H520,2),LEFT(H520,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H520,1)=\"J\",RIGHT(H520,LEN(H520)-4),RIGHT(H520,LEN(H520)-6)),\"\"))","v":"mit Einschränkung"}]
[50000437,"Goodwe","GW10KL-ET (nur Australien)",10,11,3,"Hybrid-Wechselrichter","Nein","2022-10-24","Martin Bertsch",null,null,null,null,"P(U) teilweise mit zu großer Verzögerungszeit","Ja","Nein","Ja","nicht OK","Roland Bründlinger","50314995 005","2022-08-01",null,"Vorhanden",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H521,1)=\"J\",LEFT(H521,2),LEFT(H521,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H521,1)=\"J\",RIGHT(H521,LEN(H521)-4),RIGHT(H521,LEN(H521)-6)),\"\"))","v":""}]
[50000438,"Goodwe","GW10KN-ET",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-11-28","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H522,1)=\"J\",LEFT(H522,2),LEFT(H522,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H522,1)=\"J\",RIGHT(H522,LEN(H522)-4),RIGHT(H522,LEN(H522)-6)),\"\"))","v":"mit Einschränkung"}]
[50000439,"Goodwe","GW10K-SDT-20",10,11,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-03-22","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein","Nein","Vorhanden",null,"PVP09056/21E-03","2022-04-22","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H523,1)=\"J\",LEFT(H523,2),LEFT(H523,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H523,1)=\"J\",RIGHT(H523,LEN(H523)-4),RIGHT(H523,LEN(H523)-6)),\"\"))","v":"mit Einschränkung"}]
[50000440,"Goodwe","GW10KT-DT ",10,11,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H524,1)=\"J\",LEFT(H524,2),LEFT(H524,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H524,1)=\"J\",RIGHT(H524,LEN(H524)-4),RIGHT(H524,LEN(H524)-6)),\"\"))","v":"mit Einschränkung"}]
[50000441,"Goodwe","GW12K-SDT-20",12,13.2,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-03-22","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein","Nein","Vorhanden",null,"PVP09056/21E-03","2022-04-22","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H525,1)=\"J\",LEFT(H525,2),LEFT(H525,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H525,1)=\"J\",RIGHT(H525,LEN(H525)-4),RIGHT(H525,LEN(H525)-6)),\"\"))","v":"mit Einschränkung"}]
[50000442,"Goodwe","GW12KT-DT ",12,14,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H526,1)=\"J\",LEFT(H526,2),LEFT(H526,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H526,1)=\"J\",RIGHT(H526,LEN(H526)-4),RIGHT(H526,LEN(H526)-6)),\"\"))","v":"mit Einschränkung"}]
[50000443,"Goodwe","GW15K-ET",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-15","FW: 060608",null,null,null,"Ja","Nein","Ja","Vorhanden",null,"CN23NT8A 001 ","2023-03-28","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H527,1)=\"J\",LEFT(H527,2),LEFT(H527,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H527,1)=\"J\",RIGHT(H527,LEN(H527)-4),RIGHT(H527,LEN(H527)-6)),\"\"))","v":"mit Einschränkung"}]
[50000444,"Goodwe","GW15K-SDT-20",15,16.5,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-03-22","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein","Nein","Vorhanden",null,"PVP09056/21E-03","2022-04-22","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H528,1)=\"J\",LEFT(H528,2),LEFT(H528,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H528,1)=\"J\",RIGHT(H528,LEN(H528)-4),RIGHT(H528,LEN(H528)-6)),\"\"))","v":"mit Einschränkung"}]
[50000445,"Goodwe","GW15KT-DT ",15,16.5,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H529,1)=\"J\",LEFT(H529,2),LEFT(H529,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H529,1)=\"J\",RIGHT(H529,LEN(H529)-4),RIGHT(H529,LEN(H529)-6)),\"\"))","v":"mit Einschränkung"}]
[50000446,"Goodwe","GW17K-SDT-20",17,18.7,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-03-22","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein","Nein","Vorhanden",null,"PVP09056/21E-03","2022-04-22","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H530,1)=\"J\",LEFT(H530,2),LEFT(H530,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H530,1)=\"J\",RIGHT(H530,LEN(H530)-4),RIGHT(H530,LEN(H530)-6)),\"\"))","v":"mit Einschränkung"}]
[50000447,"Goodwe","GW17KT-DT ",17,19,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H531,1)=\"J\",LEFT(H531,2),LEFT(H531,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H531,1)=\"J\",RIGHT(H531,LEN(H531)-4),RIGHT(H531,LEN(H531)-6)),\"\"))","v":"mit Einschränkung"}]
[50000448,"Goodwe","GW20K-ET",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-15","FW: 060608",null,null,null,"Ja","Nein","Ja","Vorhanden",null,"CN23NT8A 001 ","2023-03-28","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H532,1)=\"J\",LEFT(H532,2),LEFT(H532,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H532,1)=\"J\",RIGHT(H532,LEN(H532)-4),RIGHT(H532,LEN(H532)-6)),\"\"))","v":"mit Einschränkung"}]
[50000449,"Goodwe","GW20K-SDT-20",20,22,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-03-22","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein","Nein","Vorhanden",null,"PVP09056/21E-03","2022-04-22","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H533,1)=\"J\",LEFT(H533,2),LEFT(H533,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H533,1)=\"J\",RIGHT(H533,LEN(H533)-4),RIGHT(H533,LEN(H533)-6)),\"\"))","v":"mit Einschränkung"}]
[50000450,"Goodwe","GW20KT-DT ",20,22,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H534,1)=\"J\",LEFT(H534,2),LEFT(H534,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H534,1)=\"J\",RIGHT(H534,LEN(H534)-4),RIGHT(H534,LEN(H534)-6)),\"\"))","v":"mit Einschränkung"}]
[50000451,"Goodwe","GW25K-ET",25,27.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-15","FW: 060608",null,null,null,"Ja","Nein","Ja","Vorhanden",null,"CN23NT8A 001 ","2023-03-28","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H535,1)=\"J\",LEFT(H535,2),LEFT(H535,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H535,1)=\"J\",RIGHT(H535,LEN(H535)-4),RIGHT(H535,LEN(H535)-6)),\"\"))","v":"mit Einschränkung"}]
[50000452,"Goodwe","GW25K-MT ",25,27.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200622N035-R1","2020-12-28",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H536,1)=\"J\",LEFT(H536,2),LEFT(H536,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H536,1)=\"J\",RIGHT(H536,LEN(H536)-4),RIGHT(H536,LEN(H536)-6)),\"\"))","v":""}]
[50000453,"Goodwe","GW25KT-DT ",25,27.5,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2023-02-24","17.17.18; Vmax PV: 950 V DC",null,null,null,"Nein","Nein",null,"Vorhanden","Katrin Fuchs (Energie Steiermark Technik)","6082075.52","2022-10-24","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H537,1)=\"J\",LEFT(H537,2),LEFT(H537,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H537,1)=\"J\",RIGHT(H537,LEN(H537)-4),RIGHT(H537,LEN(H537)-6)),\"\"))","v":"mit Einschränkung"}]
[50000454,"Goodwe","GW29.9K-ET",29.9,29.9,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-15","FW: 060608",null,null,null,"Ja","Nein","Ja","Vorhanden",null,"CN23NT8A 001 ","2023-03-28","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H538,1)=\"J\",LEFT(H538,2),LEFT(H538,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H538,1)=\"J\",RIGHT(H538,LEN(H538)-4),RIGHT(H538,LEN(H538)-6)),\"\"))","v":"mit Einschränkung"}]
[50000455,"Goodwe","GW30K-ET",30,33,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-15","FW: 060608",null,null,null,"Ja","Nein","Ja","Vorhanden",null,"CN23NT8A 001 ","2023-03-28","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H539,1)=\"J\",LEFT(H539,2),LEFT(H539,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H539,1)=\"J\",RIGHT(H539,LEN(H539)-4),RIGHT(H539,LEN(H539)-6)),\"\"))","v":"mit Einschränkung"}]
[50000456,"Goodwe","GW30K-MT ",30,33,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200622N035-R1","2020-12-28",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H540,1)=\"J\",LEFT(H540,2),LEFT(H540,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H540,1)=\"J\",RIGHT(H540,LEN(H540)-4),RIGHT(H540,LEN(H540)-6)),\"\"))","v":""}]
[50000457,"Goodwe","GW36K-MT ",36,36,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200622N035-R1","2020-12-28",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H541,1)=\"J\",LEFT(H541,2),LEFT(H541,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H541,1)=\"J\",RIGHT(H541,LEN(H541)-4),RIGHT(H541,LEN(H541)-6)),\"\"))","v":""}]
[50000458,"Goodwe","GW50K-BTC",52.5,52.5,3,"AC-Batteriewechselrichter","Nein","2023-03-17","Christian Elbs",null,null,null,null,null,"Ja","Nein","Ja","nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H542,1)=\"J\",LEFT(H542,2),LEFT(H542,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H542,1)=\"J\",RIGHT(H542,LEN(H542)-4),RIGHT(H542,LEN(H542)-6)),\"\"))","v":""}]
[50000459,"Goodwe","GW50K-ETC",52.5,52.5,3,"Hybrid-Wechselrichter","Nein","2023-03-17","Christian Elbs",null,null,null,null,null,"Ja","Nein","Ja","nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H543,1)=\"J\",LEFT(H543,2),LEFT(H543,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H543,1)=\"J\",RIGHT(H543,LEN(H543)-4),RIGHT(H543,LEN(H543)-6)),\"\"))","v":""}]
[50000460,"Goodwe","GW50KS-MT",50,55,3,"PV-Wechselrichter","Nein","2022-12-01","Christian Elbs",null,null,null,null,null,"Nein","Nein","Nein","nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H544,1)=\"J\",LEFT(H544,2),LEFT(H544,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H544,1)=\"J\",RIGHT(H544,LEN(H544)-4),RIGHT(H544,LEN(H544)-6)),\"\"))","v":""}]
[50000461,"Goodwe","GW60KS-MT",60,66,3,"PV-Wechselrichter","Nein","2022-12-01","Christian Elbs",null,null,null,null,null,"Nein","Nein","Nein","nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H545,1)=\"J\",LEFT(H545,2),LEFT(H545,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H545,1)=\"J\",RIGHT(H545,LEN(H545)-4),RIGHT(H545,LEN(H545)-6)),\"\"))","v":""}]
[50000462,"Goodwe","GW80K-MT",80,88,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H546,1)=\"J\",LEFT(H546,2),LEFT(H546,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H546,1)=\"J\",RIGHT(H546,LEN(H546)-4),RIGHT(H546,LEN(H546)-6)),\"\"))","v":""}]
[50000463,"Goodwe","GW100K-HT",100,110,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H547,1)=\"J\",LEFT(H547,2),LEFT(H547,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H547,1)=\"J\",RIGHT(H547,LEN(H547)-4),RIGHT(H547,LEN(H547)-6)),\"\"))","v":""}]
[50000464,"Goodwe","GW110K-HT",110,121,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H548,1)=\"J\",LEFT(H548,2),LEFT(H548,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H548,1)=\"J\",RIGHT(H548,LEN(H548)-4),RIGHT(H548,LEN(H548)-6)),\"\"))","v":""}]
[50000465,"Goodwe","GW120K-HT",120,132,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H549,1)=\"J\",LEFT(H549,2),LEFT(H549,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H549,1)=\"J\",RIGHT(H549,LEN(H549)-4),RIGHT(H549,LEN(H549)-6)),\"\"))","v":""}]
[50000466,"Goodwe","GW136K-HTH",136,150,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H550,1)=\"J\",LEFT(H550,2),LEFT(H550,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H550,1)=\"J\",RIGHT(H550,LEN(H550)-4),RIGHT(H550,LEN(H550)-6)),\"\"))","v":""}]
[50000467,"Goodwe","GW225K-HT",225,247.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H551,1)=\"J\",LEFT(H551,2),LEFT(H551,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H551,1)=\"J\",RIGHT(H551,LEN(H551)-4),RIGHT(H551,LEN(H551)-6)),\"\"))","v":""}]
[50000468,"Goodwe","GW250K-HT",250,250,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H552,1)=\"J\",LEFT(H552,2),LEFT(H552,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H552,1)=\"J\",RIGHT(H552,LEN(H552)-4),RIGHT(H552,LEN(H552)-6)),\"\"))","v":""}]
[50001718,"Growatt","MIC 600TL-X",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-09-04","Martin Bertsch","2023-09-04",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"230403060GZU-002","2023-07-24",null,"VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H553,1)=\"J\",LEFT(H553,2),LEFT(H553,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H553,1)=\"J\",RIGHT(H553,LEN(H553)-4),RIGHT(H553,LEN(H553)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002237,"Growatt","NEO 600M-X",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-15","Martin Bertsch","2024-05-15",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"230731032GZU-001","2023-09-26","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H554,1)=\"J\",LEFT(H554,2),LEFT(H554,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H554,1)=\"J\",RIGHT(H554,LEN(H554)-4),RIGHT(H554,LEN(H554)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001719,"Growatt","MIC 750TL-X",0.75,0.75,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-09-04","Martin Bertsch","2023-09-04",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"230403060GZU-002","2023-07-24",null,"VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H555,1)=\"J\",LEFT(H555,2),LEFT(H555,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H555,1)=\"J\",RIGHT(H555,LEN(H555)-4),RIGHT(H555,LEN(H555)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001720,"Growatt","MIC 800TL-X",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-09-04","Martin Bertsch","2023-09-04",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"230403060GZU-002","2023-07-24",null,"VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H556,1)=\"J\",LEFT(H556,2),LEFT(H556,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H556,1)=\"J\",RIGHT(H556,LEN(H556)-4),RIGHT(H556,LEN(H556)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002238,"Growatt","NEO 800M-X",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-15","Martin Bertsch","2024-05-15",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"230731032GZU-001","2023-09-26","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H557,1)=\"J\",LEFT(H557,2),LEFT(H557,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H557,1)=\"J\",RIGHT(H557,LEN(H557)-4),RIGHT(H557,LEN(H557)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000476,"Growatt","Growatt 3000TL3-S ",null,3,3,"PV-Wechselrichter","Nein","2022-06-29",null,"2021-05-06",null,null,"2022-06-29",null,"Nein","Nein",null,"Vorhanden",null,"200109114GZU-001","2020-06-17",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H558,1)=\"J\",LEFT(H558,2),LEFT(H558,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H558,1)=\"J\",RIGHT(H558,LEN(H558)-4),RIGHT(H558,LEN(H558)-6)),\"\"))","v":""}]
[50002229,"Growatt","MOD 3000TL3-XA",3,3,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H559,1)=\"J\",LEFT(H559,2),LEFT(H559,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H559,1)=\"J\",RIGHT(H559,LEN(H559)-4),RIGHT(H559,LEN(H559)-6)),\"\"))","v":"mit Einschränkung"}]
[50000481,"Growatt","MOD 3000TL3-X",3,3.3,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H560,1)=\"J\",LEFT(H560,2),LEFT(H560,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H560,1)=\"J\",RIGHT(H560,LEN(H560)-4),RIGHT(H560,LEN(H560)-6)),\"\"))","v":"mit Einschränkung"}]
[50000482,"Growatt","MOD 3000TL3-XH",3,3.3,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H561,1)=\"J\",LEFT(H561,2),LEFT(H561,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H561,1)=\"J\",RIGHT(H561,LEN(H561)-4),RIGHT(H561,LEN(H561)-6)),\"\"))","v":"mit Einschränkung"}]
[50000485,"Growatt","Growatt 4000TL3-S ",4,4,3,"PV-Wechselrichter","Nein","2022-06-29",null,"2021-05-06",null,null,"2022-06-29",null,"Nein","Nein",null,"Vorhanden",null,"200109114GZU-001","2020-06-17",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H562,1)=\"J\",LEFT(H562,2),LEFT(H562,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H562,1)=\"J\",RIGHT(H562,LEN(H562)-4),RIGHT(H562,LEN(H562)-6)),\"\"))","v":""}]
[50002230,"Growatt","MOD 4000TL3-XA",4,4,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H563,1)=\"J\",LEFT(H563,2),LEFT(H563,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H563,1)=\"J\",RIGHT(H563,LEN(H563)-4),RIGHT(H563,LEN(H563)-6)),\"\"))","v":"mit Einschränkung"}]
[50000486,"Growatt","SPA 4000TL3 BH",4,4,3,"AC-Batteriewechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H564,1)=\"J\",LEFT(H564,2),LEFT(H564,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H564,1)=\"J\",RIGHT(H564,LEN(H564)-4),RIGHT(H564,LEN(H564)-6)),\"\"))","v":""}]
[50000487,"Growatt","SPA 4000TL3 BH-UP",4,4,3,"AC-Batteriewechselrichter","Ja","2022-08-03","Christian Elbs","2022-08-03","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H565,1)=\"J\",LEFT(H565,2),LEFT(H565,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H565,1)=\"J\",RIGHT(H565,LEN(H565)-4),RIGHT(H565,LEN(H565)-6)),\"\"))","v":""}]
[50000488,"Growatt","SPH 4000TL3 BH",4,4,3,"Hybrid-Wechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H566,1)=\"J\",LEFT(H566,2),LEFT(H566,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H566,1)=\"J\",RIGHT(H566,LEN(H566)-4),RIGHT(H566,LEN(H566)-6)),\"\"))","v":""}]
[50000489,"Growatt","SPH 4000TL3 BH-UP",4,4,3,"Hybrid-Wechselrichter","Ja","2022-08-01","Christian Elbs","2022-08-01","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H567,1)=\"J\",LEFT(H567,2),LEFT(H567,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H567,1)=\"J\",RIGHT(H567,LEN(H567)-4),RIGHT(H567,LEN(H567)-6)),\"\"))","v":""}]
[50000492,"Growatt","MOD 4000TL3-X",4,4.4000000000000004,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H568,1)=\"J\",LEFT(H568,2),LEFT(H568,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H568,1)=\"J\",RIGHT(H568,LEN(H568)-4),RIGHT(H568,LEN(H568)-6)),\"\"))","v":"mit Einschränkung"}]
[50000493,"Growatt","MOD 4000TL3-XH",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H569,1)=\"J\",LEFT(H569,2),LEFT(H569,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H569,1)=\"J\",RIGHT(H569,LEN(H569)-4),RIGHT(H569,LEN(H569)-6)),\"\"))","v":"mit Einschränkung"}]
[50000496,"Growatt","Growatt 5000TL3-S ",5,5,3,"PV-Wechselrichter","Nein","2022-06-29",null,"2021-05-06",null,null,"2022-06-29",null,"Nein","Nein",null,"Vorhanden",null,"200109114GZU-001","2020-06-17",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H570,1)=\"J\",LEFT(H570,2),LEFT(H570,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H570,1)=\"J\",RIGHT(H570,LEN(H570)-4),RIGHT(H570,LEN(H570)-6)),\"\"))","v":""}]
[50002231,"Growatt","MOD 5000TL3-XA",5,5,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H571,1)=\"J\",LEFT(H571,2),LEFT(H571,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H571,1)=\"J\",RIGHT(H571,LEN(H571)-4),RIGHT(H571,LEN(H571)-6)),\"\"))","v":"mit Einschränkung"}]
[50000497,"Growatt","SPA 5000TL3 BH",5,5,3,"AC-Batteriewechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H572,1)=\"J\",LEFT(H572,2),LEFT(H572,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H572,1)=\"J\",RIGHT(H572,LEN(H572)-4),RIGHT(H572,LEN(H572)-6)),\"\"))","v":""}]
[50000498,"Growatt","SPA 5000TL3 BH-UP",5,5,3,"AC-Batteriewechselrichter","Ja","2022-08-03","Christian Elbs","2022-08-03","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H573,1)=\"J\",LEFT(H573,2),LEFT(H573,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H573,1)=\"J\",RIGHT(H573,LEN(H573)-4),RIGHT(H573,LEN(H573)-6)),\"\"))","v":""}]
[50000500,"Growatt","SPH 5000TL3 BH",5,5,3,"Hybrid-Wechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H574,1)=\"J\",LEFT(H574,2),LEFT(H574,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H574,1)=\"J\",RIGHT(H574,LEN(H574)-4),RIGHT(H574,LEN(H574)-6)),\"\"))","v":""}]
[50000501,"Growatt","SPH 5000TL3 BH-UP",5,5,3,"Hybrid-Wechselrichter","Ja","2022-08-01","Christian Elbs","2022-08-01","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H575,1)=\"J\",LEFT(H575,2),LEFT(H575,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H575,1)=\"J\",RIGHT(H575,LEN(H575)-4),RIGHT(H575,LEN(H575)-6)),\"\"))","v":""}]
[50000503,"Growatt","MOD 5000TL3-X",5,5.5,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H576,1)=\"J\",LEFT(H576,2),LEFT(H576,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H576,1)=\"J\",RIGHT(H576,LEN(H576)-4),RIGHT(H576,LEN(H576)-6)),\"\"))","v":"mit Einschränkung"}]
[50000504,"Growatt","MOD 5000TL3-XH",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H577,1)=\"J\",LEFT(H577,2),LEFT(H577,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H577,1)=\"J\",RIGHT(H577,LEN(H577)-4),RIGHT(H577,LEN(H577)-6)),\"\"))","v":"mit Einschränkung"}]
[50000505,"Growatt","Growatt 6000TL3-S ",6,6,3,"PV-Wechselrichter","Nein","2022-06-29",null,"2021-05-06",null,null,"2022-06-29",null,"Nein","Nein",null,"Vorhanden",null,"200109114GZU-001","2020-06-17",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H578,1)=\"J\",LEFT(H578,2),LEFT(H578,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H578,1)=\"J\",RIGHT(H578,LEN(H578)-4),RIGHT(H578,LEN(H578)-6)),\"\"))","v":""}]
[50002232,"Growatt","MOD 6000TL3-XA",6,6,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H579,1)=\"J\",LEFT(H579,2),LEFT(H579,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H579,1)=\"J\",RIGHT(H579,LEN(H579)-4),RIGHT(H579,LEN(H579)-6)),\"\"))","v":"mit Einschränkung"}]
[50000506,"Growatt","SPA 6000TL3 BH",6,6,3,"AC-Batteriewechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H580,1)=\"J\",LEFT(H580,2),LEFT(H580,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H580,1)=\"J\",RIGHT(H580,LEN(H580)-4),RIGHT(H580,LEN(H580)-6)),\"\"))","v":""}]
[50000507,"Growatt","SPA 6000TL3 BH-UP",6,6,3,"AC-Batteriewechselrichter","Ja","2022-08-03","Christian Elbs","2022-08-03","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H581,1)=\"J\",LEFT(H581,2),LEFT(H581,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H581,1)=\"J\",RIGHT(H581,LEN(H581)-4),RIGHT(H581,LEN(H581)-6)),\"\"))","v":""}]
[50000508,"Growatt","SPH 6000TL3 BH",6,6,3,"Hybrid-Wechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H582,1)=\"J\",LEFT(H582,2),LEFT(H582,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H582,1)=\"J\",RIGHT(H582,LEN(H582)-4),RIGHT(H582,LEN(H582)-6)),\"\"))","v":""}]
[50000509,"Growatt","SPH 6000TL3 BH-UP",6,6,3,"Hybrid-Wechselrichter","Ja","2022-08-01","Christian Elbs","2022-08-01","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H583,1)=\"J\",LEFT(H583,2),LEFT(H583,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H583,1)=\"J\",RIGHT(H583,LEN(H583)-4),RIGHT(H583,LEN(H583)-6)),\"\"))","v":""}]
[50000510,"Growatt","MOD 6000TL3-X",6,6.6,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H584,1)=\"J\",LEFT(H584,2),LEFT(H584,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H584,1)=\"J\",RIGHT(H584,LEN(H584)-4),RIGHT(H584,LEN(H584)-6)),\"\"))","v":"mit Einschränkung"}]
[50000511,"Growatt","MOD 6000TL3-XH",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H585,1)=\"J\",LEFT(H585,2),LEFT(H585,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H585,1)=\"J\",RIGHT(H585,LEN(H585)-4),RIGHT(H585,LEN(H585)-6)),\"\"))","v":"mit Einschränkung"}]
[50002233,"Growatt","MOD 7000TL3-XA",7,7,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H586,1)=\"J\",LEFT(H586,2),LEFT(H586,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H586,1)=\"J\",RIGHT(H586,LEN(H586)-4),RIGHT(H586,LEN(H586)-6)),\"\"))","v":"mit Einschränkung"}]
[50000512,"Growatt","SPA 7000TL3 BH",7,7,3,"AC-Batteriewechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H587,1)=\"J\",LEFT(H587,2),LEFT(H587,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H587,1)=\"J\",RIGHT(H587,LEN(H587)-4),RIGHT(H587,LEN(H587)-6)),\"\"))","v":""}]
[50000513,"Growatt","SPA 7000TL3 BH-UP",7,7,3,"AC-Batteriewechselrichter","Ja","2022-08-03","Christian Elbs","2022-08-03","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H588,1)=\"J\",LEFT(H588,2),LEFT(H588,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H588,1)=\"J\",RIGHT(H588,LEN(H588)-4),RIGHT(H588,LEN(H588)-6)),\"\"))","v":""}]
[50000514,"Growatt","SPH 7000TL3 BH",7,7,3,"Hybrid-Wechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H589,1)=\"J\",LEFT(H589,2),LEFT(H589,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H589,1)=\"J\",RIGHT(H589,LEN(H589)-4),RIGHT(H589,LEN(H589)-6)),\"\"))","v":""}]
[50000515,"Growatt","SPH 7000TL3 BH-UP",7,7,3,"Hybrid-Wechselrichter","Ja","2022-08-01","Christian Elbs","2022-08-01","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H590,1)=\"J\",LEFT(H590,2),LEFT(H590,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H590,1)=\"J\",RIGHT(H590,LEN(H590)-4),RIGHT(H590,LEN(H590)-6)),\"\"))","v":""}]
[50000516,"Growatt","Growatt 7000TL3-S ",7,7.7,3,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs","2021-05-06",null,null,"2022-06-29",null,"Nein","Nein",null,"Vorhanden",null,"200109114GZU-001","2020-06-17",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H591,1)=\"J\",LEFT(H591,2),LEFT(H591,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H591,1)=\"J\",RIGHT(H591,LEN(H591)-4),RIGHT(H591,LEN(H591)-6)),\"\"))","v":""}]
[50000517,"Growatt","MOD 7000TL3-X",7,7.7,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H592,1)=\"J\",LEFT(H592,2),LEFT(H592,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H592,1)=\"J\",RIGHT(H592,LEN(H592)-4),RIGHT(H592,LEN(H592)-6)),\"\"))","v":"mit Einschränkung"}]
[50000518,"Growatt","MOD 7000TL3-XH",7,7.7,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H593,1)=\"J\",LEFT(H593,2),LEFT(H593,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H593,1)=\"J\",RIGHT(H593,LEN(H593)-4),RIGHT(H593,LEN(H593)-6)),\"\"))","v":"mit Einschränkung"}]
[50002234,"Growatt","MOD 8000TL3-XA",8,8,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H594,1)=\"J\",LEFT(H594,2),LEFT(H594,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H594,1)=\"J\",RIGHT(H594,LEN(H594)-4),RIGHT(H594,LEN(H594)-6)),\"\"))","v":"mit Einschränkung"}]
[50000519,"Growatt","SPA 8000TL3 BH",8,8,3,"AC-Batteriewechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H595,1)=\"J\",LEFT(H595,2),LEFT(H595,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H595,1)=\"J\",RIGHT(H595,LEN(H595)-4),RIGHT(H595,LEN(H595)-6)),\"\"))","v":""}]
[50000520,"Growatt","SPA 8000TL3 BH-UP",8,8,3,"AC-Batteriewechselrichter","Ja","2022-08-03","Christian Elbs","2022-08-03","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H596,1)=\"J\",LEFT(H596,2),LEFT(H596,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H596,1)=\"J\",RIGHT(H596,LEN(H596)-4),RIGHT(H596,LEN(H596)-6)),\"\"))","v":""}]
[50000521,"Growatt","SPH 8000TL3 BH",8,8,3,"Hybrid-Wechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H597,1)=\"J\",LEFT(H597,2),LEFT(H597,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H597,1)=\"J\",RIGHT(H597,LEN(H597)-4),RIGHT(H597,LEN(H597)-6)),\"\"))","v":""}]
[50000522,"Growatt","SPH 8000TL3 BH-UP",8,8,3,"Hybrid-Wechselrichter","Ja","2022-08-01","Christian Elbs","2022-08-01","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H598,1)=\"J\",LEFT(H598,2),LEFT(H598,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H598,1)=\"J\",RIGHT(H598,LEN(H598)-4),RIGHT(H598,LEN(H598)-6)),\"\"))","v":""}]
[50000523,"Growatt","Growatt 8000TL3-S ",8,8.8000000000000007,3,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs",null,null,null,"2022-06-29",null,"Nein","Nein",null,"Vorhanden",null,"200109114GZU-001","2020-06-17",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H599,1)=\"J\",LEFT(H599,2),LEFT(H599,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H599,1)=\"J\",RIGHT(H599,LEN(H599)-4),RIGHT(H599,LEN(H599)-6)),\"\"))","v":""}]
[50000524,"Growatt","MOD 8000TL3-X",8,8.8000000000000007,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H600,1)=\"J\",LEFT(H600,2),LEFT(H600,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H600,1)=\"J\",RIGHT(H600,LEN(H600)-4),RIGHT(H600,LEN(H600)-6)),\"\"))","v":"mit Einschränkung"}]
[50000525,"Growatt","MOD 8000TL3-XH",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H601,1)=\"J\",LEFT(H601,2),LEFT(H601,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H601,1)=\"J\",RIGHT(H601,LEN(H601)-4),RIGHT(H601,LEN(H601)-6)),\"\"))","v":"mit Einschränkung"}]
[50002235,"Growatt","MOD 9000TL3-XA",9,9,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H602,1)=\"J\",LEFT(H602,2),LEFT(H602,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H602,1)=\"J\",RIGHT(H602,LEN(H602)-4),RIGHT(H602,LEN(H602)-6)),\"\"))","v":"mit Einschränkung"}]
[50000526,"Growatt","Growatt 9000TL3-S ",9,9.9,3,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs","2021-05-06",null,null,"2022-06-29",null,"Nein","Nein",null,"Vorhanden",null,"200109114GZU-001","2020-06-17",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H603,1)=\"J\",LEFT(H603,2),LEFT(H603,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H603,1)=\"J\",RIGHT(H603,LEN(H603)-4),RIGHT(H603,LEN(H603)-6)),\"\"))","v":""}]
[50000527,"Growatt","MOD 9000TL3-X",9,9.9,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H604,1)=\"J\",LEFT(H604,2),LEFT(H604,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H604,1)=\"J\",RIGHT(H604,LEN(H604)-4),RIGHT(H604,LEN(H604)-6)),\"\"))","v":"mit Einschränkung"}]
[50000528,"Growatt","MOD 9000TL3-XH",9,9.9,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H605,1)=\"J\",LEFT(H605,2),LEFT(H605,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H605,1)=\"J\",RIGHT(H605,LEN(H605)-4),RIGHT(H605,LEN(H605)-6)),\"\"))","v":"mit Einschränkung"}]
[50002236,"Growatt","MOD 10KTL3-XA",10,10,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H606,1)=\"J\",LEFT(H606,2),LEFT(H606,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H606,1)=\"J\",RIGHT(H606,LEN(H606)-4),RIGHT(H606,LEN(H606)-6)),\"\"))","v":"mit Einschränkung"}]
[50000529,"Growatt","SPA 10000TL3 BH",10,10,3,"AC-Batteriewechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H607,1)=\"J\",LEFT(H607,2),LEFT(H607,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H607,1)=\"J\",RIGHT(H607,LEN(H607)-4),RIGHT(H607,LEN(H607)-6)),\"\"))","v":""}]
[50000530,"Growatt","SPA 10000TL3 BH-UP",10,10,3,"AC-Batteriewechselrichter","Ja","2022-08-03","Christian Elbs","2022-08-03","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H608,1)=\"J\",LEFT(H608,2),LEFT(H608,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H608,1)=\"J\",RIGHT(H608,LEN(H608)-4),RIGHT(H608,LEN(H608)-6)),\"\"))","v":""}]
[50000531,"Growatt","SPH 10000TL3 BH",10,10,3,"Hybrid-Wechselrichter","Nein","2022-08-11","Christian Elbs",null,null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"200109117GZU-002","2020-06-12",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H609,1)=\"J\",LEFT(H609,2),LEFT(H609,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H609,1)=\"J\",RIGHT(H609,LEN(H609)-4),RIGHT(H609,LEN(H609)-6)),\"\"))","v":""}]
[50000532,"Growatt","SPH 10000TL3 BH-UP",10,10,3,"Hybrid-Wechselrichter","Ja","2022-08-01","Christian Elbs","2022-08-01","YA1.0(YBAa-959593)",null,null,null,"Ja","Nein","Ja","Vorhanden","Meike Gelhart (Wiener Netze)","210121014GZU-009","2021-05-20",null,"OK",null,"Vorhanden","2022-08-03",null,null,null,null,null,null,{"$f":"IF(LEFT(H610,1)=\"J\",LEFT(H610,2),LEFT(H610,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H610,1)=\"J\",RIGHT(H610,LEN(H610)-4),RIGHT(H610,LEN(H610)-6)),\"\"))","v":""}]
[50000533,"Growatt","Growatt 10000TL3-S ",10,11,3,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs","2021-05-06",null,null,"2022-06-29",null,"Nein","Nein",null,"Vorhanden",null,"200109114GZU-001","2020-06-17",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H611,1)=\"J\",LEFT(H611,2),LEFT(H611,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H611,1)=\"J\",RIGHT(H611,LEN(H611)-4),RIGHT(H611,LEN(H611)-6)),\"\"))","v":""}]
[50002221,"Growatt","MID 11KTL3-XA",11,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H612,1)=\"J\",LEFT(H612,2),LEFT(H612,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H612,1)=\"J\",RIGHT(H612,LEN(H612)-4),RIGHT(H612,LEN(H612)-6)),\"\"))","v":"mit Einschränkung"}]
[50000534,"Growatt","MOD 10KTL3-X",10,11,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H613,1)=\"J\",LEFT(H613,2),LEFT(H613,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H613,1)=\"J\",RIGHT(H613,LEN(H613)-4),RIGHT(H613,LEN(H613)-6)),\"\"))","v":"mit Einschränkung"}]
[50000535,"Growatt","MOD 10KTL3-XH",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H614,1)=\"J\",LEFT(H614,2),LEFT(H614,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H614,1)=\"J\",RIGHT(H614,LEN(H614)-4),RIGHT(H614,LEN(H614)-6)),\"\"))","v":"mit Einschränkung"}]
[50002222,"Growatt","MID 12KTL3-XA",12,12,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H615,1)=\"J\",LEFT(H615,2),LEFT(H615,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H615,1)=\"J\",RIGHT(H615,LEN(H615)-4),RIGHT(H615,LEN(H615)-6)),\"\"))","v":"mit Einschränkung"}]
[50000536,"Growatt","Growatt 11000TL3-S ",11,12.1,3,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs","2021-05-06",null,null,"2022-06-29",null,"Nein","Nein",null,"Vorhanden",null,"200109114GZU-001","2020-06-17",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H616,1)=\"J\",LEFT(H616,2),LEFT(H616,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H616,1)=\"J\",RIGHT(H616,LEN(H616)-4),RIGHT(H616,LEN(H616)-6)),\"\"))","v":""}]
[50002213,"Growatt","MID 11KTL3-XH",11,12.1,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H617,1)=\"J\",LEFT(H617,2),LEFT(H617,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H617,1)=\"J\",RIGHT(H617,LEN(H617)-4),RIGHT(H617,LEN(H617)-6)),\"\"))","v":"mit Einschränkung"}]
[50000537,"Growatt","MOD 11KTL3-X",11,12.1,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H618,1)=\"J\",LEFT(H618,2),LEFT(H618,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H618,1)=\"J\",RIGHT(H618,LEN(H618)-4),RIGHT(H618,LEN(H618)-6)),\"\"))","v":"mit Einschränkung"}]
[50000538,"Growatt","MOD 11KTL3-XH",11,12.1,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H619,1)=\"J\",LEFT(H619,2),LEFT(H619,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H619,1)=\"J\",RIGHT(H619,LEN(H619)-4),RIGHT(H619,LEN(H619)-6)),\"\"))","v":"mit Einschränkung"}]
[50002223,"Growatt","MID 13KTL3-XA",13,13,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H620,1)=\"J\",LEFT(H620,2),LEFT(H620,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H620,1)=\"J\",RIGHT(H620,LEN(H620)-4),RIGHT(H620,LEN(H620)-6)),\"\"))","v":"mit Einschränkung"}]
[50002214,"Growatt","MID 12KTL3-XH",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H621,1)=\"J\",LEFT(H621,2),LEFT(H621,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H621,1)=\"J\",RIGHT(H621,LEN(H621)-4),RIGHT(H621,LEN(H621)-6)),\"\"))","v":"mit Einschränkung"}]
[50000541,"Growatt","MOD 12KTL3-X",12,13.2,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H622,1)=\"J\",LEFT(H622,2),LEFT(H622,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H622,1)=\"J\",RIGHT(H622,LEN(H622)-4),RIGHT(H622,LEN(H622)-6)),\"\"))","v":"mit Einschränkung"}]
[50000542,"Growatt","MOD 12KTL3-XH",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H623,1)=\"J\",LEFT(H623,2),LEFT(H623,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H623,1)=\"J\",RIGHT(H623,LEN(H623)-4),RIGHT(H623,LEN(H623)-6)),\"\"))","v":"mit Einschränkung"}]
[50002215,"Growatt","MID 13KTL3-XH",13,14.3,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H624,1)=\"J\",LEFT(H624,2),LEFT(H624,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H624,1)=\"J\",RIGHT(H624,LEN(H624)-4),RIGHT(H624,LEN(H624)-6)),\"\"))","v":"mit Einschränkung"}]
[50000544,"Growatt","MOD 13KTL3-X",13,14.3,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H625,1)=\"J\",LEFT(H625,2),LEFT(H625,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H625,1)=\"J\",RIGHT(H625,LEN(H625)-4),RIGHT(H625,LEN(H625)-6)),\"\"))","v":"mit Einschränkung"}]
[50000545,"Growatt","MOD 13KTL3-XH",13,14.3,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H626,1)=\"J\",LEFT(H626,2),LEFT(H626,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H626,1)=\"J\",RIGHT(H626,LEN(H626)-4),RIGHT(H626,LEN(H626)-6)),\"\"))","v":"mit Einschränkung"}]
[50002224,"Growatt","MID 15KTL3-XA",15,15,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H627,1)=\"J\",LEFT(H627,2),LEFT(H627,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H627,1)=\"J\",RIGHT(H627,LEN(H627)-4),RIGHT(H627,LEN(H627)-6)),\"\"))","v":"mit Einschränkung"}]
[50002216,"Growatt","MID 15KTL3-XH",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H628,1)=\"J\",LEFT(H628,2),LEFT(H628,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H628,1)=\"J\",RIGHT(H628,LEN(H628)-4),RIGHT(H628,LEN(H628)-6)),\"\"))","v":"mit Einschränkung"}]
[50000547,"Growatt","MOD 15KTL3-X",15,16.5,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H629,1)=\"J\",LEFT(H629,2),LEFT(H629,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H629,1)=\"J\",RIGHT(H629,LEN(H629)-4),RIGHT(H629,LEN(H629)-6)),\"\"))","v":"mit Einschränkung"}]
[50000548,"Growatt","MOD 15KTL3-XH",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2022-11-16","Inverter DNAA06510107 S38B08D00T00P0FU01M0064",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220817030GZU-001","2023-09-25","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H630,1)=\"J\",LEFT(H630,2),LEFT(H630,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H630,1)=\"J\",RIGHT(H630,LEN(H630)-4),RIGHT(H630,LEN(H630)-6)),\"\"))","v":"mit Einschränkung"}]
[50002225,"Growatt","MID 17KTL3-XA",17,17,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H631,1)=\"J\",LEFT(H631,2),LEFT(H631,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H631,1)=\"J\",RIGHT(H631,LEN(H631)-4),RIGHT(H631,LEN(H631)-6)),\"\"))","v":"mit Einschränkung"}]
[50002217,"Growatt","MID 17KTL3-XH",17,18.7,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H632,1)=\"J\",LEFT(H632,2),LEFT(H632,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H632,1)=\"J\",RIGHT(H632,LEN(H632)-4),RIGHT(H632,LEN(H632)-6)),\"\"))","v":"mit Einschränkung"}]
[50000551,"Growatt","MID 17KTL3-X1",17,18.8,3,"PV-Wechselrichter","Nein","2024-05-14","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","200426161GZU-001","2022-04-12",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H633,1)=\"J\",LEFT(H633,2),LEFT(H633,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H633,1)=\"J\",RIGHT(H633,LEN(H633)-4),RIGHT(H633,LEN(H633)-6)),\"\"))","v":""}]
[50002226,"Growatt","MID 20KTL3-XA",20,20,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H634,1)=\"J\",LEFT(H634,2),LEFT(H634,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H634,1)=\"J\",RIGHT(H634,LEN(H634)-4),RIGHT(H634,LEN(H634)-6)),\"\"))","v":"mit Einschränkung"}]
[50000553,"Growatt","MID 20KTL3-X1",20,22,3,"PV-Wechselrichter","Nein","2024-05-14","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","200426161GZU-001","2022-04-12",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H635,1)=\"J\",LEFT(H635,2),LEFT(H635,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H635,1)=\"J\",RIGHT(H635,LEN(H635)-4),RIGHT(H635,LEN(H635)-6)),\"\"))","v":""}]
[50002218,"Growatt","MID 20KTL3-XH",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H636,1)=\"J\",LEFT(H636,2),LEFT(H636,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H636,1)=\"J\",RIGHT(H636,LEN(H636)-4),RIGHT(H636,LEN(H636)-6)),\"\"))","v":"mit Einschränkung"}]
[50000554,"Growatt","MID 22KTL3-X1",22,24.2,3,"PV-Wechselrichter","Nein","2024-05-14","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","200426161GZU-001","2022-04-12",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H637,1)=\"J\",LEFT(H637,2),LEFT(H637,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H637,1)=\"J\",RIGHT(H637,LEN(H637)-4),RIGHT(H637,LEN(H637)-6)),\"\"))","v":""}]
[50002227,"Growatt","MID 25KTL3-XA",25,25,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H638,1)=\"J\",LEFT(H638,2),LEFT(H638,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H638,1)=\"J\",RIGHT(H638,LEN(H638)-4),RIGHT(H638,LEN(H638)-6)),\"\"))","v":"mit Einschränkung"}]
[50002219,"Growatt","MID 25KTL3-XH",25,27.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H639,1)=\"J\",LEFT(H639,2),LEFT(H639,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H639,1)=\"J\",RIGHT(H639,LEN(H639)-4),RIGHT(H639,LEN(H639)-6)),\"\"))","v":"mit Einschränkung"}]
[50000557,"Growatt","MID 25KTL3-X1",25,27.7,3,"PV-Wechselrichter","Nein","2024-05-14","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","200426161GZU-001","2022-04-12",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H640,1)=\"J\",LEFT(H640,2),LEFT(H640,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H640,1)=\"J\",RIGHT(H640,LEN(H640)-4),RIGHT(H640,LEN(H640)-6)),\"\"))","v":""}]
[50002228,"Growatt","MID 30KTL3-XA",30,30,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H641,1)=\"J\",LEFT(H641,2),LEFT(H641,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H641,1)=\"J\",RIGHT(H641,LEN(H641)-4),RIGHT(H641,LEN(H641)-6)),\"\"))","v":"mit Einschränkung"}]
[50002220,"Growatt","MID 30KTL3-XH",30,30,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-15","Martin Bertsch","2024-05-15","DNBa975100/ZBDB-0007 Model: S38B00D00T06P0FU01M012C",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230315052GZU-001","2023-08-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H642,1)=\"J\",LEFT(H642,2),LEFT(H642,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H642,1)=\"J\",RIGHT(H642,LEN(H642)-4),RIGHT(H642,LEN(H642)-6)),\"\"))","v":"mit Einschränkung"}]
[50000558,"Growatt","MID 30KTL3-X",30,33.299999999999997,3,"PV-Wechselrichter","Nein","2024-05-14","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","200426161GZU-001","2022-04-12",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H643,1)=\"J\",LEFT(H643,2),LEFT(H643,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H643,1)=\"J\",RIGHT(H643,LEN(H643)-4),RIGHT(H643,LEN(H643)-6)),\"\"))","v":""}]
[50000559,"Growatt","MID 33KTL3-X",33,36.6,3,"PV-Wechselrichter","Nein","2024-05-14","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","200426161GZU-001","2022-04-12",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H644,1)=\"J\",LEFT(H644,2),LEFT(H644,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H644,1)=\"J\",RIGHT(H644,LEN(H644)-4),RIGHT(H644,LEN(H644)-6)),\"\"))","v":""}]
[50000560,"Growatt","MID 36KTL3-X",36,39.6,3,"PV-Wechselrichter","Nein","2024-05-14","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","200426161GZU-001","2022-04-12",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H645,1)=\"J\",LEFT(H645,2),LEFT(H645,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H645,1)=\"J\",RIGHT(H645,LEN(H645)-4),RIGHT(H645,LEN(H645)-6)),\"\"))","v":""}]
[50000561,"Growatt","MID 40KTL3-X",40,44,3,"PV-Wechselrichter","Nein","2024-05-14","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","200426161GZU-001","2022-04-12",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H646,1)=\"J\",LEFT(H646,2),LEFT(H646,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H646,1)=\"J\",RIGHT(H646,LEN(H646)-4),RIGHT(H646,LEN(H646)-6)),\"\"))","v":""}]
[50000562,"Growatt","MAX 50KTL3 LV",50,55.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H647,1)=\"J\",LEFT(H647,2),LEFT(H647,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H647,1)=\"J\",RIGHT(H647,LEN(H647)-4),RIGHT(H647,LEN(H647)-6)),\"\"))","v":""}]
[50000563,"Growatt","MAX 60KTL3 LV",60,66.599999999999994,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H648,1)=\"J\",LEFT(H648,2),LEFT(H648,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H648,1)=\"J\",RIGHT(H648,LEN(H648)-4),RIGHT(H648,LEN(H648)-6)),\"\"))","v":""}]
[50000564,"Growatt","MAX 70KTL3 LV",70,77.7,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H649,1)=\"J\",LEFT(H649,2),LEFT(H649,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H649,1)=\"J\",RIGHT(H649,LEN(H649)-4),RIGHT(H649,LEN(H649)-6)),\"\"))","v":""}]
[50000565,"Growatt","MAX 80KTL3 LV",80,88.8,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H650,1)=\"J\",LEFT(H650,2),LEFT(H650,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H650,1)=\"J\",RIGHT(H650,LEN(H650)-4),RIGHT(H650,LEN(H650)-6)),\"\"))","v":""}]
[50000566,"Guangzhou Sanjing Electric","H2-5K-T2",5,5.5,3,"Hybrid-Wechselrichter","Nein","2022-06-21",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H651,1)=\"J\",LEFT(H651,2),LEFT(H651,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H651,1)=\"J\",RIGHT(H651,LEN(H651)-4),RIGHT(H651,LEN(H651)-6)),\"\"))","v":""}]
[50000567,"Guangzhou Sanjing Electric","H2-6K-T2",6,6.6,3,"Hybrid-Wechselrichter","Nein","2022-06-21",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H652,1)=\"J\",LEFT(H652,2),LEFT(H652,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H652,1)=\"J\",RIGHT(H652,LEN(H652)-4),RIGHT(H652,LEN(H652)-6)),\"\"))","v":""}]
[50000568,"Guangzhou Sanjing Electric","H2-8K-T2",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein","2022-06-21",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H653,1)=\"J\",LEFT(H653,2),LEFT(H653,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H653,1)=\"J\",RIGHT(H653,LEN(H653)-4),RIGHT(H653,LEN(H653)-6)),\"\"))","v":""}]
[50000569,"Guangzhou Sanjing Electric","H2-10K-T2",10,11,3,"Hybrid-Wechselrichter","Nein","2022-06-21",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H654,1)=\"J\",LEFT(H654,2),LEFT(H654,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H654,1)=\"J\",RIGHT(H654,LEN(H654)-4),RIGHT(H654,LEN(H654)-6)),\"\"))","v":""}]
[50001756,"HICONICS","HEC1.5-T6Hr2",6,6.6,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.22.31855.01","2023-04-11",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H655,1)=\"J\",LEFT(H655,2),LEFT(H655,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H655,1)=\"J\",RIGHT(H655,LEN(H655)-4),RIGHT(H655,LEN(H655)-6)),\"\"))","v":"In Prüfung"}]
[50001755,"HICONICS","HEC1.5-T8Hr2",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.22.31855.01","2023-04-11",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H656,1)=\"J\",LEFT(H656,2),LEFT(H656,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H656,1)=\"J\",RIGHT(H656,LEN(H656)-4),RIGHT(H656,LEN(H656)-6)),\"\"))","v":"In Prüfung"}]
[50001757,"HICONICS","HEC1.5-T10Hr2",10,11,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.22.31855.01","2023-04-11",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H657,1)=\"J\",LEFT(H657,2),LEFT(H657,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H657,1)=\"J\",RIGHT(H657,LEN(H657)-4),RIGHT(H657,LEN(H657)-6)),\"\"))","v":"In Prüfung"}]
[50001758,"HICONICS","HEC1.5-T12Hr2",12,13.2,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.22.31855.01","2023-04-11",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H658,1)=\"J\",LEFT(H658,2),LEFT(H658,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H658,1)=\"J\",RIGHT(H658,LEN(H658)-4),RIGHT(H658,LEN(H658)-6)),\"\"))","v":"In Prüfung"}]
[50001759,"HICONICS","HEC1.5-T15Hr2",15,16.5,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-07","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"64.290.22.31855.01","2023-04-11",null,null,null,null,null,null,"ident zu MEGAREVO",null,null,null,null,{"$f":"IF(LEFT(H659,1)=\"J\",LEFT(H659,2),LEFT(H659,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H659,1)=\"J\",RIGHT(H659,LEN(H659)-4),RIGHT(H659,LEN(H659)-6)),\"\"))","v":"In Prüfung"}]
[50000570,"hoymiles","HM-250",null,0.25,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H660,1)=\"J\",LEFT(H660,2),LEFT(H660,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H660,1)=\"J\",RIGHT(H660,LEN(H660)-4),RIGHT(H660,LEN(H660)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000571,"hoymiles","HM-250A",null,0.25,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H661,1)=\"J\",LEFT(H661,2),LEFT(H661,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H661,1)=\"J\",RIGHT(H661,LEN(H661)-4),RIGHT(H661,LEN(H661)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000572,"hoymiles","HM-250T",null,0.25,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H662,1)=\"J\",LEFT(H662,2),LEFT(H662,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H662,1)=\"J\",RIGHT(H662,LEN(H662)-4),RIGHT(H662,LEN(H662)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000573,"hoymiles","HMS-250 -1T",null,0.25,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H663,1)=\"J\",LEFT(H663,2),LEFT(H663,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H663,1)=\"J\",RIGHT(H663,LEN(H663)-4),RIGHT(H663,LEN(H663)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000574,"hoymiles","HMS-250-1A",null,0.25,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H664,1)=\"J\",LEFT(H664,2),LEFT(H664,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H664,1)=\"J\",RIGHT(H664,LEN(H664)-4),RIGHT(H664,LEN(H664)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000575,"hoymiles","HMS-250-1D",null,0.25,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H665,1)=\"J\",LEFT(H665,2),LEFT(H665,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H665,1)=\"J\",RIGHT(H665,LEN(H665)-4),RIGHT(H665,LEN(H665)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000576,"hoymiles","HM-300 ",null,0.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H666,1)=\"J\",LEFT(H666,2),LEFT(H666,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H666,1)=\"J\",RIGHT(H666,LEN(H666)-4),RIGHT(H666,LEN(H666)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000577,"hoymiles","HM-300A",null,0.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H667,1)=\"J\",LEFT(H667,2),LEFT(H667,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H667,1)=\"J\",RIGHT(H667,LEN(H667)-4),RIGHT(H667,LEN(H667)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000578,"hoymiles","HM-300T",null,0.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H668,1)=\"J\",LEFT(H668,2),LEFT(H668,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H668,1)=\"J\",RIGHT(H668,LEN(H668)-4),RIGHT(H668,LEN(H668)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000579,"hoymiles","HMS-300 -1T",null,0.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H669,1)=\"J\",LEFT(H669,2),LEFT(H669,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H669,1)=\"J\",RIGHT(H669,LEN(H669)-4),RIGHT(H669,LEN(H669)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000580,"hoymiles","HMS-300-1A",null,0.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H670,1)=\"J\",LEFT(H670,2),LEFT(H670,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H670,1)=\"J\",RIGHT(H670,LEN(H670)-4),RIGHT(H670,LEN(H670)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000581,"hoymiles","HMS-300-1D",null,0.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H671,1)=\"J\",LEFT(H671,2),LEFT(H671,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H671,1)=\"J\",RIGHT(H671,LEN(H671)-4),RIGHT(H671,LEN(H671)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000582,"hoymiles","MI-300T",0.3,0.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H672,1)=\"J\",LEFT(H672,2),LEFT(H672,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H672,1)=\"J\",RIGHT(H672,LEN(H672)-4),RIGHT(H672,LEN(H672)-6)),\"\"))","v":""}]
[50000583,"hoymiles","MI-350",0.3,0.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H673,1)=\"J\",LEFT(H673,2),LEFT(H673,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H673,1)=\"J\",RIGHT(H673,LEN(H673)-4),RIGHT(H673,LEN(H673)-6)),\"\"))","v":""}]
[50000584,"hoymiles","MI-300 ",null,0.33,1,"PV-Wechselrichter","Nein","2022-09-08","Martin Bertsch",null,null,null,"2022-09-08","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H674,1)=\"J\",LEFT(H674,2),LEFT(H674,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H674,1)=\"J\",RIGHT(H674,LEN(H674)-4),RIGHT(H674,LEN(H674)-6)),\"\"))","v":""}]
[50000585,"hoymiles","HM-350 ",null,0.35,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer",null,"2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H675,1)=\"J\",LEFT(H675,2),LEFT(H675,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H675,1)=\"J\",RIGHT(H675,LEN(H675)-4),RIGHT(H675,LEN(H675)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000586,"hoymiles","HM-350A ",null,0.35,1,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H676,1)=\"J\",LEFT(H676,2),LEFT(H676,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H676,1)=\"J\",RIGHT(H676,LEN(H676)-4),RIGHT(H676,LEN(H676)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000587,"hoymiles","MI-350T",0.35,0.35,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H677,1)=\"J\",LEFT(H677,2),LEFT(H677,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H677,1)=\"J\",RIGHT(H677,LEN(H677)-4),RIGHT(H677,LEN(H677)-6)),\"\"))","v":""}]
[50000588,"hoymiles","HM-400 ",null,0.4,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H678,1)=\"J\",LEFT(H678,2),LEFT(H678,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H678,1)=\"J\",RIGHT(H678,LEN(H678)-4),RIGHT(H678,LEN(H678)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000589,"hoymiles","HM-400A",null,0.4,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H679,1)=\"J\",LEFT(H679,2),LEFT(H679,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H679,1)=\"J\",RIGHT(H679,LEN(H679)-4),RIGHT(H679,LEN(H679)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000590,"hoymiles","HM-400T",null,0.4,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H680,1)=\"J\",LEFT(H680,2),LEFT(H680,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H680,1)=\"J\",RIGHT(H680,LEN(H680)-4),RIGHT(H680,LEN(H680)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000591,"hoymiles","HMS-400-1A",null,0.4,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-06-01","Martin Bertsch",null,null,null,null,null,null,null,null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H681,1)=\"J\",LEFT(H681,2),LEFT(H681,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H681,1)=\"J\",RIGHT(H681,LEN(H681)-4),RIGHT(H681,LEN(H681)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000592,"hoymiles","HMS-400-1D",null,0.4,1,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H682,1)=\"J\",LEFT(H682,2),LEFT(H682,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H682,1)=\"J\",RIGHT(H682,LEN(H682)-4),RIGHT(H682,LEN(H682)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000593,"hoymiles","HMS-400-1T",null,0.4,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-06-01","Martin Bertsch",null,null,null,null,null,null,null,null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H683,1)=\"J\",LEFT(H683,2),LEFT(H683,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H683,1)=\"J\",RIGHT(H683,LEN(H683)-4),RIGHT(H683,LEN(H683)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000594,"hoymiles","MI-400",0.4,0.4,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H684,1)=\"J\",LEFT(H684,2),LEFT(H684,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H684,1)=\"J\",RIGHT(H684,LEN(H684)-4),RIGHT(H684,LEN(H684)-6)),\"\"))","v":""}]
[50000595,"hoymiles","MI-400T",0.4,0.4,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H685,1)=\"J\",LEFT(H685,2),LEFT(H685,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H685,1)=\"J\",RIGHT(H685,LEN(H685)-4),RIGHT(H685,LEN(H685)-6)),\"\"))","v":""}]
[50000596,"hoymiles","HMS-450-1A",null,0.45,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-06-01","Martin Bertsch",null,null,null,null,null,null,null,null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H686,1)=\"J\",LEFT(H686,2),LEFT(H686,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H686,1)=\"J\",RIGHT(H686,LEN(H686)-4),RIGHT(H686,LEN(H686)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000597,"hoymiles","HMS-450-1D",null,0.45,1,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H687,1)=\"J\",LEFT(H687,2),LEFT(H687,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H687,1)=\"J\",RIGHT(H687,LEN(H687)-4),RIGHT(H687,LEN(H687)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000598,"hoymiles","HMS-450-1T",null,0.45,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-06-01","Martin Bertsch",null,null,null,null,null,null,null,null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H688,1)=\"J\",LEFT(H688,2),LEFT(H688,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H688,1)=\"J\",RIGHT(H688,LEN(H688)-4),RIGHT(H688,LEN(H688)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000599,"hoymiles","HM-500 ",null,0.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H689,1)=\"J\",LEFT(H689,2),LEFT(H689,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H689,1)=\"J\",RIGHT(H689,LEN(H689)-4),RIGHT(H689,LEN(H689)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000600,"hoymiles","HM-500-2D",null,0.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H690,1)=\"J\",LEFT(H690,2),LEFT(H690,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H690,1)=\"J\",RIGHT(H690,LEN(H690)-4),RIGHT(H690,LEN(H690)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000601,"hoymiles","HM-500-2T",null,0.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H691,1)=\"J\",LEFT(H691,2),LEFT(H691,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H691,1)=\"J\",RIGHT(H691,LEN(H691)-4),RIGHT(H691,LEN(H691)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000602,"hoymiles","HM-500T",null,0.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H692,1)=\"J\",LEFT(H692,2),LEFT(H692,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H692,1)=\"J\",RIGHT(H692,LEN(H692)-4),RIGHT(H692,LEN(H692)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000603,"hoymiles","HMS-500-1A",null,0.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-06-01","Martin Bertsch",null,null,null,null,null,null,null,null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H693,1)=\"J\",LEFT(H693,2),LEFT(H693,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H693,1)=\"J\",RIGHT(H693,LEN(H693)-4),RIGHT(H693,LEN(H693)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000604,"hoymiles","HMS-500-1D",null,0.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","6094000.50","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H694,1)=\"J\",LEFT(H694,2),LEFT(H694,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H694,1)=\"J\",RIGHT(H694,LEN(H694)-4),RIGHT(H694,LEN(H694)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000605,"hoymiles","HMS-500-1T",null,0.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-06-01","Martin Bertsch",null,null,null,null,null,null,null,null,"OK","Markus Radauer","BL-DG2270018-B01","2022-11-23","nicht vorhanden","OK","drei Setups je nach Blindleistungsstrategie",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H695,1)=\"J\",LEFT(H695,2),LEFT(H695,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H695,1)=\"J\",RIGHT(H695,LEN(H695)-4),RIGHT(H695,LEN(H695)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000606,"hoymiles","HM-600 ",null,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H696,1)=\"J\",LEFT(H696,2),LEFT(H696,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H696,1)=\"J\",RIGHT(H696,LEN(H696)-4),RIGHT(H696,LEN(H696)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000607,"hoymiles","HM-600-2D",null,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H697,1)=\"J\",LEFT(H697,2),LEFT(H697,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H697,1)=\"J\",RIGHT(H697,LEN(H697)-4),RIGHT(H697,LEN(H697)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000608,"hoymiles","HM-600-2T",null,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H698,1)=\"J\",LEFT(H698,2),LEFT(H698,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H698,1)=\"J\",RIGHT(H698,LEN(H698)-4),RIGHT(H698,LEN(H698)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000609,"hoymiles","HM-600T",null,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H699,1)=\"J\",LEFT(H699,2),LEFT(H699,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H699,1)=\"J\",RIGHT(H699,LEN(H699)-4),RIGHT(H699,LEN(H699)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000610,"hoymiles","HMS-600-2T",null,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180296-B03","2022-11-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H700,1)=\"J\",LEFT(H700,2),LEFT(H700,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H700,1)=\"J\",RIGHT(H700,LEN(H700)-4),RIGHT(H700,LEN(H700)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000611,"hoymiles","MI-600 ",null,0.6,1,"PV-Wechselrichter","Nein","2022-09-08","Martin Bertsch",null,null,null,"2022-09-08","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Micro-Wechselrichter 1~ - zulässig bis 0,8 kW Sum. Pn - KONFORM","F","F",null,null,{"$f":"IF(LEFT(H701,1)=\"J\",LEFT(H701,2),LEFT(H701,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H701,1)=\"J\",RIGHT(H701,LEN(H701)-4),RIGHT(H701,LEN(H701)-6)),\"\"))","v":""}]
[50000612,"hoymiles","HM-700 ",null,0.7,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H702,1)=\"J\",LEFT(H702,2),LEFT(H702,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H702,1)=\"J\",RIGHT(H702,LEN(H702)-4),RIGHT(H702,LEN(H702)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000613,"hoymiles","HM-700-2D",null,0.7,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H703,1)=\"J\",LEFT(H703,2),LEFT(H703,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H703,1)=\"J\",RIGHT(H703,LEN(H703)-4),RIGHT(H703,LEN(H703)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000614,"hoymiles","HM-700-2T",null,0.7,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H704,1)=\"J\",LEFT(H704,2),LEFT(H704,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H704,1)=\"J\",RIGHT(H704,LEN(H704)-4),RIGHT(H704,LEN(H704)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000615,"hoymiles","HM-700T",null,0.7,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H705,1)=\"J\",LEFT(H705,2),LEFT(H705,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H705,1)=\"J\",RIGHT(H705,LEN(H705)-4),RIGHT(H705,LEN(H705)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000616,"hoymiles","HMS-700-2T",null,0.7,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180296-B03","2022-11-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H706,1)=\"J\",LEFT(H706,2),LEFT(H706,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H706,1)=\"J\",RIGHT(H706,LEN(H706)-4),RIGHT(H706,LEN(H706)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000617,"hoymiles","MI-700",0.7,0.7,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H707,1)=\"J\",LEFT(H707,2),LEFT(H707,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H707,1)=\"J\",RIGHT(H707,LEN(H707)-4),RIGHT(H707,LEN(H707)-6)),\"\"))","v":""}]
[50000618,"hoymiles","HM-800 ",null,0.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H708,1)=\"J\",LEFT(H708,2),LEFT(H708,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H708,1)=\"J\",RIGHT(H708,LEN(H708)-4),RIGHT(H708,LEN(H708)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000619,"hoymiles","HM-800-2D",null,0.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H709,1)=\"J\",LEFT(H709,2),LEFT(H709,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H709,1)=\"J\",RIGHT(H709,LEN(H709)-4),RIGHT(H709,LEN(H709)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000620,"hoymiles","HM-800-2T",null,0.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H710,1)=\"J\",LEFT(H710,2),LEFT(H710,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H710,1)=\"J\",RIGHT(H710,LEN(H710)-4),RIGHT(H710,LEN(H710)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000621,"hoymiles","HM-800T",null,0.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.51","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H711,1)=\"J\",LEFT(H711,2),LEFT(H711,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H711,1)=\"J\",RIGHT(H711,LEN(H711)-4),RIGHT(H711,LEN(H711)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000622,"hoymiles","HMS-800-2T",null,0.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180296-B03","2022-11-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H712,1)=\"J\",LEFT(H712,2),LEFT(H712,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H712,1)=\"J\",RIGHT(H712,LEN(H712)-4),RIGHT(H712,LEN(H712)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000623,"hoymiles","MI-800",0.8,0.8,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H713,1)=\"J\",LEFT(H713,2),LEFT(H713,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H713,1)=\"J\",RIGHT(H713,LEN(H713)-4),RIGHT(H713,LEN(H713)-6)),\"\"))","v":""}]
[50000624,"hoymiles","HMS-900-2T",null,0.9,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180296-B03","2022-11-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H714,1)=\"J\",LEFT(H714,2),LEFT(H714,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H714,1)=\"J\",RIGHT(H714,LEN(H714)-4),RIGHT(H714,LEN(H714)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000625,"hoymiles","HM-1000 ",null,1,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H715,1)=\"J\",LEFT(H715,2),LEFT(H715,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H715,1)=\"J\",RIGHT(H715,LEN(H715)-4),RIGHT(H715,LEN(H715)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000626,"hoymiles","HM-1000-4T",null,1,1,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H716,1)=\"J\",LEFT(H716,2),LEFT(H716,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H716,1)=\"J\",RIGHT(H716,LEN(H716)-4),RIGHT(H716,LEN(H716)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000627,"hoymiles","HM-1000T",null,1,1,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H717,1)=\"J\",LEFT(H717,2),LEFT(H717,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H717,1)=\"J\",RIGHT(H717,LEN(H717)-4),RIGHT(H717,LEN(H717)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000628,"hoymiles","HMS-1000-2T",null,1,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180296-B03","2022-11-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H718,1)=\"J\",LEFT(H718,2),LEFT(H718,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H718,1)=\"J\",RIGHT(H718,LEN(H718)-4),RIGHT(H718,LEN(H718)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000629,"hoymiles","HMS-1000-4D",null,1,1,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,null,null,null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H719,1)=\"J\",LEFT(H719,2),LEFT(H719,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H719,1)=\"J\",RIGHT(H719,LEN(H719)-4),RIGHT(H719,LEN(H719)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000630,"hoymiles","MI-1000",1,1,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H720,1)=\"J\",LEFT(H720,2),LEFT(H720,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H720,1)=\"J\",RIGHT(H720,LEN(H720)-4),RIGHT(H720,LEN(H720)-6)),\"\"))","v":""}]
[50000631,"hoymiles","MI-1000T",1,1,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H721,1)=\"J\",LEFT(H721,2),LEFT(H721,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H721,1)=\"J\",RIGHT(H721,LEN(H721)-4),RIGHT(H721,LEN(H721)-6)),\"\"))","v":""}]
[50000632,"hoymiles","HM-1200 ",null,1.2,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H722,1)=\"J\",LEFT(H722,2),LEFT(H722,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H722,1)=\"J\",RIGHT(H722,LEN(H722)-4),RIGHT(H722,LEN(H722)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000633,"hoymiles","HM-1200-4D",null,1.2,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H723,1)=\"J\",LEFT(H723,2),LEFT(H723,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H723,1)=\"J\",RIGHT(H723,LEN(H723)-4),RIGHT(H723,LEN(H723)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000634,"hoymiles","HM-1200-4T",null,1.2,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H724,1)=\"J\",LEFT(H724,2),LEFT(H724,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H724,1)=\"J\",RIGHT(H724,LEN(H724)-4),RIGHT(H724,LEN(H724)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000635,"hoymiles","HM-1200T",null,1.2,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H725,1)=\"J\",LEFT(H725,2),LEFT(H725,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H725,1)=\"J\",RIGHT(H725,LEN(H725)-4),RIGHT(H725,LEN(H725)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000636,"hoymiles","MI-1200",1.2,1.2,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H726,1)=\"J\",LEFT(H726,2),LEFT(H726,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H726,1)=\"J\",RIGHT(H726,LEN(H726)-4),RIGHT(H726,LEN(H726)-6)),\"\"))","v":""}]
[50000637,"hoymiles","MI-1200T",1.2,1.2,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H727,1)=\"J\",LEFT(H727,2),LEFT(H727,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H727,1)=\"J\",RIGHT(H727,LEN(H727)-4),RIGHT(H727,LEN(H727)-6)),\"\"))","v":""}]
[50000638,"hoymiles","HMS-1400C-4T",1.4,1.4,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Martin Bertsch (OE)","BMH-ESH-P22110043","2022-12-20","nicht vorhanden","nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H728,1)=\"J\",LEFT(H728,2),LEFT(H728,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H728,1)=\"J\",RIGHT(H728,LEN(H728)-4),RIGHT(H728,LEN(H728)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000639,"hoymiles","HM-1500 ",null,1.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H729,1)=\"J\",LEFT(H729,2),LEFT(H729,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H729,1)=\"J\",RIGHT(H729,LEN(H729)-4),RIGHT(H729,LEN(H729)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000640,"hoymiles","HM-1500-4D",null,1.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H730,1)=\"J\",LEFT(H730,2),LEFT(H730,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H730,1)=\"J\",RIGHT(H730,LEN(H730)-4),RIGHT(H730,LEN(H730)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000641,"hoymiles","HM-1500-4T",null,1.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H731,1)=\"J\",LEFT(H731,2),LEFT(H731,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H731,1)=\"J\",RIGHT(H731,LEN(H731)-4),RIGHT(H731,LEN(H731)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000642,"hoymiles","HM-1500T",null,1.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-06-04","Martin Bertsch","2021-04-10",null,null,null,null,"Nein","Nein",null,"OK","Markus Radauer","6091793.50 V1.1","2021-04-10",null,"OK","drei Setups je nach Blindleistungsstrategie",null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H732,1)=\"J\",LEFT(H732,2),LEFT(H732,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H732,1)=\"J\",RIGHT(H732,LEN(H732)-4),RIGHT(H732,LEN(H732)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000643,"hoymiles","MI-1500",1.5,1.5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H733,1)=\"J\",LEFT(H733,2),LEFT(H733,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H733,1)=\"J\",RIGHT(H733,LEN(H733)-4),RIGHT(H733,LEN(H733)-6)),\"\"))","v":""}]
[50000644,"hoymiles","MI-1500T",1.5,1.5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H734,1)=\"J\",LEFT(H734,2),LEFT(H734,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H734,1)=\"J\",RIGHT(H734,LEN(H734)-4),RIGHT(H734,LEN(H734)-6)),\"\"))","v":""}]
[50000645,"hoymiles","HMS-1600-4T",null,1.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180295-B04","2023-01-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H735,1)=\"J\",LEFT(H735,2),LEFT(H735,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H735,1)=\"J\",RIGHT(H735,LEN(H735)-4),RIGHT(H735,LEN(H735)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000646,"hoymiles","HMS-1600B-4T",null,1.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180295-B04","2023-01-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H736,1)=\"J\",LEFT(H736,2),LEFT(H736,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H736,1)=\"J\",RIGHT(H736,LEN(H736)-4),RIGHT(H736,LEN(H736)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000647,"hoymiles","HMS-1600C-4T",1.6,1.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Martin Bertsch (OE)","BMH-ESH-P22110043","2022-12-20","nicht vorhanden","nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H737,1)=\"J\",LEFT(H737,2),LEFT(H737,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H737,1)=\"J\",RIGHT(H737,LEN(H737)-4),RIGHT(H737,LEN(H737)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002079,"hoymiles","HMT-1600-4T",1.6,1.6,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-01-29",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden",null,"BMH-ESH-P22120957","2023-10-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H738,1)=\"J\",LEFT(H738,2),LEFT(H738,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H738,1)=\"J\",RIGHT(H738,LEN(H738)-4),RIGHT(H738,LEN(H738)-6)),\"\"))","v":"befristet"}]
[50000648,"hoymiles","HMS-1800-4T",null,1.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180295-B04","2023-01-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H739,1)=\"J\",LEFT(H739,2),LEFT(H739,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H739,1)=\"J\",RIGHT(H739,LEN(H739)-4),RIGHT(H739,LEN(H739)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000649,"hoymiles","HMS-1800B-4T",null,1.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180295-B04","2023-01-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H740,1)=\"J\",LEFT(H740,2),LEFT(H740,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H740,1)=\"J\",RIGHT(H740,LEN(H740)-4),RIGHT(H740,LEN(H740)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000650,"hoymiles","HMS-1800C-4T",1.8,1.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Martin Bertsch (OE)","BMH-ESH-P22110043","2022-12-20","nicht vorhanden","nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H741,1)=\"J\",LEFT(H741,2),LEFT(H741,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H741,1)=\"J\",RIGHT(H741,LEN(H741)-4),RIGHT(H741,LEN(H741)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002078,"hoymiles","HMT-1800-4T",1.8,1.8,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-01-29",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden",null,"BMH-ESH-P22120957","2023-10-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H742,1)=\"J\",LEFT(H742,2),LEFT(H742,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H742,1)=\"J\",RIGHT(H742,LEN(H742)-4),RIGHT(H742,LEN(H742)-6)),\"\"))","v":"befristet"}]
[50000651,"hoymiles","HMT-1800-6T",1.8,1.8,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-07-28",null,"2024-09-30",null,"Frist wurde um 1 Monat verlängert; Testgerät wurde geliefert",null,null,null,"OK","Michael Tippmann","6117119.50","2022-04-06",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H743,1)=\"J\",LEFT(H743,2),LEFT(H743,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H743,1)=\"J\",RIGHT(H743,LEN(H743)-4),RIGHT(H743,LEN(H743)-6)),\"\"))","v":"befristet"}]
[50000652,"hoymiles","HMS-2000-4T",null,2,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180295-B04","2023-01-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H744,1)=\"J\",LEFT(H744,2),LEFT(H744,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H744,1)=\"J\",RIGHT(H744,LEN(H744)-4),RIGHT(H744,LEN(H744)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000653,"hoymiles","HMS-2000B-4T",null,2,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Markus Radauer","BL-DG2180295-B04","2023-01-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H745,1)=\"J\",LEFT(H745,2),LEFT(H745,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H745,1)=\"J\",RIGHT(H745,LEN(H745)-4),RIGHT(H745,LEN(H745)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50000654,"hoymiles","HMS-2000C-4T",2,2,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-05-26","Martin Bertsch","2023-05-23",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Martin Bertsch (OE)","BMH-ESH-P22110043","2022-12-20","nicht vorhanden","nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H746,1)=\"J\",LEFT(H746,2),LEFT(H746,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H746,1)=\"J\",RIGHT(H746,LEN(H746)-4),RIGHT(H746,LEN(H746)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002077,"hoymiles","HMT-2000-4T",2,2,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-01-29",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden",null,"BMH-ESH-P22120957","2023-10-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H747,1)=\"J\",LEFT(H747,2),LEFT(H747,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H747,1)=\"J\",RIGHT(H747,LEN(H747)-4),RIGHT(H747,LEN(H747)-6)),\"\"))","v":"befristet"}]
[50000655,"hoymiles","HMT-2250-6T",2.25,2.25,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-07-28",null,"2024-09-30",null,"Frist wurde um 1 Monat verlängert; Testgerät wurde geliefert",null,null,null,"OK","Michael Tippmann","6117119.50","2022-04-06",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H748,1)=\"J\",LEFT(H748,2),LEFT(H748,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H748,1)=\"J\",RIGHT(H748,LEN(H748)-4),RIGHT(H748,LEN(H748)-6)),\"\"))","v":"befristet"}]
[50000656,"hoymiles","HYT-5.0HV-EUG1",5,5.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-17",null,"2024-09-30",null,"finale FW Änderung zu überprüfen; Test erfolgt mit Modulwechselrichter","Ja","Nein",null,"OK","Markus Radauer","BL-DG2290901-B01","2023-01-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H749,1)=\"J\",LEFT(H749,2),LEFT(H749,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H749,1)=\"J\",RIGHT(H749,LEN(H749)-4),RIGHT(H749,LEN(H749)-6)),\"\"))","v":"befristet"}]
[50000657,"hoymiles","HYT-6.0HV-EUG1",6,6.6,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-17",null,"2024-09-30",null,"finale FW Änderung zu überprüfen; Test erfolgt mit Modulwechselrichter","Ja","Nein",null,"OK","Markus Radauer","BL-DG2290901-B01","2023-01-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H750,1)=\"J\",LEFT(H750,2),LEFT(H750,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H750,1)=\"J\",RIGHT(H750,LEN(H750)-4),RIGHT(H750,LEN(H750)-6)),\"\"))","v":"befristet"}]
[50000658,"hoymiles","HYT-8.0HV-EUG1",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-17",null,"2024-09-30",null,"finale FW Änderung zu überprüfen; Test erfolgt mit Modulwechselrichter","Ja","Nein",null,"OK","Markus Radauer","BL-DG2290901-B01","2023-01-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H751,1)=\"J\",LEFT(H751,2),LEFT(H751,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H751,1)=\"J\",RIGHT(H751,LEN(H751)-4),RIGHT(H751,LEN(H751)-6)),\"\"))","v":"befristet"}]
[50000659,"hoymiles","HYT-10.0HV-EUG1",10,11,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-17",null,"2024-09-30",null,"finale FW Änderung zu überprüfen; Test erfolgt mit Modulwechselrichter","Ja","Nein",null,"OK","Markus Radauer","BL-DG2290901-B01","2023-01-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H752,1)=\"J\",LEFT(H752,2),LEFT(H752,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H752,1)=\"J\",RIGHT(H752,LEN(H752)-4),RIGHT(H752,LEN(H752)-6)),\"\"))","v":"befristet"}]
[50000660,"hoymiles","HYT-12.0HV-EUG1",12,13.2,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-17",null,"2024-09-30",null,"finale FW Änderung zu überprüfen; Test erfolgt mit Modulwechselrichter","Ja","Nein",null,"OK","Markus Radauer","BL-DG2290901-B01","2023-01-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H753,1)=\"J\",LEFT(H753,2),LEFT(H753,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H753,1)=\"J\",RIGHT(H753,LEN(H753)-4),RIGHT(H753,LEN(H753)-6)),\"\"))","v":"befristet"}]
[50000661,"Huawei","SUN2000-2KTL-L1 ",2,2.2000000000000002,1,"Hybrid-Wechselrichter","Ja - <= 16A Anlage","2023-07-24","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein",null,"OK","Martin Bertsch (OE)","PVAT191217N030-R2","2023-06-13","nicht vorhanden","OK",null,null,null,null,"Hybridwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H754,1)=\"J\",LEFT(H754,2),LEFT(H754,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H754,1)=\"J\",RIGHT(H754,LEN(H754)-4),RIGHT(H754,LEN(H754)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000662,"Huawei","SUN2000-3KTL_M0/M1 ",3.3,3.3,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT191219N026","2020-06-24",null,"OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H755,1)=\"J\",LEFT(H755,2),LEFT(H755,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H755,1)=\"J\",RIGHT(H755,LEN(H755)-4),RIGHT(H755,LEN(H755)-6)),\"\"))","v":""}]
[50000663,"Huawei","SUN2000-3KTL-L1 ",3,3.3,1,"Hybrid-Wechselrichter","Ja - <= 16A Anlage","2023-07-24","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein",null,"OK","Martin Bertsch (OE)","PVAT191217N030-R2","2023-06-13","nicht vorhanden","OK",null,null,null,null,"Hybridwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H756,1)=\"J\",LEFT(H756,2),LEFT(H756,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H756,1)=\"J\",RIGHT(H756,LEN(H756)-4),RIGHT(H756,LEN(H756)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000664,"Huawei","SUN2000-3.68KTL-L1 ",3.68,3.68,1,"Hybrid-Wechselrichter","Ja - <= 16A Anlage","2023-07-24","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein",null,"OK","Martin Bertsch (OE)","PVAT191217N030-R2","2023-06-13","nicht vorhanden","OK",null,null,null,null,"Hybridwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H757,1)=\"J\",LEFT(H757,2),LEFT(H757,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H757,1)=\"J\",RIGHT(H757,LEN(H757)-4),RIGHT(H757,LEN(H757)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000665,"Huawei","SUN2000-4KTL-L1",4,4.4000000000000004,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H758,1)=\"J\",LEFT(H758,2),LEFT(H758,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H758,1)=\"J\",RIGHT(H758,LEN(H758)-4),RIGHT(H758,LEN(H758)-6)),\"\"))","v":""}]
[50000666,"Huawei","SUN2000-4KTL-M0/M1 ",4.4000000000000004,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT191219N026","2020-06-24",null,"OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H759,1)=\"J\",LEFT(H759,2),LEFT(H759,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H759,1)=\"J\",RIGHT(H759,LEN(H759)-4),RIGHT(H759,LEN(H759)-6)),\"\"))","v":""}]
[50000667,"Huawei","SUN2000-4.6KTL-L1",4.5999999999999996,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H760,1)=\"J\",LEFT(H760,2),LEFT(H760,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H760,1)=\"J\",RIGHT(H760,LEN(H760)-4),RIGHT(H760,LEN(H760)-6)),\"\"))","v":""}]
[50002266,"Huawei","SUN2000-5K-MAP0 (optional mit SmartGuard-63A-T0)",5,5.5,3,"Hybrid-Wechselrichter","Ja","2024-05-26","Martin Bertsch","2024-05-26",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"240122192GZU-001","2024-05-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H761,1)=\"J\",LEFT(H761,2),LEFT(H761,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H761,1)=\"J\",RIGHT(H761,LEN(H761)-4),RIGHT(H761,LEN(H761)-6)),\"\"))","v":""}]
[50000668,"Huawei","SUN2000-5KTL-L1",5,5.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H762,1)=\"J\",LEFT(H762,2),LEFT(H762,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H762,1)=\"J\",RIGHT(H762,LEN(H762)-4),RIGHT(H762,LEN(H762)-6)),\"\"))","v":""}]
[50000669,"Huawei","SUN2000-5KTL-M0/M1 ",5.5,5.5,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT191219N026","2020-06-24",null,"OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H763,1)=\"J\",LEFT(H763,2),LEFT(H763,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H763,1)=\"J\",RIGHT(H763,LEN(H763)-4),RIGHT(H763,LEN(H763)-6)),\"\"))","v":""}]
[50000670,"Huawei","SUN2000-6KTL-L1",6,6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H764,1)=\"J\",LEFT(H764,2),LEFT(H764,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H764,1)=\"J\",RIGHT(H764,LEN(H764)-4),RIGHT(H764,LEN(H764)-6)),\"\"))","v":""}]
[50002267,"Huawei","SUN2000-6K-MAP0 (optional mit SmartGuard-63A-T0)",6,6.6,3,"Hybrid-Wechselrichter","Ja","2024-05-26","Martin Bertsch","2024-05-26",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"240122192GZU-001","2024-05-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H765,1)=\"J\",LEFT(H765,2),LEFT(H765,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H765,1)=\"J\",RIGHT(H765,LEN(H765)-4),RIGHT(H765,LEN(H765)-6)),\"\"))","v":""}]
[50000671,"Huawei","SUN2000-6KTL-M0/M1 ",6.6,6.6,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT191219N026","2020-06-24",null,"OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H766,1)=\"J\",LEFT(H766,2),LEFT(H766,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H766,1)=\"J\",RIGHT(H766,LEN(H766)-4),RIGHT(H766,LEN(H766)-6)),\"\"))","v":""}]
[50002268,"Huawei","SUN2000-8K-MAP0 (optional mit SmartGuard-63A-T0)",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2024-05-26","Martin Bertsch","2024-05-26",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"240122192GZU-001","2024-05-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H767,1)=\"J\",LEFT(H767,2),LEFT(H767,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H767,1)=\"J\",RIGHT(H767,LEN(H767)-4),RIGHT(H767,LEN(H767)-6)),\"\"))","v":""}]
[50000672,"Huawei","SUN2000-8KTL-M0/M1/M2 ",8.8000000000000007,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT191219N018","2020-06-24",null,"OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H768,1)=\"J\",LEFT(H768,2),LEFT(H768,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H768,1)=\"J\",RIGHT(H768,LEN(H768)-4),RIGHT(H768,LEN(H768)-6)),\"\"))","v":""}]
[50002271,"Huawei","SUN5000-8K-MAP0 (optional mit SmartGuard-63A-T0)",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2024-05-26","Martin Bertsch","2024-05-26",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"240122192GZU-001","2024-05-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H769,1)=\"J\",LEFT(H769,2),LEFT(H769,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H769,1)=\"J\",RIGHT(H769,LEN(H769)-4),RIGHT(H769,LEN(H769)-6)),\"\"))","v":""}]
[50002269,"Huawei","SUN2000-10K-MAP0 (optional mit SmartGuard-63A-T0)",10,11,3,"Hybrid-Wechselrichter","Ja","2024-05-26","Martin Bertsch","2024-05-26",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"240122192GZU-001","2024-05-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H770,1)=\"J\",LEFT(H770,2),LEFT(H770,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H770,1)=\"J\",RIGHT(H770,LEN(H770)-4),RIGHT(H770,LEN(H770)-6)),\"\"))","v":""}]
[50000673,"Huawei","SUN2000-10KTL-M0/M1/M2",11,11,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT191219N018","2020-06-24",null,"OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H771,1)=\"J\",LEFT(H771,2),LEFT(H771,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H771,1)=\"J\",RIGHT(H771,LEN(H771)-4),RIGHT(H771,LEN(H771)-6)),\"\"))","v":""}]
[50002270,"Huawei","SUN2000-12K-MAP0 (optional mit SmartGuard-63A-T0)",12,13.2,3,"Hybrid-Wechselrichter","Ja","2024-05-26","Martin Bertsch","2024-05-26",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"240122192GZU-001","2024-05-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H772,1)=\"J\",LEFT(H772,2),LEFT(H772,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H772,1)=\"J\",RIGHT(H772,LEN(H772)-4),RIGHT(H772,LEN(H772)-6)),\"\"))","v":""}]
[50000676,"Huawei","SUN2000-12K-MB0",13.2,13.2,3,"Hybrid-Wechselrichter","Ja","2024-02-28","Martin Bertsch","2023-05-03",null,null,null,null,"Ja","Ja",null,"OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H773,1)=\"J\",LEFT(H773,2),LEFT(H773,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H773,1)=\"J\",RIGHT(H773,LEN(H773)-4),RIGHT(H773,LEN(H773)-6)),\"\"))","v":""}]
[50000674,"Huawei","SUN2000-12KTL-M0/M2 ",12,13.2,3,"PV-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT191219N018","2020-06-24","Vorhanden","OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H774,1)=\"J\",LEFT(H774,2),LEFT(H774,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H774,1)=\"J\",RIGHT(H774,LEN(H774)-4),RIGHT(H774,LEN(H774)-6)),\"\"))","v":""}]
[50000675,"Huawei","SUN2000-12KTL-M5",13.2,13.2,3,"PV-Wechselrichter","Ja","2023-09-21","Martin Bertsch","2023-05-03",null,null,null,null,"Nein","Ja","Nein","OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H775,1)=\"J\",LEFT(H775,2),LEFT(H775,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H775,1)=\"J\",RIGHT(H775,LEN(H775)-4),RIGHT(H775,LEN(H775)-6)),\"\"))","v":""}]
[50002272,"Huawei","SUN5000-12K-MAP0 (optional mit SmartGuard-63A-T0)",12,13.2,3,"Hybrid-Wechselrichter","Ja","2024-05-26","Martin Bertsch","2024-05-26",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"240122192GZU-001","2024-05-10","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H776,1)=\"J\",LEFT(H776,2),LEFT(H776,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H776,1)=\"J\",RIGHT(H776,LEN(H776)-4),RIGHT(H776,LEN(H776)-6)),\"\"))","v":""}]
[50000679,"Huawei","SUN2000-15K-MB0",16.5,16.5,3,"Hybrid-Wechselrichter","Ja","2024-02-28","Martin Bertsch","2023-05-03",null,null,null,null,"Ja","Ja",null,"OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H777,1)=\"J\",LEFT(H777,2),LEFT(H777,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H777,1)=\"J\",RIGHT(H777,LEN(H777)-4),RIGHT(H777,LEN(H777)-6)),\"\"))","v":""}]
[50000677,"Huawei","SUN2000-15KTL-M0/M2/M3 ",15,16.5,3,"PV-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200511N092","2020-10-15","Vorhanden","OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H778,1)=\"J\",LEFT(H778,2),LEFT(H778,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H778,1)=\"J\",RIGHT(H778,LEN(H778)-4),RIGHT(H778,LEN(H778)-6)),\"\"))","v":""}]
[50000678,"Huawei","SUN2000-15KTL-M5",16.5,16.5,3,"PV-Wechselrichter","Ja","2023-09-21","Martin Bertsch","2023-05-03",null,null,null,null,"Nein","Ja","Nein","OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H779,1)=\"J\",LEFT(H779,2),LEFT(H779,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H779,1)=\"J\",RIGHT(H779,LEN(H779)-4),RIGHT(H779,LEN(H779)-6)),\"\"))","v":""}]
[50000682,"Huawei","SUN2000-17K-MB0",18.7,18.7,3,"Hybrid-Wechselrichter","Ja","2024-02-28","Martin Bertsch","2023-05-03",null,null,null,null,"Ja","Ja",null,"OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H780,1)=\"J\",LEFT(H780,2),LEFT(H780,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H780,1)=\"J\",RIGHT(H780,LEN(H780)-4),RIGHT(H780,LEN(H780)-6)),\"\"))","v":""}]
[50000680,"Huawei","SUN2000-17KTL-M0/M2/M3 ",17,18.7,3,"PV-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200511N092","2020-10-15","Vorhanden","OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H781,1)=\"J\",LEFT(H781,2),LEFT(H781,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H781,1)=\"J\",RIGHT(H781,LEN(H781)-4),RIGHT(H781,LEN(H781)-6)),\"\"))","v":""}]
[50000681,"Huawei","SUN2000-17KTL-M5",18.7,18.7,3,"PV-Wechselrichter","Ja","2023-09-21","Martin Bertsch","2023-05-03",null,null,null,null,"Nein","Ja","Nein","OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H782,1)=\"J\",LEFT(H782,2),LEFT(H782,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H782,1)=\"J\",RIGHT(H782,LEN(H782)-4),RIGHT(H782,LEN(H782)-6)),\"\"))","v":""}]
[50000685,"Huawei","SUN2000-20K-MB0",22,22,3,"Hybrid-Wechselrichter","Ja","2024-02-28","Martin Bertsch","2023-05-03",null,null,null,null,"Ja","Ja",null,"OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H783,1)=\"J\",LEFT(H783,2),LEFT(H783,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H783,1)=\"J\",RIGHT(H783,LEN(H783)-4),RIGHT(H783,LEN(H783)-6)),\"\"))","v":""}]
[50000683,"Huawei","SUN2000-20KTL-M0/M2/M3 ",20,22,3,"PV-Wechselrichter","Ja",null,null,"2021-11-29","SUN2000MAV100R001C00SPC139",null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200511N092","2020-10-15","Vorhanden","OK","nicht vorhanden","Vorhanden","2021-11-29",null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H784,1)=\"J\",LEFT(H784,2),LEFT(H784,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H784,1)=\"J\",RIGHT(H784,LEN(H784)-4),RIGHT(H784,LEN(H784)-6)),\"\"))","v":""}]
[50000684,"Huawei","SUN2000-20KTL-M5",22,22,3,"PV-Wechselrichter","Ja","2023-09-21","Martin Bertsch","2023-05-03",null,null,null,null,"Nein","Ja","Nein","OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H785,1)=\"J\",LEFT(H785,2),LEFT(H785,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H785,1)=\"J\",RIGHT(H785,LEN(H785)-4),RIGHT(H785,LEN(H785)-6)),\"\"))","v":""}]
[50000688,"Huawei","SUN2000-25K-MB0",27.5,27.5,3,"Hybrid-Wechselrichter","Ja","2024-02-28","Martin Bertsch","2023-05-03",null,null,null,null,"Ja","Ja",null,"OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H786,1)=\"J\",LEFT(H786,2),LEFT(H786,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H786,1)=\"J\",RIGHT(H786,LEN(H786)-4),RIGHT(H786,LEN(H786)-6)),\"\"))","v":""}]
[50000686,"Huawei","SUN2000-25KTL",25,27.5,3,"PV-Wechselrichter","Nein","2022-07-18","Christian Elbs",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H787,1)=\"J\",LEFT(H787,2),LEFT(H787,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H787,1)=\"J\",RIGHT(H787,LEN(H787)-4),RIGHT(H787,LEN(H787)-6)),\"\"))","v":""}]
[50000687,"Huawei","SUN2000-25KTL-M5",27.5,27.5,3,"PV-Wechselrichter","Ja","2023-09-21","Martin Bertsch","2023-05-03",null,null,null,null,"Nein","Ja","Nein","OK","Martin Bertsch (OE)","64.290.22.31348.02","2023-06-26","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H788,1)=\"J\",LEFT(H788,2),LEFT(H788,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H788,1)=\"J\",RIGHT(H788,LEN(H788)-4),RIGHT(H788,LEN(H788)-6)),\"\"))","v":""}]
[50000689,"Huawei","SUN2000-30KTL-M3 ",30,30,3,"PV-Wechselrichter","Ja","2022-07-29",null,"2021-05-07",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200511N092","2020-10-15","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F",null,"statische Begrenzung Scheinleitung auf 30 kVA, daher kein NA Schutz erforderlich",{"$f":"IF(LEFT(H789,1)=\"J\",LEFT(H789,2),LEFT(H789,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H789,1)=\"J\",RIGHT(H789,LEN(H789)-4),RIGHT(H789,LEN(H789)-6)),\"\"))","v":""}]
[50000690,"Huawei","SUN2000-33KTL-A ",30,33,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200609N040","2020-06-29",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H790,1)=\"J\",LEFT(H790,2),LEFT(H790,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H790,1)=\"J\",RIGHT(H790,LEN(H790)-4),RIGHT(H790,LEN(H790)-6)),\"\"))","v":""}]
[50000691,"Huawei","SUN2000-36KTL ",40,40,3,"PV-Wechselrichter","Nein","2022-08-23","Christian Elbs",null,null,null,"2022-08-23","Laut Kurt Reinagel ist update nicht mehr möglich, altes Modell","Nein","Nein",null,"Vorhanden",null,"PVAT200609N040","2020-06-29","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H791,1)=\"J\",LEFT(H791,2),LEFT(H791,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H791,1)=\"J\",RIGHT(H791,LEN(H791)-4),RIGHT(H791,LEN(H791)-6)),\"\"))","v":""}]
[50000692,"Huawei","SUN2000-36KTL-M3 ",40,40,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200511N092","2020-10-15","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H792,1)=\"J\",LEFT(H792,2),LEFT(H792,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H792,1)=\"J\",RIGHT(H792,LEN(H792)-4),RIGHT(H792,LEN(H792)-6)),\"\"))","v":""}]
[50000693,"Huawei","SUN2000-40KTL-M3 ",44,44,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200511N092","2020-10-15","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H793,1)=\"J\",LEFT(H793,2),LEFT(H793,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H793,1)=\"J\",RIGHT(H793,LEN(H793)-4),RIGHT(H793,LEN(H793)-6)),\"\"))","v":""}]
[50000694,"Huawei","SUN2000-50KTL-M0 ",55,55,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200609N040-1-R1","2020-08-18","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+B+R25","F","F",null,null,{"$f":"IF(LEFT(H794,1)=\"J\",LEFT(H794,2),LEFT(H794,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H794,1)=\"J\",RIGHT(H794,LEN(H794)-4),RIGHT(H794,LEN(H794)-6)),\"\"))","v":""}]
[50000695,"Huawei","SUN2000-50KTL-M3",55,55,3,"PV-Wechselrichter","Ja","2023-09-18","Martin Bertsch","2023-02-24",null,null,null,null,"Nein","Nein","Nein","OK","Roland Bründlinger","64.290.22.30908.02","2023-07-17","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H795,1)=\"J\",LEFT(H795,2),LEFT(H795,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H795,1)=\"J\",RIGHT(H795,LEN(H795)-4),RIGHT(H795,LEN(H795)-6)),\"\"))","v":""}]
[50000696,"Huawei","SUN2000-60KTL-M0 ",66,66,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200609N040-1-R1","2020-08-18","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+B+R25","F","F",null,null,{"$f":"IF(LEFT(H796,1)=\"J\",LEFT(H796,2),LEFT(H796,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H796,1)=\"J\",RIGHT(H796,LEN(H796)-4),RIGHT(H796,LEN(H796)-6)),\"\"))","v":""}]
[50000697,"Huawei","SUN2000-100KTL-M1 ",110,110,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"PVAT200609N040-2-R1","2020-08-27","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+B+R25","F","F",null,null,{"$f":"IF(LEFT(H797,1)=\"J\",LEFT(H797,2),LEFT(H797,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H797,1)=\"J\",RIGHT(H797,LEN(H797)-4),RIGHT(H797,LEN(H797)-6)),\"\"))","v":""}]
[50000698,"Huawei","SUN2000-100KTL-M2",110,110,3,"PV-Wechselrichter","Ja","2023-09-18","Martin Bertsch","2023-02-24",null,null,null,null,"Nein",null,null,"OK","Martin Bertsch (OE)","CN239ABL 001","2023-07-03","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H798,1)=\"J\",LEFT(H798,2),LEFT(H798,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H798,1)=\"J\",RIGHT(H798,LEN(H798)-4),RIGHT(H798,LEN(H798)-6)),\"\"))","v":""}]
[50000699,"Huawei","SUN2000-105KTL-H1",116,116,3,"PV-Wechselrichter","Nein - Typ B","2023-04-25","Christian Elbs",null,null,null,null,"800V AC Wechselrichter","Nein","Nein","Nein","nicht vorhanden",null,null,null,"Vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H799,1)=\"J\",LEFT(H799,2),LEFT(H799,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H799,1)=\"J\",RIGHT(H799,LEN(H799)-4),RIGHT(H799,LEN(H799)-6)),\"\"))","v":"Typ B"}]
[50001915,"Huawei","LUNA2000-100KTL-M1",110,120,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2023-10-19",null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","CN23ZY9T 001","2023-02-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H800,1)=\"J\",LEFT(H800,2),LEFT(H800,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H800,1)=\"J\",RIGHT(H800,LEN(H800)-4),RIGHT(H800,LEN(H800)-6)),\"\"))","v":""}]
[50000700,"Huawei","SUN2000-115KTL-M2",125,125,3,"PV-Wechselrichter","Ja","2023-09-18","Martin Bertsch","2023-02-24",null,null,null,null,"Nein",null,null,"OK","Martin Bertsch (OE)","CN239ABL 001","2023-07-03","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H801,1)=\"J\",LEFT(H801,2),LEFT(H801,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H801,1)=\"J\",RIGHT(H801,LEN(H801)-4),RIGHT(H801,LEN(H801)-6)),\"\"))","v":""}]
[50002282,"HUAWEI","SUN2000-150K-MG0",165,165,3,"PV-Wechselrichter","Ja","2024-06-04","Martin Bertsch","2024-06-04",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"231019075GZU-001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H802,1)=\"J\",LEFT(H802,2),LEFT(H802,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H802,1)=\"J\",RIGHT(H802,LEN(H802)-4),RIGHT(H802,LEN(H802)-6)),\"\"))","v":""}]
[50002283,"HUAWEI","SUN5000-150K-MG0",165,165,3,"PV-Wechselrichter","Ja","2024-06-04","Martin Bertsch","2024-06-04",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"231019075GZU-001","2024-05-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H803,1)=\"J\",LEFT(H803,2),LEFT(H803,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H803,1)=\"J\",RIGHT(H803,LEN(H803)-4),RIGHT(H803,LEN(H803)-6)),\"\"))","v":""}]
[50000701,"Huawei","SUN2000-185KTL-H1",185,185,3,"PV-Wechselrichter","Nein - Typ B",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H804,1)=\"J\",LEFT(H804,2),LEFT(H804,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H804,1)=\"J\",RIGHT(H804,LEN(H804)-4),RIGHT(H804,LEN(H804)-6)),\"\"))","v":"Typ B"}]
[50000702,"Huawei","SUN2000-215KTL-H0",215,215,3,"PV-Wechselrichter","Nein - Typ B",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H805,1)=\"J\",LEFT(H805,2),LEFT(H805,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H805,1)=\"J\",RIGHT(H805,LEN(H805)-4),RIGHT(H805,LEN(H805)-6)),\"\"))","v":"Typ B"}]
[50001917,"HUAYU","HY-300-Plus",0.3,0.3,1,"PV-Wechselrichter","Ja - <= 800W Anlage",44910,"Martin Bertsch","2022-11-03",null,null,null,null,null,null,null,"VDE4105/4110",null,null,null,null,"VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H806,1)=\"J\",LEFT(H806,2),LEFT(H806,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H806,1)=\"J\",RIGHT(H806,LEN(H806)-4),RIGHT(H806,LEN(H806)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000704,"HUAYU","HY-500-Plus",0.5,0.5,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2022-12-15","Martin Bertsch","2022-11-03",null,null,null,null,null,null,null,"VDE4105/4110",null,null,null,null,"VDE4105/4111",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H807,1)=\"J\",LEFT(H807,2),LEFT(H807,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H807,1)=\"J\",RIGHT(H807,LEN(H807)-4),RIGHT(H807,LEN(H807)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000705,"HUAYU","HY-600-Plus",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2022-12-15","Martin Bertsch","2022-11-03",null,null,null,null,null,null,null,"VDE4105/4110",null,null,null,null,"VDE4105/4112",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H808,1)=\"J\",LEFT(H808,2),LEFT(H808,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H808,1)=\"J\",RIGHT(H808,LEN(H808)-4),RIGHT(H808,LEN(H808)-6)),\"\"))","v":"<= 800W Anlage"}]
[50000706,"HUAYU","HY-800-Plus",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2022-12-15","Martin Bertsch","2022-11-03",null,null,null,null,null,null,null,"VDE4105/4110",null,null,null,null,"VDE4105/4113",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H809,1)=\"J\",LEFT(H809,2),LEFT(H809,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H809,1)=\"J\",RIGHT(H809,LEN(H809)-4),RIGHT(H809,LEN(H809)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002209,"INVERX","XLiT5",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2024-05-13","Software_Master_Version: SIHXXTH_01_1_ARM.01.011 Main_DSP_Software_Version: SIHXXTH_01_1_MDSP.01.014",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6189754.50","2024-05-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H810,1)=\"J\",LEFT(H810,2),LEFT(H810,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H810,1)=\"J\",RIGHT(H810,LEN(H810)-4),RIGHT(H810,LEN(H810)-6)),\"\"))","v":"mit Einschränkung"}]
[50002210,"INVERX","XLiT6",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2024-05-13","Software_Master_Version: SIHXXTH_01_1_ARM.01.011 Main_DSP_Software_Version: SIHXXTH_01_1_MDSP.01.014",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6189754.50","2024-05-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H811,1)=\"J\",LEFT(H811,2),LEFT(H811,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H811,1)=\"J\",RIGHT(H811,LEN(H811)-4),RIGHT(H811,LEN(H811)-6)),\"\"))","v":"mit Einschränkung"}]
[50002211,"INVERX","XLiT8",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2024-05-13","Software_Master_Version: SIHXXTH_01_1_ARM.01.011 Main_DSP_Software_Version: SIHXXTH_01_1_MDSP.01.014",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6189754.50","2024-05-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H812,1)=\"J\",LEFT(H812,2),LEFT(H812,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H812,1)=\"J\",RIGHT(H812,LEN(H812)-4),RIGHT(H812,LEN(H812)-6)),\"\"))","v":"mit Einschränkung"}]
[50002212,"INVERX","XLiT10",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-05-13","Martin Bertsch","2024-05-13","Software_Master_Version: SIHXXTH_01_1_ARM.01.011 Main_DSP_Software_Version: SIHXXTH_01_1_MDSP.01.014",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6189754.50","2024-05-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H813,1)=\"J\",LEFT(H813,2),LEFT(H813,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H813,1)=\"J\",RIGHT(H813,LEN(H813)-4),RIGHT(H813,LEN(H813)-6)),\"\"))","v":"mit Einschränkung"}]
[50000707,"Kaco","blueplanet 3.0 NX1 M2",null,3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H814,1)=\"J\",LEFT(H814,2),LEFT(H814,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H814,1)=\"J\",RIGHT(H814,LEN(H814)-4),RIGHT(H814,LEN(H814)-6)),\"\"))","v":""}]
[50000708,"Kaco","blueplanet 3.0 NX3 M2 WM OD IIG0",3,3,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","64.290.22.30919.01","2023-04-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H815,1)=\"J\",LEFT(H815,2),LEFT(H815,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H815,1)=\"J\",RIGHT(H815,LEN(H815)-4),RIGHT(H815,LEN(H815)-6)),\"\"))","v":"befristet"}]
[50000709,"Kaco","blueplanet 3.7 NX1 M2",null,3.68,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H816,1)=\"J\",LEFT(H816,2),LEFT(H816,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H816,1)=\"J\",RIGHT(H816,LEN(H816)-4),RIGHT(H816,LEN(H816)-6)),\"\"))","v":""}]
[50000710,"Kaco","blueplanet 4.0 NX1 M2",null,4,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H817,1)=\"J\",LEFT(H817,2),LEFT(H817,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H817,1)=\"J\",RIGHT(H817,LEN(H817)-4),RIGHT(H817,LEN(H817)-6)),\"\"))","v":""}]
[50000711,"Kaco","blueplanet 5.0 NX1 M2",null,5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H818,1)=\"J\",LEFT(H818,2),LEFT(H818,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H818,1)=\"J\",RIGHT(H818,LEN(H818)-4),RIGHT(H818,LEN(H818)-6)),\"\"))","v":""}]
[50000712,"Kaco","blueplanet 5.0 NX3 M2 WM OD IIG0",5,5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","64.290.22.30919.01","2023-04-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H819,1)=\"J\",LEFT(H819,2),LEFT(H819,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H819,1)=\"J\",RIGHT(H819,LEN(H819)-4),RIGHT(H819,LEN(H819)-6)),\"\"))","v":"befristet"}]
[50000713,"Kaco","blueplanet 8.0 NX3 M2 WM OD IIG0",8,8,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","64.290.22.30919.01","2023-04-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H820,1)=\"J\",LEFT(H820,2),LEFT(H820,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H820,1)=\"J\",RIGHT(H820,LEN(H820)-4),RIGHT(H820,LEN(H820)-6)),\"\"))","v":"befristet"}]
[50000714,"Kaco","blueplanet 10.0 NX3 M2 WM OD IIG0",10,10,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","64.290.22.30919.01","2023-04-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H821,1)=\"J\",LEFT(H821,2),LEFT(H821,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H821,1)=\"J\",RIGHT(H821,LEN(H821)-4),RIGHT(H821,LEN(H821)-6)),\"\"))","v":"befristet"}]
[50000715,"Kaco","blueplanet hybrid 10.0 TL3",9.9,11,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2024-04-24","Martin Bertsch","2023-06-26","8.26.9.2.19","2024-04-30","2024-04-30","vom Hersteller abgekündigt.","ja",null,null,"Vorhanden",null,"21PP664-02_0","2022-03-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H822,1)=\"J\",LEFT(H822,2),LEFT(H822,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H822,1)=\"J\",RIGHT(H822,LEN(H822)-4),RIGHT(H822,LEN(H822)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000716,"Kaco","blueplanet 15.0 NX3 M2 WM OD IIG0",15,15,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","64.290.22.30919.01","2023-04-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H823,1)=\"J\",LEFT(H823,2),LEFT(H823,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H823,1)=\"J\",RIGHT(H823,LEN(H823)-4),RIGHT(H823,LEN(H823)-6)),\"\"))","v":"befristet"}]
[50000717,"Kaco","blueplanet 20.0 NX3 M2 WM OD IIG0",20,20,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","64.290.22.30919.01","2023-04-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H824,1)=\"J\",LEFT(H824,2),LEFT(H824,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H824,1)=\"J\",RIGHT(H824,LEN(H824)-4),RIGHT(H824,LEN(H824)-6)),\"\"))","v":"befristet"}]
[50000723,"Kaco","blueplanet gridsave 50.0 TL3-S B1 WM OD IIGB",52,52,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-10-21",null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht OK",null,"18TH0378-OVE-directive R25_0","2021-03-25",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM AB","F","F",null,null,{"$f":"IF(LEFT(H825,1)=\"J\",LEFT(H825,2),LEFT(H825,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H825,1)=\"J\",RIGHT(H825,LEN(H825)-4),RIGHT(H825,LEN(H825)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000724,"Kaco","blueplanet gridsave 50.0 TL3-S B1 WM OD IIGL",52,52,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-10-21",null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht OK",null,"18TH0378-OVE-directive R25_0","2021-03-25",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM AB","F","F",null,null,{"$f":"IF(LEFT(H826,1)=\"J\",LEFT(H826,2),LEFT(H826,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H826,1)=\"J\",RIGHT(H826,LEN(H826)-4),RIGHT(H826,LEN(H826)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000725,"Kaco","blueplanet gridsave 50.0 TL3-S B1 WM OD IIGM",52,52,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-10-21",null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht OK",null,"18TH0378-OVE-directive R25_0","2021-03-25",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM AB","F","F",null,null,{"$f":"IF(LEFT(H827,1)=\"J\",LEFT(H827,2),LEFT(H827,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H827,1)=\"J\",RIGHT(H827,LEN(H827)-4),RIGHT(H827,LEN(H827)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000726,"Kaco","blueplanet gridsave 50.0 TL3-S B1 WM OD IIGX",52,52,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-10-21",null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht OK",null,"18TH0378-OVE-directive R25_0","2021-03-25",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM AB","F","F",null,null,{"$f":"IF(LEFT(H828,1)=\"J\",LEFT(H828,2),LEFT(H828,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H828,1)=\"J\",RIGHT(H828,LEN(H828)-4),RIGHT(H828,LEN(H828)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50002018,"Kaco","KACO blueplanet 50.0 TL3 M1 WM OD FRGX",50,52,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H829,1)=\"J\",LEFT(H829,2),LEFT(H829,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H829,1)=\"J\",RIGHT(H829,LEN(H829)-4),RIGHT(H829,LEN(H829)-6)),\"\"))","v":""}]
[50002015,"Kaco","KACO blueplanet 50.0 TL3 M1 WM OD IIGB",50,52,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H830,1)=\"J\",LEFT(H830,2),LEFT(H830,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H830,1)=\"J\",RIGHT(H830,LEN(H830)-4),RIGHT(H830,LEN(H830)-6)),\"\"))","v":""}]
[50002014,"Kaco","KACO blueplanet 50.0 TL3 M1 WM OD IIGM",50,52,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H831,1)=\"J\",LEFT(H831,2),LEFT(H831,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H831,1)=\"J\",RIGHT(H831,LEN(H831)-4),RIGHT(H831,LEN(H831)-6)),\"\"))","v":""}]
[50002017,"Kaco","KACO blueplanet 50.0 TL3 M1 WM OD IIGS",50,52,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H832,1)=\"J\",LEFT(H832,2),LEFT(H832,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H832,1)=\"J\",RIGHT(H832,LEN(H832)-4),RIGHT(H832,LEN(H832)-6)),\"\"))","v":""}]
[50002016,"Kaco","KACO blueplanet 50.0 TL3 M1 WM OD IIGX",50,52,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H833,1)=\"J\",LEFT(H833,2),LEFT(H833,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H833,1)=\"J\",RIGHT(H833,LEN(H833)-4),RIGHT(H833,LEN(H833)-6)),\"\"))","v":""}]
[50002022,"Kaco","KACO blueplanet 60.0 TL3 M1 WM OD FRGX",60,60,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H834,1)=\"J\",LEFT(H834,2),LEFT(H834,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H834,1)=\"J\",RIGHT(H834,LEN(H834)-4),RIGHT(H834,LEN(H834)-6)),\"\"))","v":""}]
[50002020,"Kaco","KACO blueplanet 60.0 TL3 M1 WM OD IIGB",60,60,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H835,1)=\"J\",LEFT(H835,2),LEFT(H835,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H835,1)=\"J\",RIGHT(H835,LEN(H835)-4),RIGHT(H835,LEN(H835)-6)),\"\"))","v":""}]
[50002019,"Kaco","KACO blueplanet 60.0 TL3 M1 WM OD IIGM",60,60,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H836,1)=\"J\",LEFT(H836,2),LEFT(H836,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H836,1)=\"J\",RIGHT(H836,LEN(H836)-4),RIGHT(H836,LEN(H836)-6)),\"\"))","v":""}]
[50002021,"Kaco","KACO blueplanet 60.0 TL3 M1 WM OD IIGX",60,60,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H837,1)=\"J\",LEFT(H837,2),LEFT(H837,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H837,1)=\"J\",RIGHT(H837,LEN(H837)-4),RIGHT(H837,LEN(H837)-6)),\"\"))","v":""}]
[50002024,"Kaco","KACO blueplanet 60.0 TL3 M1 WM OD KRGB",60,60,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H838,1)=\"J\",LEFT(H838,2),LEFT(H838,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H838,1)=\"J\",RIGHT(H838,LEN(H838)-4),RIGHT(H838,LEN(H838)-6)),\"\"))","v":""}]
[50002023,"Kaco","KACO blueplanet 60.0 TL3 M1 WM OD TWGB",60,60,3,"PV-Wechselrichter","Ja","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"15TH0250-OVE-directive R25_1","2023-12-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H839,1)=\"J\",LEFT(H839,2),LEFT(H839,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H839,1)=\"J\",RIGHT(H839,LEN(H839)-4),RIGHT(H839,LEN(H839)-6)),\"\"))","v":""}]
[50000733,"Kaco","blueplanet 87.0 TL3 M1 WM OD IIF0",87,87,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H840,1)=\"J\",LEFT(H840,2),LEFT(H840,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H840,1)=\"J\",RIGHT(H840,LEN(H840)-4),RIGHT(H840,LEN(H840)-6)),\"\"))","v":"befristet"}]
[50000734,"Kaco","blueplanet 87.0 TL3 M1 WM OD IIFX",87,87,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H841,1)=\"J\",LEFT(H841,2),LEFT(H841,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H841,1)=\"J\",RIGHT(H841,LEN(H841)-4),RIGHT(H841,LEN(H841)-6)),\"\"))","v":"befristet"}]
[50000735,"Kaco","blueplanet 92.0 TL3 M1 WM OD IIG0",92,92,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H842,1)=\"J\",LEFT(H842,2),LEFT(H842,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H842,1)=\"J\",RIGHT(H842,LEN(H842)-4),RIGHT(H842,LEN(H842)-6)),\"\"))","v":"befristet"}]
[50000736,"Kaco","blueplanet 92.0 TL3 M1 WM OD IIGX",92,92,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H843,1)=\"J\",LEFT(H843,2),LEFT(H843,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H843,1)=\"J\",RIGHT(H843,LEN(H843)-4),RIGHT(H843,LEN(H843)-6)),\"\"))","v":"befristet"}]
[50000737,"Kaco","blueplanet gs 92.0 TL3-S B1 WM OD IIGL ",92,92,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H844,1)=\"J\",LEFT(H844,2),LEFT(H844,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H844,1)=\"J\",RIGHT(H844,LEN(H844)-4),RIGHT(H844,LEN(H844)-6)),\"\"))","v":"befristet"}]
[50000738,"Kaco","blueplanet gs 92.0 TL3-S B1 WM OD IIGM ",92,92,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H845,1)=\"J\",LEFT(H845,2),LEFT(H845,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H845,1)=\"J\",RIGHT(H845,LEN(H845)-4),RIGHT(H845,LEN(H845)-6)),\"\"))","v":"befristet"}]
[50000739,"Kaco","blueplanet gs 92.0 TL3-S B1 WM OD IIGX ",92,92,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H846,1)=\"J\",LEFT(H846,2),LEFT(H846,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H846,1)=\"J\",RIGHT(H846,LEN(H846)-4),RIGHT(H846,LEN(H846)-6)),\"\"))","v":"befristet"}]
[50002301,"Kaco","blueplanet 100 NX3 M8 WM OD IIGM",100,100,3,"PV-Wechselrichter","Ja, befristet","2024-06-19","Martin Bertsch","2024-06-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden",null,"713249653-12","2024-05-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H847,1)=\"J\",LEFT(H847,2),LEFT(H847,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H847,1)=\"J\",RIGHT(H847,LEN(H847)-4),RIGHT(H847,LEN(H847)-6)),\"\"))","v":"befristet"}]
[50002300,"Kaco","blueplanet 100 NX3 M8 WM OD IIGX",100,100,3,"PV-Wechselrichter","Ja, befristet","2024-06-19","Martin Bertsch","2024-06-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden",null,"713249653-12","2024-05-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H848,1)=\"J\",LEFT(H848,2),LEFT(H848,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H848,1)=\"J\",RIGHT(H848,LEN(H848)-4),RIGHT(H848,LEN(H848)-6)),\"\"))","v":"befristet"}]
[50000740,"Kaco","blueplanet 105 TL3 M1 WM OD IIG0",105,105,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H849,1)=\"J\",LEFT(H849,2),LEFT(H849,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H849,1)=\"J\",RIGHT(H849,LEN(H849)-4),RIGHT(H849,LEN(H849)-6)),\"\"))","v":"befristet"}]
[50000741,"Kaco","blueplanet 105 TL3 M1 WM OD IIGX",105,105,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H850,1)=\"J\",LEFT(H850,2),LEFT(H850,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H850,1)=\"J\",RIGHT(H850,LEN(H850)-4),RIGHT(H850,LEN(H850)-6)),\"\"))","v":"befristet"}]
[50000742,"Kaco","blueplanet gs 110 TL3-S B1 WM OD IIKL ",110,110,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H851,1)=\"J\",LEFT(H851,2),LEFT(H851,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H851,1)=\"J\",RIGHT(H851,LEN(H851)-4),RIGHT(H851,LEN(H851)-6)),\"\"))","v":"befristet"}]
[50000743,"Kaco","blueplanet gs 110 TL3-S B1 WM OD IIKM ",110,110,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H852,1)=\"J\",LEFT(H852,2),LEFT(H852,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H852,1)=\"J\",RIGHT(H852,LEN(H852)-4),RIGHT(H852,LEN(H852)-6)),\"\"))","v":"befristet"}]
[50000744,"Kaco","blueplanet gs 110 TL3-S B1 WM OD IIKX ",110,110,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H853,1)=\"J\",LEFT(H853,2),LEFT(H853,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H853,1)=\"J\",RIGHT(H853,LEN(H853)-4),RIGHT(H853,LEN(H853)-6)),\"\"))","v":"befristet"}]
[50002299,"Kaco","blueplanet 125 NX3 M10 WM OD IIGM",125,125,3,"PV-Wechselrichter","Ja, befristet","2024-06-19","Martin Bertsch","2024-06-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden",null,"713249653-12","2024-05-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H854,1)=\"J\",LEFT(H854,2),LEFT(H854,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H854,1)=\"J\",RIGHT(H854,LEN(H854)-4),RIGHT(H854,LEN(H854)-6)),\"\"))","v":"befristet"}]
[50002298,"Kaco","blueplanet 125 NX3 M10 WM OD IIGX",125,125,3,"PV-Wechselrichter","Ja, befristet","2024-06-19","Martin Bertsch","2024-06-19",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden",null,"713249653-12","2024-05-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H855,1)=\"J\",LEFT(H855,2),LEFT(H855,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H855,1)=\"J\",RIGHT(H855,LEN(H855)-4),RIGHT(H855,LEN(H855)-6)),\"\"))","v":"befristet"}]
[50000745,"Kaco","blueplanet 137 TL3 M1 WM OD IIP0",null,137,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H856,1)=\"J\",LEFT(H856,2),LEFT(H856,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H856,1)=\"J\",RIGHT(H856,LEN(H856)-4),RIGHT(H856,LEN(H856)-6)),\"\"))","v":"befristet"}]
[50000746,"Kaco","blueplanet 137 TL3 M1 WM OD IIPX",null,137,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H857,1)=\"J\",LEFT(H857,2),LEFT(H857,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H857,1)=\"J\",RIGHT(H857,LEN(H857)-4),RIGHT(H857,LEN(H857)-6)),\"\"))","v":"befristet"}]
[50000747,"Kaco","blueplanet gs 137 TL3-S B1 WM OD IIPL ",137,137,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H858,1)=\"J\",LEFT(H858,2),LEFT(H858,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H858,1)=\"J\",RIGHT(H858,LEN(H858)-4),RIGHT(H858,LEN(H858)-6)),\"\"))","v":"befristet"}]
[50000748,"Kaco","blueplanet gs 137 TL3-S B1 WM OD IIPM ",137,137,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H859,1)=\"J\",LEFT(H859,2),LEFT(H859,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H859,1)=\"J\",RIGHT(H859,LEN(H859)-4),RIGHT(H859,LEN(H859)-6)),\"\"))","v":"befristet"}]
[50000749,"Kaco","blueplanet gs 137 TL3-S B1 WM OD IIPX",137,137,3,"AC-Batteriewechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H860,1)=\"J\",LEFT(H860,2),LEFT(H860,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H860,1)=\"J\",RIGHT(H860,LEN(H860)-4),RIGHT(H860,LEN(H860)-6)),\"\"))","v":"befristet"}]
[50000750,"Kaco","blueplanet 125 TL3 M1 WM OD IIK0",125,137.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ","F","F",null,null,{"$f":"IF(LEFT(H861,1)=\"J\",LEFT(H861,2),LEFT(H861,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H861,1)=\"J\",RIGHT(H861,LEN(H861)-4),RIGHT(H861,LEN(H861)-6)),\"\"))","v":"befristet"}]
[50000751,"Kaco","blueplanet 125 TL3 M1 WM OD IIKX",125,137.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ","F","F",null,null,{"$f":"IF(LEFT(H862,1)=\"J\",LEFT(H862,2),LEFT(H862,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H862,1)=\"J\",RIGHT(H862,LEN(H862)-4),RIGHT(H862,LEN(H862)-6)),\"\"))","v":"befristet"}]
[50000752,"Kaco","blueplanet 125 TL3 M1 WM OD IIP0",125,137.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ","F","F",null,null,{"$f":"IF(LEFT(H863,1)=\"J\",LEFT(H863,2),LEFT(H863,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H863,1)=\"J\",RIGHT(H863,LEN(H863)-4),RIGHT(H863,LEN(H863)-6)),\"\"))","v":"befristet"}]
[50000753,"Kaco","blueplanet 125 TL3 M1 WM OD IIPX",125,137.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ","F","F",null,null,{"$f":"IF(LEFT(H864,1)=\"J\",LEFT(H864,2),LEFT(H864,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H864,1)=\"J\",RIGHT(H864,LEN(H864)-4),RIGHT(H864,LEN(H864)-6)),\"\"))","v":"befristet"}]
[50000754,"Kaco","blueplanet 150 TL3 M1 WM OD IIQ0",null,150,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H865,1)=\"J\",LEFT(H865,2),LEFT(H865,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H865,1)=\"J\",RIGHT(H865,LEN(H865)-4),RIGHT(H865,LEN(H865)-6)),\"\"))","v":"befristet"}]
[50000755,"Kaco","blueplanet 150 TL3 M1 WM OD IIQX",null,150,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H866,1)=\"J\",LEFT(H866,2),LEFT(H866,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H866,1)=\"J\",RIGHT(H866,LEN(H866)-4),RIGHT(H866,LEN(H866)-6)),\"\"))","v":"befristet"}]
[50000756,"Kaco","blueplanet 155 TL3 M1 WM OD IIP0",155,155,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H867,1)=\"J\",LEFT(H867,2),LEFT(H867,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H867,1)=\"J\",RIGHT(H867,LEN(H867)-4),RIGHT(H867,LEN(H867)-6)),\"\"))","v":"befristet"}]
[50000757,"Kaco","blueplanet 155 TL3 M1 WM OD IIPX",155,155,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H868,1)=\"J\",LEFT(H868,2),LEFT(H868,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H868,1)=\"J\",RIGHT(H868,LEN(H868)-4),RIGHT(H868,LEN(H868)-6)),\"\"))","v":"befristet"}]
[50000758,"Kaco","blueplanet 165 TL3 M1 WM OD IIQ0",165,165,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H869,1)=\"J\",LEFT(H869,2),LEFT(H869,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H869,1)=\"J\",RIGHT(H869,LEN(H869)-4),RIGHT(H869,LEN(H869)-6)),\"\"))","v":"befristet"}]
[50000759,"Kaco","blueplanet 165 TL3 M1 WM OD IIQX",165,165,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-03",null,"2024-09-30",null,null,"Nein","Nein","Nein","nicht OK","Roland Bründlinger","20581-1-TR, 20278-1-TR and 21252-1-TR","2022-04-13",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H870,1)=\"J\",LEFT(H870,2),LEFT(H870,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H870,1)=\"J\",RIGHT(H870,LEN(H870)-4),RIGHT(H870,LEN(H870)-6)),\"\"))","v":"befristet"}]
[50000760,"Kärnten Solar","PANTA I0 ",10,10,3,"Hybrid-Wechselrichter","Nein","2022-10-17","Christian Elbs","2022-05-23",null,null,"2022-10-06","Keine Rückmeldung zum fehlerhaften Prüfbericht","Ja","Nein",null,"nicht OK","Martin Bertsch (OE)","PVAT200119N030-R1","2020-12-09",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H871,1)=\"J\",LEFT(H871,2),LEFT(H871,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H871,1)=\"J\",RIGHT(H871,LEN(H871)-4),RIGHT(H871,LEN(H871)-6)),\"\"))","v":""}]
[50000761,"Katek / Steca","Steca AJ 275-12",null,0.2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H872,1)=\"J\",LEFT(H872,2),LEFT(H872,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H872,1)=\"J\",RIGHT(H872,LEN(H872)-4),RIGHT(H872,LEN(H872)-6)),\"\"))","v":""}]
[50000762,"Katek / Steca","Steca AJ 350-24",null,0.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H873,1)=\"J\",LEFT(H873,2),LEFT(H873,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H873,1)=\"J\",RIGHT(H873,LEN(H873)-4),RIGHT(H873,LEN(H873)-6)),\"\"))","v":""}]
[50000763,"Katek / Steca","Steca AJ 400-48",null,0.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H874,1)=\"J\",LEFT(H874,2),LEFT(H874,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H874,1)=\"J\",RIGHT(H874,LEN(H874)-4),RIGHT(H874,LEN(H874)-6)),\"\"))","v":""}]
[50000764,"Katek / Steca","Steca AJ 700-48",null,0.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H875,1)=\"J\",LEFT(H875,2),LEFT(H875,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H875,1)=\"J\",RIGHT(H875,LEN(H875)-4),RIGHT(H875,LEN(H875)-6)),\"\"))","v":""}]
[50000765,"Katek / Steca","Steca Xtender XTS 900-12",null,0.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H876,1)=\"J\",LEFT(H876,2),LEFT(H876,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H876,1)=\"J\",RIGHT(H876,LEN(H876)-4),RIGHT(H876,LEN(H876)-6)),\"\"))","v":""}]
[50000766,"Katek / Steca","Steca Xtender XTS 1200-24",null,0.65,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H877,1)=\"J\",LEFT(H877,2),LEFT(H877,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H877,1)=\"J\",RIGHT(H877,LEN(H877)-4),RIGHT(H877,LEN(H877)-6)),\"\"))","v":""}]
[50000767,"Katek / Steca","Steca Xtender XTS 1400-48",null,0.75,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H878,1)=\"J\",LEFT(H878,2),LEFT(H878,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H878,1)=\"J\",RIGHT(H878,LEN(H878)-4),RIGHT(H878,LEN(H878)-6)),\"\"))","v":""}]
[50000768,"Katek / Steca","Steca AJ 1000-12",null,0.8,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H879,1)=\"J\",LEFT(H879,2),LEFT(H879,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H879,1)=\"J\",RIGHT(H879,LEN(H879)-4),RIGHT(H879,LEN(H879)-6)),\"\"))","v":""}]
[50000769,"Katek / Steca","Steca Solarix PLI 1000-12",1,1,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H880,1)=\"J\",LEFT(H880,2),LEFT(H880,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H880,1)=\"J\",RIGHT(H880,LEN(H880)-4),RIGHT(H880,LEN(H880)-6)),\"\"))","v":""}]
[50000770,"Katek / Steca","Steca Xtender XTM 1500-12",null,1.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H881,1)=\"J\",LEFT(H881,2),LEFT(H881,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H881,1)=\"J\",RIGHT(H881,LEN(H881)-4),RIGHT(H881,LEN(H881)-6)),\"\"))","v":""}]
[50000771,"Katek / Steca","StecaGrid 1511 ",1.5,1.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-03-07","Christian Elbs","2023-01-11",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","18TH0316-OVE-directive R25_2","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3ph bis Sum 11,04kVA Konform TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H882,1)=\"J\",LEFT(H882,2),LEFT(H882,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H882,1)=\"J\",RIGHT(H882,LEN(H882)-4),RIGHT(H882,LEN(H882)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000772,"Katek / Steca","Steca AJ 2100-12",null,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H883,1)=\"J\",LEFT(H883,2),LEFT(H883,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H883,1)=\"J\",RIGHT(H883,LEN(H883)-4),RIGHT(H883,LEN(H883)-6)),\"\"))","v":""}]
[50000773,"Katek / Steca","Steca AJ 2400-24",null,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H884,1)=\"J\",LEFT(H884,2),LEFT(H884,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H884,1)=\"J\",RIGHT(H884,LEN(H884)-4),RIGHT(H884,LEN(H884)-6)),\"\"))","v":""}]
[50000774,"Katek / Steca","Steca Xtender XTM 2000-12",null,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H885,1)=\"J\",LEFT(H885,2),LEFT(H885,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H885,1)=\"J\",RIGHT(H885,LEN(H885)-4),RIGHT(H885,LEN(H885)-6)),\"\"))","v":""}]
[50000775,"Katek / Steca","Steca Xtender XTM 2400-24",null,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H886,1)=\"J\",LEFT(H886,2),LEFT(H886,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H886,1)=\"J\",RIGHT(H886,LEN(H886)-4),RIGHT(H886,LEN(H886)-6)),\"\"))","v":""}]
[50000776,"Katek / Steca","Steca Xtender XTM 2600-48",null,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H887,1)=\"J\",LEFT(H887,2),LEFT(H887,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H887,1)=\"J\",RIGHT(H887,LEN(H887)-4),RIGHT(H887,LEN(H887)-6)),\"\"))","v":""}]
[50000777,"Katek / Steca","StecaGrid 2011 ",2,2,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-03-07","Christian Elbs","2023-01-11",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","18TH0316-OVE-directive R25_2","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3ph bis Sum 11,04kVA Konform TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H888,1)=\"J\",LEFT(H888,2),LEFT(H888,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H888,1)=\"J\",RIGHT(H888,LEN(H888)-4),RIGHT(H888,LEN(H888)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000778,"Katek / Steca","Steca Xtender XTH 3000-12",null,2.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H889,1)=\"J\",LEFT(H889,2),LEFT(H889,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H889,1)=\"J\",RIGHT(H889,LEN(H889)-4),RIGHT(H889,LEN(H889)-6)),\"\"))","v":""}]
[50000779,"Katek / Steca","StecaGrid 2511 ",2.5,2.5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-03-07","Christian Elbs","2023-01-11",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","18TH0316-OVE-directive R25_2","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3ph bis Sum 11,04kVA Konform TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H890,1)=\"J\",LEFT(H890,2),LEFT(H890,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H890,1)=\"J\",RIGHT(H890,LEN(H890)-4),RIGHT(H890,LEN(H890)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000780,"Katek / Steca","Solarix PLI 2400-24-24",2.4,3,1,"USV-Anwendung","Ja","2022-07-18",null,"2022-07-18",null,null,null,null,"Ja","Nein","Ja","nicht vorhanden","Martin Bertsch (OE)",null,null,null,null,null,null,null,null,"USV-Anwendung - kein R25 Prüfbericht erforderlich",null,null,null,null,{"$f":"IF(LEFT(H891,1)=\"J\",LEFT(H891,2),LEFT(H891,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H891,1)=\"J\",RIGHT(H891,LEN(H891)-4),RIGHT(H891,LEN(H891)-6)),\"\"))","v":""}]
[50000781,"Katek / Steca","Steca Solarix PLI 2400-24",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H892,1)=\"J\",LEFT(H892,2),LEFT(H892,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H892,1)=\"J\",RIGHT(H892,LEN(H892)-4),RIGHT(H892,LEN(H892)-6)),\"\"))","v":""}]
[50000782,"Katek / Steca","Steca Xtender XTM 3500-24",null,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H893,1)=\"J\",LEFT(H893,2),LEFT(H893,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H893,1)=\"J\",RIGHT(H893,LEN(H893)-4),RIGHT(H893,LEN(H893)-6)),\"\"))","v":""}]
[50000783,"Katek / Steca","StecaGrid 3011 ",3,3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-03-07","Christian Elbs","2023-01-11",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","18TH0316-OVE-directive R25_2","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3ph bis Sum 11,04kVA Konform TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H894,1)=\"J\",LEFT(H894,2),LEFT(H894,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H894,1)=\"J\",RIGHT(H894,LEN(H894)-4),RIGHT(H894,LEN(H894)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000784,"Katek / Steca","StecaGrid 3011_2 ",3,3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-03-07","Christian Elbs","2023-01-11",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","18TH0316-OVE-directive R25_2","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3ph bis Sum 11,04kVA Konform TOR ERZ A",null,null,null,null,{"$f":"IF(LEFT(H895,1)=\"J\",LEFT(H895,2),LEFT(H895,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H895,1)=\"J\",RIGHT(H895,LEN(H895)-4),RIGHT(H895,LEN(H895)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000785,"Katek / Steca","StecaGrid 3213",3.2,3.2,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-06-08",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","13TH0511-OVE-directive R25_1","2021-06-08",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H896,1)=\"J\",LEFT(H896,2),LEFT(H896,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H896,1)=\"J\",RIGHT(H896,LEN(H896)-4),RIGHT(H896,LEN(H896)-6)),\"\"))","v":""}]
[50000786,"Katek / Steca","Steca Xtender XTM 4000-48",null,3.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H897,1)=\"J\",LEFT(H897,2),LEFT(H897,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H897,1)=\"J\",RIGHT(H897,LEN(H897)-4),RIGHT(H897,LEN(H897)-6)),\"\"))","v":""}]
[50000787,"Katek / Steca","StecaGrid 3611 ",3.68,3.68,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-03-07","Christian Elbs","2023-01-11",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","18TH0316-OVE-directive R25_2","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3ph bis Sum 11,04kVA Konform TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H898,1)=\"J\",LEFT(H898,2),LEFT(H898,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H898,1)=\"J\",RIGHT(H898,LEN(H898)-4),RIGHT(H898,LEN(H898)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000788,"Katek / Steca","StecaGrid 3611_2 ",3.68,3.68,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-03-07","Christian Elbs","2023-01-11",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","18TH0316-OVE-directive R25_2","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3ph bis Sum 11,04kVA Konform TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H899,1)=\"J\",LEFT(H899,2),LEFT(H899,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H899,1)=\"J\",RIGHT(H899,LEN(H899)-4),RIGHT(H899,LEN(H899)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000789,"Katek / Steca","StecaGrid 4013",4,4,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-06-08",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","13TH0511-OVE-directive R25_1","2021-06-08",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25",null,null,"Verbauter Wechselrichter Refusol",null,{"$f":"IF(LEFT(H900,1)=\"J\",LEFT(H900,2),LEFT(H900,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H900,1)=\"J\",RIGHT(H900,LEN(H900)-4),RIGHT(H900,LEN(H900)-6)),\"\"))","v":""}]
[50000790,"Katek / Steca","StecaGrid 4213 ",4.2,4.2,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH0374-Hybird-OVE-Directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F","Verbauter Wechselrichter Sinexcel",null,{"$f":"IF(LEFT(H901,1)=\"J\",LEFT(H901,2),LEFT(H901,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H901,1)=\"J\",RIGHT(H901,LEN(H901)-4),RIGHT(H901,LEN(H901)-6)),\"\"))","v":""}]
[50000791,"Katek / Steca","Steca Xtender XTH 5000-24",null,4.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H902,1)=\"J\",LEFT(H902,2),LEFT(H902,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H902,1)=\"J\",RIGHT(H902,LEN(H902)-4),RIGHT(H902,LEN(H902)-6)),\"\"))","v":""}]
[50000792,"Katek / Steca","StecaGrid 4611_2",4.5999999999999996,4.5999999999999996,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-03-07","Christian Elbs","2023-01-11","Ländereinstellung TOR Erzeuger setzt das Limit auf 3,68 kVA",null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","18TH0316-OVE-directive R25_2","2021-06-15",null,"OK",null,null,null,null,null,null,null,"Verbauter Wechselrichter SolaxPower",null,{"$f":"IF(LEFT(H903,1)=\"J\",LEFT(H903,2),LEFT(H903,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H903,1)=\"J\",RIGHT(H903,LEN(H903)-4),RIGHT(H903,LEN(H903)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000793,"Katek / Steca","Solarix PLI 5000-48",5,5,1,"USV-Anwendung","Ja","2022-07-18",null,"2022-07-18",null,null,null,null,"Ja","Nein","Ja","nicht vorhanden","Martin Bertsch (OE)",null,null,null,null,null,null,null,null,"USV-Anwendung - kein R25 Prüfbericht erforderlich",null,null,null,null,{"$f":"IF(LEFT(H904,1)=\"J\",LEFT(H904,2),LEFT(H904,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H904,1)=\"J\",RIGHT(H904,LEN(H904)-4),RIGHT(H904,LEN(H904)-6)),\"\"))","v":""}]
[50000794,"Katek / Steca","Steca Solarix PLI 5000-48",5,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H905,1)=\"J\",LEFT(H905,2),LEFT(H905,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H905,1)=\"J\",RIGHT(H905,LEN(H905)-4),RIGHT(H905,LEN(H905)-6)),\"\"))","v":""}]
[50000795,"Katek / Steca","Steca Xtender XTH 6000-48",null,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H906,1)=\"J\",LEFT(H906,2),LEFT(H906,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H906,1)=\"J\",RIGHT(H906,LEN(H906)-4),RIGHT(H906,LEN(H906)-6)),\"\"))","v":""}]
[50000796,"Katek / Steca","StecaGrid 5011_2",5,5,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-03-07","Christian Elbs","2023-01-11","Ländereinstellung TOR Erzeuger setzt das Limit auf 3,68 kVA",null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","18TH0316-OVE-directive R25_2","2021-06-15",null,"OK",null,null,null,null,null,null,null,"Verbauter Wechselrichter SolaxPower",null,{"$f":"IF(LEFT(H907,1)=\"J\",LEFT(H907,2),LEFT(H907,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H907,1)=\"J\",RIGHT(H907,LEN(H907)-4),RIGHT(H907,LEN(H907)-6)),\"\"))","v":"<= 16A Anlage"}]
[50000797,"Katek / Steca","StecaGrid 5013",5,5,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-06-08",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","13TH0511-OVE-directive R25_1","2021-06-08",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25",null,null,"Verbauter Wechselrichter SolaxPower",null,{"$f":"IF(LEFT(H908,1)=\"J\",LEFT(H908,2),LEFT(H908,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H908,1)=\"J\",RIGHT(H908,LEN(H908)-4),RIGHT(H908,LEN(H908)-6)),\"\"))","v":""}]
[50000798,"Katek / Steca","StecaGrid 5513 ",5.5,5.5,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH0374-Hybird-OVE-Directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H909,1)=\"J\",LEFT(H909,2),LEFT(H909,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H909,1)=\"J\",RIGHT(H909,LEN(H909)-4),RIGHT(H909,LEN(H909)-6)),\"\"))","v":""}]
[50000799,"Katek / Steca","StecaGrid 6013",6,6,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-06-08",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","13TH0511-OVE-directive R25_1","2021-06-08",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25",null,null,"Verbauter Wechselrichter Goodwe",null,{"$f":"IF(LEFT(H910,1)=\"J\",LEFT(H910,2),LEFT(H910,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H910,1)=\"J\",RIGHT(H910,LEN(H910)-4),RIGHT(H910,LEN(H910)-6)),\"\"))","v":""}]
[50000800,"Katek / Steca","Steca Xtender XTH 8000-48",null,7,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H911,1)=\"J\",LEFT(H911,2),LEFT(H911,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H911,1)=\"J\",RIGHT(H911,LEN(H911)-4),RIGHT(H911,LEN(H911)-6)),\"\"))","v":""}]
[50000801,"Katek / Steca","StecaGrid 7013 ",7,7,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH0374-Hybird-OVE-Directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F","Verbauter Wechselrichter SolaxPower",null,{"$f":"IF(LEFT(H912,1)=\"J\",LEFT(H912,2),LEFT(H912,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H912,1)=\"J\",RIGHT(H912,LEN(H912)-4),RIGHT(H912,LEN(H912)-6)),\"\"))","v":""}]
[50000802,"Katek / Steca","StecaGrid 8513 ",8.5,8.5,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH0374-Hybird-OVE-Directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F","Verbauter Wechselrichter SolaxPower",null,{"$f":"IF(LEFT(H913,1)=\"J\",LEFT(H913,2),LEFT(H913,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H913,1)=\"J\",RIGHT(H913,LEN(H913)-4),RIGHT(H913,LEN(H913)-6)),\"\"))","v":""}]
[50000803,"Katek / Steca","StecaGrid 10013 ",10,10,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH0374-Hybird-OVE-Directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H914,1)=\"J\",LEFT(H914,2),LEFT(H914,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H914,1)=\"J\",RIGHT(H914,LEN(H914)-4),RIGHT(H914,LEN(H914)-6)),\"\"))","v":""}]
[50002297,"KEHUA","ESI215-100K-M",100,110,3,"AC-Batteriewechselrichter","Nein - In Prüfung","2024-06-19","Martin Bertsch",null,null,null,null,null,null,null,null,"Vorhanden",null,"PVP03133/24E-01","2024-05-30",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H915,1)=\"J\",LEFT(H915,2),LEFT(H915,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H915,1)=\"J\",RIGHT(H915,LEN(H915)-4),RIGHT(H915,LEN(H915)-6)),\"\"))","v":"In Prüfung"}]
[50000804,"KEHUA TECH","iStoragE3 5K",5,5.5,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-10-23","Martin Bertsch","2023-06-15",null,"2023-10-23","2023-10-23",null,"Ja","Nein",null,"Vorhanden",null,"64.290.23.30467.01","2023-05-29",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H916,1)=\"J\",LEFT(H916,2),LEFT(H916,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H916,1)=\"J\",RIGHT(H916,LEN(H916)-4),RIGHT(H916,LEN(H916)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000805,"KEHUA TECH","iStoragE3 6K",6,6.6,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-10-23","Martin Bertsch","2023-06-15",null,"2023-10-23","2023-10-23",null,"Ja","Nein",null,"Vorhanden",null,"64.290.23.30467.01","2023-05-29",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H917,1)=\"J\",LEFT(H917,2),LEFT(H917,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H917,1)=\"J\",RIGHT(H917,LEN(H917)-4),RIGHT(H917,LEN(H917)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000806,"KEHUA TECH","iStoragE3 8K",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-10-23","Martin Bertsch","2023-06-15",null,"2023-10-23","2023-10-23",null,"Ja","Nein",null,"Vorhanden",null,"64.290.23.30467.01","2023-05-29",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H918,1)=\"J\",LEFT(H918,2),LEFT(H918,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H918,1)=\"J\",RIGHT(H918,LEN(H918)-4),RIGHT(H918,LEN(H918)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000807,"KEHUA TECH","iStoragE3 10K",10,11,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-10-23","Martin Bertsch","2023-06-15",null,"2023-10-23","2023-10-23",null,"Ja","Nein",null,"Vorhanden",null,"64.290.23.30467.01","2023-05-29",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H919,1)=\"J\",LEFT(H919,2),LEFT(H919,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H919,1)=\"J\",RIGHT(H919,LEN(H919)-4),RIGHT(H919,LEN(H919)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000808,"KEHUA TECH","iStoragE3 12K",12,12,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-10-23","Martin Bertsch","2023-06-15",null,"2023-10-23","2023-10-23",null,"Ja","Nein",null,"Vorhanden",null,"64.290.23.30467.01","2023-05-29",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H920,1)=\"J\",LEFT(H920,2),LEFT(H920,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H920,1)=\"J\",RIGHT(H920,LEN(H920)-4),RIGHT(H920,LEN(H920)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50002295,"KONTRON","StecaGrid SolBrid 10-3-2 (optional mit Steca hy-switch)",10,10,3,"Hybrid-Wechselrichter","Ja, befristet","2024-06-17","Martin Bertsch","2024-06-19",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"23TH0372-OVE-directive R25_0","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H921,1)=\"J\",LEFT(H921,2),LEFT(H921,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H921,1)=\"J\",RIGHT(H921,LEN(H921)-4),RIGHT(H921,LEN(H921)-6)),\"\"))","v":"befristet"}]
[50002296,"KONTRON","StecaGrid SolBrid 10-3-4 (optional mit Steca hy-switch)",10,10,3,"Hybrid-Wechselrichter","Ja, befristet","2024-06-17","Martin Bertsch","2024-06-19",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"23TH0372-OVE-directive R25_0","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H922,1)=\"J\",LEFT(H922,2),LEFT(H922,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H922,1)=\"J\",RIGHT(H922,LEN(H922)-4),RIGHT(H922,LEN(H922)-6)),\"\"))","v":"befristet"}]
[50000809,"KOPP GERMANY","KOPP.Kuara 5.0-3-AC",5,5.5,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H923,1)=\"J\",LEFT(H923,2),LEFT(H923,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H923,1)=\"J\",RIGHT(H923,LEN(H923)-4),RIGHT(H923,LEN(H923)-6)),\"\"))","v":"mit Einschränkung"}]
[50000810,"KOPP GERMANY","KOPP.Kuara 5.0-3-H",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H924,1)=\"J\",LEFT(H924,2),LEFT(H924,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H924,1)=\"J\",RIGHT(H924,LEN(H924)-4),RIGHT(H924,LEN(H924)-6)),\"\"))","v":"mit Einschränkung"}]
[50000811,"KOPP GERMANY","KOPP.Kuara 6.0-3-AC",6,6.6,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H925,1)=\"J\",LEFT(H925,2),LEFT(H925,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H925,1)=\"J\",RIGHT(H925,LEN(H925)-4),RIGHT(H925,LEN(H925)-6)),\"\"))","v":"mit Einschränkung"}]
[50000812,"KOPP GERMANY","KOPP.Kuara 6.0-3-H",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H926,1)=\"J\",LEFT(H926,2),LEFT(H926,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H926,1)=\"J\",RIGHT(H926,LEN(H926)-4),RIGHT(H926,LEN(H926)-6)),\"\"))","v":"mit Einschränkung"}]
[50000813,"KOPP GERMANY","KOPP.Kuara 8.0-3-AC",8,8.8000000000000007,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H927,1)=\"J\",LEFT(H927,2),LEFT(H927,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H927,1)=\"J\",RIGHT(H927,LEN(H927)-4),RIGHT(H927,LEN(H927)-6)),\"\"))","v":"mit Einschränkung"}]
[50000814,"KOPP GERMANY","KOPP.Kuara 8.0-3-H",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H928,1)=\"J\",LEFT(H928,2),LEFT(H928,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H928,1)=\"J\",RIGHT(H928,LEN(H928)-4),RIGHT(H928,LEN(H928)-6)),\"\"))","v":"mit Einschränkung"}]
[50000815,"KOPP GERMANY","KOPP.Kuara 10.0-3-AC",10,11,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H929,1)=\"J\",LEFT(H929,2),LEFT(H929,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H929,1)=\"J\",RIGHT(H929,LEN(H929)-4),RIGHT(H929,LEN(H929)-6)),\"\"))","v":"mit Einschränkung"}]
[50000816,"KOPP GERMANY","KOPP.Kuara 10.0-3-H",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H930,1)=\"J\",LEFT(H930,2),LEFT(H930,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H930,1)=\"J\",RIGHT(H930,LEN(H930)-4),RIGHT(H930,LEN(H930)-6)),\"\"))","v":"mit Einschränkung"}]
[50000817,"KOPP GERMANY","KOPP.Kuara 12.0-3-AC ",12,13.2,3,"AC-Batteriewechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H931,1)=\"J\",LEFT(H931,2),LEFT(H931,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H931,1)=\"J\",RIGHT(H931,LEN(H931)-4),RIGHT(H931,LEN(H931)-6)),\"\"))","v":"mit Einschränkung"}]
[50000818,"KOPP GERMANY","KOPP.Kuara 12.0-3-H",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-23","Martin Bertsch","2023-04-27","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CGDY-ESH-P23031401","2023-04-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H932,1)=\"J\",LEFT(H932,2),LEFT(H932,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H932,1)=\"J\",RIGHT(H932,LEN(H932)-4),RIGHT(H932,LEN(H932)-6)),\"\"))","v":"mit Einschränkung"}]
[50000819,"Kostal","PIKO MP plus 1.5-1 ",1.5,1.5,1,"Hybrid-Wechselrichter","Ja","2022-06-07",null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"18TH0316-PIKO-Hybrid-OVE-directive R5_3","2021-06-15",null,"nicht OK",null,null,null,null,"FRT passt nicht",null,null,null,null,{"$f":"IF(LEFT(H933,1)=\"J\",LEFT(H933,2),LEFT(H933,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H933,1)=\"J\",RIGHT(H933,LEN(H933)-4),RIGHT(H933,LEN(H933)-6)),\"\"))","v":""}]
[50000820,"Kostal","PIKO MP plus 2.0-1 ",2,2,1,"Hybrid-Wechselrichter","Ja","2022-06-07",null,"2021-03-26",null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"18TH0316-PIKO-Hybrid-OVE-directive R5_3","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H934,1)=\"J\",LEFT(H934,2),LEFT(H934,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H934,1)=\"J\",RIGHT(H934,LEN(H934)-4),RIGHT(H934,LEN(H934)-6)),\"\"))","v":""}]
[50000821,"Kostal","PIKO MP plus 2.5-1 ",2.5,2.5,1,"Hybrid-Wechselrichter","Ja","2022-06-07",null,"2021-03-26",null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"18TH0316-PIKO-Hybrid-OVE-directive R5_3","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H935,1)=\"J\",LEFT(H935,2),LEFT(H935,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H935,1)=\"J\",RIGHT(H935,LEN(H935)-4),RIGHT(H935,LEN(H935)-6)),\"\"))","v":""}]
[50000822,"Kostal","PIKO IQ 3.0 ",3,3,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H936,1)=\"J\",LEFT(H936,2),LEFT(H936,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H936,1)=\"J\",RIGHT(H936,LEN(H936)-4),RIGHT(H936,LEN(H936)-6)),\"\"))","v":""}]
[50000823,"Kostal","PIKO MP plus 3.0-1 ",3,3,1,"Hybrid-Wechselrichter","Ja","2022-06-07",null,"2021-03-26",null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"18TH0316-PIKO-Hybrid-OVE-directive R5_3","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H937,1)=\"J\",LEFT(H937,2),LEFT(H937,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H937,1)=\"J\",RIGHT(H937,LEN(H937)-4),RIGHT(H937,LEN(H937)-6)),\"\"))","v":""}]
[50000824,"Kostal","PIKO MP plus 3.0-2 ",3,3,1,"Hybrid-Wechselrichter","Ja","2022-06-07",null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"18TH0316-PIKO-Hybrid-OVE-directive R5_3","2021-06-15",null,"nicht OK",null,null,null,null,"FRT passt nicht",null,null,null,null,{"$f":"IF(LEFT(H938,1)=\"J\",LEFT(H938,2),LEFT(H938,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H938,1)=\"J\",RIGHT(H938,LEN(H938)-4),RIGHT(H938,LEN(H938)-6)),\"\"))","v":""}]
[50000825,"Kostal","PLENTICORE plus 3.0 ",3,3,3,"Hybrid-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H939,1)=\"J\",LEFT(H939,2),LEFT(H939,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H939,1)=\"J\",RIGHT(H939,LEN(H939)-4),RIGHT(H939,LEN(H939)-6)),\"\"))","v":""}]
[50000826,"Kostal","PLENTICORE plus 3.0 G2",3,3,3,"Hybrid-Wechselrichter","Ja","2022-09-05","Christian Elbs","2022-09-05",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0374-Hybrid-G2-OVE-directive R25_0","2022-08-10",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H940,1)=\"J\",LEFT(H940,2),LEFT(H940,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H940,1)=\"J\",RIGHT(H940,LEN(H940)-4),RIGHT(H940,LEN(H940)-6)),\"\"))","v":""}]
[50000827,"Kostal","PIKO MP plus 3.6-1 ",3.68,3.7,1,"Hybrid-Wechselrichter","Ja","2022-06-07",null,"2021-03-26",null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"18TH0316-PIKO-Hybrid-OVE-directive R5_3","2021-06-15",null,"OK",null,null,null,null,"Stringwechselrichter 1~ nur 3~ Anschluss gestattet - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H941,1)=\"J\",LEFT(H941,2),LEFT(H941,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H941,1)=\"J\",RIGHT(H941,LEN(H941)-4),RIGHT(H941,LEN(H941)-6)),\"\"))","v":""}]
[50000828,"Kostal","PIKO MP plus 3.6-2 ",3.68,3.7,1,"Hybrid-Wechselrichter","Ja","2022-06-07",null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"18TH0316-PIKO-Hybrid-OVE-directive R5_3","2021-06-15",null,"nicht OK",null,null,null,null,"FRT passt nicht",null,null,null,null,{"$f":"IF(LEFT(H942,1)=\"J\",LEFT(H942,2),LEFT(H942,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H942,1)=\"J\",RIGHT(H942,LEN(H942)-4),RIGHT(H942,LEN(H942)-6)),\"\"))","v":""}]
[50000829,"Kostal","PIKO IQ 4.2 ",4.2,4.2,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H943,1)=\"J\",LEFT(H943,2),LEFT(H943,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H943,1)=\"J\",RIGHT(H943,LEN(H943)-4),RIGHT(H943,LEN(H943)-6)),\"\"))","v":""}]
[50000830,"Kostal","PLENTICORE plus 4.2 ",4.2,4.2,3,"Hybrid-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H944,1)=\"J\",LEFT(H944,2),LEFT(H944,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H944,1)=\"J\",RIGHT(H944,LEN(H944)-4),RIGHT(H944,LEN(H944)-6)),\"\"))","v":""}]
[50000831,"Kostal","PLENTICORE plus 4.2 G2",4.2,4.2,3,"Hybrid-Wechselrichter","Ja","2022-09-05","Christian Elbs","2022-09-05",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0374-Hybrid-G2-OVE-directive R25_0","2022-08-10",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H945,1)=\"J\",LEFT(H945,2),LEFT(H945,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H945,1)=\"J\",RIGHT(H945,LEN(H945)-4),RIGHT(H945,LEN(H945)-6)),\"\"))","v":""}]
[50000832,"Kostal","PIKO MP plus 4.6-2 ",4.5999999999999996,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein","2022-06-07",null,null,null,null,null,null,null,null,null,"Vorhanden",null,"18TH0316-PIKO-Hybrid-OVE-directive R5_3","2021-06-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H946,1)=\"J\",LEFT(H946,2),LEFT(H946,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H946,1)=\"J\",RIGHT(H946,LEN(H946)-4),RIGHT(H946,LEN(H946)-6)),\"\"))","v":""}]
[50000833,"Kostal","PIKO MP plus 5.0-2 ",5,5,1,"Hybrid-Wechselrichter","Nein","2022-06-07",null,null,null,null,null,null,null,null,null,"Vorhanden",null,"18TH0316-PIKO-Hybrid-OVE-directive R5_3","2021-06-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H947,1)=\"J\",LEFT(H947,2),LEFT(H947,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H947,1)=\"J\",RIGHT(H947,LEN(H947)-4),RIGHT(H947,LEN(H947)-6)),\"\"))","v":""}]
[50000834,"Kostal","PIKO IQ 5.5 ",5.5,5.5,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H948,1)=\"J\",LEFT(H948,2),LEFT(H948,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H948,1)=\"J\",RIGHT(H948,LEN(H948)-4),RIGHT(H948,LEN(H948)-6)),\"\"))","v":""}]
[50000835,"Kostal","PLENTICORE BI 5.5/13  ",5.5,5.5,3,"AC-Batteriewechselrichter","Ja","2022-06-07",null,"2022-06-07",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0374-OVE-directive R25_0","2019-09-17",null,"OK",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H949,1)=\"J\",LEFT(H949,2),LEFT(H949,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H949,1)=\"J\",RIGHT(H949,LEN(H949)-4),RIGHT(H949,LEN(H949)-6)),\"\"))","v":""}]
[50000836,"Kostal","PLENTICORE BI 5.5/26  ",5.5,5.5,3,"AC-Batteriewechselrichter","Ja","2022-06-07",null,"2022-06-07",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0374-OVE-directive R25_0","2019-09-17",null,"OK",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H950,1)=\"J\",LEFT(H950,2),LEFT(H950,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H950,1)=\"J\",RIGHT(H950,LEN(H950)-4),RIGHT(H950,LEN(H950)-6)),\"\"))","v":""}]
[50000837,"Kostal","PLENTICORE BI 5.5/26 G2",5,5.5,3,"AC-Batteriewechselrichter","Ja","2023-05-22","Martin Bertsch","2023-05-22",null,null,null,null,null,null,null,"Vorhanden",null,"19TH0374_BI-G2-OVE-directive R25_0","2023-03-14",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H951,1)=\"J\",LEFT(H951,2),LEFT(H951,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H951,1)=\"J\",RIGHT(H951,LEN(H951)-4),RIGHT(H951,LEN(H951)-6)),\"\"))","v":""}]
[50000838,"Kostal","PLENTICORE plus 5.5 ",5.5,5.5,3,"Hybrid-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H952,1)=\"J\",LEFT(H952,2),LEFT(H952,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H952,1)=\"J\",RIGHT(H952,LEN(H952)-4),RIGHT(H952,LEN(H952)-6)),\"\"))","v":""}]
[50000839,"Kostal","PLENTICORE plus 5.5 G2",5.5,5.5,3,"Hybrid-Wechselrichter","Ja","2022-09-05","Christian Elbs","2022-09-05",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0374-Hybrid-G2-OVE-directive R25_0","2022-08-10",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H953,1)=\"J\",LEFT(H953,2),LEFT(H953,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H953,1)=\"J\",RIGHT(H953,LEN(H953)-4),RIGHT(H953,LEN(H953)-6)),\"\"))","v":""}]
[50000840,"Kostal","PIKO IQ 7.0 ",7,7,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H954,1)=\"J\",LEFT(H954,2),LEFT(H954,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H954,1)=\"J\",RIGHT(H954,LEN(H954)-4),RIGHT(H954,LEN(H954)-6)),\"\"))","v":""}]
[50000841,"Kostal","PLENTICORE plus 7.0 ",7,7,3,"Hybrid-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H955,1)=\"J\",LEFT(H955,2),LEFT(H955,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H955,1)=\"J\",RIGHT(H955,LEN(H955)-4),RIGHT(H955,LEN(H955)-6)),\"\"))","v":""}]
[50000842,"Kostal","PLENTICORE plus 7.0 G2",7,7,3,"Hybrid-Wechselrichter","Ja","2022-09-05","Christian Elbs","2022-09-05",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0374-Hybrid-G2-OVE-directive R25_0","2022-08-10",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H956,1)=\"J\",LEFT(H956,2),LEFT(H956,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H956,1)=\"J\",RIGHT(H956,LEN(H956)-4),RIGHT(H956,LEN(H956)-6)),\"\"))","v":""}]
[50002092,"Kostal","PLENTICORE S G3",6.3,7,3,"PV-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-07-31",null,null,"Nein",null,"Nein","Vorhanden",null,"22PP512-04_0","2024-03-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H957,1)=\"J\",LEFT(H957,2),LEFT(H957,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H957,1)=\"J\",RIGHT(H957,LEN(H957)-4),RIGHT(H957,LEN(H957)-6)),\"\"))","v":"befristet"}]
[50000843,"Kostal","PIKO IQ 8.5 ",8.5,8.5,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H958,1)=\"J\",LEFT(H958,2),LEFT(H958,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H958,1)=\"J\",RIGHT(H958,LEN(H958)-4),RIGHT(H958,LEN(H958)-6)),\"\"))","v":""}]
[50000844,"Kostal","PLENTICORE plus 8.5 ",8.5,8.5,3,"Hybrid-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H959,1)=\"J\",LEFT(H959,2),LEFT(H959,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H959,1)=\"J\",RIGHT(H959,LEN(H959)-4),RIGHT(H959,LEN(H959)-6)),\"\"))","v":""}]
[50000845,"Kostal","PLENTICORE plus 8.5 G2",8.5,8.5,3,"Hybrid-Wechselrichter","Ja","2022-09-05","Christian Elbs","2022-09-05",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0374-Hybrid-G2-OVE-directive R25_0","2022-08-10",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H960,1)=\"J\",LEFT(H960,2),LEFT(H960,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H960,1)=\"J\",RIGHT(H960,LEN(H960)-4),RIGHT(H960,LEN(H960)-6)),\"\"))","v":""}]
[50000846,"Kostal","PIKO 10 ",10,10,3,"PV-Wechselrichter","Ja","2022-07-04","Christian Elbs",null,"6.17",null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"19TH0373-OVE-directive R25_0","2021-06-14","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F","Verbauter Wechselrichter SolaxPower",null,{"$f":"IF(LEFT(H961,1)=\"J\",LEFT(H961,2),LEFT(H961,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H961,1)=\"J\",RIGHT(H961,LEN(H961)-4),RIGHT(H961,LEN(H961)-6)),\"\"))","v":""}]
[50000847,"Kostal","PIKO IQ 10.0",10,10,3,"PV-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H962,1)=\"J\",LEFT(H962,2),LEFT(H962,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H962,1)=\"J\",RIGHT(H962,LEN(H962)-4),RIGHT(H962,LEN(H962)-6)),\"\"))","v":""}]
[50000848,"Kostal","PLENTICORE BI 10/26  ",10,10,3,"AC-Batteriewechselrichter","Ja","2022-06-07",null,"2022-06-07",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0374-OVE-directive R25_0","2019-09-17",null,"OK",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H963,1)=\"J\",LEFT(H963,2),LEFT(H963,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H963,1)=\"J\",RIGHT(H963,LEN(H963)-4),RIGHT(H963,LEN(H963)-6)),\"\"))","v":""}]
[50000849,"Kostal","PLENTICORE BI 10/26 G2  ",9,10,3,"AC-Batteriewechselrichter","Ja","2023-05-22","Martin Bertsch","2023-05-22",null,null,null,null,null,null,null,"Vorhanden",null,"19TH0374_BI-G2-OVE-directive R25_0","2023-03-14",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H964,1)=\"J\",LEFT(H964,2),LEFT(H964,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H964,1)=\"J\",RIGHT(H964,LEN(H964)-4),RIGHT(H964,LEN(H964)-6)),\"\"))","v":""}]
[50000850,"Kostal","PLENTICORE plus 10.0 ",10,10,3,"Hybrid-Wechselrichter","Ja","2023-03-07","Christian Elbs","2021-03-16",null,null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","19TH03774-Hybrid-OVE-directive R25_0","2021-03-16",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H965,1)=\"J\",LEFT(H965,2),LEFT(H965,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H965,1)=\"J\",RIGHT(H965,LEN(H965)-4),RIGHT(H965,LEN(H965)-6)),\"\"))","v":""}]
[50000851,"Kostal","PLENTICORE plus 10.0 G2",10,10,3,"Hybrid-Wechselrichter","Ja","2022-09-05","Christian Elbs","2022-09-05",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0374-Hybrid-G2-OVE-directive R25_0","2022-08-10",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H966,1)=\"J\",LEFT(H966,2),LEFT(H966,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H966,1)=\"J\",RIGHT(H966,LEN(H966)-4),RIGHT(H966,LEN(H966)-6)),\"\"))","v":""}]
[50000852,"Kostal","PIKO 12 ",12,12,3,"PV-Wechselrichter","Ja","2022-07-04","Christian Elbs",null,"6.17",null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"19TH0373-OVE-directive R25_0","2021-06-14","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H967,1)=\"J\",LEFT(H967,2),LEFT(H967,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H967,1)=\"J\",RIGHT(H967,LEN(H967)-4),RIGHT(H967,LEN(H967)-6)),\"\"))","v":""}]
[50002091,"Kostal","PLENTICORE M G3",11.25,12.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-07-31",null,null,"Nein",null,"Nein","Vorhanden",null,"22PP512-04_0","2024-03-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H968,1)=\"J\",LEFT(H968,2),LEFT(H968,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H968,1)=\"J\",RIGHT(H968,LEN(H968)-4),RIGHT(H968,LEN(H968)-6)),\"\"))","v":"befristet"}]
[50000853,"Kostal","PIKO 15 ",15,15,3,"PV-Wechselrichter","Ja","2022-07-04","Christian Elbs",null,"6.17",null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"19TH0373-OVE-directive R25_0","2021-06-14","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H969,1)=\"J\",LEFT(H969,2),LEFT(H969,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H969,1)=\"J\",RIGHT(H969,LEN(H969)-4),RIGHT(H969,LEN(H969)-6)),\"\"))","v":""}]
[50000854,"Kostal","PIKO 17 ",17,17,3,"PV-Wechselrichter","Ja","2022-07-04","Christian Elbs",null,"6.17",null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"19TH0373-OVE-directive R25_0","2021-06-14","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H970,1)=\"J\",LEFT(H970,2),LEFT(H970,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H970,1)=\"J\",RIGHT(H970,LEN(H970)-4),RIGHT(H970,LEN(H970)-6)),\"\"))","v":""}]
[50000855,"Kostal","PIKO 20 ",20,20,3,"PV-Wechselrichter","Ja","2022-07-04","Christian Elbs",null,"6.17",null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"19TH0373-OVE-directive R25_0","2021-06-14","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H971,1)=\"J\",LEFT(H971,2),LEFT(H971,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H971,1)=\"J\",RIGHT(H971,LEN(H971)-4),RIGHT(H971,LEN(H971)-6)),\"\"))","v":""}]
[50002090,"Kostal","PLENTICORE L G3",18,20,3,"PV-Wechselrichter","Ja, befristet","2024-05-20","Martin Bertsch","2024-05-20",null,"2024-07-31",null,null,"Nein",null,"Nein","Vorhanden",null,"22PP512-04_0","2024-03-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H972,1)=\"J\",LEFT(H972,2),LEFT(H972,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H972,1)=\"J\",RIGHT(H972,LEN(H972)-4),RIGHT(H972,LEN(H972)-6)),\"\"))","v":"befristet"}]
[50000856,"Kostal","PIKO CI 30",30,33,3,"PV-Wechselrichter","Ja","2023-05-08","Martin Bertsch","2022-06-15",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger","PV2105WDG0066-1-R2","2022-11-02","Vorhanden","OK",null,null,null,null,null,"F","F",null,null,{"$f":"IF(LEFT(H973,1)=\"J\",LEFT(H973,2),LEFT(H973,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H973,1)=\"J\",RIGHT(H973,LEN(H973)-4),RIGHT(H973,LEN(H973)-6)),\"\"))","v":""}]
[50000857,"Kostal","PIKO CI 50",55,55,3,"PV-Wechselrichter","Ja","2023-06-21","Martin Bertsch",null,null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger","PV2105WDG0065","2021-10-20","Vorhanden","OK",null,null,null,"Ja, keine N-Überwachung durch ENS","Stringwechselrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H974,1)=\"J\",LEFT(H974,2),LEFT(H974,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H974,1)=\"J\",RIGHT(H974,LEN(H974)-4),RIGHT(H974,LEN(H974)-6)),\"\"))","v":""}]
[50000858,"Kostal","PIKO CI 60",66,66,3,"PV-Wechselrichter","Ja","2023-06-21","Martin Bertsch",null,null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger","PV2105WDG0065","2021-10-20","Vorhanden","OK",null,null,null,"Ja, keine N-Überwachung durch ENS","Stringwechselrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H975,1)=\"J\",LEFT(H975,2),LEFT(H975,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H975,1)=\"J\",RIGHT(H975,LEN(H975)-4),RIGHT(H975,LEN(H975)-6)),\"\"))","v":""}]
[50001680,"KOYOE","KY-EST06KH ",6,6,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H976,1)=\"J\",LEFT(H976,2),LEFT(H976,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H976,1)=\"J\",RIGHT(H976,LEN(H976)-4),RIGHT(H976,LEN(H976)-6)),\"\"))","v":""}]
[50002259,"KOYOE","KY-EST06KH-A",6,6,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H977,1)=\"J\",LEFT(H977,2),LEFT(H977,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H977,1)=\"J\",RIGHT(H977,LEN(H977)-4),RIGHT(H977,LEN(H977)-6)),\"\"))","v":""}]
[50001699,"KOYOE","KY-EST06KH-S",6,6,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H978,1)=\"J\",LEFT(H978,2),LEFT(H978,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H978,1)=\"J\",RIGHT(H978,LEN(H978)-4),RIGHT(H978,LEN(H978)-6)),\"\"))","v":""}]
[50000860,"KOYOE","KY-EST08KH ",8,8,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H979,1)=\"J\",LEFT(H979,2),LEFT(H979,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H979,1)=\"J\",RIGHT(H979,LEN(H979)-4),RIGHT(H979,LEN(H979)-6)),\"\"))","v":""}]
[50002260,"KOYOE","KY-EST08KH-A",8,8,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H980,1)=\"J\",LEFT(H980,2),LEFT(H980,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H980,1)=\"J\",RIGHT(H980,LEN(H980)-4),RIGHT(H980,LEN(H980)-6)),\"\"))","v":""}]
[50001700,"KOYOE","KY-EST08KH-S",8,8,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H981,1)=\"J\",LEFT(H981,2),LEFT(H981,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H981,1)=\"J\",RIGHT(H981,LEN(H981)-4),RIGHT(H981,LEN(H981)-6)),\"\"))","v":""}]
[50000861,"KOYOE","KY-EST10KH ",10,10,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H982,1)=\"J\",LEFT(H982,2),LEFT(H982,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H982,1)=\"J\",RIGHT(H982,LEN(H982)-4),RIGHT(H982,LEN(H982)-6)),\"\"))","v":""}]
[50002261,"KOYOE","KY-EST10KH-A",10,10,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H983,1)=\"J\",LEFT(H983,2),LEFT(H983,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H983,1)=\"J\",RIGHT(H983,LEN(H983)-4),RIGHT(H983,LEN(H983)-6)),\"\"))","v":""}]
[50001701,"KOYOE","KY-EST10KH-S",10,10,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H984,1)=\"J\",LEFT(H984,2),LEFT(H984,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H984,1)=\"J\",RIGHT(H984,LEN(H984)-4),RIGHT(H984,LEN(H984)-6)),\"\"))","v":""}]
[50000862,"KOYOE","KY-EST12KH ",12,12,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H985,1)=\"J\",LEFT(H985,2),LEFT(H985,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H985,1)=\"J\",RIGHT(H985,LEN(H985)-4),RIGHT(H985,LEN(H985)-6)),\"\"))","v":""}]
[50002262,"KOYOE","KY-EST12KH-A",12,12,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H986,1)=\"J\",LEFT(H986,2),LEFT(H986,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H986,1)=\"J\",RIGHT(H986,LEN(H986)-4),RIGHT(H986,LEN(H986)-6)),\"\"))","v":""}]
[50001702,"KOYOE","KY-EST12KH-S",12,12,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H987,1)=\"J\",LEFT(H987,2),LEFT(H987,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H987,1)=\"J\",RIGHT(H987,LEN(H987)-4),RIGHT(H987,LEN(H987)-6)),\"\"))","v":""}]
[50000863,"KOYOE","KY-EST15KH",15,15,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H988,1)=\"J\",LEFT(H988,2),LEFT(H988,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H988,1)=\"J\",RIGHT(H988,LEN(H988)-4),RIGHT(H988,LEN(H988)-6)),\"\"))","v":""}]
[50002263,"KOYOE","KY-EST15KH-A",15,15,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H989,1)=\"J\",LEFT(H989,2),LEFT(H989,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H989,1)=\"J\",RIGHT(H989,LEN(H989)-4),RIGHT(H989,LEN(H989)-6)),\"\"))","v":""}]
[50001703,"KOYOE","KY-EST15KH-S",15,15,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H990,1)=\"J\",LEFT(H990,2),LEFT(H990,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H990,1)=\"J\",RIGHT(H990,LEN(H990)-4),RIGHT(H990,LEN(H990)-6)),\"\"))","v":""}]
[50000864,"KOYOE","KY-EST17KH ",17,17,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H991,1)=\"J\",LEFT(H991,2),LEFT(H991,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H991,1)=\"J\",RIGHT(H991,LEN(H991)-4),RIGHT(H991,LEN(H991)-6)),\"\"))","v":""}]
[50002264,"KOYOE","KY-EST17KH-A",17,17,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H992,1)=\"J\",LEFT(H992,2),LEFT(H992,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H992,1)=\"J\",RIGHT(H992,LEN(H992)-4),RIGHT(H992,LEN(H992)-6)),\"\"))","v":""}]
[50001704,"KOYOE","KY-EST17KH-S",17,17,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H993,1)=\"J\",LEFT(H993,2),LEFT(H993,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H993,1)=\"J\",RIGHT(H993,LEN(H993)-4),RIGHT(H993,LEN(H993)-6)),\"\"))","v":""}]
[50000865,"KOYOE","KY-EST20KH ",20,20,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H994,1)=\"J\",LEFT(H994,2),LEFT(H994,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H994,1)=\"J\",RIGHT(H994,LEN(H994)-4),RIGHT(H994,LEN(H994)-6)),\"\"))","v":""}]
[50002265,"KOYOE","KY-EST20KH-A",20,20,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H995,1)=\"J\",LEFT(H995,2),LEFT(H995,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H995,1)=\"J\",RIGHT(H995,LEN(H995)-4),RIGHT(H995,LEN(H995)-6)),\"\"))","v":""}]
[50001705,"KOYOE","KY-EST20KH-S",20,20,3,"Hybrid-Wechselrichter","Nein","2024-05-22","Martin Bertsch",null,null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger","CIPL-ESH-P23111559","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H996,1)=\"J\",LEFT(H996,2),LEFT(H996,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H996,1)=\"J\",RIGHT(H996,LEN(H996)-4),RIGHT(H996,LEN(H996)-6)),\"\"))","v":""}]
[50000866,"KSTAR","E8KT",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein","2023-10-18","Martin Bertsch",null,null,null,null,"Gerät wurde beim AIT überprüft; erfüllt Network Code nicht.",null,null,null,"Vorhanden",null,"64.290.23.30352.01","2023-03-25",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H997,1)=\"J\",LEFT(H997,2),LEFT(H997,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H997,1)=\"J\",RIGHT(H997,LEN(H997)-4),RIGHT(H997,LEN(H997)-6)),\"\"))","v":""}]
[50000867,"KSTAR","E10KT",10,11,3,"Hybrid-Wechselrichter","Nein","2023-10-18","Martin Bertsch",null,null,null,null,"Gerät wurde beim AIT überprüft; erfüllt Network Code nicht.",null,null,null,"Vorhanden",null,"64.290.23.30352.01","2023-03-25",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H998,1)=\"J\",LEFT(H998,2),LEFT(H998,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H998,1)=\"J\",RIGHT(H998,LEN(H998)-4),RIGHT(H998,LEN(H998)-6)),\"\"))","v":""}]
[50000868,"KSTAR","E12KT",12,13.2,3,"Hybrid-Wechselrichter","Nein","2023-10-18","Martin Bertsch",null,null,null,null,"Gerät wurde beim AIT überprüft; erfüllt Network Code nicht.",null,null,null,"Vorhanden",null,"64.290.23.30352.01","2023-03-25",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H999,1)=\"J\",LEFT(H999,2),LEFT(H999,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H999,1)=\"J\",RIGHT(H999,LEN(H999)-4),RIGHT(H999,LEN(H999)-6)),\"\"))","v":""}]
[50000869,"KSTAR","KSG-25KT-M0",25,27.5,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1000,1)=\"J\",LEFT(H1000,2),LEFT(H1000,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1000,1)=\"J\",RIGHT(H1000,LEN(H1000)-4),RIGHT(H1000,LEN(H1000)-6)),\"\"))","v":"In Prüfung"}]
[50000870,"KSTAR","KSG-25KT-M1",25,27.5,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1001,1)=\"J\",LEFT(H1001,2),LEFT(H1001,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1001,1)=\"J\",RIGHT(H1001,LEN(H1001)-4),RIGHT(H1001,LEN(H1001)-6)),\"\"))","v":"In Prüfung"}]
[50000871,"KSTAR","KSG-25KT-M2",25,27.5,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1002,1)=\"J\",LEFT(H1002,2),LEFT(H1002,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1002,1)=\"J\",RIGHT(H1002,LEN(H1002)-4),RIGHT(H1002,LEN(H1002)-6)),\"\"))","v":"In Prüfung"}]
[50000872,"KSTAR","KSG-25KT-M3",25,27.5,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1003,1)=\"J\",LEFT(H1003,2),LEFT(H1003,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1003,1)=\"J\",RIGHT(H1003,LEN(H1003)-4),RIGHT(H1003,LEN(H1003)-6)),\"\"))","v":"In Prüfung"}]
[50000873,"KSTAR","KSG-30KT-M0",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1004,1)=\"J\",LEFT(H1004,2),LEFT(H1004,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1004,1)=\"J\",RIGHT(H1004,LEN(H1004)-4),RIGHT(H1004,LEN(H1004)-6)),\"\"))","v":"In Prüfung"}]
[50000874,"KSTAR","KSG-30KT-M1",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1005,1)=\"J\",LEFT(H1005,2),LEFT(H1005,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1005,1)=\"J\",RIGHT(H1005,LEN(H1005)-4),RIGHT(H1005,LEN(H1005)-6)),\"\"))","v":"In Prüfung"}]
[50000875,"KSTAR","KSG-30KT-M2",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1006,1)=\"J\",LEFT(H1006,2),LEFT(H1006,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1006,1)=\"J\",RIGHT(H1006,LEN(H1006)-4),RIGHT(H1006,LEN(H1006)-6)),\"\"))","v":"In Prüfung"}]
[50000876,"KSTAR","KSG-30KT-M3",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1007,1)=\"J\",LEFT(H1007,2),LEFT(H1007,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1007,1)=\"J\",RIGHT(H1007,LEN(H1007)-4),RIGHT(H1007,LEN(H1007)-6)),\"\"))","v":"In Prüfung"}]
[50000877,"KSTAR","KSG-30KT-M4",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1008,1)=\"J\",LEFT(H1008,2),LEFT(H1008,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1008,1)=\"J\",RIGHT(H1008,LEN(H1008)-4),RIGHT(H1008,LEN(H1008)-6)),\"\"))","v":"In Prüfung"}]
[50000878,"KSTAR","KSG-30KT-M5",30,33,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1009,1)=\"J\",LEFT(H1009,2),LEFT(H1009,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1009,1)=\"J\",RIGHT(H1009,LEN(H1009)-4),RIGHT(H1009,LEN(H1009)-6)),\"\"))","v":"In Prüfung"}]
[50000879,"KSTAR","KSG-33KT-M0",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1010,1)=\"J\",LEFT(H1010,2),LEFT(H1010,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1010,1)=\"J\",RIGHT(H1010,LEN(H1010)-4),RIGHT(H1010,LEN(H1010)-6)),\"\"))","v":"In Prüfung"}]
[50000880,"KSTAR","KSG-33KT-M1",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1011,1)=\"J\",LEFT(H1011,2),LEFT(H1011,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1011,1)=\"J\",RIGHT(H1011,LEN(H1011)-4),RIGHT(H1011,LEN(H1011)-6)),\"\"))","v":"In Prüfung"}]
[50000881,"KSTAR","KSG-33KT-M2",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1012,1)=\"J\",LEFT(H1012,2),LEFT(H1012,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1012,1)=\"J\",RIGHT(H1012,LEN(H1012)-4),RIGHT(H1012,LEN(H1012)-6)),\"\"))","v":"In Prüfung"}]
[50000882,"KSTAR","KSG-33KT-M3",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1013,1)=\"J\",LEFT(H1013,2),LEFT(H1013,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1013,1)=\"J\",RIGHT(H1013,LEN(H1013)-4),RIGHT(H1013,LEN(H1013)-6)),\"\"))","v":"In Prüfung"}]
[50000883,"KSTAR","KSG-33KT-M4",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1014,1)=\"J\",LEFT(H1014,2),LEFT(H1014,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1014,1)=\"J\",RIGHT(H1014,LEN(H1014)-4),RIGHT(H1014,LEN(H1014)-6)),\"\"))","v":"In Prüfung"}]
[50000884,"KSTAR","KSG-33KT-M5",33,36.299999999999997,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1015,1)=\"J\",LEFT(H1015,2),LEFT(H1015,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1015,1)=\"J\",RIGHT(H1015,LEN(H1015)-4),RIGHT(H1015,LEN(H1015)-6)),\"\"))","v":"In Prüfung"}]
[50000885,"KSTAR","KSG-36KT-M0",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1016,1)=\"J\",LEFT(H1016,2),LEFT(H1016,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1016,1)=\"J\",RIGHT(H1016,LEN(H1016)-4),RIGHT(H1016,LEN(H1016)-6)),\"\"))","v":"In Prüfung"}]
[50000886,"KSTAR","KSG-36KT-M1",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1017,1)=\"J\",LEFT(H1017,2),LEFT(H1017,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1017,1)=\"J\",RIGHT(H1017,LEN(H1017)-4),RIGHT(H1017,LEN(H1017)-6)),\"\"))","v":"In Prüfung"}]
[50000887,"KSTAR","KSG-36KT-M2",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1018,1)=\"J\",LEFT(H1018,2),LEFT(H1018,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1018,1)=\"J\",RIGHT(H1018,LEN(H1018)-4),RIGHT(H1018,LEN(H1018)-6)),\"\"))","v":"In Prüfung"}]
[50000888,"KSTAR","KSG-36KT-M3",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1019,1)=\"J\",LEFT(H1019,2),LEFT(H1019,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1019,1)=\"J\",RIGHT(H1019,LEN(H1019)-4),RIGHT(H1019,LEN(H1019)-6)),\"\"))","v":"In Prüfung"}]
[50000889,"KSTAR","KSG-36KT-M4",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1020,1)=\"J\",LEFT(H1020,2),LEFT(H1020,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1020,1)=\"J\",RIGHT(H1020,LEN(H1020)-4),RIGHT(H1020,LEN(H1020)-6)),\"\"))","v":"In Prüfung"}]
[50000890,"KSTAR","KSG-36KT-M5",36,39.6,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1021,1)=\"J\",LEFT(H1021,2),LEFT(H1021,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1021,1)=\"J\",RIGHT(H1021,LEN(H1021)-4),RIGHT(H1021,LEN(H1021)-6)),\"\"))","v":"In Prüfung"}]
[50000891,"KSTAR","KSG-40KT-M0",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1022,1)=\"J\",LEFT(H1022,2),LEFT(H1022,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1022,1)=\"J\",RIGHT(H1022,LEN(H1022)-4),RIGHT(H1022,LEN(H1022)-6)),\"\"))","v":"In Prüfung"}]
[50000892,"KSTAR","KSG-40KT-M1",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1023,1)=\"J\",LEFT(H1023,2),LEFT(H1023,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1023,1)=\"J\",RIGHT(H1023,LEN(H1023)-4),RIGHT(H1023,LEN(H1023)-6)),\"\"))","v":"In Prüfung"}]
[50000893,"KSTAR","KSG-40KT-M2",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1024,1)=\"J\",LEFT(H1024,2),LEFT(H1024,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1024,1)=\"J\",RIGHT(H1024,LEN(H1024)-4),RIGHT(H1024,LEN(H1024)-6)),\"\"))","v":"In Prüfung"}]
[50000894,"KSTAR","KSG-40KT-M3",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1025,1)=\"J\",LEFT(H1025,2),LEFT(H1025,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1025,1)=\"J\",RIGHT(H1025,LEN(H1025)-4),RIGHT(H1025,LEN(H1025)-6)),\"\"))","v":"In Prüfung"}]
[50000895,"KSTAR","KSG-40KT-M4",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1026,1)=\"J\",LEFT(H1026,2),LEFT(H1026,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1026,1)=\"J\",RIGHT(H1026,LEN(H1026)-4),RIGHT(H1026,LEN(H1026)-6)),\"\"))","v":"In Prüfung"}]
[50000896,"KSTAR","KSG-40KT-M5",40,44,3,"PV-Wechselrichter","Nein - In Prüfung","2023-04-11","Karl Scheida",null,null,null,null,null,null,null,null,"vorhanden",null,"BL-DG22B0710-B01","2023-02-13",null,"nicht OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1027,1)=\"J\",LEFT(H1027,2),LEFT(H1027,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1027,1)=\"J\",RIGHT(H1027,LEN(H1027)-4),RIGHT(H1027,LEN(H1027)-6)),\"\"))","v":"In Prüfung"}]
[50001750,"LG Electronics","ESS Home 8 D008KE1N211",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2023-02-22","Christian Elbs",null,"R1664",null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","50328210 002","2021-03-10",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - ggf. NETZUMSCHALTBOX - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1028,1)=\"J\",LEFT(H1028,2),LEFT(H1028,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1028,1)=\"J\",RIGHT(H1028,LEN(H1028)-4),RIGHT(H1028,LEN(H1028)-6)),\"\"))","v":""}]
[50000898,"LG Electronics","ESS Home 10 D010KE1N211",10,11,3,"Hybrid-Wechselrichter","Ja","2023-02-22","Christian Elbs",null,"R1664",null,null,null,"Ja","Ja","Nein","OK","Christian Elbs","50328210 002","2021-03-10",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - ggf. NETZUMSCHALTBOX -  KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1029,1)=\"J\",LEFT(H1029,2),LEFT(H1029,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1029,1)=\"J\",RIGHT(H1029,LEN(H1029)-4),RIGHT(H1029,LEN(H1029)-6)),\"\"))","v":""}]
[50002072,"Lux Power","LXP 3600 ACS",0.3634,0.3634,1,"Hybrid-Wechselrichter","Ja - nur für Eigenverbrauch","2024-01-19","Martin Bertsch","2024-01-19",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"220513JH001-EG-DE-001","2022-08-29",null,"VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1030,1)=\"J\",LEFT(H1030,2),LEFT(H1030,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1030,1)=\"J\",RIGHT(H1030,LEN(H1030)-4),RIGHT(H1030,LEN(H1030)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000899,"luxra","luxra SK-L 3.0 ",3,3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","T","F",null,null,{"$f":"IF(LEFT(H1031,1)=\"J\",LEFT(H1031,2),LEFT(H1031,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1031,1)=\"J\",RIGHT(H1031,LEN(H1031)-4),RIGHT(H1031,LEN(H1031)-6)),\"\"))","v":""}]
[50000900,"luxra","luxra ES-S/ES-M/ES-L",4,4,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1032,1)=\"J\",LEFT(H1032,2),LEFT(H1032,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1032,1)=\"J\",RIGHT(H1032,LEN(H1032)-4),RIGHT(H1032,LEN(H1032)-6)),\"\"))","v":""}]
[50000901,"luxra","luxra SK-L 4200 ",4.2,4.2,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","T","F",null,null,{"$f":"IF(LEFT(H1033,1)=\"J\",LEFT(H1033,2),LEFT(H1033,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1033,1)=\"J\",RIGHT(H1033,LEN(H1033)-4),RIGHT(H1033,LEN(H1033)-6)),\"\"))","v":""}]
[50000902,"luxra","luxra SK-L 5500 ",5.5,5.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","T","F",null,null,{"$f":"IF(LEFT(H1034,1)=\"J\",LEFT(H1034,2),LEFT(H1034,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1034,1)=\"J\",RIGHT(H1034,LEN(H1034)-4),RIGHT(H1034,LEN(H1034)-6)),\"\"))","v":""}]
[50000903,"luxra","luxra SK-L 7000 ",7,7,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM ","T","F",null,null,{"$f":"IF(LEFT(H1035,1)=\"J\",LEFT(H1035,2),LEFT(H1035,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1035,1)=\"J\",RIGHT(H1035,LEN(H1035)-4),RIGHT(H1035,LEN(H1035)-6)),\"\"))","v":""}]
[50000904,"luxra","luxra SK-L 8300 ",8.3000000000000007,8.3000000000000007,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Nicht mehr am Markt","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - nicht mehr am Markt","T","F",null,null,{"$f":"IF(LEFT(H1036,1)=\"J\",LEFT(H1036,2),LEFT(H1036,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1036,1)=\"J\",RIGHT(H1036,LEN(H1036)-4),RIGHT(H1036,LEN(H1036)-6)),\"\"))","v":""}]
[50000905,"luxra","luxra SK-L 10100 ",10,10,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Nicht mehr am Markt","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - nicht mehr am Markt","T","F",null,null,{"$f":"IF(LEFT(H1037,1)=\"J\",LEFT(H1037,2),LEFT(H1037,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1037,1)=\"J\",RIGHT(H1037,LEN(H1037)-4),RIGHT(H1037,LEN(H1037)-6)),\"\"))","v":""}]
[50001972,"Maschinenfabrik Reinhausen","GRIDCON PCS",70.099999999999994,86,3,"AC-Batteriewechselrichter","Nein - Typ B","2023-11-21","Martin Bertsch","2023-11-21",null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1038,1)=\"J\",LEFT(H1038,2),LEFT(H1038,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1038,1)=\"J\",RIGHT(H1038,LEN(H1038)-4),RIGHT(H1038,LEN(H1038)-6)),\"\"))","v":"Typ B"}]
[50000906,"MAVEL","H22",null,22,3,"Frequenzumformer","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Frequenzumformer 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1039,1)=\"J\",LEFT(H1039,2),LEFT(H1039,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1039,1)=\"J\",RIGHT(H1039,LEN(H1039)-4),RIGHT(H1039,LEN(H1039)-6)),\"\"))","v":""}]
[50000907,"MAVEL","H96",100,100,3,"Frequenzumformer","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1040,1)=\"J\",LEFT(H1040,2),LEFT(H1040,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1040,1)=\"J\",RIGHT(H1040,LEN(H1040)-4),RIGHT(H1040,LEN(H1040)-6)),\"\"))","v":""}]
[50000908,"MEGAREVO","R6KH3",6,6.6,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-17",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein","Ja","Vorhanden",null,"64.290.22.31135.01","2023-02-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1041,1)=\"J\",LEFT(H1041,2),LEFT(H1041,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1041,1)=\"J\",RIGHT(H1041,LEN(H1041)-4),RIGHT(H1041,LEN(H1041)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000909,"MEGAREVO","R8KH3",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-17",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein","Ja","Vorhanden",null,"64.290.22.31135.01","2023-02-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1042,1)=\"J\",LEFT(H1042,2),LEFT(H1042,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1042,1)=\"J\",RIGHT(H1042,LEN(H1042)-4),RIGHT(H1042,LEN(H1042)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000910,"MEGAREVO","R10KH3",10,11,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-17",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein","Ja","Vorhanden",null,"64.290.22.31135.01","2023-02-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1043,1)=\"J\",LEFT(H1043,2),LEFT(H1043,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1043,1)=\"J\",RIGHT(H1043,LEN(H1043)-4),RIGHT(H1043,LEN(H1043)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000911,"MEGAREVO","R12KH3",12,13.2,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-17",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein","Ja","Vorhanden",null,"64.290.22.31135.01","2023-02-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1044,1)=\"J\",LEFT(H1044,2),LEFT(H1044,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1044,1)=\"J\",RIGHT(H1044,LEN(H1044)-4),RIGHT(H1044,LEN(H1044)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000912,"MEGAREVO","R15KH3",15,16.5,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-09-26","Martin Bertsch","2023-05-17",null,"2023-09-30","2023-10-01","Testgerät wurde nicht bereitgestellt","Ja","Nein","Ja","Vorhanden",null,"64.290.22.31135.01","2023-02-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1045,1)=\"J\",LEFT(H1045,2),LEFT(H1045,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1045,1)=\"J\",RIGHT(H1045,LEN(H1045)-4),RIGHT(H1045,LEN(H1045)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000913,"MPP SOLAR  ","MPI 10K",10,10,3,"Hybrid-Wechselrichter","Nein","2023-02-21","Christian Elbs",null,null,null,null,"Ländereinstellung fehlerhaft",null,null,null,"nicht OK","Roland Bründlinger","PVAT2108WDG0244","2021-09-14",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1046,1)=\"J\",LEFT(H1046,2),LEFT(H1046,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1046,1)=\"J\",RIGHT(H1046,LEN(H1046)-4),RIGHT(H1046,LEN(H1046)-6)),\"\"))","v":""}]
[50000914,"MPP SOLAR INC","PIP-2424HSP",2.4,2.4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1047,1)=\"J\",LEFT(H1047,2),LEFT(H1047,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1047,1)=\"J\",RIGHT(H1047,LEN(H1047)-4),RIGHT(H1047,LEN(H1047)-6)),\"\"))","v":""}]
[50000915,"MPP SOLAR INC","PIP-2424MSP",2.4,2.4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1048,1)=\"J\",LEFT(H1048,2),LEFT(H1048,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1048,1)=\"J\",RIGHT(H1048,LEN(H1048)-4),RIGHT(H1048,LEN(H1048)-6)),\"\"))","v":""}]
[50000916,"MPP SOLAR INC","Hybrid V2-3048",3,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1049,1)=\"J\",LEFT(H1049,2),LEFT(H1049,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1049,1)=\"J\",RIGHT(H1049,LEN(H1049)-4),RIGHT(H1049,LEN(H1049)-6)),\"\"))","v":""}]
[50000917,"MPP SOLAR INC","Hybrid V-3048",3,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1050,1)=\"J\",LEFT(H1050,2),LEFT(H1050,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1050,1)=\"J\",RIGHT(H1050,LEN(H1050)-4),RIGHT(H1050,LEN(H1050)-6)),\"\"))","v":""}]
[50000918,"MPP SOLAR INC","PIP-2424HSE1",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1051,1)=\"J\",LEFT(H1051,2),LEFT(H1051,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1051,1)=\"J\",RIGHT(H1051,LEN(H1051)-4),RIGHT(H1051,LEN(H1051)-6)),\"\"))","v":""}]
[50000919,"MPP SOLAR INC","PIP-2424MSE1",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1052,1)=\"J\",LEFT(H1052,2),LEFT(H1052,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1052,1)=\"J\",RIGHT(H1052,LEN(H1052)-4),RIGHT(H1052,LEN(H1052)-6)),\"\"))","v":""}]
[50000920,"MPP SOLAR INC","PIP-3024GK",3,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1053,1)=\"J\",LEFT(H1053,2),LEFT(H1053,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1053,1)=\"J\",RIGHT(H1053,LEN(H1053)-4),RIGHT(H1053,LEN(H1053)-6)),\"\"))","v":""}]
[50000921,"MPP SOLAR INC","PIP-3024MK",3,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1054,1)=\"J\",LEFT(H1054,2),LEFT(H1054,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1054,1)=\"J\",RIGHT(H1054,LEN(H1054)-4),RIGHT(H1054,LEN(H1054)-6)),\"\"))","v":""}]
[50000922,"MPP SOLAR INC","PIP-3624MAX",3.6,3.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1055,1)=\"J\",LEFT(H1055,2),LEFT(H1055,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1055,1)=\"J\",RIGHT(H1055,LEN(H1055)-4),RIGHT(H1055,LEN(H1055)-6)),\"\"))","v":""}]
[50000923,"MPP SOLAR INC","U 3624GK",3.6,3.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1056,1)=\"J\",LEFT(H1056,2),LEFT(H1056,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1056,1)=\"J\",RIGHT(H1056,LEN(H1056)-4),RIGHT(H1056,LEN(H1056)-6)),\"\"))","v":""}]
[50000924,"MPP SOLAR INC","Hybrid V-4048",4,4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1057,1)=\"J\",LEFT(H1057,2),LEFT(H1057,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1057,1)=\"J\",RIGHT(H1057,LEN(H1057)-4),RIGHT(H1057,LEN(H1057)-6)),\"\"))","v":""}]
[50000925,"MPP SOLAR INC","PIP-4024HSP",4,4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1058,1)=\"J\",LEFT(H1058,2),LEFT(H1058,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1058,1)=\"J\",RIGHT(H1058,LEN(H1058)-4),RIGHT(H1058,LEN(H1058)-6)),\"\"))","v":""}]
[50000926,"MPP SOLAR INC","PIP-4024MSP",4,4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1059,1)=\"J\",LEFT(H1059,2),LEFT(H1059,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1059,1)=\"J\",RIGHT(H1059,LEN(H1059)-4),RIGHT(H1059,LEN(H1059)-6)),\"\"))","v":""}]
[50000927,"MPP SOLAR INC","Hybrid V2-5048",5,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1060,1)=\"J\",LEFT(H1060,2),LEFT(H1060,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1060,1)=\"J\",RIGHT(H1060,LEN(H1060)-4),RIGHT(H1060,LEN(H1060)-6)),\"\"))","v":""}]
[50000928,"MPP SOLAR INC","Hybrid V-5048",5,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1061,1)=\"J\",LEFT(H1061,2),LEFT(H1061,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1061,1)=\"J\",RIGHT(H1061,LEN(H1061)-4),RIGHT(H1061,LEN(H1061)-6)),\"\"))","v":""}]
[50000929,"MPP SOLAR INC","MPI HYBRID 5K ",null,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ nur 3~ Anschluss gestattet - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1062,1)=\"J\",LEFT(H1062,2),LEFT(H1062,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1062,1)=\"J\",RIGHT(H1062,LEN(H1062)-4),RIGHT(H1062,LEN(H1062)-6)),\"\"))","v":""}]
[50000930,"MPP SOLAR INC","PIP-5048GK",5,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1063,1)=\"J\",LEFT(H1063,2),LEFT(H1063,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1063,1)=\"J\",RIGHT(H1063,LEN(H1063)-4),RIGHT(H1063,LEN(H1063)-6)),\"\"))","v":""}]
[50000931,"MPP SOLAR INC","PIP-5048MGX",5,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1064,1)=\"J\",LEFT(H1064,2),LEFT(H1064,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1064,1)=\"J\",RIGHT(H1064,LEN(H1064)-4),RIGHT(H1064,LEN(H1064)-6)),\"\"))","v":""}]
[50000932,"MPP SOLAR INC","PIP-5048MK",5,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1065,1)=\"J\",LEFT(H1065,2),LEFT(H1065,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1065,1)=\"J\",RIGHT(H1065,LEN(H1065)-4),RIGHT(H1065,LEN(H1065)-6)),\"\"))","v":""}]
[50000933,"MPP SOLAR INC","PIP-5048MKX",5,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1066,1)=\"J\",LEFT(H1066,2),LEFT(H1066,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1066,1)=\"J\",RIGHT(H1066,LEN(H1066)-4),RIGHT(H1066,LEN(H1066)-6)),\"\"))","v":""}]
[50000934,"MPP SOLAR INC","MPI HYBRID 5.5K ",null,5.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ nur 3~ Anschluss gestattet - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1067,1)=\"J\",LEFT(H1067,2),LEFT(H1067,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1067,1)=\"J\",RIGHT(H1067,LEN(H1067)-4),RIGHT(H1067,LEN(H1067)-6)),\"\"))","v":""}]
[50000935,"MPP SOLAR INC","U 5648GK",5.6,5.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1068,1)=\"J\",LEFT(H1068,2),LEFT(H1068,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1068,1)=\"J\",RIGHT(H1068,LEN(H1068)-4),RIGHT(H1068,LEN(H1068)-6)),\"\"))","v":""}]
[50000936,"MPP SOLAR INC","U 5648MS",5.6,5.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1069,1)=\"J\",LEFT(H1069,2),LEFT(H1069,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1069,1)=\"J\",RIGHT(H1069,LEN(H1069)-4),RIGHT(H1069,LEN(H1069)-6)),\"\"))","v":""}]
[50000937,"MPP SOLAR INC","3P Hybrid V-6KW",6,6,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1070,1)=\"J\",LEFT(H1070,2),LEFT(H1070,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1070,1)=\"J\",RIGHT(H1070,LEN(H1070)-4),RIGHT(H1070,LEN(H1070)-6)),\"\"))","v":""}]
[50000938,"MPP SOLAR INC","PIP-7248MAX",7.2,7.2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1071,1)=\"J\",LEFT(H1071,2),LEFT(H1071,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1071,1)=\"J\",RIGHT(H1071,LEN(H1071)-4),RIGHT(H1071,LEN(H1071)-6)),\"\"))","v":""}]
[50000939,"MPP SOLAR INC","PIP-8048MAX",8,8,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1072,1)=\"J\",LEFT(H1072,2),LEFT(H1072,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1072,1)=\"J\",RIGHT(H1072,LEN(H1072)-4),RIGHT(H1072,LEN(H1072)-6)),\"\"))","v":""}]
[50000940,"MPP SOLAR INC","3P Hybrid V-9KW",9,9,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1073,1)=\"J\",LEFT(H1073,2),LEFT(H1073,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1073,1)=\"J\",RIGHT(H1073,LEN(H1073)-4),RIGHT(H1073,LEN(H1073)-6)),\"\"))","v":""}]
[50000941,"MPP SOLAR INC","MPI HYBRID 10K ",null,10,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1074,1)=\"J\",LEFT(H1074,2),LEFT(H1074,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1074,1)=\"J\",RIGHT(H1074,LEN(H1074)-4),RIGHT(H1074,LEN(H1074)-6)),\"\"))","v":""}]
[50000942,"MPP SOLAR INC","HV V3 30KW",30,30,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1075,1)=\"J\",LEFT(H1075,2),LEFT(H1075,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1075,1)=\"J\",RIGHT(H1075,LEN(H1075)-4),RIGHT(H1075,LEN(H1075)-6)),\"\"))","v":""}]
[50000943,"M-TEC Energy Systems GmbH","EnergyButler 4kW-3P",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch",null,"V1.05","2023-05-31","2023-06-01",null,"Ja",null,null,"nicht OK","Martin Bertsch (OE)","6120072.50","2022-03-25",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1076,1)=\"J\",LEFT(H1076,2),LEFT(H1076,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1076,1)=\"J\",RIGHT(H1076,LEN(H1076)-4),RIGHT(H1076,LEN(H1076)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000944,"M-TEC Energy Systems GmbH","EnergyButler 4kW-3P-3G25",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1077,1)=\"J\",LEFT(H1077,2),LEFT(H1077,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1077,1)=\"J\",RIGHT(H1077,LEN(H1077)-4),RIGHT(H1077,LEN(H1077)-6)),\"\"))","v":"mit Einschränkung"}]
[50000945,"M-TEC Energy Systems GmbH","EnergyButler 5kW-3P",5,5.5,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch",null,"V1.05","2023-05-31","2023-06-01",null,"Ja",null,null,"nicht OK","Martin Bertsch (OE)","6120072.50","2022-03-25",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1078,1)=\"J\",LEFT(H1078,2),LEFT(H1078,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1078,1)=\"J\",RIGHT(H1078,LEN(H1078)-4),RIGHT(H1078,LEN(H1078)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000946,"M-TEC Energy Systems GmbH","EnergyButler 5kW-3P-3G25",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1079,1)=\"J\",LEFT(H1079,2),LEFT(H1079,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1079,1)=\"J\",RIGHT(H1079,LEN(H1079)-4),RIGHT(H1079,LEN(H1079)-6)),\"\"))","v":"mit Einschränkung"}]
[50000947,"M-TEC Energy Systems GmbH","EnergyButler 6kW-3P",6,6.6,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch",null,"V1.05","2023-05-31","2023-06-01",null,"Ja",null,null,"nicht OK","Martin Bertsch (OE)","6120072.50","2022-03-25",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1080,1)=\"J\",LEFT(H1080,2),LEFT(H1080,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1080,1)=\"J\",RIGHT(H1080,LEN(H1080)-4),RIGHT(H1080,LEN(H1080)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000948,"M-TEC Energy Systems GmbH","EnergyButler 6kW-3P-3G25",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1081,1)=\"J\",LEFT(H1081,2),LEFT(H1081,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1081,1)=\"J\",RIGHT(H1081,LEN(H1081)-4),RIGHT(H1081,LEN(H1081)-6)),\"\"))","v":"mit Einschränkung"}]
[50000949,"M-TEC Energy Systems GmbH","EnergyButler 8kW-3P",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch",null,"V1.05","2023-05-31","2023-06-01",null,"Ja",null,null,"nicht OK","Martin Bertsch (OE)","6120072.50","2022-03-25",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1082,1)=\"J\",LEFT(H1082,2),LEFT(H1082,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1082,1)=\"J\",RIGHT(H1082,LEN(H1082)-4),RIGHT(H1082,LEN(H1082)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000950,"M-TEC Energy Systems GmbH","EnergyButler 8kW-3P-3G25",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1083,1)=\"J\",LEFT(H1083,2),LEFT(H1083,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1083,1)=\"J\",RIGHT(H1083,LEN(H1083)-4),RIGHT(H1083,LEN(H1083)-6)),\"\"))","v":"mit Einschränkung"}]
[50000951,"M-TEC Energy Systems GmbH","EnergyButler 10kW-3P",10,11,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch",null,"V1.05","2023-05-31","2023-06-01",null,"Ja",null,null,"nicht OK","Martin Bertsch (OE)","6120072.50","2022-03-25",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1084,1)=\"J\",LEFT(H1084,2),LEFT(H1084,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1084,1)=\"J\",RIGHT(H1084,LEN(H1084)-4),RIGHT(H1084,LEN(H1084)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000952,"M-TEC Energy Systems GmbH","EnergyButler 10kW-3P-3G25",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1085,1)=\"J\",LEFT(H1085,2),LEFT(H1085,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1085,1)=\"J\",RIGHT(H1085,LEN(H1085)-4),RIGHT(H1085,LEN(H1085)-6)),\"\"))","v":"mit Einschränkung"}]
[50000953,"M-TEC Energy Systems GmbH","EnergyButler 10kW-3P-3G40",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1086,1)=\"J\",LEFT(H1086,2),LEFT(H1086,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1086,1)=\"J\",RIGHT(H1086,LEN(H1086)-4),RIGHT(H1086,LEN(H1086)-6)),\"\"))","v":"mit Einschränkung"}]
[50000954,"M-TEC Energy Systems GmbH","EnergyButler 12kW-3P",12,13.2,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch","2022-10-18","V1.05","2023-05-31","2023-06-01",null,"Ja",null,null,"nicht OK","Martin Bertsch (OE)","6120072.50","2022-03-25",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1087,1)=\"J\",LEFT(H1087,2),LEFT(H1087,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1087,1)=\"J\",RIGHT(H1087,LEN(H1087)-4),RIGHT(H1087,LEN(H1087)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50000955,"M-TEC Energy Systems GmbH","EnergyButler 12kW-3P-3G25",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1088,1)=\"J\",LEFT(H1088,2),LEFT(H1088,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1088,1)=\"J\",RIGHT(H1088,LEN(H1088)-4),RIGHT(H1088,LEN(H1088)-6)),\"\"))","v":"mit Einschränkung"}]
[50000956,"M-TEC Energy Systems GmbH","EnergyButler 12kW-3P-3G40",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1089,1)=\"J\",LEFT(H1089,2),LEFT(H1089,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1089,1)=\"J\",RIGHT(H1089,LEN(H1089)-4),RIGHT(H1089,LEN(H1089)-6)),\"\"))","v":"mit Einschränkung"}]
[50000957,"M-TEC Energy Systems GmbH","EnergyButler 15kW-3P-3G40",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1090,1)=\"J\",LEFT(H1090,2),LEFT(H1090,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1090,1)=\"J\",RIGHT(H1090,LEN(H1090)-4),RIGHT(H1090,LEN(H1090)-6)),\"\"))","v":"mit Einschränkung"}]
[50000958,"M-TEC Energy Systems GmbH","EnergyButler 20kW-3P-3G40",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1091,1)=\"J\",LEFT(H1091,2),LEFT(H1091,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1091,1)=\"J\",RIGHT(H1091,LEN(H1091)-4),RIGHT(H1091,LEN(H1091)-6)),\"\"))","v":"mit Einschränkung"}]
[50000959,"neoom","KJUUBE LIGHT NEA HV-SO 5KW",5,5,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden",null,50368718002,"2020-03-06",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ -  KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1092,1)=\"J\",LEFT(H1092,2),LEFT(H1092,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1092,1)=\"J\",RIGHT(H1092,LEN(H1092)-4),RIGHT(H1092,LEN(H1092)-6)),\"\"))","v":""}]
[50000960,"neoom","KJUUBE NEA HV-SO 5KW",5,5,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden",null,50368718002,"2020-03-06",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1093,1)=\"J\",LEFT(H1093,2),LEFT(H1093,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1093,1)=\"J\",RIGHT(H1093,LEN(H1093)-4),RIGHT(H1093,LEN(H1093)-6)),\"\"))","v":""}]
[50000961,"neoom","KJUUBE LIGHT USV HV-GW 5KW",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-10-18","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1094,1)=\"J\",LEFT(H1094,2),LEFT(H1094,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1094,1)=\"J\",RIGHT(H1094,LEN(H1094)-4),RIGHT(H1094,LEN(H1094)-6)),\"\"))","v":"mit Einschränkung"}]
[50000962,"neoom","KJUUBE LIGHT NEA HV-SO 6KW",6,6,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden",null,50368718002,"2020-03-06",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1095,1)=\"J\",LEFT(H1095,2),LEFT(H1095,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1095,1)=\"J\",RIGHT(H1095,LEN(H1095)-4),RIGHT(H1095,LEN(H1095)-6)),\"\"))","v":""}]
[50000963,"neoom","KJUUBE NEA HV-SO 6KW",6,6,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden",null,50368718002,"2020-03-06",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ -  KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H1096,1)=\"J\",LEFT(H1096,2),LEFT(H1096,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1096,1)=\"J\",RIGHT(H1096,LEN(H1096)-4),RIGHT(H1096,LEN(H1096)-6)),\"\"))","v":""}]
[50000964,"neoom","KJUUBE LIGHT NEA + SOLAX X3-Hybrid-6.0",6,6.6,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch","2023-06-27",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1097,1)=\"J\",LEFT(H1097,2),LEFT(H1097,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1097,1)=\"J\",RIGHT(H1097,LEN(H1097)-4),RIGHT(H1097,LEN(H1097)-6)),\"\"))","v":""}]
[50000965,"neoom","KJUUBE LIGHT USV HV-GW 6KW",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-10-18","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1098,1)=\"J\",LEFT(H1098,2),LEFT(H1098,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1098,1)=\"J\",RIGHT(H1098,LEN(H1098)-4),RIGHT(H1098,LEN(H1098)-6)),\"\"))","v":"mit Einschränkung"}]
[50000966,"neoom","KJUUBE LIGHT NEA HV-SO 8KW",8,8,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden",null,50368718002,"2020-03-06",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1099,1)=\"J\",LEFT(H1099,2),LEFT(H1099,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1099,1)=\"J\",RIGHT(H1099,LEN(H1099)-4),RIGHT(H1099,LEN(H1099)-6)),\"\"))","v":""}]
[50000967,"neoom","KJUUBE NEA HV-SO 8KW",8,8,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden",null,50368718002,"2020-03-06",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ -  KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H1100,1)=\"J\",LEFT(H1100,2),LEFT(H1100,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1100,1)=\"J\",RIGHT(H1100,LEN(H1100)-4),RIGHT(H1100,LEN(H1100)-6)),\"\"))","v":""}]
[50000968,"neoom","KJUUBE LIGHT NEA + SOLAX X3-Hybrid-8.0",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch","2023-06-27",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1101,1)=\"J\",LEFT(H1101,2),LEFT(H1101,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1101,1)=\"J\",RIGHT(H1101,LEN(H1101)-4),RIGHT(H1101,LEN(H1101)-6)),\"\"))","v":""}]
[50000969,"neoom","KJUUBE LIGHT USV HV-GW 8KW",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-10-18","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1102,1)=\"J\",LEFT(H1102,2),LEFT(H1102,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1102,1)=\"J\",RIGHT(H1102,LEN(H1102)-4),RIGHT(H1102,LEN(H1102)-6)),\"\"))","v":"mit Einschränkung"}]
[50000970,"neoom","KJUUBE LIGHT NEA HV-SO 10KW",10,10,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden",null,50368718002,"2020-03-06",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ -  KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1103,1)=\"J\",LEFT(H1103,2),LEFT(H1103,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1103,1)=\"J\",RIGHT(H1103,LEN(H1103)-4),RIGHT(H1103,LEN(H1103)-6)),\"\"))","v":""}]
[50000971,"neoom","KJUUBE NEA HV-SO 10KW",10,10,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch",null,null,null,null,null,"Ja",null,null,"Vorhanden",null,50368718002,"2020-03-06",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ -  KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H1104,1)=\"J\",LEFT(H1104,2),LEFT(H1104,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1104,1)=\"J\",RIGHT(H1104,LEN(H1104)-4),RIGHT(H1104,LEN(H1104)-6)),\"\"))","v":""}]
[50002190,"neoom","KJUUBE Light + NEEO HYD 10KTL",10,11,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1105,1)=\"J\",LEFT(H1105,2),LEFT(H1105,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1105,1)=\"J\",RIGHT(H1105,LEN(H1105)-4),RIGHT(H1105,LEN(H1105)-6)),\"\"))","v":"befristet"}]
[50000972,"neoom","KJUUBE LIGHT NEA + SOLAX X3-Hybrid-10.0",10,11,3,"Hybrid-Wechselrichter","Ja","2023-08-28","Martin Bertsch","2023-06-27",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1106,1)=\"J\",LEFT(H1106,2),LEFT(H1106,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1106,1)=\"J\",RIGHT(H1106,LEN(H1106)-4),RIGHT(H1106,LEN(H1106)-6)),\"\"))","v":""}]
[50000973,"neoom","KJUUBE LIGHT S UPS + SOFAR HYD 10KTL-3PH",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2023-06-27","Firmware Version: V112351_51_51",null,null,null,"Ja","Nein",null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1107,1)=\"J\",LEFT(H1107,2),LEFT(H1107,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1107,1)=\"J\",RIGHT(H1107,LEN(H1107)-4),RIGHT(H1107,LEN(H1107)-6)),\"\"))","v":"mit Einschränkung"}]
[50000974,"neoom","KJUUBE LIGHT S USV + GOODWE GW10K-ET",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2023-06-27","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1108,1)=\"J\",LEFT(H1108,2),LEFT(H1108,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1108,1)=\"J\",RIGHT(H1108,LEN(H1108)-4),RIGHT(H1108,LEN(H1108)-6)),\"\"))","v":"mit Einschränkung"}]
[50000975,"neoom","KJUUBE LIGHT USV HV-GW 10KW",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-04","Martin Bertsch","2022-10-18","FW: 090922",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","50314995 005","2022-08-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1109,1)=\"J\",LEFT(H1109,2),LEFT(H1109,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1109,1)=\"J\",RIGHT(H1109,LEN(H1109)-4),RIGHT(H1109,LEN(H1109)-6)),\"\"))","v":"mit Einschränkung"}]
[50002142,"neoom","NEEO HYD 10KTL-3PH",10,11,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1110,1)=\"J\",LEFT(H1110,2),LEFT(H1110,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1110,1)=\"J\",RIGHT(H1110,LEN(H1110)-4),RIGHT(H1110,LEN(H1110)-6)),\"\"))","v":"befristet"}]
[50002184,"neoom","STAAK + NEEO HYD 10KTL",10,11,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1111,1)=\"J\",LEFT(H1111,2),LEFT(H1111,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1111,1)=\"J\",RIGHT(H1111,LEN(H1111)-4),RIGHT(H1111,LEN(H1111)-6)),\"\"))","v":"befristet"}]
[50002187,"neoom","STAAK Eco + NEEO HYD 10KTL",10,11,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1112,1)=\"J\",LEFT(H1112,2),LEFT(H1112,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1112,1)=\"J\",RIGHT(H1112,LEN(H1112)-4),RIGHT(H1112,LEN(H1112)-6)),\"\"))","v":"befristet"}]
[50002191,"neoom","KJUUBE Light + NEEO HYD 15KTL",15,16.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1113,1)=\"J\",LEFT(H1113,2),LEFT(H1113,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1113,1)=\"J\",RIGHT(H1113,LEN(H1113)-4),RIGHT(H1113,LEN(H1113)-6)),\"\"))","v":"befristet"}]
[50000976,"neoom","KJUUBE LIGHT S UPS + SOFAR HYD 15KTL-3PH ",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2023-06-27","Firmware Version: V112351_51_51",null,null,null,"Ja","Nein",null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1114,1)=\"J\",LEFT(H1114,2),LEFT(H1114,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1114,1)=\"J\",RIGHT(H1114,LEN(H1114)-4),RIGHT(H1114,LEN(H1114)-6)),\"\"))","v":"mit Einschränkung"}]
[50002143,"neoom","NEEO HYD 15KTL-3PH",15,16.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1115,1)=\"J\",LEFT(H1115,2),LEFT(H1115,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1115,1)=\"J\",RIGHT(H1115,LEN(H1115)-4),RIGHT(H1115,LEN(H1115)-6)),\"\"))","v":"befristet"}]
[50002185,"neoom","STAAK + NEEO HYD 15KTL",15,16.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1116,1)=\"J\",LEFT(H1116,2),LEFT(H1116,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1116,1)=\"J\",RIGHT(H1116,LEN(H1116)-4),RIGHT(H1116,LEN(H1116)-6)),\"\"))","v":"befristet"}]
[50002188,"neoom","STAAK Eco + NEEO HYD 15KTL",15,16.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1117,1)=\"J\",LEFT(H1117,2),LEFT(H1117,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1117,1)=\"J\",RIGHT(H1117,LEN(H1117)-4),RIGHT(H1117,LEN(H1117)-6)),\"\"))","v":"befristet"}]
[50002192,"neoom","KJUUBE Light + NEEO HYD 20KTL",20,22,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1118,1)=\"J\",LEFT(H1118,2),LEFT(H1118,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1118,1)=\"J\",RIGHT(H1118,LEN(H1118)-4),RIGHT(H1118,LEN(H1118)-6)),\"\"))","v":"befristet"}]
[50000977,"neoom","KJUUBE LIGHT S UPS + SOFAR HYD 20KTL-3PH ",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2023-06-27","Firmware Version: V112351_51_51",null,null,null,"Ja","Nein",null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1119,1)=\"J\",LEFT(H1119,2),LEFT(H1119,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1119,1)=\"J\",RIGHT(H1119,LEN(H1119)-4),RIGHT(H1119,LEN(H1119)-6)),\"\"))","v":"mit Einschränkung"}]
[50002144,"neoom","NEEO HYD 20KTL-3PH",20,22,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1120,1)=\"J\",LEFT(H1120,2),LEFT(H1120,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1120,1)=\"J\",RIGHT(H1120,LEN(H1120)-4),RIGHT(H1120,LEN(H1120)-6)),\"\"))","v":"befristet"}]
[50002186,"neoom","STAAK + NEEO HYD 20KTL",20,22,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1121,1)=\"J\",LEFT(H1121,2),LEFT(H1121,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1121,1)=\"J\",RIGHT(H1121,LEN(H1121)-4),RIGHT(H1121,LEN(H1121)-6)),\"\"))","v":"befristet"}]
[50002189,"neoom","STAAK Eco + NEEO HYD 20KTL",20,22,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-04-22",null,"2024-09-30",null,null,"Ja","Nein",null,"Vorhanden",null,"240204116GZU-001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1122,1)=\"J\",LEFT(H1122,2),LEFT(H1122,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1122,1)=\"J\",RIGHT(H1122,LEN(H1122)-4),RIGHT(H1122,LEN(H1122)-6)),\"\"))","v":"befristet"}]
[50000978,"neoom","BLOKK LIGHT NEA 30 kVA",30,30,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-10-02","Martin Bertsch",null,null,null,null,null,"Nein",null,null,"Vorhanden",null,"CN21GNUV001","2021-02-02",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - NETZUMSCHALTBOX - KONFORM TOR ERZ AB",null,null,null,null,{"$f":"IF(LEFT(H1123,1)=\"J\",LEFT(H1123,2),LEFT(H1123,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1123,1)=\"J\",RIGHT(H1123,LEN(H1123)-4),RIGHT(H1123,LEN(H1123)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000979,"neoom","BLOKK Light 50kW",50,50,3,"AC-Batteriewechselrichter","Nein - Typ B","2023-08-28","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,"18TH0270-OVE-directive R25_1","2022-07-07","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1124,1)=\"J\",LEFT(H1124,2),LEFT(H1124,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1124,1)=\"J\",RIGHT(H1124,LEN(H1124)-4),RIGHT(H1124,LEN(H1124)-6)),\"\"))","v":"Typ B"}]
[50001849,"neoom","BLOKK LIGHT NEA 60 kVA",60,60,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-10-02","Martin Bertsch","2023-10-02",null,null,null,null,null,null,null,"Vorhanden",null,"CN21GNUV001","2021-02-02",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1125,1)=\"J\",LEFT(H1125,2),LEFT(H1125,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1125,1)=\"J\",RIGHT(H1125,LEN(H1125)-4),RIGHT(H1125,LEN(H1125)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000980,"neoom","BLOKK",88,88,3,"AC-Batteriewechselrichter","Nein - Typ B","2023-08-28","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,"18TH0270-OVE-directive R25_1","2022-07-07","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1126,1)=\"J\",LEFT(H1126,2),LEFT(H1126,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1126,1)=\"J\",RIGHT(H1126,LEN(H1126)-4),RIGHT(H1126,LEN(H1126)-6)),\"\"))","v":"Typ B"}]
[50000981,"neoom","BLOKK LIGHT",88,88,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-28","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"18TH0270-OVE","2021-03-19","Vorhanden","nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM TOR ERZ AB",null,null,null,null,{"$f":"IF(LEFT(H1127,1)=\"J\",LEFT(H1127,2),LEFT(H1127,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1127,1)=\"J\",RIGHT(H1127,LEN(H1127)-4),RIGHT(H1127,LEN(H1127)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000982,"neoom","BLOKK Light 88kW",88,88,3,"AC-Batteriewechselrichter","Nein - Typ B","2023-08-28","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,"18TH0270-OVE-directive R25_1","2022-07-07","Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1128,1)=\"J\",LEFT(H1128,2),LEFT(H1128,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1128,1)=\"J\",RIGHT(H1128,LEN(H1128)-4),RIGHT(H1128,LEN(H1128)-6)),\"\"))","v":"Typ B"}]
[50000983,"neoom","BLOKK ",90,90,3,"AC-Batteriewechselrichter","Nein","2023-08-28","Martin Bertsch",null,null,null,null,null,"Nein",null,null,"VDE4105/4110",null,"18TH0270-OVE","2021-03-19",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM TOR ERZ AB","F","F",null,null,{"$f":"IF(LEFT(H1129,1)=\"J\",LEFT(H1129,2),LEFT(H1129,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1129,1)=\"J\",RIGHT(H1129,LEN(H1129)-4),RIGHT(H1129,LEN(H1129)-6)),\"\"))","v":""}]
[50001850,"neoom","BLOKK LIGHT NEA 90 kVA",90,90,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-10-02","Martin Bertsch","2023-10-02",null,null,null,null,null,null,null,"Vorhanden",null,"CN21GNUV001","2021-02-02",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1130,1)=\"J\",LEFT(H1130,2),LEFT(H1130,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1130,1)=\"J\",RIGHT(H1130,LEN(H1130)-4),RIGHT(H1130,LEN(H1130)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001851,"neoom","BLOKK LIGHT NEA 120 kVA",120,120,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-10-02","Martin Bertsch","2023-10-02",null,null,null,null,null,null,null,"Vorhanden",null,"CN21GNUV001","2021-02-02",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1131,1)=\"J\",LEFT(H1131,2),LEFT(H1131,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1131,1)=\"J\",RIGHT(H1131,LEN(H1131)-4),RIGHT(H1131,LEN(H1131)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000984,"neoom","BL300/398,0-1.1 AC",null,300,3,"AC-Batteriewechselrichter","Nein - Typ B","2023-08-28","Martin Bertsch",null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein",null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1132,1)=\"J\",LEFT(H1132,2),LEFT(H1132,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1132,1)=\"J\",RIGHT(H1132,LEN(H1132)-4),RIGHT(H1132,LEN(H1132)-6)),\"\"))","v":"Typ B"}]
[50000985,"NEP","BDM 300",0.3,0.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1133,1)=\"J\",LEFT(H1133,2),LEFT(H1133,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1133,1)=\"J\",RIGHT(H1133,LEN(H1133)-4),RIGHT(H1133,LEN(H1133)-6)),\"\"))","v":""}]
[50000986,"NEP","BDM 500",0.55000000000000004,0.55000000000000004,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1134,1)=\"J\",LEFT(H1134,2),LEFT(H1134,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1134,1)=\"J\",RIGHT(H1134,LEN(H1134)-4),RIGHT(H1134,LEN(H1134)-6)),\"\"))","v":""}]
[50000987,"NEP","BDM-600",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2023-11-22","Martin Bertsch","2023-11-22","FW 0x9200 ",null,null,null,"Nein","Nein","Nein","OK","Michael Tippmann","64.290.20.30267.03","2022-01-10","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1135,1)=\"J\",LEFT(H1135,2),LEFT(H1135,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1135,1)=\"J\",RIGHT(H1135,LEN(H1135)-4),RIGHT(H1135,LEN(H1135)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50000988,"NEP","BDM-800",0.75,0.75,1,"PV-Wechselrichter","Ja - <= 16A Anlage, mit Einschränkung","2023-11-22","Martin Bertsch","2023-11-22","FW 0x9200 ",null,null,null,"Nein","Nein","Nein","OK","Michael Tippmann","64.290.20.30267.03","2022-01-10","nicht vorhanden","OK","Vorhanden",null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1136,1)=\"J\",LEFT(H1136,2),LEFT(H1136,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1136,1)=\"J\",RIGHT(H1136,LEN(H1136)-4),RIGHT(H1136,LEN(H1136)-6)),\"\"))","v":"<= 16A Anlage, mit Einschränkung"}]
[50000989,"NGEN","STAR-H3-5.0-E",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-05-11","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1137,1)=\"J\",LEFT(H1137,2),LEFT(H1137,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1137,1)=\"J\",RIGHT(H1137,LEN(H1137)-4),RIGHT(H1137,LEN(H1137)-6)),\"\"))","v":"mit Einschränkung"}]
[50000990,"NGEN","STAR-H3-6.0-E",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-05-11","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1138,1)=\"J\",LEFT(H1138,2),LEFT(H1138,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1138,1)=\"J\",RIGHT(H1138,LEN(H1138)-4),RIGHT(H1138,LEN(H1138)-6)),\"\"))","v":"mit Einschränkung"}]
[50000991,"NGEN","STAR-H3-8.0-E",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-05-11","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1139,1)=\"J\",LEFT(H1139,2),LEFT(H1139,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1139,1)=\"J\",RIGHT(H1139,LEN(H1139)-4),RIGHT(H1139,LEN(H1139)-6)),\"\"))","v":"mit Einschränkung"}]
[50000992,"NGEN","STAR-H3-10.0-E",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-05-11","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1140,1)=\"J\",LEFT(H1140,2),LEFT(H1140,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1140,1)=\"J\",RIGHT(H1140,LEN(H1140)-4),RIGHT(H1140,LEN(H1140)-6)),\"\"))","v":"mit Einschränkung"}]
[50000993,"NGEN","STAR-H3-12.0-E",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-05-11","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1141,1)=\"J\",LEFT(H1141,2),LEFT(H1141,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1141,1)=\"J\",RIGHT(H1141,LEN(H1141)-4),RIGHT(H1141,LEN(H1141)-6)),\"\"))","v":"mit Einschränkung"}]
[50002273,"NORD HT AS","EcoMaster 3P 5.0",5,5.5,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 008","2024-01-15","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1142,1)=\"J\",LEFT(H1142,2),LEFT(H1142,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1142,1)=\"J\",RIGHT(H1142,LEN(H1142)-4),RIGHT(H1142,LEN(H1142)-6)),\"\"))","v":""}]
[50002274,"NORD HT AS","EcoMaster 3P 6.0",6,6.6,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 008","2024-01-15","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1143,1)=\"J\",LEFT(H1143,2),LEFT(H1143,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1143,1)=\"J\",RIGHT(H1143,LEN(H1143)-4),RIGHT(H1143,LEN(H1143)-6)),\"\"))","v":""}]
[50002275,"NORD HT AS","EcoMaster 3P 8.0",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 008","2024-01-15","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1144,1)=\"J\",LEFT(H1144,2),LEFT(H1144,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1144,1)=\"J\",RIGHT(H1144,LEN(H1144)-4),RIGHT(H1144,LEN(H1144)-6)),\"\"))","v":""}]
[50002276,"NORD HT AS","EcoMaster 3P 10.0",10,11,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 008","2024-01-15","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1145,1)=\"J\",LEFT(H1145,2),LEFT(H1145,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1145,1)=\"J\",RIGHT(H1145,LEN(H1145)-4),RIGHT(H1145,LEN(H1145)-6)),\"\"))","v":""}]
[50002277,"NORD HT AS","EcoMaster 3P 12.0",12,13.2,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 008","2024-01-15","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1146,1)=\"J\",LEFT(H1146,2),LEFT(H1146,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1146,1)=\"J\",RIGHT(H1146,LEN(H1146)-4),RIGHT(H1146,LEN(H1146)-6)),\"\"))","v":""}]
[50002278,"NORD HT AS","EcoMaster 3P 15.0",15,15,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 008","2024-01-15","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1147,1)=\"J\",LEFT(H1147,2),LEFT(H1147,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1147,1)=\"J\",RIGHT(H1147,LEN(H1147)-4),RIGHT(H1147,LEN(H1147)-6)),\"\"))","v":""}]
[50000994,"PIXII","PowerShaper 3.3kW/YYkWh",3.3,3.3,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1148,1)=\"J\",LEFT(H1148,2),LEFT(H1148,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1148,1)=\"J\",RIGHT(H1148,LEN(H1148)-4),RIGHT(H1148,LEN(H1148)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001008,"PIXII","PowerShaper 6.7kW/YYkWh",6.7,6.7,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1149,1)=\"J\",LEFT(H1149,2),LEFT(H1149,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1149,1)=\"J\",RIGHT(H1149,LEN(H1149)-4),RIGHT(H1149,LEN(H1149)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000995,"PIXII","PowerShaper 10kW/YYkWh",10,10,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1150,1)=\"J\",LEFT(H1150,2),LEFT(H1150,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1150,1)=\"J\",RIGHT(H1150,LEN(H1150)-4),RIGHT(H1150,LEN(H1150)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000996,"PIXII","PowerShaper 13.3kW/YYkWh",13.3,13.3,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1151,1)=\"J\",LEFT(H1151,2),LEFT(H1151,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1151,1)=\"J\",RIGHT(H1151,LEN(H1151)-4),RIGHT(H1151,LEN(H1151)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000997,"PIXII","PowerShaper 16.7kW/YYkWh",16.7,16.7,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1152,1)=\"J\",LEFT(H1152,2),LEFT(H1152,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1152,1)=\"J\",RIGHT(H1152,LEN(H1152)-4),RIGHT(H1152,LEN(H1152)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000998,"PIXII","PowerShaper 20kW/YYkWh",20,20,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1153,1)=\"J\",LEFT(H1153,2),LEFT(H1153,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1153,1)=\"J\",RIGHT(H1153,LEN(H1153)-4),RIGHT(H1153,LEN(H1153)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50000999,"PIXII","PowerShaper 23.3kW/YYkWh",23.3,23.3,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1154,1)=\"J\",LEFT(H1154,2),LEFT(H1154,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1154,1)=\"J\",RIGHT(H1154,LEN(H1154)-4),RIGHT(H1154,LEN(H1154)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001000,"PIXII","PowerShaper 26.7kW/YYkWh",26.7,26.7,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1155,1)=\"J\",LEFT(H1155,2),LEFT(H1155,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1155,1)=\"J\",RIGHT(H1155,LEN(H1155)-4),RIGHT(H1155,LEN(H1155)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001001,"PIXII","PowerShaper 30kW/YYkWh",30,30,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1156,1)=\"J\",LEFT(H1156,2),LEFT(H1156,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1156,1)=\"J\",RIGHT(H1156,LEN(H1156)-4),RIGHT(H1156,LEN(H1156)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001002,"PIXII","PowerShaper 40kW/YYkWh",30,30,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1157,1)=\"J\",LEFT(H1157,2),LEFT(H1157,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1157,1)=\"J\",RIGHT(H1157,LEN(H1157)-4),RIGHT(H1157,LEN(H1157)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001003,"PIXII","PowerShaper 33kW/YYkWh",33,33,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1158,1)=\"J\",LEFT(H1158,2),LEFT(H1158,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1158,1)=\"J\",RIGHT(H1158,LEN(H1158)-4),RIGHT(H1158,LEN(H1158)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001004,"PIXII","PowerShaper 36.7kW/YYkWh",36.700000000000003,36.700000000000003,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1159,1)=\"J\",LEFT(H1159,2),LEFT(H1159,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1159,1)=\"J\",RIGHT(H1159,LEN(H1159)-4),RIGHT(H1159,LEN(H1159)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001005,"PIXII","PowerShaper 43.3kW/YYkWh",43.3,43.3,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1160,1)=\"J\",LEFT(H1160,2),LEFT(H1160,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1160,1)=\"J\",RIGHT(H1160,LEN(H1160)-4),RIGHT(H1160,LEN(H1160)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001006,"PIXII","PowerShaper 46.7kW/YYkWh",46.7,46.7,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1161,1)=\"J\",LEFT(H1161,2),LEFT(H1161,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1161,1)=\"J\",RIGHT(H1161,LEN(H1161)-4),RIGHT(H1161,LEN(H1161)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001007,"PIXII","PowerShaper 50kW/YYkWh",50,50,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-08-18","Martin Bertsch","2023-08-18",null,null,null,null,"Nein","Nein","Nein","VDE4105","Martin Bertsch (OE)","19PP137-05_0","2020-05-12","nicht vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1162,1)=\"J\",LEFT(H1162,2),LEFT(H1162,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1162,1)=\"J\",RIGHT(H1162,LEN(H1162)-4),RIGHT(H1162,LEN(H1162)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50002029,"PRAMAC","420P050",50,50,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2024-03-12","Martin Bertsch","2024-03-12",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"23TH0331-OVE-directive R25_0","2023-11-29",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1163,1)=\"J\",LEFT(H1163,2),LEFT(H1163,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1163,1)=\"J\",RIGHT(H1163,LEN(H1163)-4),RIGHT(H1163,LEN(H1163)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50002030,"PRAMAC","421P050",50,50,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2024-03-12","Martin Bertsch","2024-03-12",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"23TH0331-OVE-directive R25_0","2023-11-29",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1164,1)=\"J\",LEFT(H1164,2),LEFT(H1164,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1164,1)=\"J\",RIGHT(H1164,LEN(H1164)-4),RIGHT(H1164,LEN(H1164)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50002031,"PRAMAC","420P088",88,88,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2024-03-12","Martin Bertsch","2024-03-12",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"23TH0331-OVE-directive R25_0","2023-11-29",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1165,1)=\"J\",LEFT(H1165,2),LEFT(H1165,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1165,1)=\"J\",RIGHT(H1165,LEN(H1165)-4),RIGHT(H1165,LEN(H1165)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50002028,"PRAMAC","421P100",88,88,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2024-03-12","Martin Bertsch","2024-03-12",null,null,null,null,"Ja","Ja","Nein","Vorhanden",null,"23TH0331-OVE-directive R25_0","2023-11-29",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1166,1)=\"J\",LEFT(H1166,2),LEFT(H1166,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1166,1)=\"J\",RIGHT(H1166,LEN(H1166)-4),RIGHT(H1166,LEN(H1166)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001009,"Q Cells","Q.HOME ESS AC-G2",3,3,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1167,1)=\"J\",LEFT(H1167,2),LEFT(H1167,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1167,1)=\"J\",RIGHT(H1167,LEN(H1167)-4),RIGHT(H1167,LEN(H1167)-6)),\"\"))","v":""}]
[50001010,"Q Cells","Q.Volt HYB-G3 3.0 kW 1P",null,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1168,1)=\"J\",LEFT(H1168,2),LEFT(H1168,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1168,1)=\"J\",RIGHT(H1168,LEN(H1168)-4),RIGHT(H1168,LEN(H1168)-6)),\"\"))","v":""}]
[50001011,"Q Cells","Q.Volt HYB-G3 3.7 kW 1P",null,3.68,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1169,1)=\"J\",LEFT(H1169,2),LEFT(H1169,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1169,1)=\"J\",RIGHT(H1169,LEN(H1169)-4),RIGHT(H1169,LEN(H1169)-6)),\"\"))","v":""}]
[50001012,"Q Cells","Q.HOME ESS HYB-G2",4.5999999999999996,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1170,1)=\"J\",LEFT(H1170,2),LEFT(H1170,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1170,1)=\"J\",RIGHT(H1170,LEN(H1170)-4),RIGHT(H1170,LEN(H1170)-6)),\"\"))","v":""}]
[50002065,"Q Cells","Q.VOLT H5.0 T-F",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1171,1)=\"J\",LEFT(H1171,2),LEFT(H1171,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1171,1)=\"J\",RIGHT(H1171,LEN(H1171)-4),RIGHT(H1171,LEN(H1171)-6)),\"\"))","v":"mit Einschränkung"}]
[50001013,"Q Cells","Q.Volt HYB-G3 5.0 kW 3P",5,5.5,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1172,1)=\"J\",LEFT(H1172,2),LEFT(H1172,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1172,1)=\"J\",RIGHT(H1172,LEN(H1172)-4),RIGHT(H1172,LEN(H1172)-6)),\"\"))","v":""}]
[50001014,"Q Cells","Q.Volt HYB-G3 5.0 kW 3P-D",5,5.5,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1173,1)=\"J\",LEFT(H1173,2),LEFT(H1173,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1173,1)=\"J\",RIGHT(H1173,LEN(H1173)-4),RIGHT(H1173,LEN(H1173)-6)),\"\"))","v":""}]
[50002066,"Q Cells","Q.VOLT H6.0 T-F",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1174,1)=\"J\",LEFT(H1174,2),LEFT(H1174,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1174,1)=\"J\",RIGHT(H1174,LEN(H1174)-4),RIGHT(H1174,LEN(H1174)-6)),\"\"))","v":"mit Einschränkung"}]
[50001015,"Q Cells","Q.Volt HYB-G3 6.0 kW 3P",6,6.6,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1175,1)=\"J\",LEFT(H1175,2),LEFT(H1175,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1175,1)=\"J\",RIGHT(H1175,LEN(H1175)-4),RIGHT(H1175,LEN(H1175)-6)),\"\"))","v":""}]
[50001016,"Q Cells","Q.Volt HYB-G3 6.0 kW 3P-D",6,6.6,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1176,1)=\"J\",LEFT(H1176,2),LEFT(H1176,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1176,1)=\"J\",RIGHT(H1176,LEN(H1176)-4),RIGHT(H1176,LEN(H1176)-6)),\"\"))","v":""}]
[50002067,"Q Cells","Q.VOLT H8.0 T-F",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1177,1)=\"J\",LEFT(H1177,2),LEFT(H1177,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1177,1)=\"J\",RIGHT(H1177,LEN(H1177)-4),RIGHT(H1177,LEN(H1177)-6)),\"\"))","v":"mit Einschränkung"}]
[50001017,"Q Cells","Q.Volt HYB-G3 8.0 kW 3P",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1178,1)=\"J\",LEFT(H1178,2),LEFT(H1178,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1178,1)=\"J\",RIGHT(H1178,LEN(H1178)-4),RIGHT(H1178,LEN(H1178)-6)),\"\"))","v":""}]
[50001018,"Q Cells","Q.Volt HYB-G3 8.0 kW 3P-D",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1179,1)=\"J\",LEFT(H1179,2),LEFT(H1179,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1179,1)=\"J\",RIGHT(H1179,LEN(H1179)-4),RIGHT(H1179,LEN(H1179)-6)),\"\"))","v":""}]
[50002068,"Q Cells","Q.VOLT H10.0 T-F",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1180,1)=\"J\",LEFT(H1180,2),LEFT(H1180,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1180,1)=\"J\",RIGHT(H1180,LEN(H1180)-4),RIGHT(H1180,LEN(H1180)-6)),\"\"))","v":"mit Einschränkung"}]
[50001019,"Q Cells","Q.Volt HYB-G3 10.0 kW 3P",10,11,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1181,1)=\"J\",LEFT(H1181,2),LEFT(H1181,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1181,1)=\"J\",RIGHT(H1181,LEN(H1181)-4),RIGHT(H1181,LEN(H1181)-6)),\"\"))","v":""}]
[50001020,"Q Cells","Q.Volt HYB-G3 10.0 kW 3P-D",10,11,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1182,1)=\"J\",LEFT(H1182,2),LEFT(H1182,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1182,1)=\"J\",RIGHT(H1182,LEN(H1182)-4),RIGHT(H1182,LEN(H1182)-6)),\"\"))","v":""}]
[50002069,"Q Cells","Q.VOLT H12.0 T-F",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-01-30","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365-R2","2023-04-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1183,1)=\"J\",LEFT(H1183,2),LEFT(H1183,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1183,1)=\"J\",RIGHT(H1183,LEN(H1183)-4),RIGHT(H1183,LEN(H1183)-6)),\"\"))","v":"mit Einschränkung"}]
[50001021,"Q Cells","Q.Volt HYB-G3 12.0 kW 3P",12,13.2,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1184,1)=\"J\",LEFT(H1184,2),LEFT(H1184,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1184,1)=\"J\",RIGHT(H1184,LEN(H1184)-4),RIGHT(H1184,LEN(H1184)-6)),\"\"))","v":""}]
[50001022,"Q Cells","Q.Volt HYB-G3 12.0 kW 3P-D",12,13.2,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1185,1)=\"J\",LEFT(H1185,2),LEFT(H1185,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1185,1)=\"J\",RIGHT(H1185,LEN(H1185)-4),RIGHT(H1185,LEN(H1185)-6)),\"\"))","v":""}]
[50001023,"Q Cells","Q.Volt HYB-G3 15.0 kW 3P",15,15,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1186,1)=\"J\",LEFT(H1186,2),LEFT(H1186,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1186,1)=\"J\",RIGHT(H1186,LEN(H1186)-4),RIGHT(H1186,LEN(H1186)-6)),\"\"))","v":""}]
[50001024,"Q Cells","Q.Volt HYB-G3 15.0 kW 3P-D",15,15,3,"Hybrid-Wechselrichter","Ja","2022-07-28",null,null,null,null,null,null,null,null,null,"OK","Roland Bründlinger","CN2182YH 001","2021-07-19",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1187,1)=\"J\",LEFT(H1187,2),LEFT(H1187,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1187,1)=\"J\",RIGHT(H1187,LEN(H1187)-4),RIGHT(H1187,LEN(H1187)-6)),\"\"))","v":""}]
[50001025,"RCT Power GmbH","Power Inverter 4.0 ",4,6.3,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0431","2020-06-09",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1188,1)=\"J\",LEFT(H1188,2),LEFT(H1188,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1188,1)=\"J\",RIGHT(H1188,LEN(H1188)-4),RIGHT(H1188,LEN(H1188)-6)),\"\"))","v":""}]
[50001026,"RCT Power GmbH","Power Inverter 6.0 ",6,6.3,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0431","2020-06-09",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1189,1)=\"J\",LEFT(H1189,2),LEFT(H1189,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1189,1)=\"J\",RIGHT(H1189,LEN(H1189)-4),RIGHT(H1189,LEN(H1189)-6)),\"\"))","v":""}]
[50001027,"RCT Power GmbH","Power Storage AC 4.0",4,6.3,3,"AC-Batteriewechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0431","2020-06-09",null,"OK",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1190,1)=\"J\",LEFT(H1190,2),LEFT(H1190,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1190,1)=\"J\",RIGHT(H1190,LEN(H1190)-4),RIGHT(H1190,LEN(H1190)-6)),\"\"))","v":""}]
[50001028,"RCT Power GmbH","Power Storage AC 6.0",6,6.3,3,"AC-Batteriewechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0431","2020-06-09",null,"OK",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1191,1)=\"J\",LEFT(H1191,2),LEFT(H1191,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1191,1)=\"J\",RIGHT(H1191,LEN(H1191)-4),RIGHT(H1191,LEN(H1191)-6)),\"\"))","v":""}]
[50001029,"RCT Power GmbH","Power Storage DC 4.0",4,6.3,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"19TH0431","2020-06-09",null,"OK",null,null,null,null,"Batteriespeicher 3~ DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1192,1)=\"J\",LEFT(H1192,2),LEFT(H1192,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1192,1)=\"J\",RIGHT(H1192,LEN(H1192)-4),RIGHT(H1192,LEN(H1192)-6)),\"\"))","v":""}]
[50001030,"RCT Power GmbH","Power Storage DC 6.0",6,6.3,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"19TH0431","2020-06-09",null,"OK",null,null,null,null,"Batteriespeicher 3~ DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1193,1)=\"J\",LEFT(H1193,2),LEFT(H1193,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1193,1)=\"J\",RIGHT(H1193,LEN(H1193)-4),RIGHT(H1193,LEN(H1193)-6)),\"\"))","v":""}]
[50001031,"RCT Power GmbH","Power Storage DC 10.0 ",9.9,10.5,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"19TH0431-DC 10.0","2020-12-02",null,"OK",null,null,null,null,"Batteriespeicher 3~ DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1194,1)=\"J\",LEFT(H1194,2),LEFT(H1194,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1194,1)=\"J\",RIGHT(H1194,LEN(H1194)-4),RIGHT(H1194,LEN(H1194)-6)),\"\"))","v":""}]
[50001032,"RCT Power GmbH","Power Storage DC 8.0 ",8,10.5,3,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"19TH0431-DC 10.0","2020-12-02",null,"OK",null,null,null,null,"Batteriespeicher 3~ DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1195,1)=\"J\",LEFT(H1195,2),LEFT(H1195,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1195,1)=\"J\",RIGHT(H1195,LEN(H1195)-4),RIGHT(H1195,LEN(H1195)-6)),\"\"))","v":""}]
[50002044,"RECO","RHT-4K-25",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1196,1)=\"J\",LEFT(H1196,2),LEFT(H1196,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1196,1)=\"J\",RIGHT(H1196,LEN(H1196)-4),RIGHT(H1196,LEN(H1196)-6)),\"\"))","v":"mit Einschränkung"}]
[50002045,"RECO","RHT-5K-25",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1197,1)=\"J\",LEFT(H1197,2),LEFT(H1197,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1197,1)=\"J\",RIGHT(H1197,LEN(H1197)-4),RIGHT(H1197,LEN(H1197)-6)),\"\"))","v":"mit Einschränkung"}]
[50002046,"RECO","RHT-6K-25",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1198,1)=\"J\",LEFT(H1198,2),LEFT(H1198,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1198,1)=\"J\",RIGHT(H1198,LEN(H1198)-4),RIGHT(H1198,LEN(H1198)-6)),\"\"))","v":"mit Einschränkung"}]
[50002047,"RECO","RHT-8K-25",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1199,1)=\"J\",LEFT(H1199,2),LEFT(H1199,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1199,1)=\"J\",RIGHT(H1199,LEN(H1199)-4),RIGHT(H1199,LEN(H1199)-6)),\"\"))","v":"mit Einschränkung"}]
[50002048,"RECO","RHT-10K-25",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1200,1)=\"J\",LEFT(H1200,2),LEFT(H1200,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1200,1)=\"J\",RIGHT(H1200,LEN(H1200)-4),RIGHT(H1200,LEN(H1200)-6)),\"\"))","v":"mit Einschränkung"}]
[50002049,"RECO","RHT-10K-40",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1201,1)=\"J\",LEFT(H1201,2),LEFT(H1201,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1201,1)=\"J\",RIGHT(H1201,LEN(H1201)-4),RIGHT(H1201,LEN(H1201)-6)),\"\"))","v":"mit Einschränkung"}]
[50002050,"RECO","RHT-12K-25",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1202,1)=\"J\",LEFT(H1202,2),LEFT(H1202,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1202,1)=\"J\",RIGHT(H1202,LEN(H1202)-4),RIGHT(H1202,LEN(H1202)-6)),\"\"))","v":"mit Einschränkung"}]
[50002051,"RECO","RHT-12K-40",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1203,1)=\"J\",LEFT(H1203,2),LEFT(H1203,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1203,1)=\"J\",RIGHT(H1203,LEN(H1203)-4),RIGHT(H1203,LEN(H1203)-6)),\"\"))","v":"mit Einschränkung"}]
[50002052,"RECO","RHT-15K-40",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1204,1)=\"J\",LEFT(H1204,2),LEFT(H1204,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1204,1)=\"J\",RIGHT(H1204,LEN(H1204)-4),RIGHT(H1204,LEN(H1204)-6)),\"\"))","v":"mit Einschränkung"}]
[50002053,"RECO","RHT-20K-40",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Rartin Bertsch","2024-01-05","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1205,1)=\"J\",LEFT(H1205,2),LEFT(H1205,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1205,1)=\"J\",RIGHT(H1205,LEN(H1205)-4),RIGHT(H1205,LEN(H1205)-6)),\"\"))","v":"mit Einschränkung"}]
[50001033,"REFUsol","REFUsol 20K ",null,20,3,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1206,1)=\"J\",LEFT(H1206,2),LEFT(H1206,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1206,1)=\"J\",RIGHT(H1206,LEN(H1206)-4),RIGHT(H1206,LEN(H1206)-6)),\"\"))","v":""}]
[50001034,"REFUsol","REFUsol 20K-2T",20,22,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1207,1)=\"J\",LEFT(H1207,2),LEFT(H1207,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1207,1)=\"J\",RIGHT(H1207,LEN(H1207)-4),RIGHT(H1207,LEN(H1207)-6)),\"\"))","v":""}]
[50001035,"REFUsol","REFUsol 33K-2T",33,36.299999999999997,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1208,1)=\"J\",LEFT(H1208,2),LEFT(H1208,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1208,1)=\"J\",RIGHT(H1208,LEN(H1208)-4),RIGHT(H1208,LEN(H1208)-6)),\"\"))","v":""}]
[50001036,"REFUsol","REFUsol 50K-3T",50,50,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1209,1)=\"J\",LEFT(H1209,2),LEFT(H1209,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1209,1)=\"J\",RIGHT(H1209,LEN(H1209)-4),RIGHT(H1209,LEN(H1209)-6)),\"\"))","v":""}]
[50001037,"REFUsol","REFUstore 50K",null,50,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-03-19",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"18TH0270","2021-03-19",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1210,1)=\"J\",LEFT(H1210,2),LEFT(H1210,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1210,1)=\"J\",RIGHT(H1210,LEN(H1210)-4),RIGHT(H1210,LEN(H1210)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001038,"REFUsol","REFUstore 88K",null,88,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-03-19",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"18TH0270","2021-03-19",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1211,1)=\"J\",LEFT(H1211,2),LEFT(H1211,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1211,1)=\"J\",RIGHT(H1211,LEN(H1211)-4),RIGHT(H1211,LEN(H1211)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001039,"REFUsol","REFUsol 100k",null,100,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"18TH0270","2021-03-19",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1212,1)=\"J\",LEFT(H1212,2),LEFT(H1212,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1212,1)=\"J\",RIGHT(H1212,LEN(H1212)-4),RIGHT(H1212,LEN(H1212)-6)),\"\"))","v":""}]
[50001040,"REFUsol","REFUstore 100K",null,100,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-03-19",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"18TH0270","2021-03-19",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1213,1)=\"J\",LEFT(H1213,2),LEFT(H1213,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1213,1)=\"J\",RIGHT(H1213,LEN(H1213)-4),RIGHT(H1213,LEN(H1213)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001041,"RENAC","N3-HV-5.0",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-08","V1.05",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","ABRE-ESH-P22120410","2023-07-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1214,1)=\"J\",LEFT(H1214,2),LEFT(H1214,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1214,1)=\"J\",RIGHT(H1214,LEN(H1214)-4),RIGHT(H1214,LEN(H1214)-6)),\"\"))","v":"mit Einschränkung"}]
[50001042,"RENAC","N3-HV-6.0",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-08","V1.05",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","ABRE-ESH-P22120410","2023-07-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1215,1)=\"J\",LEFT(H1215,2),LEFT(H1215,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1215,1)=\"J\",RIGHT(H1215,LEN(H1215)-4),RIGHT(H1215,LEN(H1215)-6)),\"\"))","v":"mit Einschränkung"}]
[50001043,"RENAC","N3-HV-8.0",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-08","V1.05",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","ABRE-ESH-P22120410","2023-07-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1216,1)=\"J\",LEFT(H1216,2),LEFT(H1216,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1216,1)=\"J\",RIGHT(H1216,LEN(H1216)-4),RIGHT(H1216,LEN(H1216)-6)),\"\"))","v":"mit Einschränkung"}]
[50001044,"RENAC","N3-HV-10.0",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-08","V1.05",null,null,null,"Ja","Nein","Nein","Vorhanden","Martin Bertsch (OE)","ABRE-ESH-P22120410","2023-07-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1217,1)=\"J\",LEFT(H1217,2),LEFT(H1217,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1217,1)=\"J\",RIGHT(H1217,LEN(H1217)-4),RIGHT(H1217,LEN(H1217)-6)),\"\"))","v":"mit Einschränkung"}]
[50001045,"SAJ","H2-5K-T2",5,5.5,3,"Hybrid-Wechselrichter","Ja","2023-10-05","Martin Bertsch","2023-06-29","FW-Version V4.023 ; Ländersetup: V1.012 Österreich Tor Erzeuger",null,null,null,"Ja","Nein",null,"Vorhanden","Martin Bertsch (OE)","CN239J52 001","2023-02-28","nicht vorhanden","OK",null,null,null,null,"Gerät wurde am 23.09.2023 im Auftrag von OE beim AIT geprüft. Mit aktueller FW fehlerfrei.",null,null,null,null,{"$f":"IF(LEFT(H1218,1)=\"J\",LEFT(H1218,2),LEFT(H1218,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1218,1)=\"J\",RIGHT(H1218,LEN(H1218)-4),RIGHT(H1218,LEN(H1218)-6)),\"\"))","v":""}]
[50001046,"SAJ","HS2-5K-T2-X",5,5.5,3,"Hybrid-Wechselrichter","Ja","2023-10-05","Martin Bertsch","2023-05-19","FW-Version V4.023 ; Ländersetup: V1.012 Österreich Tor Erzeuger",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","BSWO-ESH-P22100456-R1","2023-04-23","nicht vorhanden","OK",null,null,null,null,"Gerät wurde am 23.09.2023 im Auftrag von OE beim AIT geprüft. Mit aktueller FW fehlerfrei.",null,null,null,null,{"$f":"IF(LEFT(H1219,1)=\"J\",LEFT(H1219,2),LEFT(H1219,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1219,1)=\"J\",RIGHT(H1219,LEN(H1219)-4),RIGHT(H1219,LEN(H1219)-6)),\"\"))","v":""}]
[50001047,"SAJ","H2-6K-T2",6,6.6,3,"Hybrid-Wechselrichter","Ja","2023-10-05","Martin Bertsch","2023-06-29","FW-Version V4.023 ; Ländersetup: V1.012 Österreich Tor Erzeuger",null,null,null,"Ja","Nein",null,"Vorhanden","Martin Bertsch (OE)","CN239J52 001","2023-02-28","nicht vorhanden","OK",null,null,null,null,"Gerät wurde am 23.09.2023 im Auftrag von OE beim AIT geprüft. Mit aktueller FW fehlerfrei.",null,null,null,null,{"$f":"IF(LEFT(H1220,1)=\"J\",LEFT(H1220,2),LEFT(H1220,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1220,1)=\"J\",RIGHT(H1220,LEN(H1220)-4),RIGHT(H1220,LEN(H1220)-6)),\"\"))","v":""}]
[50001048,"SAJ","HS2-6K-T2-X",6,6.6,3,"Hybrid-Wechselrichter","Ja","2023-10-05","Martin Bertsch","2023-05-19","FW-Version V4.023 ; Ländersetup: V1.012 Österreich Tor Erzeuger",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","BSWO-ESH-P22100456-R1","2023-04-23","nicht vorhanden","OK",null,null,null,null,"Gerät wurde am 23.09.2023 im Auftrag von OE beim AIT geprüft. Mit aktueller FW fehlerfrei.",null,null,null,null,{"$f":"IF(LEFT(H1221,1)=\"J\",LEFT(H1221,2),LEFT(H1221,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1221,1)=\"J\",RIGHT(H1221,LEN(H1221)-4),RIGHT(H1221,LEN(H1221)-6)),\"\"))","v":""}]
[50001049,"SAJ","H2-8K-T2",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2023-10-05","Martin Bertsch","2023-06-29","FW-Version V4.023 ; Ländersetup: V1.012 Österreich Tor Erzeuger",null,null,null,"Ja","Nein",null,"Vorhanden","Martin Bertsch (OE)","CN239J52 001","2023-02-28","nicht vorhanden","OK",null,null,null,null,"Gerät wurde am 23.09.2023 im Auftrag von OE beim AIT geprüft. Mit aktueller FW fehlerfrei.",null,null,null,null,{"$f":"IF(LEFT(H1222,1)=\"J\",LEFT(H1222,2),LEFT(H1222,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1222,1)=\"J\",RIGHT(H1222,LEN(H1222)-4),RIGHT(H1222,LEN(H1222)-6)),\"\"))","v":""}]
[50001050,"SAJ","HS2-8K-T2-X",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2023-10-05","Martin Bertsch","2023-05-19","FW-Version V4.023 ; Ländersetup: V1.012 Österreich Tor Erzeuger",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","BSWO-ESH-P22100456-R1","2023-04-23","nicht vorhanden","OK",null,null,null,null,"Gerät wurde am 23.09.2023 im Auftrag von OE beim AIT geprüft. Mit aktueller FW fehlerfrei.",null,null,null,null,{"$f":"IF(LEFT(H1223,1)=\"J\",LEFT(H1223,2),LEFT(H1223,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1223,1)=\"J\",RIGHT(H1223,LEN(H1223)-4),RIGHT(H1223,LEN(H1223)-6)),\"\"))","v":""}]
[50001051,"SAJ","H2-10K-T2",10,11,3,"Hybrid-Wechselrichter","Ja","2023-10-05","Martin Bertsch","2023-06-29","FW-Version V4.023 ; Ländersetup: V1.012 Österreich Tor Erzeuger",null,null,null,"Ja","Nein",null,"Vorhanden","Martin Bertsch (OE)","CN239J52 001","2023-02-28","nicht vorhanden","OK",null,null,null,null,"Gerät wurde am 23.09.2023 im Auftrag von OE beim AIT geprüft. Mit aktueller FW fehlerfrei.",null,null,null,null,{"$f":"IF(LEFT(H1224,1)=\"J\",LEFT(H1224,2),LEFT(H1224,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1224,1)=\"J\",RIGHT(H1224,LEN(H1224)-4),RIGHT(H1224,LEN(H1224)-6)),\"\"))","v":""}]
[50002132,"SAJ","H2-10K-T3",10,11,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1225,1)=\"J\",LEFT(H1225,2),LEFT(H1225,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1225,1)=\"J\",RIGHT(H1225,LEN(H1225)-4),RIGHT(H1225,LEN(H1225)-6)),\"\"))","v":""}]
[50001052,"SAJ","HS2-10K-T2-X",10,11,3,"Hybrid-Wechselrichter","Ja","2023-10-05","Martin Bertsch","2023-05-19","FW-Version V4.023 ; Ländersetup: V1.012 Österreich Tor Erzeuger",null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","BSWO-ESH-P22100456-R1","2023-04-23","nicht vorhanden","OK",null,null,null,null,"Gerät wurde am 23.09.2023 im Auftrag von OE beim AIT geprüft. Mit aktueller FW fehlerfrei.",null,null,null,null,{"$f":"IF(LEFT(H1226,1)=\"J\",LEFT(H1226,2),LEFT(H1226,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1226,1)=\"J\",RIGHT(H1226,LEN(H1226)-4),RIGHT(H1226,LEN(H1226)-6)),\"\"))","v":""}]
[50002133,"SAJ","H2-12K-T3",12,13.2,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1227,1)=\"J\",LEFT(H1227,2),LEFT(H1227,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1227,1)=\"J\",RIGHT(H1227,LEN(H1227)-4),RIGHT(H1227,LEN(H1227)-6)),\"\"))","v":""}]
[50002138,"SAJ","H2-15K-T2",15,16.5,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1228,1)=\"J\",LEFT(H1228,2),LEFT(H1228,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1228,1)=\"J\",RIGHT(H1228,LEN(H1228)-4),RIGHT(H1228,LEN(H1228)-6)),\"\"))","v":""}]
[50002134,"SAJ","H2-15K-T3",15,16.5,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1229,1)=\"J\",LEFT(H1229,2),LEFT(H1229,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1229,1)=\"J\",RIGHT(H1229,LEN(H1229)-4),RIGHT(H1229,LEN(H1229)-6)),\"\"))","v":""}]
[50001957,"SAJ","R6-15K-T2-32",15,16.5,3,"PV-Wechselrichter","Ja","2023-10-30","Martin Bertsch","2023-10-30",null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","CN23ZLHH 001","2023-08-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1230,1)=\"J\",LEFT(H1230,2),LEFT(H1230,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1230,1)=\"J\",RIGHT(H1230,LEN(H1230)-4),RIGHT(H1230,LEN(H1230)-6)),\"\"))","v":""}]
[50001958,"SAJ","R6-17K-T2-32",17,18.7,3,"PV-Wechselrichter","Ja","2023-10-30","Martin Bertsch","2023-10-30",null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","CN23ZLHH 001","2023-08-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1231,1)=\"J\",LEFT(H1231,2),LEFT(H1231,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1231,1)=\"J\",RIGHT(H1231,LEN(H1231)-4),RIGHT(H1231,LEN(H1231)-6)),\"\"))","v":""}]
[50002139,"SAJ","H2-20K-T2",20,22,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1232,1)=\"J\",LEFT(H1232,2),LEFT(H1232,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1232,1)=\"J\",RIGHT(H1232,LEN(H1232)-4),RIGHT(H1232,LEN(H1232)-6)),\"\"))","v":""}]
[50002135,"SAJ","H2-20K-T3",20,22,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1233,1)=\"J\",LEFT(H1233,2),LEFT(H1233,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1233,1)=\"J\",RIGHT(H1233,LEN(H1233)-4),RIGHT(H1233,LEN(H1233)-6)),\"\"))","v":""}]
[50001959,"SAJ","R6-20K-T2-32",20,22,3,"PV-Wechselrichter","Ja","2023-10-30","Martin Bertsch","2023-10-30",null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","CN23ZLHH 001","2023-08-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1234,1)=\"J\",LEFT(H1234,2),LEFT(H1234,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1234,1)=\"J\",RIGHT(H1234,LEN(H1234)-4),RIGHT(H1234,LEN(H1234)-6)),\"\"))","v":""}]
[50001960,"SAJ","R6-22K-T2-32",22,24.2,3,"PV-Wechselrichter","Ja","2023-10-30","Martin Bertsch","2023-10-30",null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","CN23ZLHH 001","2023-08-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1235,1)=\"J\",LEFT(H1235,2),LEFT(H1235,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1235,1)=\"J\",RIGHT(H1235,LEN(H1235)-4),RIGHT(H1235,LEN(H1235)-6)),\"\"))","v":""}]
[50002140,"SAJ","H2-25K-T3-BE",25,25,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1236,1)=\"J\",LEFT(H1236,2),LEFT(H1236,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1236,1)=\"J\",RIGHT(H1236,LEN(H1236)-4),RIGHT(H1236,LEN(H1236)-6)),\"\"))","v":""}]
[50002136,"SAJ","H2-25K-T3",25,27.5,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1237,1)=\"J\",LEFT(H1237,2),LEFT(H1237,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1237,1)=\"J\",RIGHT(H1237,LEN(H1237)-4),RIGHT(H1237,LEN(H1237)-6)),\"\"))","v":""}]
[50001961,"SAJ","R6-25K-T2-32",25,27.5,3,"PV-Wechselrichter","Ja","2023-10-30","Martin Bertsch","2023-10-30",null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","CN23ZLHH 001","2023-08-06","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1238,1)=\"J\",LEFT(H1238,2),LEFT(H1238,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1238,1)=\"J\",RIGHT(H1238,LEN(H1238)-4),RIGHT(H1238,LEN(H1238)-6)),\"\"))","v":""}]
[50001809,"SAJ","R6-25K-T3-32",25,27.5,3,"PV-Wechselrichter","Ja","2023-10-16","Martin Bertsch","2023-10-06",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN232PZU 001","2023-08-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1239,1)=\"J\",LEFT(H1239,2),LEFT(H1239,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1239,1)=\"J\",RIGHT(H1239,LEN(H1239)-4),RIGHT(H1239,LEN(H1239)-6)),\"\"))","v":""}]
[50002141,"SAJ","H2-30K-T3-DE",29.99,29.99,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1240,1)=\"J\",LEFT(H1240,2),LEFT(H1240,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1240,1)=\"J\",RIGHT(H1240,LEN(H1240)-4),RIGHT(H1240,LEN(H1240)-6)),\"\"))","v":""}]
[50002137,"SAJ","H2-30K-T3",30,33,3,"Hybrid-Wechselrichter","Ja","2024-05-07","Martin Bertsch","2024-05-07",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN24KQE0 001","2024-04-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1241,1)=\"J\",LEFT(H1241,2),LEFT(H1241,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1241,1)=\"J\",RIGHT(H1241,LEN(H1241)-4),RIGHT(H1241,LEN(H1241)-6)),\"\"))","v":""}]
[50001810,"SAJ","R6-30K-T3-32",30,33,3,"PV-Wechselrichter","Ja","2023-10-16","Martin Bertsch","2023-10-06",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN232PZU 001","2023-08-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1242,1)=\"J\",LEFT(H1242,2),LEFT(H1242,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1242,1)=\"J\",RIGHT(H1242,LEN(H1242)-4),RIGHT(H1242,LEN(H1242)-6)),\"\"))","v":""}]
[50001811,"SAJ","R6-33K-T3-32",33,36.299999999999997,3,"PV-Wechselrichter","Ja","2023-10-16","Martin Bertsch","2023-10-06",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN232PZU 001","2023-08-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1243,1)=\"J\",LEFT(H1243,2),LEFT(H1243,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1243,1)=\"J\",RIGHT(H1243,LEN(H1243)-4),RIGHT(H1243,LEN(H1243)-6)),\"\"))","v":""}]
[50001812,"SAJ","R6-36K-T3-32",36,39.6,3,"PV-Wechselrichter","Ja","2023-10-16","Martin Bertsch","2023-10-06",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN232PZU 001","2023-08-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1244,1)=\"J\",LEFT(H1244,2),LEFT(H1244,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1244,1)=\"J\",RIGHT(H1244,LEN(H1244)-4),RIGHT(H1244,LEN(H1244)-6)),\"\"))","v":""}]
[50001813,"SAJ","R6-36K-T4-32",36,39.6,3,"PV-Wechselrichter","Ja","2023-10-16","Martin Bertsch","2023-10-06",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN232PZU 001","2023-08-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1245,1)=\"J\",LEFT(H1245,2),LEFT(H1245,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1245,1)=\"J\",RIGHT(H1245,LEN(H1245)-4),RIGHT(H1245,LEN(H1245)-6)),\"\"))","v":""}]
[50001814,"SAJ","R6-40K-T4-32",40,44,3,"PV-Wechselrichter","Ja","2023-10-16","Martin Bertsch","2023-10-06",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN232PZU 001","2023-08-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1246,1)=\"J\",LEFT(H1246,2),LEFT(H1246,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1246,1)=\"J\",RIGHT(H1246,LEN(H1246)-4),RIGHT(H1246,LEN(H1246)-6)),\"\"))","v":""}]
[50001815,"SAJ","R6-50K-T4-32",50,55,3,"PV-Wechselrichter","Ja","2023-10-16","Martin Bertsch","2023-10-06",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN232PZU 001","2023-08-07","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1247,1)=\"J\",LEFT(H1247,2),LEFT(H1247,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1247,1)=\"J\",RIGHT(H1247,LEN(H1247)-4),RIGHT(H1247,LEN(H1247)-6)),\"\"))","v":""}]
[50002202,"SAKO","SKY300M1-EU-230",0.3,0.3,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-13","Martin Bertsch","2024-05-13",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"230124RECO01","2023-06-08","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1248,1)=\"J\",LEFT(H1248,2),LEFT(H1248,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1248,1)=\"J\",RIGHT(H1248,LEN(H1248)-4),RIGHT(H1248,LEN(H1248)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002203,"SAKO","SKY400M1-EU-230",0.4,0.4,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-13","Martin Bertsch","2024-05-13",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"230124RECO01","2023-06-08","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1249,1)=\"J\",LEFT(H1249,2),LEFT(H1249,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1249,1)=\"J\",RIGHT(H1249,LEN(H1249)-4),RIGHT(H1249,LEN(H1249)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002204,"SAKO","SKY500M1-EU-230",0.5,0.5,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-13","Martin Bertsch","2024-05-13",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"230124RECO01","2023-06-08","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1250,1)=\"J\",LEFT(H1250,2),LEFT(H1250,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1250,1)=\"J\",RIGHT(H1250,LEN(H1250)-4),RIGHT(H1250,LEN(H1250)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002205,"SAKO","SKY600M1-EU-230",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-13","Martin Bertsch","2024-05-13",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"230124RECO01","2023-06-08","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1251,1)=\"J\",LEFT(H1251,2),LEFT(H1251,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1251,1)=\"J\",RIGHT(H1251,LEN(H1251)-4),RIGHT(H1251,LEN(H1251)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002206,"SAKO","SKY800M1-EU-230",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-13","Martin Bertsch","2024-05-13",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"230124RECO01","2023-06-08","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1252,1)=\"J\",LEFT(H1252,2),LEFT(H1252,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1252,1)=\"J\",RIGHT(H1252,LEN(H1252)-4),RIGHT(H1252,LEN(H1252)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001974,"SAX","PRIMO-1-6-5-230",3.68,3.68,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-03","Martin Bertsch","2024-01-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden",null,"20TH0533-OVE-directive R25_0","2023-10-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1253,1)=\"J\",LEFT(H1253,2),LEFT(H1253,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1253,1)=\"J\",RIGHT(H1253,LEN(H1253)-4),RIGHT(H1253,LEN(H1253)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50001973,"SAX","PRIMO-2-6-5-230",3.68,3.68,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-03","Martin Bertsch","2024-01-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden",null,"20TH0533-OVE-directive R25_0","2023-10-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1254,1)=\"J\",LEFT(H1254,2),LEFT(H1254,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1254,1)=\"J\",RIGHT(H1254,LEN(H1254)-4),RIGHT(H1254,LEN(H1254)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50001053,"Schachner","Schachner Generator mit FU (5 kW) ",null,5,3,"Windenergie-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Windenergiewechselrichter 3~ inselbetriebsfähig - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1255,1)=\"J\",LEFT(H1255,2),LEFT(H1255,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1255,1)=\"J\",RIGHT(H1255,LEN(H1255)-4),RIGHT(H1255,LEN(H1255)-6)),\"\"))","v":""}]
[50001054,"SENEC","SENEC.HOME V2.1 2.5",null,1.25,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1256,1)=\"J\",LEFT(H1256,2),LEFT(H1256,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1256,1)=\"J\",RIGHT(H1256,LEN(H1256)-4),RIGHT(H1256,LEN(H1256)-6)),\"\"))","v":""}]
[50001055,"SENEC","SENEC.HOME V2.1 10.0",null,2.5,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1257,1)=\"J\",LEFT(H1257,2),LEFT(H1257,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1257,1)=\"J\",RIGHT(H1257,LEN(H1257)-4),RIGHT(H1257,LEN(H1257)-6)),\"\"))","v":""}]
[50001056,"SENEC","SENEC.HOME V2.1 5.0",null,2.5,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1258,1)=\"J\",LEFT(H1258,2),LEFT(H1258,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1258,1)=\"J\",RIGHT(H1258,LEN(H1258)-4),RIGHT(H1258,LEN(H1258)-6)),\"\"))","v":""}]
[50001057,"SENEC","SENEC.HOME V2.1 7.5",null,2.5,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1259,1)=\"J\",LEFT(H1259,2),LEFT(H1259,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1259,1)=\"J\",RIGHT(H1259,LEN(H1259)-4),RIGHT(H1259,LEN(H1259)-6)),\"\"))","v":""}]
[50001058,"SENEC","SENEC.HOME V3 hybrid 10.0",null,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1260,1)=\"J\",LEFT(H1260,2),LEFT(H1260,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1260,1)=\"J\",RIGHT(H1260,LEN(H1260)-4),RIGHT(H1260,LEN(H1260)-6)),\"\"))","v":""}]
[50001059,"SENEC","SENEC.HOME V3 hybrid 2.5",null,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1261,1)=\"J\",LEFT(H1261,2),LEFT(H1261,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1261,1)=\"J\",RIGHT(H1261,LEN(H1261)-4),RIGHT(H1261,LEN(H1261)-6)),\"\"))","v":""}]
[50001060,"SENEC","SENEC.HOME V3 hybrid 5.0",null,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1262,1)=\"J\",LEFT(H1262,2),LEFT(H1262,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1262,1)=\"J\",RIGHT(H1262,LEN(H1262)-4),RIGHT(H1262,LEN(H1262)-6)),\"\"))","v":""}]
[50001061,"SENEC","SENEC.HOME V3 hybrid 7.5",null,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1263,1)=\"J\",LEFT(H1263,2),LEFT(H1263,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1263,1)=\"J\",RIGHT(H1263,LEN(H1263)-4),RIGHT(H1263,LEN(H1263)-6)),\"\"))","v":""}]
[50001062,"SENEC","SENEC.HOME V3 hybrid duo 10.0",null,9.1999999999999993,2,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1264,1)=\"J\",LEFT(H1264,2),LEFT(H1264,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1264,1)=\"J\",RIGHT(H1264,LEN(H1264)-4),RIGHT(H1264,LEN(H1264)-6)),\"\"))","v":""}]
[50001063,"SENEC","SENEC.HOME V3 hybrid duo 2.5",null,9.1999999999999993,2,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1265,1)=\"J\",LEFT(H1265,2),LEFT(H1265,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1265,1)=\"J\",RIGHT(H1265,LEN(H1265)-4),RIGHT(H1265,LEN(H1265)-6)),\"\"))","v":""}]
[50001064,"SENEC","SENEC.HOME V3 hybrid duo 5.0",null,9.1999999999999993,2,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1266,1)=\"J\",LEFT(H1266,2),LEFT(H1266,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1266,1)=\"J\",RIGHT(H1266,LEN(H1266)-4),RIGHT(H1266,LEN(H1266)-6)),\"\"))","v":""}]
[50001065,"SENEC","SENEC.HOME V3 hybrid duo 7.5",null,9.1999999999999993,2,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1267,1)=\"J\",LEFT(H1267,2),LEFT(H1267,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1267,1)=\"J\",RIGHT(H1267,LEN(H1267)-4),RIGHT(H1267,LEN(H1267)-6)),\"\"))","v":""}]
[50001862,"Senergy","SE 17KTL-D3",17,18.7,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1268,1)=\"J\",LEFT(H1268,2),LEFT(H1268,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1268,1)=\"J\",RIGHT(H1268,LEN(H1268)-4),RIGHT(H1268,LEN(H1268)-6)),\"\"))","v":"befristet"}]
[50001868,"Senergy","SE 17KTL-D3/EU",17,18.7,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1269,1)=\"J\",LEFT(H1269,2),LEFT(H1269,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1269,1)=\"J\",RIGHT(H1269,LEN(H1269)-4),RIGHT(H1269,LEN(H1269)-6)),\"\"))","v":"befristet"}]
[50001863,"Senergy","SE 20KTL-D3",20,22,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1270,1)=\"J\",LEFT(H1270,2),LEFT(H1270,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1270,1)=\"J\",RIGHT(H1270,LEN(H1270)-4),RIGHT(H1270,LEN(H1270)-6)),\"\"))","v":"befristet"}]
[50001869,"Senergy","SE 20KTL-D3/EU ",20,22,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1271,1)=\"J\",LEFT(H1271,2),LEFT(H1271,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1271,1)=\"J\",RIGHT(H1271,LEN(H1271)-4),RIGHT(H1271,LEN(H1271)-6)),\"\"))","v":"befristet"}]
[50001864,"Senergy","SE 22KTL-D3",22,24.2,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1272,1)=\"J\",LEFT(H1272,2),LEFT(H1272,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1272,1)=\"J\",RIGHT(H1272,LEN(H1272)-4),RIGHT(H1272,LEN(H1272)-6)),\"\"))","v":"befristet"}]
[50001870,"Senergy","SE 22KTL-D3/EU",22,24.2,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1273,1)=\"J\",LEFT(H1273,2),LEFT(H1273,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1273,1)=\"J\",RIGHT(H1273,LEN(H1273)-4),RIGHT(H1273,LEN(H1273)-6)),\"\"))","v":"befristet"}]
[50001865,"Senergy","SE 25KTL-D3 ",25,27.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1274,1)=\"J\",LEFT(H1274,2),LEFT(H1274,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1274,1)=\"J\",RIGHT(H1274,LEN(H1274)-4),RIGHT(H1274,LEN(H1274)-6)),\"\"))","v":"befristet"}]
[50001871,"Senergy","SE 25KTL-D3/EU",25,27.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1275,1)=\"J\",LEFT(H1275,2),LEFT(H1275,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1275,1)=\"J\",RIGHT(H1275,LEN(H1275)-4),RIGHT(H1275,LEN(H1275)-6)),\"\"))","v":"befristet"}]
[50001866,"Senergy","SE 28KTL-D3",28,30.8,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1276,1)=\"J\",LEFT(H1276,2),LEFT(H1276,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1276,1)=\"J\",RIGHT(H1276,LEN(H1276)-4),RIGHT(H1276,LEN(H1276)-6)),\"\"))","v":"befristet"}]
[50001872,"Senergy","SE 28KTL-D3/EU ",28,30.8,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1277,1)=\"J\",LEFT(H1277,2),LEFT(H1277,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1277,1)=\"J\",RIGHT(H1277,LEN(H1277)-4),RIGHT(H1277,LEN(H1277)-6)),\"\"))","v":"befristet"}]
[50001867,"Senergy","SE 30KTL-D3",30,33,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1278,1)=\"J\",LEFT(H1278,2),LEFT(H1278,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1278,1)=\"J\",RIGHT(H1278,LEN(H1278)-4),RIGHT(H1278,LEN(H1278)-6)),\"\"))","v":"befristet"}]
[50001873,"Senergy","SE 30KTL-D3/EU",30,33,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1279,1)=\"J\",LEFT(H1279,2),LEFT(H1279,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1279,1)=\"J\",RIGHT(H1279,LEN(H1279)-4),RIGHT(H1279,LEN(H1279)-6)),\"\"))","v":"befristet"}]
[50001874,"Senergy","SE 30KTL-D3/EU-CSB",30,33,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",3001,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0066-R2","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1280,1)=\"J\",LEFT(H1280,2),LEFT(H1280,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1280,1)=\"J\",RIGHT(H1280,LEN(H1280)-4),RIGHT(H1280,LEN(H1280)-6)),\"\"))","v":"befristet"}]
[50001852,"Senergy","SE 50KTL",50,55,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1281,1)=\"J\",LEFT(H1281,2),LEFT(H1281,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1281,1)=\"J\",RIGHT(H1281,LEN(H1281)-4),RIGHT(H1281,LEN(H1281)-6)),\"\"))","v":"befristet"}]
[50001855,"Senergy","SE 50KTL-D3/EU",50,55,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1282,1)=\"J\",LEFT(H1282,2),LEFT(H1282,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1282,1)=\"J\",RIGHT(H1282,LEN(H1282)-4),RIGHT(H1282,LEN(H1282)-6)),\"\"))","v":"befristet"}]
[50001853,"Senergy","SE 50KTL-Q3/EU",50,55,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1283,1)=\"J\",LEFT(H1283,2),LEFT(H1283,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1283,1)=\"J\",RIGHT(H1283,LEN(H1283)-4),RIGHT(H1283,LEN(H1283)-6)),\"\"))","v":"befristet"}]
[50001856,"Senergy","SE 50KTL-Q3/EU-CSB",50,55,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1284,1)=\"J\",LEFT(H1284,2),LEFT(H1284,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1284,1)=\"J\",RIGHT(H1284,LEN(H1284)-4),RIGHT(H1284,LEN(H1284)-6)),\"\"))","v":"befristet"}]
[50001854,"Senergy","SE 50KTL-S3/EU",50,55,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1285,1)=\"J\",LEFT(H1285,2),LEFT(H1285,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1285,1)=\"J\",RIGHT(H1285,LEN(H1285)-4),RIGHT(H1285,LEN(H1285)-6)),\"\"))","v":"befristet"}]
[50001857,"Senergy","SE 60KTL",60,66,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1286,1)=\"J\",LEFT(H1286,2),LEFT(H1286,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1286,1)=\"J\",RIGHT(H1286,LEN(H1286)-4),RIGHT(H1286,LEN(H1286)-6)),\"\"))","v":"befristet"}]
[50001860,"Senergy","SE 60KTL-D3/EU",60,66,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1287,1)=\"J\",LEFT(H1287,2),LEFT(H1287,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1287,1)=\"J\",RIGHT(H1287,LEN(H1287)-4),RIGHT(H1287,LEN(H1287)-6)),\"\"))","v":"befristet"}]
[50001858,"Senergy","SE 60KTL-Q3/EU",60,66,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1288,1)=\"J\",LEFT(H1288,2),LEFT(H1288,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1288,1)=\"J\",RIGHT(H1288,LEN(H1288)-4),RIGHT(H1288,LEN(H1288)-6)),\"\"))","v":"befristet"}]
[50001861,"Senergy","SE 60KTL-Q3/EU-CSB",60,66,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1289,1)=\"J\",LEFT(H1289,2),LEFT(H1289,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1289,1)=\"J\",RIGHT(H1289,LEN(H1289)-4),RIGHT(H1289,LEN(H1289)-6)),\"\"))","v":"befristet"}]
[50001859,"Senergy","SE 60KTL-S3/EU",60,66,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",600101,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2105WDG0065-1-R2","2023-05-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1290,1)=\"J\",LEFT(H1290,2),LEFT(H1290,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1290,1)=\"J\",RIGHT(H1290,LEN(H1290)-4),RIGHT(H1290,LEN(H1290)-6)),\"\"))","v":"befristet"}]
[50001799,"SHEENPLUS","SP_HYB-T_04K",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1291,1)=\"J\",LEFT(H1291,2),LEFT(H1291,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1291,1)=\"J\",RIGHT(H1291,LEN(H1291)-4),RIGHT(H1291,LEN(H1291)-6)),\"\"))","v":"mit Einschränkung"}]
[50001800,"SHEENPLUS","SP_HYB-T_05K",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1292,1)=\"J\",LEFT(H1292,2),LEFT(H1292,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1292,1)=\"J\",RIGHT(H1292,LEN(H1292)-4),RIGHT(H1292,LEN(H1292)-6)),\"\"))","v":"mit Einschränkung"}]
[50001801,"SHEENPLUS","SP_HYB-T_06K",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1293,1)=\"J\",LEFT(H1293,2),LEFT(H1293,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1293,1)=\"J\",RIGHT(H1293,LEN(H1293)-4),RIGHT(H1293,LEN(H1293)-6)),\"\"))","v":"mit Einschränkung"}]
[50001802,"SHEENPLUS","SP_HYB-T_08K",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1294,1)=\"J\",LEFT(H1294,2),LEFT(H1294,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1294,1)=\"J\",RIGHT(H1294,LEN(H1294)-4),RIGHT(H1294,LEN(H1294)-6)),\"\"))","v":"mit Einschränkung"}]
[50001805,"SHEENPLUS","SP_HYB-T_10K",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1295,1)=\"J\",LEFT(H1295,2),LEFT(H1295,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1295,1)=\"J\",RIGHT(H1295,LEN(H1295)-4),RIGHT(H1295,LEN(H1295)-6)),\"\"))","v":"mit Einschränkung"}]
[50001803,"SHEENPLUS","SP_HYB-T_10K-25",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1296,1)=\"J\",LEFT(H1296,2),LEFT(H1296,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1296,1)=\"J\",RIGHT(H1296,LEN(H1296)-4),RIGHT(H1296,LEN(H1296)-6)),\"\"))","v":"mit Einschränkung"}]
[50001806,"SHEENPLUS","SP_HYB-T_12K",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1297,1)=\"J\",LEFT(H1297,2),LEFT(H1297,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1297,1)=\"J\",RIGHT(H1297,LEN(H1297)-4),RIGHT(H1297,LEN(H1297)-6)),\"\"))","v":"mit Einschränkung"}]
[50001804,"SHEENPLUS","SP_HYB-T_12K-25",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1298,1)=\"J\",LEFT(H1298,2),LEFT(H1298,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1298,1)=\"J\",RIGHT(H1298,LEN(H1298)-4),RIGHT(H1298,LEN(H1298)-6)),\"\"))","v":"mit Einschränkung"}]
[50001807,"SHEENPLUS","SP_HYB-T_15K",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1299,1)=\"J\",LEFT(H1299,2),LEFT(H1299,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1299,1)=\"J\",RIGHT(H1299,LEN(H1299)-4),RIGHT(H1299,LEN(H1299)-6)),\"\"))","v":"mit Einschränkung"}]
[50001808,"SHEENPLUS","SP_HYB-T_20K",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-19","Martin Bertsch","2023-09-13","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","HC23072604-EG-AT-001","2023-09-05","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1300,1)=\"J\",LEFT(H1300,2),LEFT(H1300,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1300,1)=\"J\",RIGHT(H1300,LEN(H1300)-4),RIGHT(H1300,LEN(H1300)-6)),\"\"))","v":"mit Einschränkung"}]
[50001930,"SIGENERGY","Sigen Hybrid 5.0 TP",5,5.5,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1301,1)=\"J\",LEFT(H1301,2),LEFT(H1301,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1301,1)=\"J\",RIGHT(H1301,LEN(H1301)-4),RIGHT(H1301,LEN(H1301)-6)),\"\"))","v":""}]
[50001948,"SIGENERGY","Sigen PV Max 5.0 TP",5,5.5,3,"PV-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1302,1)=\"J\",LEFT(H1302,2),LEFT(H1302,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1302,1)=\"J\",RIGHT(H1302,LEN(H1302)-4),RIGHT(H1302,LEN(H1302)-6)),\"\"))","v":""}]
[50001939,"SIGENERGY","SigenStor AC 5.0 TP ",5,5.5,3,"AC-Batteriewechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1303,1)=\"J\",LEFT(H1303,2),LEFT(H1303,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1303,1)=\"J\",RIGHT(H1303,LEN(H1303)-4),RIGHT(H1303,LEN(H1303)-6)),\"\"))","v":""}]
[50001921,"SIGENERGY","SigenStor EC 5.0 TP ",5,5.5,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1304,1)=\"J\",LEFT(H1304,2),LEFT(H1304,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1304,1)=\"J\",RIGHT(H1304,LEN(H1304)-4),RIGHT(H1304,LEN(H1304)-6)),\"\"))","v":""}]
[50001931,"SIGENERGY","Sigen Hybrid 6.0 TP",6,6.6,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1305,1)=\"J\",LEFT(H1305,2),LEFT(H1305,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1305,1)=\"J\",RIGHT(H1305,LEN(H1305)-4),RIGHT(H1305,LEN(H1305)-6)),\"\"))","v":""}]
[50001949,"SIGENERGY","Sigen PV Max 6.0 TP",6,6.6,3,"PV-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1306,1)=\"J\",LEFT(H1306,2),LEFT(H1306,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1306,1)=\"J\",RIGHT(H1306,LEN(H1306)-4),RIGHT(H1306,LEN(H1306)-6)),\"\"))","v":""}]
[50001940,"SIGENERGY","SigenStor AC 6.0 TP ",6,6.6,3,"AC-Batteriewechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1307,1)=\"J\",LEFT(H1307,2),LEFT(H1307,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1307,1)=\"J\",RIGHT(H1307,LEN(H1307)-4),RIGHT(H1307,LEN(H1307)-6)),\"\"))","v":""}]
[50001922,"SIGENERGY","SigenStor EC 6.0 TP ",6,6.6,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1308,1)=\"J\",LEFT(H1308,2),LEFT(H1308,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1308,1)=\"J\",RIGHT(H1308,LEN(H1308)-4),RIGHT(H1308,LEN(H1308)-6)),\"\"))","v":""}]
[50001932,"SIGENERGY","Sigen Hybrid 8.0 TP",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1309,1)=\"J\",LEFT(H1309,2),LEFT(H1309,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1309,1)=\"J\",RIGHT(H1309,LEN(H1309)-4),RIGHT(H1309,LEN(H1309)-6)),\"\"))","v":""}]
[50001950,"SIGENERGY","Sigen PV Max 8.0 TP",8,8.8000000000000007,3,"PV-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1310,1)=\"J\",LEFT(H1310,2),LEFT(H1310,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1310,1)=\"J\",RIGHT(H1310,LEN(H1310)-4),RIGHT(H1310,LEN(H1310)-6)),\"\"))","v":""}]
[50001941,"SIGENERGY","SigenStor AC 8.0 TP ",8,8.8000000000000007,3,"AC-Batteriewechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1311,1)=\"J\",LEFT(H1311,2),LEFT(H1311,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1311,1)=\"J\",RIGHT(H1311,LEN(H1311)-4),RIGHT(H1311,LEN(H1311)-6)),\"\"))","v":""}]
[50001923,"SIGENERGY","SigenStor EC 8.0 TP ",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1312,1)=\"J\",LEFT(H1312,2),LEFT(H1312,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1312,1)=\"J\",RIGHT(H1312,LEN(H1312)-4),RIGHT(H1312,LEN(H1312)-6)),\"\"))","v":""}]
[50001933,"SIGENERGY","Sigen Hybrid 10.0 TP",10,11,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1313,1)=\"J\",LEFT(H1313,2),LEFT(H1313,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1313,1)=\"J\",RIGHT(H1313,LEN(H1313)-4),RIGHT(H1313,LEN(H1313)-6)),\"\"))","v":""}]
[50001951,"SIGENERGY","Sigen PV Max 10,0 TP",10,11,3,"PV-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1314,1)=\"J\",LEFT(H1314,2),LEFT(H1314,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1314,1)=\"J\",RIGHT(H1314,LEN(H1314)-4),RIGHT(H1314,LEN(H1314)-6)),\"\"))","v":""}]
[50001942,"SIGENERGY","SigenStor AC 10.0 TP ",10,11,3,"AC-Batteriewechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1315,1)=\"J\",LEFT(H1315,2),LEFT(H1315,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1315,1)=\"J\",RIGHT(H1315,LEN(H1315)-4),RIGHT(H1315,LEN(H1315)-6)),\"\"))","v":""}]
[50001924,"SIGENERGY","SigenStor EC 10.0 TP ",10,11,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1316,1)=\"J\",LEFT(H1316,2),LEFT(H1316,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1316,1)=\"J\",RIGHT(H1316,LEN(H1316)-4),RIGHT(H1316,LEN(H1316)-6)),\"\"))","v":""}]
[50001934,"SIGENERGY","Sigen Hybrid 12.0 TP",12,13.2,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1317,1)=\"J\",LEFT(H1317,2),LEFT(H1317,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1317,1)=\"J\",RIGHT(H1317,LEN(H1317)-4),RIGHT(H1317,LEN(H1317)-6)),\"\"))","v":""}]
[50001952,"SIGENERGY","Sigen PV Max 12.0 TP",12,13.2,3,"PV-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1318,1)=\"J\",LEFT(H1318,2),LEFT(H1318,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1318,1)=\"J\",RIGHT(H1318,LEN(H1318)-4),RIGHT(H1318,LEN(H1318)-6)),\"\"))","v":""}]
[50001943,"SIGENERGY","SigenStor AC 12.0 TP ",12,13.2,3,"AC-Batteriewechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1319,1)=\"J\",LEFT(H1319,2),LEFT(H1319,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1319,1)=\"J\",RIGHT(H1319,LEN(H1319)-4),RIGHT(H1319,LEN(H1319)-6)),\"\"))","v":""}]
[50001925,"SIGENERGY","SigenStor EC 12.0 TP ",12,13.2,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1320,1)=\"J\",LEFT(H1320,2),LEFT(H1320,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1320,1)=\"J\",RIGHT(H1320,LEN(H1320)-4),RIGHT(H1320,LEN(H1320)-6)),\"\"))","v":""}]
[50001935,"SIGENERGY","Sigen Hybrid 15.0 TP",15,16.5,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1321,1)=\"J\",LEFT(H1321,2),LEFT(H1321,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1321,1)=\"J\",RIGHT(H1321,LEN(H1321)-4),RIGHT(H1321,LEN(H1321)-6)),\"\"))","v":""}]
[50001953,"SIGENERGY","Sigen PV Max 15.0 TP",15,16.5,3,"PV-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1322,1)=\"J\",LEFT(H1322,2),LEFT(H1322,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1322,1)=\"J\",RIGHT(H1322,LEN(H1322)-4),RIGHT(H1322,LEN(H1322)-6)),\"\"))","v":""}]
[50001944,"SIGENERGY","SigenStor AC 15.0 TP ",15,16.5,3,"AC-Batteriewechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1323,1)=\"J\",LEFT(H1323,2),LEFT(H1323,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1323,1)=\"J\",RIGHT(H1323,LEN(H1323)-4),RIGHT(H1323,LEN(H1323)-6)),\"\"))","v":""}]
[50001926,"SIGENERGY","SigenStor EC 15.0 TP ",15,16.5,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1324,1)=\"J\",LEFT(H1324,2),LEFT(H1324,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1324,1)=\"J\",RIGHT(H1324,LEN(H1324)-4),RIGHT(H1324,LEN(H1324)-6)),\"\"))","v":""}]
[50001936,"SIGENERGY","Sigen Hybrid 17.0 TP",17,18.7,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1325,1)=\"J\",LEFT(H1325,2),LEFT(H1325,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1325,1)=\"J\",RIGHT(H1325,LEN(H1325)-4),RIGHT(H1325,LEN(H1325)-6)),\"\"))","v":""}]
[50001954,"SIGENERGY","Sigen PV Max 17.0 TP",17,18.7,3,"PV-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1326,1)=\"J\",LEFT(H1326,2),LEFT(H1326,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1326,1)=\"J\",RIGHT(H1326,LEN(H1326)-4),RIGHT(H1326,LEN(H1326)-6)),\"\"))","v":""}]
[50001945,"SIGENERGY","SigenStor AC 17.0 TP ",17,18.7,3,"AC-Batteriewechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1327,1)=\"J\",LEFT(H1327,2),LEFT(H1327,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1327,1)=\"J\",RIGHT(H1327,LEN(H1327)-4),RIGHT(H1327,LEN(H1327)-6)),\"\"))","v":""}]
[50001927,"SIGENERGY","SigenStor EC 17.0 TP ",17,18.7,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1328,1)=\"J\",LEFT(H1328,2),LEFT(H1328,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1328,1)=\"J\",RIGHT(H1328,LEN(H1328)-4),RIGHT(H1328,LEN(H1328)-6)),\"\"))","v":""}]
[50001937,"SIGENERGY","Sigen Hybrid 20.0 TP",20,22,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1329,1)=\"J\",LEFT(H1329,2),LEFT(H1329,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1329,1)=\"J\",RIGHT(H1329,LEN(H1329)-4),RIGHT(H1329,LEN(H1329)-6)),\"\"))","v":""}]
[50001955,"SIGENERGY","Sigen PV Max 20.0 TP",20,22,3,"PV-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1330,1)=\"J\",LEFT(H1330,2),LEFT(H1330,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1330,1)=\"J\",RIGHT(H1330,LEN(H1330)-4),RIGHT(H1330,LEN(H1330)-6)),\"\"))","v":""}]
[50001946,"SIGENERGY","SigenStor AC 20.0 TP ",20,22,3,"AC-Batteriewechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1331,1)=\"J\",LEFT(H1331,2),LEFT(H1331,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1331,1)=\"J\",RIGHT(H1331,LEN(H1331)-4),RIGHT(H1331,LEN(H1331)-6)),\"\"))","v":""}]
[50001928,"SIGENERGY","SigenStor EC 20.0 TP ",20,22,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1332,1)=\"J\",LEFT(H1332,2),LEFT(H1332,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1332,1)=\"J\",RIGHT(H1332,LEN(H1332)-4),RIGHT(H1332,LEN(H1332)-6)),\"\"))","v":""}]
[50001938,"SIGENERGY","Sigen Hybrid 25.0 TP",25,27.5,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1333,1)=\"J\",LEFT(H1333,2),LEFT(H1333,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1333,1)=\"J\",RIGHT(H1333,LEN(H1333)-4),RIGHT(H1333,LEN(H1333)-6)),\"\"))","v":""}]
[50001956,"SIGENERGY","Sigen PV Max 25.0 TP",25,27.5,3,"PV-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1334,1)=\"J\",LEFT(H1334,2),LEFT(H1334,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1334,1)=\"J\",RIGHT(H1334,LEN(H1334)-4),RIGHT(H1334,LEN(H1334)-6)),\"\"))","v":""}]
[50001947,"SIGENERGY","SigenStor AC 25.0 TP ",25,27.5,3,"AC-Batteriewechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1335,1)=\"J\",LEFT(H1335,2),LEFT(H1335,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1335,1)=\"J\",RIGHT(H1335,LEN(H1335)-4),RIGHT(H1335,LEN(H1335)-6)),\"\"))","v":""}]
[50001929,"SIGENERGY","SigenStor EC 25.0 TP ",25,27.5,3,"Hybrid-Wechselrichter","Ja","2023-10-27","Martin Bertsch","2023-10-27",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"230705114GZU-001","2023-10-24","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1336,1)=\"J\",LEFT(H1336,2),LEFT(H1336,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1336,1)=\"J\",RIGHT(H1336,LEN(H1336)-4),RIGHT(H1336,LEN(H1336)-6)),\"\"))","v":""}]
[50002193,"SINENG","SN25PT-X",25,27.5,3,"PV-Wechselrichter","Nein","2024-05-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23O4X1 001","2023-10-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1337,1)=\"J\",LEFT(H1337,2),LEFT(H1337,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1337,1)=\"J\",RIGHT(H1337,LEN(H1337)-4),RIGHT(H1337,LEN(H1337)-6)),\"\"))","v":""}]
[50002194,"SINENG","SN30PT",30,33,3,"PV-Wechselrichter","Nein","2024-05-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23O4X1 001","2023-10-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1338,1)=\"J\",LEFT(H1338,2),LEFT(H1338,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1338,1)=\"J\",RIGHT(H1338,LEN(H1338)-4),RIGHT(H1338,LEN(H1338)-6)),\"\"))","v":""}]
[50002195,"SINENG","SN33PT",33,36.299999999999997,3,"PV-Wechselrichter","Nein","2024-05-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23O4X1 001","2023-10-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1339,1)=\"J\",LEFT(H1339,2),LEFT(H1339,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1339,1)=\"J\",RIGHT(H1339,LEN(H1339)-4),RIGHT(H1339,LEN(H1339)-6)),\"\"))","v":""}]
[50002196,"SINENG","SN36PT",36,39.6,3,"PV-Wechselrichter","Nein","2024-05-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23O4X1 001","2023-10-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1340,1)=\"J\",LEFT(H1340,2),LEFT(H1340,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1340,1)=\"J\",RIGHT(H1340,LEN(H1340)-4),RIGHT(H1340,LEN(H1340)-6)),\"\"))","v":""}]
[50002197,"SINENG","SN40PT",40,44,3,"PV-Wechselrichter","Nein","2024-05-23","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23O4X1 001","2023-10-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1341,1)=\"J\",LEFT(H1341,2),LEFT(H1341,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1341,1)=\"J\",RIGHT(H1341,LEN(H1341)-4),RIGHT(H1341,LEN(H1341)-6)),\"\"))","v":""}]
[50002198,"SINENG","SN50PT",50,55,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-23","Martin Bertsch","2024-05-13","DSP1 SW Ver,243000D03K DSP2 SW Ver,2430000030 DSP3 SW Ver,0000040000 Safety Para Ver,0000400000",null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23EG3X 001","2023-10-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1342,1)=\"J\",LEFT(H1342,2),LEFT(H1342,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1342,1)=\"J\",RIGHT(H1342,LEN(H1342)-4),RIGHT(H1342,LEN(H1342)-6)),\"\"))","v":"mit Einschränkung"}]
[50002199,"SINENG","SN50PT-B",50,55,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-23","Martin Bertsch","2024-05-13","DSP1 SW Ver,243000D03K DSP2 SW Ver,2430000030 DSP3 SW Ver,0000040000 Safety Para Ver,0000400000",null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23EG3X 001","2023-10-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1343,1)=\"J\",LEFT(H1343,2),LEFT(H1343,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1343,1)=\"J\",RIGHT(H1343,LEN(H1343)-4),RIGHT(H1343,LEN(H1343)-6)),\"\"))","v":"mit Einschränkung"}]
[50002200,"SINENG","SN60PT",60,66,3,"PV-Wechselrichter","Ja - mit Einschränkung","2024-05-23","Martin Bertsch","2024-05-13","DSP1 SW Ver,243000D03K DSP2 SW Ver,2430000030 DSP3 SW Ver,0000040000 Safety Para Ver,0000400000",null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23EG3X 001","2023-10-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1344,1)=\"J\",LEFT(H1344,2),LEFT(H1344,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1344,1)=\"J\",RIGHT(H1344,LEN(H1344)-4),RIGHT(H1344,LEN(H1344)-6)),\"\"))","v":"mit Einschränkung"}]
[50001066,"Sinexcel","PWS2-29M-EX",29.9,29.9,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-08-05",null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"CN21GNUV 001","2021-02-02",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt -NETZUMSCHALTBOX- KONFORM TOR ERZ A+R25","F","F","Prüfbericht von Kostal Piko IQ 5.5",null,{"$f":"IF(LEFT(H1345,1)=\"J\",LEFT(H1345,2),LEFT(H1345,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1345,1)=\"J\",RIGHT(H1345,LEN(H1345)-4),RIGHT(H1345,LEN(H1345)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50002070,"Sinexcel","PWS2-29P-EX",29.9,29.9,3,"Hybrid-Wechselrichter","Ja","2024-01-19","Martin Bertsch","2024-01-19",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"64.290.21.30882.01","2022-07-04",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1346,1)=\"J\",LEFT(H1346,2),LEFT(H1346,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1346,1)=\"J\",RIGHT(H1346,LEN(H1346)-4),RIGHT(H1346,LEN(H1346)-6)),\"\"))","v":""}]
[50001067,"Sinexcel","PWS2-30M-EX",30,33,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-08-05",null,null,null,null,"Ja","Ja",null,"Vorhanden",null,"CN21GNUV 002","2021-02-03",null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt -NETZUMSCHALTBOX- KONFORM TOR ERZ A+R25","F","F","Prüfbericht von Kostal Piko IQ 10.0",null,{"$f":"IF(LEFT(H1347,1)=\"J\",LEFT(H1347,2),LEFT(H1347,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1347,1)=\"J\",RIGHT(H1347,LEN(H1347)-4),RIGHT(H1347,LEN(H1347)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50002071,"Sinexcel","PWS2-30P-EX",30,33,3,"Hybrid-Wechselrichter","Ja","2024-01-19","Martin Bertsch","2024-01-19",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"64.290.21.30882.01","2022-07-04",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1348,1)=\"J\",LEFT(H1348,2),LEFT(H1348,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1348,1)=\"J\",RIGHT(H1348,LEN(H1348)-4),RIGHT(H1348,LEN(H1348)-6)),\"\"))","v":""}]
[50001068,"Sinexcel","PWG2-50K-EX",50,50,3,"Hybrid-Wechselrichter","Nein","2022-06-10",null,null,null,null,null,null,null,null,null,"Vorhanden",null,"64.290.20.30509.01","2020-10-16",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1349,1)=\"J\",LEFT(H1349,2),LEFT(H1349,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1349,1)=\"J\",RIGHT(H1349,LEN(H1349)-4),RIGHT(H1349,LEN(H1349)-6)),\"\"))","v":""}]
[50001069,"Sinexcel","PWS1-50K-EX",null,50,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1350,1)=\"J\",LEFT(H1350,2),LEFT(H1350,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1350,1)=\"J\",RIGHT(H1350,LEN(H1350)-4),RIGHT(H1350,LEN(H1350)-6)),\"\"))","v":""}]
[50001070,"Sinexcel","PWG2-100K-EX",100,100,3,"Hybrid-Wechselrichter","Nein","2022-06-10",null,null,null,null,null,null,null,null,null,"Vorhanden",null,"64.290.20.30509.01","2020-10-16",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1351,1)=\"J\",LEFT(H1351,2),LEFT(H1351,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1351,1)=\"J\",RIGHT(H1351,LEN(H1351)-4),RIGHT(H1351,LEN(H1351)-6)),\"\"))","v":""}]
[50001071,"Sinexcel","PWS1-100K-EX",null,100,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1352,1)=\"J\",LEFT(H1352,2),LEFT(H1352,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1352,1)=\"J\",RIGHT(H1352,LEN(H1352)-4),RIGHT(H1352,LEN(H1352)-6)),\"\"))","v":""}]
[50001072,"Sinexcel","PWS1-150K-EX",null,150,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1353,1)=\"J\",LEFT(H1353,2),LEFT(H1353,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1353,1)=\"J\",RIGHT(H1353,LEN(H1353)-4),RIGHT(H1353,LEN(H1353)-6)),\"\"))","v":""}]
[50001073,"Sinexcel","PWS1-250K-EX",null,250,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1354,1)=\"J\",LEFT(H1354,2),LEFT(H1354,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1354,1)=\"J\",RIGHT(H1354,LEN(H1354)-4),RIGHT(H1354,LEN(H1354)-6)),\"\"))","v":""}]
[50001074,"Sinexcel","PWS1-500KTL-EX",500,500,3,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1355,1)=\"J\",LEFT(H1355,2),LEFT(H1355,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1355,1)=\"J\",RIGHT(H1355,LEN(H1355)-4),RIGHT(H1355,LEN(H1355)-6)),\"\"))","v":""}]
[50001075,"SMA","Sunny Boy 1.5-1VL-40",1.5,1.5,1,"PV-Wechselrichter","Ja",null,null,null,null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","14TH0397","2021-01-27",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1356,1)=\"J\",LEFT(H1356,2),LEFT(H1356,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1356,1)=\"J\",RIGHT(H1356,LEN(H1356)-4),RIGHT(H1356,LEN(H1356)-6)),\"\"))","v":""}]
[50001076,"SMA","Sunny Boy 2.0-1VL-40",2,2,1,"PV-Wechselrichter","Ja",null,null,null,null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","14TH0397","2021-01-27",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1357,1)=\"J\",LEFT(H1357,2),LEFT(H1357,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1357,1)=\"J\",RIGHT(H1357,LEN(H1357)-4),RIGHT(H1357,LEN(H1357)-6)),\"\"))","v":""}]
[50001077,"SMA","Sunny Boy 2.5-1VL-40",2.5,2.5,1,"PV-Wechselrichter","Ja",null,null,null,null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","14TH0397","2021-01-27",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1358,1)=\"J\",LEFT(H1358,2),LEFT(H1358,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1358,1)=\"J\",RIGHT(H1358,LEN(H1358)-4),RIGHT(H1358,LEN(H1358)-6)),\"\"))","v":""}]
[50001078,"SMA","Sunny Boy STORAGE 2.5",2.5,2.5,1,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1359,1)=\"J\",LEFT(H1359,2),LEFT(H1359,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1359,1)=\"J\",RIGHT(H1359,LEN(H1359)-4),RIGHT(H1359,LEN(H1359)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001079,"SMA","Sunny Boy 3.0-1AV-41 ",3,3,1,"PV-Wechselrichter","Ja",null,null,"2021-01-27",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","16TH0348","2021-01-27",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1360,1)=\"J\",LEFT(H1360,2),LEFT(H1360,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1360,1)=\"J\",RIGHT(H1360,LEN(H1360)-4),RIGHT(H1360,LEN(H1360)-6)),\"\"))","v":""}]
[50001080,"SMA","Sunny Tripower 3.0-3AV-40 ",3,3,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","18TH0325","2020-12-04",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1361,1)=\"J\",LEFT(H1361,2),LEFT(H1361,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1361,1)=\"J\",RIGHT(H1361,LEN(H1361)-4),RIGHT(H1361,LEN(H1361)-6)),\"\"))","v":""}]
[50001081,"SMA","Sunny Island 4.4M-13",3.3,3.3,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,"2021-03-01","Nicht mehr am Markt","Ja","Ja",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - nur 3~ zul. mit Einstellung Österreich bis Summe Sn 11,04 kVA - KONFORM TOR ERZ A+R25","T","F",null,null,{"$f":"IF(LEFT(H1362,1)=\"J\",LEFT(H1362,2),LEFT(H1362,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1362,1)=\"J\",RIGHT(H1362,LEN(H1362)-4),RIGHT(H1362,LEN(H1362)-6)),\"\"))","v":""}]
[50001082,"SMA","Sunny Boy 3.6-1AV-41 ",3.68,3.68,1,"PV-Wechselrichter","Ja",null,null,"2021-01-27",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","16TH0348","2021-01-27",null,"OK",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1363,1)=\"J\",LEFT(H1363,2),LEFT(H1363,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1363,1)=\"J\",RIGHT(H1363,LEN(H1363)-4),RIGHT(H1363,LEN(H1363)-6)),\"\"))","v":""}]
[50001083,"SMA","Sunny Boy STORAGE 3.7-10",3.68,3.68,1,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-05-06",null,null,null,null,"Ja","Nein",null,"OK","Christian Elbs","17TH0338","2021-01-28",null,"OK",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - nur 3~ zul. mit Einstellung Österreich bis Summe Sn 11,04 kVA - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1364,1)=\"J\",LEFT(H1364,2),LEFT(H1364,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1364,1)=\"J\",RIGHT(H1364,LEN(H1364)-4),RIGHT(H1364,LEN(H1364)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001084,"SMA","Sunny Boy 4.0 ",4,4,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1365,1)=\"J\",LEFT(H1365,2),LEFT(H1365,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1365,1)=\"J\",RIGHT(H1365,LEN(H1365)-4),RIGHT(H1365,LEN(H1365)-6)),\"\"))","v":""}]
[50001085,"SMA","Sunny Tripower 4.0-3AV-40 ",4,4,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","18TH0325","2020-12-04",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1366,1)=\"J\",LEFT(H1366,2),LEFT(H1366,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1366,1)=\"J\",RIGHT(H1366,LEN(H1366)-4),RIGHT(H1366,LEN(H1366)-6)),\"\"))","v":""}]
[50001086,"SMA","Sunny Island 6.0H",4.5999999999999996,4.5999999999999996,1,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2022-08-16","Christian Elbs","2021-05-06",null,null,null,null,"Ja","Ja",null,"OK","Christian Elbs","13TH0287","2021-03-17",null,"OK",null,null,null,null,"Betrieb auch mit Multicluster-Box möglich, integriertes Bender Relais auf 40ms einstellen --> USV-ähnlich","F","F",null,null,{"$f":"IF(LEFT(H1367,1)=\"J\",LEFT(H1367,2),LEFT(H1367,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1367,1)=\"J\",RIGHT(H1367,LEN(H1367)-4),RIGHT(H1367,LEN(H1367)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001087,"SMA","Sunny Boy 5.0 ",5,5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1368,1)=\"J\",LEFT(H1368,2),LEFT(H1368,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1368,1)=\"J\",RIGHT(H1368,LEN(H1368)-4),RIGHT(H1368,LEN(H1368)-6)),\"\"))","v":""}]
[50001088,"SMA","Sunny Boy STORAGE 5.0-10",5,5,1,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2022-06-07","Christian Elbs",null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"OK","Christian Elbs","17TH0338","2021-01-28",null,"OK",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1369,1)=\"J\",LEFT(H1369,2),LEFT(H1369,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1369,1)=\"J\",RIGHT(H1369,LEN(H1369)-4),RIGHT(H1369,LEN(H1369)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001089,"SMA","Sunny Tripower 5.0-3AV-40 ",5,5,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","18TH0325","2020-12-04",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1370,1)=\"J\",LEFT(H1370,2),LEFT(H1370,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1370,1)=\"J\",RIGHT(H1370,LEN(H1370)-4),RIGHT(H1370,LEN(H1370)-6)),\"\"))","v":""}]
[50001090,"SMA","Sunny Tripower 5.0-3SE-40",5,5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung, befristet","2024-05-26","Martin Bertsch","2023-02-24","3.4.16.R.","2024-09-30",null,null,"Ja","Nein","Ja","nicht OK","Ferdinand Flach","CN2162FH 002","2022-06-01",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1371,1)=\"J\",LEFT(H1371,2),LEFT(H1371,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1371,1)=\"J\",RIGHT(H1371,LEN(H1371)-4),RIGHT(H1371,LEN(H1371)-6)),\"\"))","v":"mit Einschränkung, befristet"}]
[50001091,"SMA","Sunny Boy 6.0",6,6,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1372,1)=\"J\",LEFT(H1372,2),LEFT(H1372,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1372,1)=\"J\",RIGHT(H1372,LEN(H1372)-4),RIGHT(H1372,LEN(H1372)-6)),\"\"))","v":""}]
[50001092,"SMA","Sunny Boy STORAGE 6.0-10",6,6,1,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2022-06-07","Christian Elbs",null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"OK","Christian Elbs","17TH0338","2021-01-28",null,"OK",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1373,1)=\"J\",LEFT(H1373,2),LEFT(H1373,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1373,1)=\"J\",RIGHT(H1373,LEN(H1373)-4),RIGHT(H1373,LEN(H1373)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001093,"SMA","Sunny Island 8.0H",6,6,1,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2022-08-16","Christian Elbs","2021-05-06",null,null,null,null,"Ja","Ja",null,"OK","Christian Elbs","13TH0287","2021-03-17",null,"OK",null,null,null,null,"Betrieb auch mit Multicluster-Box möglich, integriertes Bender Relais auf 40ms einstellen --> USV-ähnlich","F","F",null,null,{"$f":"IF(LEFT(H1374,1)=\"J\",LEFT(H1374,2),LEFT(H1374,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1374,1)=\"J\",RIGHT(H1374,LEN(H1374)-4),RIGHT(H1374,LEN(H1374)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001094,"SMA","Sunny Tripower 6.0-3AV-40 ",6,6,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","18TH0325","2020-12-04",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1375,1)=\"J\",LEFT(H1375,2),LEFT(H1375,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1375,1)=\"J\",RIGHT(H1375,LEN(H1375)-4),RIGHT(H1375,LEN(H1375)-6)),\"\"))","v":""}]
[50001095,"SMA","Sunny Tripower 6.0-3SE-40",6,6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung, befristet","2024-05-26","Martin Bertsch","2023-02-24","3.4.16.R.","2024-09-30",null,null,"Ja","Nein","Ja","nicht OK","Ferdinand Flach","CN2162FH 002","2022-06-01",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1376,1)=\"J\",LEFT(H1376,2),LEFT(H1376,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1376,1)=\"J\",RIGHT(H1376,LEN(H1376)-4),RIGHT(H1376,LEN(H1376)-6)),\"\"))","v":"mit Einschränkung, befristet"}]
[50001096,"SMA","Sunny Tripower 8.0-3AV-40 ",8,8,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","18TH0325","2020-12-04",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1377,1)=\"J\",LEFT(H1377,2),LEFT(H1377,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1377,1)=\"J\",RIGHT(H1377,LEN(H1377)-4),RIGHT(H1377,LEN(H1377)-6)),\"\"))","v":""}]
[50001097,"SMA","Sunny Tripower 8.0-3SE-40",8,8,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung, befristet","2024-05-26","Martin Bertsch","2023-02-24","3.4.16.R.","2024-09-30",null,null,"Ja","Nein","Ja","nicht OK","Ferdinand Flach","CN2162FH 002","2022-06-01",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1378,1)=\"J\",LEFT(H1378,2),LEFT(H1378,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1378,1)=\"J\",RIGHT(H1378,LEN(H1378)-4),RIGHT(H1378,LEN(H1378)-6)),\"\"))","v":"mit Einschränkung, befristet"}]
[50001098,"SMA","Sunny Tripower 10.0-3AV-40 ",10,10,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","18TH0325","2020-12-04",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1379,1)=\"J\",LEFT(H1379,2),LEFT(H1379,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1379,1)=\"J\",RIGHT(H1379,LEN(H1379)-4),RIGHT(H1379,LEN(H1379)-6)),\"\"))","v":""}]
[50001099,"SMA","Sunny Tripower 10.0-3SE-40",10,10,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung, befristet","2024-05-26","Martin Bertsch","2023-02-24","3.4.16.R.","2024-09-30",null,null,"Ja","Nein","Ja","nicht OK","Ferdinand Flach","CN2162FH 002","2022-06-01",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1380,1)=\"J\",LEFT(H1380,2),LEFT(H1380,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1380,1)=\"J\",RIGHT(H1380,LEN(H1380)-4),RIGHT(H1380,LEN(H1380)-6)),\"\"))","v":"mit Einschränkung, befristet"}]
[50001100,"SMA","Sunny Tripower 12-50",12,12,3,"PV-Wechselrichter","Ja","2023-05-08","Martin Bertsch","2022-11-16",null,null,null,null,null,null,null,"OK","Ferdinand Flach","713254379-007","2023-03-02","Vorhanden","OK",null,"Vorhanden","2022-12-15",null,null,null,null,null,null,{"$f":"IF(LEFT(H1381,1)=\"J\",LEFT(H1381,2),LEFT(H1381,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1381,1)=\"J\",RIGHT(H1381,LEN(H1381)-4),RIGHT(H1381,LEN(H1381)-6)),\"\"))","v":""}]
[50001101,"SMA","Sunny Tripower 15000TL-30 ",15,15,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","14TH0304","2020-11-12",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1382,1)=\"J\",LEFT(H1382,2),LEFT(H1382,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1382,1)=\"J\",RIGHT(H1382,LEN(H1382)-4),RIGHT(H1382,LEN(H1382)-6)),\"\"))","v":""}]
[50001102,"SMA","Sunny Tripower 15-50",15,15,3,"PV-Wechselrichter","Ja","2023-05-08","Martin Bertsch","2022-11-16",null,null,null,null,null,null,null,"OK","Ferdinand Flach","713254379-007","2023-03-02","Vorhanden","OK",null,"Vorhanden","2022-12-15",null,null,null,null,null,null,{"$f":"IF(LEFT(H1383,1)=\"J\",LEFT(H1383,2),LEFT(H1383,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1383,1)=\"J\",RIGHT(H1383,LEN(H1383)-4),RIGHT(H1383,LEN(H1383)-6)),\"\"))","v":""}]
[50001103,"SMA","Sunny Tripower 17000TL-30 ",15,15,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","14TH0304","2020-11-12",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1384,1)=\"J\",LEFT(H1384,2),LEFT(H1384,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1384,1)=\"J\",RIGHT(H1384,LEN(H1384)-4),RIGHT(H1384,LEN(H1384)-6)),\"\"))","v":""}]
[50001104,"SMA","Sunny Tripower 20000TL-30 ",20,20,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","14TH0304","2020-11-12",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1385,1)=\"J\",LEFT(H1385,2),LEFT(H1385,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1385,1)=\"J\",RIGHT(H1385,LEN(H1385)-4),RIGHT(H1385,LEN(H1385)-6)),\"\"))","v":""}]
[50001105,"SMA","Sunny Tripower 20-50",20,20,3,"PV-Wechselrichter","Ja","2023-05-08","Martin Bertsch","2022-11-16",null,null,null,null,null,null,null,"OK","Ferdinand Flach","713254379-007","2023-03-02","Vorhanden","OK",null,"Vorhanden","2022-12-15",null,null,null,null,null,null,{"$f":"IF(LEFT(H1386,1)=\"J\",LEFT(H1386,2),LEFT(H1386,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1386,1)=\"J\",RIGHT(H1386,LEN(H1386)-4),RIGHT(H1386,LEN(H1386)-6)),\"\"))","v":""}]
[50001106,"SMA","Sunny Tripower 25000TL-30 ",25,25,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Christian Elbs","14TH0304","2020-11-12","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1387,1)=\"J\",LEFT(H1387,2),LEFT(H1387,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1387,1)=\"J\",RIGHT(H1387,LEN(H1387)-4),RIGHT(H1387,LEN(H1387)-6)),\"\"))","v":""}]
[50001107,"SMA","Sunny Tripower 25-50",25,25,3,"PV-Wechselrichter","Ja","2023-05-08","Martin Bertsch","2022-11-16",null,null,null,null,null,null,null,"OK","Ferdinand Flach","713254379-007","2023-03-02","Vorhanden","OK",null,"Vorhanden","2022-12-15",null,null,null,null,null,null,{"$f":"IF(LEFT(H1388,1)=\"J\",LEFT(H1388,2),LEFT(H1388,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1388,1)=\"J\",RIGHT(H1388,LEN(H1388)-4),RIGHT(H1388,LEN(H1388)-6)),\"\"))","v":""}]
[50001108,"SMA","SI30-20",30,30,3,"AC-Batteriewechselrichter","Ja","2023-10-06","Martin Bertsch","2023-06-19",null,null,null,null,null,null,null,"OK","Martin Bertsch (OE)","22TH0488-OVE-directive R25_0","2023-05-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1389,1)=\"J\",LEFT(H1389,2),LEFT(H1389,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1389,1)=\"J\",RIGHT(H1389,LEN(H1389)-4),RIGHT(H1389,LEN(H1389)-6)),\"\"))","v":""}]
[50001109,"SMA","STPS30-20",30,30,3,"AC-Batteriewechselrichter","Ja","2023-10-06","Martin Bertsch","2023-06-19",null,null,null,null,null,null,null,"OK","Martin Bertsch (OE)","22TH0488-OVE-directive R25_0","2023-05-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1390,1)=\"J\",LEFT(H1390,2),LEFT(H1390,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1390,1)=\"J\",RIGHT(H1390,LEN(H1390)-4),RIGHT(H1390,LEN(H1390)-6)),\"\"))","v":""}]
[50001110,"SMA","SI50-20",50,50,3,"AC-Batteriewechselrichter","Ja","2023-10-06","Martin Bertsch","2023-06-19",null,null,null,null,null,null,null,"OK","Martin Bertsch (OE)","22TH0488-OVE-directive R25_0","2023-05-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1391,1)=\"J\",LEFT(H1391,2),LEFT(H1391,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1391,1)=\"J\",RIGHT(H1391,LEN(H1391)-4),RIGHT(H1391,LEN(H1391)-6)),\"\"))","v":""}]
[50001111,"SMA","STPS50-20",50,50,3,"AC-Batteriewechselrichter","Ja","2023-10-06","Martin Bertsch","2023-06-19",null,null,null,null,null,null,null,"OK","Martin Bertsch (OE)","22TH0488-OVE-directive R25_0","2023-05-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1392,1)=\"J\",LEFT(H1392,2),LEFT(H1392,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1392,1)=\"J\",RIGHT(H1392,LEN(H1392)-4),RIGHT(H1392,LEN(H1392)-6)),\"\"))","v":""}]
[50001112,"SMA","Sunny Tripower 50-40 ",50,50,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"17TH0199-OVE-directive R25_1","2021-03-05",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1393,1)=\"J\",LEFT(H1393,2),LEFT(H1393,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1393,1)=\"J\",RIGHT(H1393,LEN(H1393)-4),RIGHT(H1393,LEN(H1393)-6)),\"\"))","v":""}]
[50001113,"SMA","Sunny Tripower 50-41",50,50,3,"PV-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,"17TH0199-OVE-directive R25_1","2021-03-05",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1394,1)=\"J\",LEFT(H1394,2),LEFT(H1394,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1394,1)=\"J\",RIGHT(H1394,LEN(H1394)-4),RIGHT(H1394,LEN(H1394)-6)),\"\"))","v":""}]
[50001114,"SMA","Sunny Tripower Storage 60",75,75,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-06-15","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein",null,"nicht OK","Roland Bründlinger","14TH0075","2021-09-09",null,"OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - NICHT EINSPEISERELEVANT - KONFORM TOR ERZ A",null,null,null,null,{"$f":"IF(LEFT(H1395,1)=\"J\",LEFT(H1395,2),LEFT(H1395,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1395,1)=\"J\",RIGHT(H1395,LEN(H1395)-4),RIGHT(H1395,LEN(H1395)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001115,"SMA","Sunny Highpower PEAK3 100-20",100,100,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1396,1)=\"J\",LEFT(H1396,2),LEFT(H1396,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1396,1)=\"J\",RIGHT(H1396,LEN(H1396)-4),RIGHT(H1396,LEN(H1396)-6)),\"\"))","v":""}]
[50001116,"SMA","Sunny Highpower PEAK3 100-21",100,100,3,"PV-Wechselrichter","Nein - Typ B","2022-12-15","Christian Elbs",null,null,null,null,"Kein Prüfbericht nach OVE R25 daher nicht für Typ A, für Typ B,C,D OK","Nein","Nein","Nein","nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1397,1)=\"J\",LEFT(H1397,2),LEFT(H1397,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1397,1)=\"J\",RIGHT(H1397,LEN(H1397)-4),RIGHT(H1397,LEN(H1397)-6)),\"\"))","v":"Typ B"}]
[50001117,"SMA","Sunny Tripower CORE2 110-60 ",110,110,3,"PV-Wechselrichter","Ja","2023-05-17","Martin Bertsch","2022-11-30","1.01.02.R",null,null,null,"Nein","Nein","Nein","OK","Christian Elbs","CN20FNS4 001","2020-12-16","Vorhanden","OK","Vorhanden",null,null,"Ja, keine N-Überwachung durch ENS","Stringwechselrichter 3~ - KONFORM TOR ERZ A+B+R25","F","F",null,null,{"$f":"IF(LEFT(H1398,1)=\"J\",LEFT(H1398,2),LEFT(H1398,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1398,1)=\"J\",RIGHT(H1398,LEN(H1398)-4),RIGHT(H1398,LEN(H1398)-6)),\"\"))","v":""}]
[50001118,"SMA","Sunny Highpower PEAK3 150-20",150,150,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1399,1)=\"J\",LEFT(H1399,2),LEFT(H1399,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1399,1)=\"J\",RIGHT(H1399,LEN(H1399)-4),RIGHT(H1399,LEN(H1399)-6)),\"\"))","v":""}]
[50001119,"SMA","Sunny Highpower PEAK3 150-21",150,150,3,"PV-Wechselrichter","Nein - Typ B","2022-12-15","Christian Elbs",null,null,null,null,"Kein Prüfbericht nach OVE R25 daher nicht für Typ A, für Typ B,C,D OK","Nein","Nein","Nein","nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1400,1)=\"J\",LEFT(H1400,2),LEFT(H1400,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1400,1)=\"J\",RIGHT(H1400,LEN(H1400)-4),RIGHT(H1400,LEN(H1400)-6)),\"\"))","v":"Typ B"}]
[50001120,"SMA","Sunny Highpower PEAK3 172-21",172,172,3,"PV-Wechselrichter","Nein - Typ B","2022-12-15","Christian Elbs",null,null,null,null,"Kein Prüfbericht nach OVE R25 daher nicht für Typ A, für Typ B,C,D OK","Nein","Nein","Nein","nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1401,1)=\"J\",LEFT(H1401,2),LEFT(H1401,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1401,1)=\"J\",RIGHT(H1401,LEN(H1401)-4),RIGHT(H1401,LEN(H1401)-6)),\"\"))","v":"Typ B"}]
[50001121,"SMA","Sunny Highpower PEAK3 180-21",180,180,3,"PV-Wechselrichter","Nein - Typ B","2022-12-15","Christian Elbs",null,null,null,null,"Kein Prüfbericht nach OVE R25 daher nicht für Typ A, für Typ B,C,D OK","Nein","Nein","Nein","nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1402,1)=\"J\",LEFT(H1402,2),LEFT(H1402,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1402,1)=\"J\",RIGHT(H1402,LEN(H1402)-4),RIGHT(H1402,LEN(H1402)-6)),\"\"))","v":"Typ B"}]
[50001122,"SOFAR","SOFAR 3.3KTLX-G3",3,3.3,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1403,1)=\"J\",LEFT(H1403,2),LEFT(H1403,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1403,1)=\"J\",RIGHT(H1403,LEN(H1403)-4),RIGHT(H1403,LEN(H1403)-6)),\"\"))","v":"befristet"}]
[50001123,"SOFAR","SOFAR 3KTLM-G3",3,3.3,1,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-08-29",null,"2024-09-30",null,null,null,null,null,"OK","Martin Bertsch (OE)","210120056GZU-001","2023-01-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1404,1)=\"J\",LEFT(H1404,2),LEFT(H1404,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1404,1)=\"J\",RIGHT(H1404,LEN(H1404)-4),RIGHT(H1404,LEN(H1404)-6)),\"\"))","v":"befristet"}]
[50001124,"SOFAR","SOFAR 3.6KTLM-G3",3.68,3.68,1,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-08-29",null,"2024-09-30",null,null,null,null,null,"OK","Martin Bertsch (OE)","210120056GZU-001","2023-01-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1405,1)=\"J\",LEFT(H1405,2),LEFT(H1405,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1405,1)=\"J\",RIGHT(H1405,LEN(H1405)-4),RIGHT(H1405,LEN(H1405)-6)),\"\"))","v":"befristet"}]
[50001125,"SOFAR","SOFAR 4.4KTLX-G3",4,4.4000000000000004,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1406,1)=\"J\",LEFT(H1406,2),LEFT(H1406,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1406,1)=\"J\",RIGHT(H1406,LEN(H1406)-4),RIGHT(H1406,LEN(H1406)-6)),\"\"))","v":"befristet"}]
[50001126,"SOFAR","SOFAR 5KTLX-G3-A",5,5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1407,1)=\"J\",LEFT(H1407,2),LEFT(H1407,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1407,1)=\"J\",RIGHT(H1407,LEN(H1407)-4),RIGHT(H1407,LEN(H1407)-6)),\"\"))","v":"befristet"}]
[50001127,"SOFAR","HYD 5KTL-3PH",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-03","Martin Bertsch","2022-06-30","Firmware Version: V112351_51_51",null,null,null,null,null,null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1408,1)=\"J\",LEFT(H1408,2),LEFT(H1408,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1408,1)=\"J\",RIGHT(H1408,LEN(H1408)-4),RIGHT(H1408,LEN(H1408)-6)),\"\"))","v":"mit Einschränkung"}]
[50001128,"SOFAR","ME 5KTL-3PH",5,5.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-11-21",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","PVAT102WDG0105","2021-03-31",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1409,1)=\"J\",LEFT(H1409,2),LEFT(H1409,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1409,1)=\"J\",RIGHT(H1409,LEN(H1409)-4),RIGHT(H1409,LEN(H1409)-6)),\"\"))","v":"befristet"}]
[50001129,"SOFAR","SOFAR 5.5KTLX-G3",5,5.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1410,1)=\"J\",LEFT(H1410,2),LEFT(H1410,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1410,1)=\"J\",RIGHT(H1410,LEN(H1410)-4),RIGHT(H1410,LEN(H1410)-6)),\"\"))","v":"befristet"}]
[50001130,"SOFAR","HYD 6KTL-3PH",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-03","Martin Bertsch","2022-06-30","Firmware Version: V112351_51_51",null,null,null,null,null,null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R26","F","F",null,null,{"$f":"IF(LEFT(H1411,1)=\"J\",LEFT(H1411,2),LEFT(H1411,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1411,1)=\"J\",RIGHT(H1411,LEN(H1411)-4),RIGHT(H1411,LEN(H1411)-6)),\"\"))","v":"mit Einschränkung"}]
[50001131,"SOFAR","ME 6KTL-3PH",6,6.6,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-11-21",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","PVAT102WDG0105","2021-03-31",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1412,1)=\"J\",LEFT(H1412,2),LEFT(H1412,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1412,1)=\"J\",RIGHT(H1412,LEN(H1412)-4),RIGHT(H1412,LEN(H1412)-6)),\"\"))","v":"befristet"}]
[50001132,"SOFAR","SOFAR 6.6KTLX-G3",6,6.6,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1413,1)=\"J\",LEFT(H1413,2),LEFT(H1413,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1413,1)=\"J\",RIGHT(H1413,LEN(H1413)-4),RIGHT(H1413,LEN(H1413)-6)),\"\"))","v":"befristet"}]
[50001133,"SOFAR","HYD 8KTL-3PH",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-03","Martin Bertsch","2022-06-30","Firmware Version: V112351_51_51",null,null,null,null,null,null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R27","F","F",null,null,{"$f":"IF(LEFT(H1414,1)=\"J\",LEFT(H1414,2),LEFT(H1414,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1414,1)=\"J\",RIGHT(H1414,LEN(H1414)-4),RIGHT(H1414,LEN(H1414)-6)),\"\"))","v":"mit Einschränkung"}]
[50001134,"SOFAR","ME 8KTL-3PH",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-11-21",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","PVAT102WDG0105","2021-03-31",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1415,1)=\"J\",LEFT(H1415,2),LEFT(H1415,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1415,1)=\"J\",RIGHT(H1415,LEN(H1415)-4),RIGHT(H1415,LEN(H1415)-6)),\"\"))","v":"befristet"}]
[50001135,"SOFAR","SOFAR 8.8KTLX-G3",8,8.8000000000000007,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1416,1)=\"J\",LEFT(H1416,2),LEFT(H1416,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1416,1)=\"J\",RIGHT(H1416,LEN(H1416)-4),RIGHT(H1416,LEN(H1416)-6)),\"\"))","v":"befristet"}]
[50001136,"SOFAR","SOFAR 8.8KTLX-G3-A",8,8.8000000000000007,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1417,1)=\"J\",LEFT(H1417,2),LEFT(H1417,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1417,1)=\"J\",RIGHT(H1417,LEN(H1417)-4),RIGHT(H1417,LEN(H1417)-6)),\"\"))","v":"befristet"}]
[50001137,"SOFAR","SOFAR 10KTLX-G3-A",10,10,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1418,1)=\"J\",LEFT(H1418,2),LEFT(H1418,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1418,1)=\"J\",RIGHT(H1418,LEN(H1418)-4),RIGHT(H1418,LEN(H1418)-6)),\"\"))","v":"befristet"}]
[50001138,"SOFAR","HYD 10KTL-3PH",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-03","Martin Bertsch","2022-06-30","Firmware Version: V112351_51_51",null,null,null,null,null,null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R28","F","F",null,null,{"$f":"IF(LEFT(H1419,1)=\"J\",LEFT(H1419,2),LEFT(H1419,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1419,1)=\"J\",RIGHT(H1419,LEN(H1419)-4),RIGHT(H1419,LEN(H1419)-6)),\"\"))","v":"mit Einschränkung"}]
[50001139,"SOFAR","ME 10KTL-3PH",10,11,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-11-21",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","PVAT102WDG0105","2021-03-31",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1420,1)=\"J\",LEFT(H1420,2),LEFT(H1420,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1420,1)=\"J\",RIGHT(H1420,LEN(H1420)-4),RIGHT(H1420,LEN(H1420)-6)),\"\"))","v":"befristet"}]
[50001140,"SOFAR","SOFAR 11KTLX-G3",10,11,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1421,1)=\"J\",LEFT(H1421,2),LEFT(H1421,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1421,1)=\"J\",RIGHT(H1421,LEN(H1421)-4),RIGHT(H1421,LEN(H1421)-6)),\"\"))","v":"befristet"}]
[50001141,"SOFAR","SOFAR 11KTLX-G3-A",10,11,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1422,1)=\"J\",LEFT(H1422,2),LEFT(H1422,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1422,1)=\"J\",RIGHT(H1422,LEN(H1422)-4),RIGHT(H1422,LEN(H1422)-6)),\"\"))","v":"befristet"}]
[50001142,"SOFAR","SOFAR 12KTLX-G3",12,13.2,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-001","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1423,1)=\"J\",LEFT(H1423,2),LEFT(H1423,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1423,1)=\"J\",RIGHT(H1423,LEN(H1423)-4),RIGHT(H1423,LEN(H1423)-6)),\"\"))","v":"befristet"}]
[50001143,"SOFAR","HYD 15KTL-3PH",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-03","Martin Bertsch","2022-06-30","Firmware Version: V112351_51_51",null,null,null,null,null,null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R29","F","F",null,null,{"$f":"IF(LEFT(H1424,1)=\"J\",LEFT(H1424,2),LEFT(H1424,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1424,1)=\"J\",RIGHT(H1424,LEN(H1424)-4),RIGHT(H1424,LEN(H1424)-6)),\"\"))","v":"mit Einschränkung"}]
[50001144,"SOFAR","ME 15KTL-3PH",15,16.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-11-21",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","PVAT102WDG0105","2021-03-31",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1425,1)=\"J\",LEFT(H1425,2),LEFT(H1425,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1425,1)=\"J\",RIGHT(H1425,LEN(H1425)-4),RIGHT(H1425,LEN(H1425)-6)),\"\"))","v":"befristet"}]
[50001145,"SOFAR","SOFAR 15KTLX-G3",15,16.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-10-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1426,1)=\"J\",LEFT(H1426,2),LEFT(H1426,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1426,1)=\"J\",RIGHT(H1426,LEN(H1426)-4),RIGHT(H1426,LEN(H1426)-6)),\"\"))","v":"befristet"}]
[50001146,"SOFAR","SOFAR 17KTLX-G3",17,18.7,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-10-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1427,1)=\"J\",LEFT(H1427,2),LEFT(H1427,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1427,1)=\"J\",RIGHT(H1427,LEN(H1427)-4),RIGHT(H1427,LEN(H1427)-6)),\"\"))","v":"befristet"}]
[50001147,"SOFAR","HYD 20KTL-3PH",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-03","Martin Bertsch","2022-06-30","Firmware Version: V112351_51_51",null,null,null,null,null,null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R30","F","F",null,null,{"$f":"IF(LEFT(H1428,1)=\"J\",LEFT(H1428,2),LEFT(H1428,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1428,1)=\"J\",RIGHT(H1428,LEN(H1428)-4),RIGHT(H1428,LEN(H1428)-6)),\"\"))","v":"mit Einschränkung"}]
[50001148,"SOFAR","ME 20KTL-3PH",20,22,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-11-21",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","PVAT102WDG0105","2021-03-31",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1429,1)=\"J\",LEFT(H1429,2),LEFT(H1429,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1429,1)=\"J\",RIGHT(H1429,LEN(H1429)-4),RIGHT(H1429,LEN(H1429)-6)),\"\"))","v":"befristet"}]
[50001149,"SOFAR","SOFAR 20KTL-G2",20,22,3,"PV-Wechselrichter","Nein","2022-09-13","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1430,1)=\"J\",LEFT(H1430,2),LEFT(H1430,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1430,1)=\"J\",RIGHT(H1430,LEN(H1430)-4),RIGHT(H1430,LEN(H1430)-6)),\"\"))","v":""}]
[50001150,"SOFAR","SOFAR 20KTLX-G3",20,22,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-10-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1431,1)=\"J\",LEFT(H1431,2),LEFT(H1431,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1431,1)=\"J\",RIGHT(H1431,LEN(H1431)-4),RIGHT(H1431,LEN(H1431)-6)),\"\"))","v":"befristet"}]
[50001151,"SOFAR","SOFAR 22KTLX-G3",22,24.2,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-10-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1432,1)=\"J\",LEFT(H1432,2),LEFT(H1432,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1432,1)=\"J\",RIGHT(H1432,LEN(H1432)-4),RIGHT(H1432,LEN(H1432)-6)),\"\"))","v":"befristet"}]
[50001152,"SOFAR","SOFAR 24KTLX-G3",24,26.4,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-10-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1433,1)=\"J\",LEFT(H1433,2),LEFT(H1433,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1433,1)=\"J\",RIGHT(H1433,LEN(H1433)-4),RIGHT(H1433,LEN(H1433)-6)),\"\"))","v":"befristet"}]
[50001153,"SOFAR","SOFAR 25KTL-G2",25,27.5,3,"PV-Wechselrichter","Nein","2022-09-13","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1434,1)=\"J\",LEFT(H1434,2),LEFT(H1434,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1434,1)=\"J\",RIGHT(H1434,LEN(H1434)-4),RIGHT(H1434,LEN(H1434)-6)),\"\"))","v":""}]
[50001154,"SOFAR","SOFAR 25KTLX-G3",25,28,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1435,1)=\"J\",LEFT(H1435,2),LEFT(H1435,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1435,1)=\"J\",RIGHT(H1435,LEN(H1435)-4),RIGHT(H1435,LEN(H1435)-6)),\"\"))","v":"befristet"}]
[50001155,"SOFAR","SOFAR 30KTLX-G3-A",29.9,29.9,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1436,1)=\"J\",LEFT(H1436,2),LEFT(H1436,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1436,1)=\"J\",RIGHT(H1436,LEN(H1436)-4),RIGHT(H1436,LEN(H1436)-6)),\"\"))","v":"befristet"}]
[50001156,"SOFAR","SOFAR 30KTL-G2",30,33,3,"PV-Wechselrichter","Nein","2022-09-13","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1437,1)=\"J\",LEFT(H1437,2),LEFT(H1437,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1437,1)=\"J\",RIGHT(H1437,LEN(H1437)-4),RIGHT(H1437,LEN(H1437)-6)),\"\"))","v":""}]
[50001157,"SOFAR","SOFAR 30KTLX-G3",30,34,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1438,1)=\"J\",LEFT(H1438,2),LEFT(H1438,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1438,1)=\"J\",RIGHT(H1438,LEN(H1438)-4),RIGHT(H1438,LEN(H1438)-6)),\"\"))","v":"befristet"}]
[50001158,"SOFAR","SOFAR 33KTL-G2",33,36.299999999999997,3,"PV-Wechselrichter","Nein","2022-09-13","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1439,1)=\"J\",LEFT(H1439,2),LEFT(H1439,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1439,1)=\"J\",RIGHT(H1439,LEN(H1439)-4),RIGHT(H1439,LEN(H1439)-6)),\"\"))","v":""}]
[50001159,"SOFAR","SOFAR 33KTLX-G3",33,37,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1440,1)=\"J\",LEFT(H1440,2),LEFT(H1440,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1440,1)=\"J\",RIGHT(H1440,LEN(H1440)-4),RIGHT(H1440,LEN(H1440)-6)),\"\"))","v":"befristet"}]
[50001160,"SOFAR","SOFAR 36KTLX-G3",36,40,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1441,1)=\"J\",LEFT(H1441,2),LEFT(H1441,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1441,1)=\"J\",RIGHT(H1441,LEN(H1441)-4),RIGHT(H1441,LEN(H1441)-6)),\"\"))","v":"befristet"}]
[50001161,"SOFAR","SOFAR 40KTLX-G3",40,44,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1442,1)=\"J\",LEFT(H1442,2),LEFT(H1442,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1442,1)=\"J\",RIGHT(H1442,LEN(H1442)-4),RIGHT(H1442,LEN(H1442)-6)),\"\"))","v":"befristet"}]
[50001162,"SOFAR","SOFAR 40KTLX-G3-HV",40,44,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1443,1)=\"J\",LEFT(H1443,2),LEFT(H1443,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1443,1)=\"J\",RIGHT(H1443,LEN(H1443)-4),RIGHT(H1443,LEN(H1443)-6)),\"\"))","v":"befristet"}]
[50001163,"SOFAR","SOFAR 45KTLX-G3",45,50,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1444,1)=\"J\",LEFT(H1444,2),LEFT(H1444,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1444,1)=\"J\",RIGHT(H1444,LEN(H1444)-4),RIGHT(H1444,LEN(H1444)-6)),\"\"))","v":"befristet"}]
[50001164,"SOFAR","SOFAR 50KTL",50,50,3,"PV-Wechselrichter","Nein","2022-09-13","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1445,1)=\"J\",LEFT(H1445,2),LEFT(H1445,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1445,1)=\"J\",RIGHT(H1445,LEN(H1445)-4),RIGHT(H1445,LEN(H1445)-6)),\"\"))","v":""}]
[50001165,"SOFAR","SOFAR 50KTLX-G3",50,55,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1446,1)=\"J\",LEFT(H1446,2),LEFT(H1446,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1446,1)=\"J\",RIGHT(H1446,LEN(H1446)-4),RIGHT(H1446,LEN(H1446)-6)),\"\"))","v":"befristet"}]
[50001166,"SOFAR","SOFAR 50KTLX-G3-HV",50,55,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,"vermutlich gleiche Fehler wie beim Hybridgerät",null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1447,1)=\"J\",LEFT(H1447,2),LEFT(H1447,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1447,1)=\"J\",RIGHT(H1447,LEN(H1447)-4),RIGHT(H1447,LEN(H1447)-6)),\"\"))","v":"befristet"}]
[50001167,"SOFAR","SOFAR 60KTL",60,60,3,"PV-Wechselrichter","Nein","2022-09-13","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1448,1)=\"J\",LEFT(H1448,2),LEFT(H1448,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1448,1)=\"J\",RIGHT(H1448,LEN(H1448)-4),RIGHT(H1448,LEN(H1448)-6)),\"\"))","v":""}]
[50001168,"SOFAR","SOFAR 60KTLX-G3",60,66,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1449,1)=\"J\",LEFT(H1449,2),LEFT(H1449,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1449,1)=\"J\",RIGHT(H1449,LEN(H1449)-4),RIGHT(H1449,LEN(H1449)-6)),\"\"))","v":"befristet"}]
[50001169,"SOFAR","SOFAR 70KTL-G2",70,75,3,"PV-Wechselrichter","Nein","2022-09-13","Martin Bertsch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1450,1)=\"J\",LEFT(H1450,2),LEFT(H1450,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1450,1)=\"J\",RIGHT(H1450,LEN(H1450)-4),RIGHT(H1450,LEN(H1450)-6)),\"\"))","v":""}]
[50001170,"SOFAR","SOFAR 75KTL",75,75,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-10-31",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1451,1)=\"J\",LEFT(H1451,2),LEFT(H1451,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1451,1)=\"J\",RIGHT(H1451,LEN(H1451)-4),RIGHT(H1451,LEN(H1451)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001171,"SOFAR","SOFAR 75KTLX-G3",75,75,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1452,1)=\"J\",LEFT(H1452,2),LEFT(H1452,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1452,1)=\"J\",RIGHT(H1452,LEN(H1452)-4),RIGHT(H1452,LEN(H1452)-6)),\"\"))","v":"befristet"}]
[50001172,"SOFAR","SOFAR 70KTLX-G3",70,77,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1453,1)=\"J\",LEFT(H1453,2),LEFT(H1453,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1453,1)=\"J\",RIGHT(H1453,LEN(H1453)-4),RIGHT(H1453,LEN(H1453)-6)),\"\"))","v":"befristet"}]
[50001173,"SOFAR","SOFAR 80KTL",80,88,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-10-31",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1454,1)=\"J\",LEFT(H1454,2),LEFT(H1454,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1454,1)=\"J\",RIGHT(H1454,LEN(H1454)-4),RIGHT(H1454,LEN(H1454)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001174,"SOFAR","SOFAR 80KTLX-G3",80,88,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1455,1)=\"J\",LEFT(H1455,2),LEFT(H1455,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1455,1)=\"J\",RIGHT(H1455,LEN(H1455)-4),RIGHT(H1455,LEN(H1455)-6)),\"\"))","v":"befristet"}]
[50001175,"SOFAR","SOFAR 100KTLX-G4",100,100,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","221215056GZU-007","2023-05-11","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1456,1)=\"J\",LEFT(H1456,2),LEFT(H1456,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1456,1)=\"J\",RIGHT(H1456,LEN(H1456)-4),RIGHT(H1456,LEN(H1456)-6)),\"\"))","v":"befristet"}]
[50001176,"SOFAR","SOFAR 100KTL",100,110,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-10-31",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21","Vorhanden","nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1457,1)=\"J\",LEFT(H1457,2),LEFT(H1457,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1457,1)=\"J\",RIGHT(H1457,LEN(H1457)-4),RIGHT(H1457,LEN(H1457)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001177,"SOFAR","SOFAR 100KTL-HV",100,110,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-10-31",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1458,1)=\"J\",LEFT(H1458,2),LEFT(H1458,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1458,1)=\"J\",RIGHT(H1458,LEN(H1458)-4),RIGHT(H1458,LEN(H1458)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001178,"SOFAR","SOFAR 110KTLX-G4",100,110,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","221215056GZU-007","2023-05-11","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1459,1)=\"J\",LEFT(H1459,2),LEFT(H1459,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1459,1)=\"J\",RIGHT(H1459,LEN(H1459)-4),RIGHT(H1459,LEN(H1459)-6)),\"\"))","v":"befristet"}]
[50001179,"SOFAR","SOFAR 110KTL",110,121,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-10-31",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1460,1)=\"J\",LEFT(H1460,2),LEFT(H1460,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1460,1)=\"J\",RIGHT(H1460,LEN(H1460)-4),RIGHT(H1460,LEN(H1460)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001180,"SOFAR","SOFAR 125KTLX-G4",110,125,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","221215056GZU-007","2023-05-11","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1461,1)=\"J\",LEFT(H1461,2),LEFT(H1461,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1461,1)=\"J\",RIGHT(H1461,LEN(H1461)-4),RIGHT(H1461,LEN(H1461)-6)),\"\"))","v":"befristet"}]
[50001181,"SOFAR","SOFAR 125KTLX-G4-A",125,125,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","221215056GZU-007","2023-05-11","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1462,1)=\"J\",LEFT(H1462,2),LEFT(H1462,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1462,1)=\"J\",RIGHT(H1462,LEN(H1462)-4),RIGHT(H1462,LEN(H1462)-6)),\"\"))","v":"befristet"}]
[50001182,"SOFAR","SOFAR 125KTL-HV",125,137,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-10-31",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1463,1)=\"J\",LEFT(H1463,2),LEFT(H1463,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1463,1)=\"J\",RIGHT(H1463,LEN(H1463)-4),RIGHT(H1463,LEN(H1463)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001183,"SOFAR","SOFAR 136KTL-HV",136,150,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-10-31",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1464,1)=\"J\",LEFT(H1464,2),LEFT(H1464,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1464,1)=\"J\",RIGHT(H1464,LEN(H1464)-4),RIGHT(H1464,LEN(H1464)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001184,"SolarEdge","SE2200H ",2.2000000000000002,2.2000000000000002,1,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-34_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1465,1)=\"J\",LEFT(H1465,2),LEFT(H1465,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1465,1)=\"J\",RIGHT(H1465,LEN(H1465)-4),RIGHT(H1465,LEN(H1465)-6)),\"\"))","v":""}]
[50001185,"SolarEdge","SE2200H SESTI",2.2000000000000002,2.2000000000000002,1,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-35_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1466,1)=\"J\",LEFT(H1466,2),LEFT(H1466,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1466,1)=\"J\",RIGHT(H1466,LEN(H1466)-4),RIGHT(H1466,LEN(H1466)-6)),\"\"))","v":""}]
[50001186,"SolarEdge","SE3000H ",3,3,1,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-34_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1467,1)=\"J\",LEFT(H1467,2),LEFT(H1467,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1467,1)=\"J\",RIGHT(H1467,LEN(H1467)-4),RIGHT(H1467,LEN(H1467)-6)),\"\"))","v":""}]
[50001187,"SolarEdge","SE3000H SESTI",3,3,1,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-35_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1468,1)=\"J\",LEFT(H1468,2),LEFT(H1468,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1468,1)=\"J\",RIGHT(H1468,LEN(H1468)-4),RIGHT(H1468,LEN(H1468)-6)),\"\"))","v":""}]
[50001188,"SolarEdge","SE3K ",3,3,3,"PV-Wechselrichter","Nein","2023-02-21","Christian Elbs","2021-05-06",null,null,"2023-02-21","Ist in der aktuellen Version des Prüfberichts entfernt worden","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1469,1)=\"J\",LEFT(H1469,2),LEFT(H1469,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1469,1)=\"J\",RIGHT(H1469,LEN(H1469)-4),RIGHT(H1469,LEN(H1469)-6)),\"\"))","v":""}]
[50001189,"SolarEdge","SE3500H ",3.5,3.5,1,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-34_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1470,1)=\"J\",LEFT(H1470,2),LEFT(H1470,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1470,1)=\"J\",RIGHT(H1470,LEN(H1470)-4),RIGHT(H1470,LEN(H1470)-6)),\"\"))","v":""}]
[50001190,"SolarEdge","SE3500H SESTI",3.5,3.5,1,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-35_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1471,1)=\"J\",LEFT(H1471,2),LEFT(H1471,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1471,1)=\"J\",RIGHT(H1471,LEN(H1471)-4),RIGHT(H1471,LEN(H1471)-6)),\"\"))","v":""}]
[50001191,"SolarEdge","SE3680H ",3.68,3.68,1,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-34_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1472,1)=\"J\",LEFT(H1472,2),LEFT(H1472,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1472,1)=\"J\",RIGHT(H1472,LEN(H1472)-4),RIGHT(H1472,LEN(H1472)-6)),\"\"))","v":""}]
[50001192,"SolarEdge","SE3680H SESTI",3.68,3.68,1,"Hybrid-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-35_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1473,1)=\"J\",LEFT(H1473,2),LEFT(H1473,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1473,1)=\"J\",RIGHT(H1473,LEN(H1473)-4),RIGHT(H1473,LEN(H1473)-6)),\"\"))","v":""}]
[50001193,"SolarEdge","StorEdge SE3680H-RWSAC",3.68,3.68,1,"AC-Batteriewechselrichter","Nein","2022-11-21","Martin Bertsch",null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1474,1)=\"J\",LEFT(H1474,2),LEFT(H1474,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1474,1)=\"J\",RIGHT(H1474,LEN(H1474)-4),RIGHT(H1474,LEN(H1474)-6)),\"\"))","v":""}]
[50001194,"SolarEdge","SE4000H ",4,4,1,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-34_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3~ bis Sum. Sn 11,04 kVA - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1475,1)=\"J\",LEFT(H1475,2),LEFT(H1475,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1475,1)=\"J\",RIGHT(H1475,LEN(H1475)-4),RIGHT(H1475,LEN(H1475)-6)),\"\"))","v":""}]
[50001195,"SolarEdge","SE4000H SESTI",4,4,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"16PP115-35_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1476,1)=\"J\",LEFT(H1476,2),LEFT(H1476,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1476,1)=\"J\",RIGHT(H1476,LEN(H1476)-4),RIGHT(H1476,LEN(H1476)-6)),\"\"))","v":""}]
[50001196,"SolarEdge","SE4K ",4,4,3,"PV-Wechselrichter","Nein","2023-02-21","Christian Elbs","2021-05-06",null,null,"2023-02-21","Ist in der aktuellen Version des Prüfberichts entfernt worden","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1477,1)=\"J\",LEFT(H1477,2),LEFT(H1477,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1477,1)=\"J\",RIGHT(H1477,LEN(H1477)-4),RIGHT(H1477,LEN(H1477)-6)),\"\"))","v":""}]
[50001197,"SolarEdge","SE4600H ",4.5999999999999996,4.5999999999999996,1,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-34_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3~ bis Sum. Sn 11,04 kVA - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1478,1)=\"J\",LEFT(H1478,2),LEFT(H1478,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1478,1)=\"J\",RIGHT(H1478,LEN(H1478)-4),RIGHT(H1478,LEN(H1478)-6)),\"\"))","v":""}]
[50001198,"SolarEdge","SE4600H SESTI",4.5999999999999996,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"16PP115-35_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1479,1)=\"J\",LEFT(H1479,2),LEFT(H1479,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1479,1)=\"J\",RIGHT(H1479,LEN(H1479)-4),RIGHT(H1479,LEN(H1479)-6)),\"\"))","v":""}]
[50001199,"SolarEdge","SE5000H ",5,5,1,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-34_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3~ bis Sum. Sn 11,04 kVA - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1480,1)=\"J\",LEFT(H1480,2),LEFT(H1480,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1480,1)=\"J\",RIGHT(H1480,LEN(H1480)-4),RIGHT(H1480,LEN(H1480)-6)),\"\"))","v":""}]
[50001200,"SolarEdge","SE5000H SESTI",5,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"16PP115-35_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1481,1)=\"J\",LEFT(H1481,2),LEFT(H1481,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1481,1)=\"J\",RIGHT(H1481,LEN(H1481)-4),RIGHT(H1481,LEN(H1481)-6)),\"\"))","v":""}]
[50001201,"SolarEdge","SE5K ",5,5,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1482,1)=\"J\",LEFT(H1482,2),LEFT(H1482,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1482,1)=\"J\",RIGHT(H1482,LEN(H1482)-4),RIGHT(H1482,LEN(H1482)-6)),\"\"))","v":""}]
[50001202,"SolarEdge","SE5K-RWB ",5,5,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1483,1)=\"J\",LEFT(H1483,2),LEFT(H1483,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1483,1)=\"J\",RIGHT(H1483,LEN(H1483)-4),RIGHT(H1483,LEN(H1483)-6)),\"\"))","v":""}]
[50001203,"SolarEdge","SE5K-RWB48",5,5,3,"Hybrid-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2023-01-25",null,null,null,null,"Ja",null,null,"OK","MM","22TH0188-OVE-directive R25_3","2023-05-23",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1484,1)=\"J\",LEFT(H1484,2),LEFT(H1484,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1484,1)=\"J\",RIGHT(H1484,LEN(H1484)-4),RIGHT(H1484,LEN(H1484)-6)),\"\"))","v":""}]
[50001204,"SolarEdge","SE5K-RWS ",5,5,3,"Hybrid-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1485,1)=\"J\",LEFT(H1485,2),LEFT(H1485,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1485,1)=\"J\",RIGHT(H1485,LEN(H1485)-4),RIGHT(H1485,LEN(H1485)-6)),\"\"))","v":""}]
[50001205,"SolarEdge","StorEdge SE5000H-RWSAC",5,5,1,"AC-Batteriewechselrichter","Nein","2023-03-28","Martin Bertsch","2021-05-06",null,null,"2023-03-28",null,"Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Nur als Batteriewechselrichter 1~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1486,1)=\"J\",LEFT(H1486,2),LEFT(H1486,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1486,1)=\"J\",RIGHT(H1486,LEN(H1486)-4),RIGHT(H1486,LEN(H1486)-6)),\"\"))","v":""}]
[50001206,"SolarEdge","SE6000H ",6,6,1,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"16PP115-34_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Stringwechselrichter 1~ - zulässig 3~ bis Sum. Sn 11,04 kVA - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1487,1)=\"J\",LEFT(H1487,2),LEFT(H1487,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1487,1)=\"J\",RIGHT(H1487,LEN(H1487)-4),RIGHT(H1487,LEN(H1487)-6)),\"\"))","v":""}]
[50001207,"SolarEdge","SE6000H SESTI",6,6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"16PP115-35_0","2020-12-07",null,"Vorhanden",null,null,null,null,"Batteriespeicher 1~ - AC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1488,1)=\"J\",LEFT(H1488,2),LEFT(H1488,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1488,1)=\"J\",RIGHT(H1488,LEN(H1488)-4),RIGHT(H1488,LEN(H1488)-6)),\"\"))","v":""}]
[50001208,"SolarEdge","SE6K ",6,6,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1489,1)=\"J\",LEFT(H1489,2),LEFT(H1489,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1489,1)=\"J\",RIGHT(H1489,LEN(H1489)-4),RIGHT(H1489,LEN(H1489)-6)),\"\"))","v":""}]
[50001209,"SolarEdge","SE7K ",7,7,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1490,1)=\"J\",LEFT(H1490,2),LEFT(H1490,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1490,1)=\"J\",RIGHT(H1490,LEN(H1490)-4),RIGHT(H1490,LEN(H1490)-6)),\"\"))","v":""}]
[50001210,"SolarEdge","SE7K-RWB48",7,7,3,"Hybrid-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2023-01-25",null,null,null,null,"Ja",null,null,"OK","MM","22TH0188-OVE-directive R25_3","2023-05-23",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1491,1)=\"J\",LEFT(H1491,2),LEFT(H1491,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1491,1)=\"J\",RIGHT(H1491,LEN(H1491)-4),RIGHT(H1491,LEN(H1491)-6)),\"\"))","v":""}]
[50001211,"SolarEdge","SE7K-RWS ",7,7,3,"Hybrid-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1492,1)=\"J\",LEFT(H1492,2),LEFT(H1492,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1492,1)=\"J\",RIGHT(H1492,LEN(H1492)-4),RIGHT(H1492,LEN(H1492)-6)),\"\"))","v":""}]
[50001212,"SolarEdge","SE8K ",8,8,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1493,1)=\"J\",LEFT(H1493,2),LEFT(H1493,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1493,1)=\"J\",RIGHT(H1493,LEN(H1493)-4),RIGHT(H1493,LEN(H1493)-6)),\"\"))","v":""}]
[50001213,"SolarEdge","SE8K-RWB48",8,8,3,"Hybrid-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2023-01-25",null,null,null,null,"Ja",null,null,"OK","MM","22TH0188-OVE-directive R25_3","2023-05-23",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1494,1)=\"J\",LEFT(H1494,2),LEFT(H1494,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1494,1)=\"J\",RIGHT(H1494,LEN(H1494)-4),RIGHT(H1494,LEN(H1494)-6)),\"\"))","v":""}]
[50001214,"SolarEdge","SE8K-RWS ",8,8,3,"Hybrid-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1495,1)=\"J\",LEFT(H1495,2),LEFT(H1495,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1495,1)=\"J\",RIGHT(H1495,LEN(H1495)-4),RIGHT(H1495,LEN(H1495)-6)),\"\"))","v":""}]
[50001215,"SolarEdge","SE9K ",9,9,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1496,1)=\"J\",LEFT(H1496,2),LEFT(H1496,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1496,1)=\"J\",RIGHT(H1496,LEN(H1496)-4),RIGHT(H1496,LEN(H1496)-6)),\"\"))","v":""}]
[50001216,"SolarEdge","SE10K ",10,10,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1497,1)=\"J\",LEFT(H1497,2),LEFT(H1497,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1497,1)=\"J\",RIGHT(H1497,LEN(H1497)-4),RIGHT(H1497,LEN(H1497)-6)),\"\"))","v":""}]
[50001217,"SolarEdge","SE10K-RWB48",10,10,3,"Hybrid-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2023-01-25",null,null,null,null,"Ja",null,null,"OK","MM","22TH0188-OVE-directive R25_3","2023-05-23",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1498,1)=\"J\",LEFT(H1498,2),LEFT(H1498,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1498,1)=\"J\",RIGHT(H1498,LEN(H1498)-4),RIGHT(H1498,LEN(H1498)-6)),\"\"))","v":""}]
[50001218,"SolarEdge","SE10K-RWS ",10,10,3,"Hybrid-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Hybridstromrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1499,1)=\"J\",LEFT(H1499,2),LEFT(H1499,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1499,1)=\"J\",RIGHT(H1499,LEN(H1499)-4),RIGHT(H1499,LEN(H1499)-6)),\"\"))","v":""}]
[50001219,"SolarEdge","SE12,5K ",12.5,12.5,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1500,1)=\"J\",LEFT(H1500,2),LEFT(H1500,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1500,1)=\"J\",RIGHT(H1500,LEN(H1500)-4),RIGHT(H1500,LEN(H1500)-6)),\"\"))","v":""}]
[50001220,"SolarEdge","SE15K ",15,15,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24",null,"OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1501,1)=\"J\",LEFT(H1501,2),LEFT(H1501,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1501,1)=\"J\",RIGHT(H1501,LEN(H1501)-4),RIGHT(H1501,LEN(H1501)-6)),\"\"))","v":""}]
[50001221,"SolarEdge","SE16K ",16,16,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1502,1)=\"J\",LEFT(H1502,2),LEFT(H1502,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1502,1)=\"J\",RIGHT(H1502,LEN(H1502)-4),RIGHT(H1502,LEN(H1502)-6)),\"\"))","v":""}]
[50001222,"SolarEdge","SE17K ",17,17,3,"PV-Wechselrichter","Ja","2023-10-19","Martin Bertsch","2021-05-06",null,null,null,null,"Nein","Nein",null,"OK","Roland Bründlinger (AIT)","10TH02222-OVE-directive R25_4","2023-08-24","Vorhanden","OK",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1503,1)=\"J\",LEFT(H1503,2),LEFT(H1503,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1503,1)=\"J\",RIGHT(H1503,LEN(H1503)-4),RIGHT(H1503,LEN(H1503)-6)),\"\"))","v":""}]
[50001971,"SolarEdge","SE20K",20,22,3,"PV-Wechselrichter","Ja","2023-11-17","Martin Bertsch","2023-11-17",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0534-OVE-directive R25_3","2023-11-10",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1504,1)=\"J\",LEFT(H1504,2),LEFT(H1504,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1504,1)=\"J\",RIGHT(H1504,LEN(H1504)-4),RIGHT(H1504,LEN(H1504)-6)),\"\"))","v":""}]
[50001223,"SolarEdge","SE25K ",25,25,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0534-OVE-directive R25_3","2023-11-10","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1505,1)=\"J\",LEFT(H1505,2),LEFT(H1505,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1505,1)=\"J\",RIGHT(H1505,LEN(H1505)-4),RIGHT(H1505,LEN(H1505)-6)),\"\"))","v":""}]
[50001224,"SolarEdge","SE27.6K ",27.6,27.6,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0534-OVE-directive R25_3","2023-11-10","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1506,1)=\"J\",LEFT(H1506,2),LEFT(H1506,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1506,1)=\"J\",RIGHT(H1506,LEN(H1506)-4),RIGHT(H1506,LEN(H1506)-6)),\"\"))","v":""}]
[50001225,"SolarEdge","SE30K ",30,30,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0534-OVE-directive R25_3","2023-11-10","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1507,1)=\"J\",LEFT(H1507,2),LEFT(H1507,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1507,1)=\"J\",RIGHT(H1507,LEN(H1507)-4),RIGHT(H1507,LEN(H1507)-6)),\"\"))","v":""}]
[50001226,"SolarEdge","SE33.3K ",33.299999999999997,33.299999999999997,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"19TH0534-OVE-directive R25_3","2023-11-10","Vorhanden","nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1508,1)=\"J\",LEFT(H1508,2),LEFT(H1508,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1508,1)=\"J\",RIGHT(H1508,LEN(H1508)-4),RIGHT(H1508,LEN(H1508)-6)),\"\"))","v":""}]
[50001227,"SolarEdge","SE40K ",40,40,3,"PV-Wechselrichter","Nein","2022-07-14","Christian Elbs",null,null,null,"2022-07-14",null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1509,1)=\"J\",LEFT(H1509,2),LEFT(H1509,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1509,1)=\"J\",RIGHT(H1509,LEN(H1509)-4),RIGHT(H1509,LEN(H1509)-6)),\"\"))","v":""}]
[50001228,"SolarEdge","SE55K ",55,55,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"17TH0209-OVE-directive R25_0","2021-02-24","Vorhanden","Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1510,1)=\"J\",LEFT(H1510,2),LEFT(H1510,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1510,1)=\"J\",RIGHT(H1510,LEN(H1510)-4),RIGHT(H1510,LEN(H1510)-6)),\"\"))","v":""}]
[50001229,"SolarEdge","SE66.6K ",66.599999999999994,66.599999999999994,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"20TH0532-OVE-directive R25_0","2021-02-24","Vorhanden","Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1511,1)=\"J\",LEFT(H1511,2),LEFT(H1511,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1511,1)=\"J\",RIGHT(H1511,LEN(H1511)-4),RIGHT(H1511,LEN(H1511)-6)),\"\"))","v":""}]
[50001230,"SolarEdge","SE82.8K ",82.8,82.8,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"17TH0209-OVE-directive R25_0","2021-02-24","Vorhanden","Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1512,1)=\"J\",LEFT(H1512,2),LEFT(H1512,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1512,1)=\"J\",RIGHT(H1512,LEN(H1512)-4),RIGHT(H1512,LEN(H1512)-6)),\"\"))","v":""}]
[50001231,"SolarEdge","SE90K ",90,90,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"20TH0532-OVE-directive R25_0","2021-02-24","Vorhanden","Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1513,1)=\"J\",LEFT(H1513,2),LEFT(H1513,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1513,1)=\"J\",RIGHT(H1513,LEN(H1513)-4),RIGHT(H1513,LEN(H1513)-6)),\"\"))","v":""}]
[50001232,"SolarEdge","SE100K ",100,100,3,"PV-Wechselrichter","Ja",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"20TH0532-OVE-directive R25_0","2021-02-24","Vorhanden","Vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1514,1)=\"J\",LEFT(H1514,2),LEFT(H1514,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1514,1)=\"J\",RIGHT(H1514,LEN(H1514)-4),RIGHT(H1514,LEN(H1514)-6)),\"\"))","v":""}]
[50001233,"SolarEdge","SE120K",120,120,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1515,1)=\"J\",LEFT(H1515,2),LEFT(H1515,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1515,1)=\"J\",RIGHT(H1515,LEN(H1515)-4),RIGHT(H1515,LEN(H1515)-6)),\"\"))","v":""}]
[50002160,"Solarinvert","BAT 600-24",0.46,0.51100000000000001,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1516,1)=\"J\",LEFT(H1516,2),LEFT(H1516,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1516,1)=\"J\",RIGHT(H1516,LEN(H1516)-4),RIGHT(H1516,LEN(H1516)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002146,"Solarinvert","SOL 600-17",0.46,0.51100000000000001,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1517,1)=\"J\",LEFT(H1517,2),LEFT(H1517,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1517,1)=\"J\",RIGHT(H1517,LEN(H1517)-4),RIGHT(H1517,LEN(H1517)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002168,"Solarinvert","WIN 600-12",0.47,0.54,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1518,1)=\"J\",LEFT(H1518,2),LEFT(H1518,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1518,1)=\"J\",RIGHT(H1518,LEN(H1518)-4),RIGHT(H1518,LEN(H1518)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002161,"Solarinvert","BAT 600-48",0.5,0.55600000000000005,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1519,1)=\"J\",LEFT(H1519,2),LEFT(H1519,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1519,1)=\"J\",RIGHT(H1519,LEN(H1519)-4),RIGHT(H1519,LEN(H1519)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002169,"Solarinvert","WIN 600-24",0.48,0.56999999999999995,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1520,1)=\"J\",LEFT(H1520,2),LEFT(H1520,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1520,1)=\"J\",RIGHT(H1520,LEN(H1520)-4),RIGHT(H1520,LEN(H1520)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002147,"Solarinvert","SOL 700-35",0.56000000000000005,0.622,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1521,1)=\"J\",LEFT(H1521,2),LEFT(H1521,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1521,1)=\"J\",RIGHT(H1521,LEN(H1521)-4),RIGHT(H1521,LEN(H1521)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002148,"Solarinvert","SOL 900-60",0.74,0.82199999999999995,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1522,1)=\"J\",LEFT(H1522,2),LEFT(H1522,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1522,1)=\"J\",RIGHT(H1522,LEN(H1522)-4),RIGHT(H1522,LEN(H1522)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002181,"Solarinvert","WIN 1000-160",0.81,0.9,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1523,1)=\"J\",LEFT(H1523,2),LEFT(H1523,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1523,1)=\"J\",RIGHT(H1523,LEN(H1523)-4),RIGHT(H1523,LEN(H1523)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002170,"Solarinvert","WIN 1000-24",0.78,0.9,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1524,1)=\"J\",LEFT(H1524,2),LEFT(H1524,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1524,1)=\"J\",RIGHT(H1524,LEN(H1524)-4),RIGHT(H1524,LEN(H1524)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002172,"Solarinvert","WIN 1000-48",0.8,0.9,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1525,1)=\"J\",LEFT(H1525,2),LEFT(H1525,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1525,1)=\"J\",RIGHT(H1525,LEN(H1525)-4),RIGHT(H1525,LEN(H1525)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002171,"Solarinvert","WIN 1200-24",0.93,1.07,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1526,1)=\"J\",LEFT(H1526,2),LEFT(H1526,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1526,1)=\"J\",RIGHT(H1526,LEN(H1526)-4),RIGHT(H1526,LEN(H1526)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002162,"Solarinvert","BAT 1200-24",0.98,1.089,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1527,1)=\"J\",LEFT(H1527,2),LEFT(H1527,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1527,1)=\"J\",RIGHT(H1527,LEN(H1527)-4),RIGHT(H1527,LEN(H1527)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002149,"Solarinvert","SOL 1200-60",1,1.111,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1528,1)=\"J\",LEFT(H1528,2),LEFT(H1528,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1528,1)=\"J\",RIGHT(H1528,LEN(H1528)-4),RIGHT(H1528,LEN(H1528)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002150,"Solarinvert","SOL 1200-90",1,1.111,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1529,1)=\"J\",LEFT(H1529,2),LEFT(H1529,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1529,1)=\"J\",RIGHT(H1529,LEN(H1529)-4),RIGHT(H1529,LEN(H1529)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002151,"Solarinvert","SOL 1300-35",1,1.111,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1530,1)=\"J\",LEFT(H1530,2),LEFT(H1530,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1530,1)=\"J\",RIGHT(H1530,LEN(H1530)-4),RIGHT(H1530,LEN(H1530)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002163,"Solarinvert","BAT 1200-48",1.06,1.1779999999999999,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1531,1)=\"J\",LEFT(H1531,2),LEFT(H1531,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1531,1)=\"J\",RIGHT(H1531,LEN(H1531)-4),RIGHT(H1531,LEN(H1531)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002153,"Solarinvert","SOL 1500-90",1.27,1.411,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1532,1)=\"J\",LEFT(H1532,2),LEFT(H1532,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1532,1)=\"J\",RIGHT(H1532,LEN(H1532)-4),RIGHT(H1532,LEN(H1532)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002173,"Solarinvert","WIN 1500-48",1.18,1.47,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1533,1)=\"J\",LEFT(H1533,2),LEFT(H1533,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1533,1)=\"J\",RIGHT(H1533,LEN(H1533)-4),RIGHT(H1533,LEN(H1533)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002180,"Solarinvert","WIN 1600-120",1.29,1.5,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1534,1)=\"J\",LEFT(H1534,2),LEFT(H1534,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1534,1)=\"J\",RIGHT(H1534,LEN(H1534)-4),RIGHT(H1534,LEN(H1534)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002152,"Solarinvert","SOL 1600-60",1.36,1.5109999999999999,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1535,1)=\"J\",LEFT(H1535,2),LEFT(H1535,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1535,1)=\"J\",RIGHT(H1535,LEN(H1535)-4),RIGHT(H1535,LEN(H1535)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002154,"Solarinvert","SOL 1800-35",1.5,1.667,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1536,1)=\"J\",LEFT(H1536,2),LEFT(H1536,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1536,1)=\"J\",RIGHT(H1536,LEN(H1536)-4),RIGHT(H1536,LEN(H1536)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002177,"Solarinvert","WIN 2000-120",1.61,1.81,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1537,1)=\"J\",LEFT(H1537,2),LEFT(H1537,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1537,1)=\"J\",RIGHT(H1537,LEN(H1537)-4),RIGHT(H1537,LEN(H1537)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002174,"Solarinvert","WIN 2000-48",1.58,1.81,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1538,1)=\"J\",LEFT(H1538,2),LEFT(H1538,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1538,1)=\"J\",RIGHT(H1538,LEN(H1538)-4),RIGHT(H1538,LEN(H1538)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002155,"Solarinvert","SOL 2000-60",1.66,1.8440000000000001,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1539,1)=\"J\",LEFT(H1539,2),LEFT(H1539,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1539,1)=\"J\",RIGHT(H1539,LEN(H1539)-4),RIGHT(H1539,LEN(H1539)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002156,"Solarinvert","SOL 2000-90",1.66,1.8440000000000001,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1540,1)=\"J\",LEFT(H1540,2),LEFT(H1540,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1540,1)=\"J\",RIGHT(H1540,LEN(H1540)-4),RIGHT(H1540,LEN(H1540)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002164,"Solarinvert","BAT 2000-48",1.7,1.889,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1541,1)=\"J\",LEFT(H1541,2),LEFT(H1541,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1541,1)=\"J\",RIGHT(H1541,LEN(H1541)-4),RIGHT(H1541,LEN(H1541)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002166,"Solarinvert","BAT 2000-96",1.75,1.944,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1542,1)=\"J\",LEFT(H1542,2),LEFT(H1542,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1542,1)=\"J\",RIGHT(H1542,LEN(H1542)-4),RIGHT(H1542,LEN(H1542)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002178,"Solarinvert","WIN 2500-120",1.99,2.15,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1543,1)=\"J\",LEFT(H1543,2),LEFT(H1543,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1543,1)=\"J\",RIGHT(H1543,LEN(H1543)-4),RIGHT(H1543,LEN(H1543)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002157,"Solarinvert","SOL 2400-90",1.94,2.1560000000000001,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1544,1)=\"J\",LEFT(H1544,2),LEFT(H1544,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1544,1)=\"J\",RIGHT(H1544,LEN(H1544)-4),RIGHT(H1544,LEN(H1544)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002158,"Solarinvert","SOL 2600-60",2.2000000000000002,2.444,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1545,1)=\"J\",LEFT(H1545,2),LEFT(H1545,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1545,1)=\"J\",RIGHT(H1545,LEN(H1545)-4),RIGHT(H1545,LEN(H1545)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002165,"Solarinvert","BAT 2800-48",2.4,2.6669999999999998,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1546,1)=\"J\",LEFT(H1546,2),LEFT(H1546,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1546,1)=\"J\",RIGHT(H1546,LEN(H1546)-4),RIGHT(H1546,LEN(H1546)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002175,"Solarinvert","WIN 2800-48",2.4,2.6669999999999998,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1547,1)=\"J\",LEFT(H1547,2),LEFT(H1547,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1547,1)=\"J\",RIGHT(H1547,LEN(H1547)-4),RIGHT(H1547,LEN(H1547)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002179,"Solarinvert","WIN 3000-120",2.39,2.71,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1548,1)=\"J\",LEFT(H1548,2),LEFT(H1548,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1548,1)=\"J\",RIGHT(H1548,LEN(H1548)-4),RIGHT(H1548,LEN(H1548)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002159,"Solarinvert","SOL 3000-90",2.5499999999999998,2.8330000000000002,1,"PV-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1549,1)=\"J\",LEFT(H1549,2),LEFT(H1549,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1549,1)=\"J\",RIGHT(H1549,LEN(H1549)-4),RIGHT(H1549,LEN(H1549)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002183,"Solarinvert","WIN 3200-160",2.7,3,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1550,1)=\"J\",LEFT(H1550,2),LEFT(H1550,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1550,1)=\"J\",RIGHT(H1550,LEN(H1550)-4),RIGHT(H1550,LEN(H1550)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002176,"Solarinvert","WIN 3200-48",2.7,3,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1551,1)=\"J\",LEFT(H1551,2),LEFT(H1551,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1551,1)=\"J\",RIGHT(H1551,LEN(H1551)-4),RIGHT(H1551,LEN(H1551)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002167,"Solarinvert","BAT 3200-96",2.8,3.1110000000000002,1,"AC-Batteriewechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1552,1)=\"J\",LEFT(H1552,2),LEFT(H1552,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1552,1)=\"J\",RIGHT(H1552,LEN(H1552)-4),RIGHT(H1552,LEN(H1552)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50002182,"Solarinvert","WIN 3600-120",2.91,3.2280000000000002,1,"Windenergie-Wechselrichter","Ja - <= 16A Anlage, befristet","2024-04-23","Martin Bertsch","2024-04-29","da cosphi(U) max. Anlagengröße 3,68 kVA","2024-07-31",null,null,"Nein","Nein","Nein","Vorhanden","Roland Bründlinger (AIT)","19TH0278-OVE-directive R25_0","2024-04-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1553,1)=\"J\",LEFT(H1553,2),LEFT(H1553,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1553,1)=\"J\",RIGHT(H1553,LEN(H1553)-4),RIGHT(H1553,LEN(H1553)-6)),\"\"))","v":"<= 16A Anlage, befristet"}]
[50001271,"SolarMax","1000SP",1,1.1000000000000001,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1554,1)=\"J\",LEFT(H1554,2),LEFT(H1554,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1554,1)=\"J\",RIGHT(H1554,LEN(H1554)-4),RIGHT(H1554,LEN(H1554)-6)),\"\"))","v":""}]
[50001272,"SolarMax","1500SP",1.5,1.65,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1555,1)=\"J\",LEFT(H1555,2),LEFT(H1555,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1555,1)=\"J\",RIGHT(H1555,LEN(H1555)-4),RIGHT(H1555,LEN(H1555)-6)),\"\"))","v":""}]
[50001273,"SolarMax","2000SP",2,2.2000000000000002,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1556,1)=\"J\",LEFT(H1556,2),LEFT(H1556,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1556,1)=\"J\",RIGHT(H1556,LEN(H1556)-4),RIGHT(H1556,LEN(H1556)-6)),\"\"))","v":""}]
[50001274,"SolarMax","2300ES-AC",2.2000000000000002,2.2000000000000002,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1557,1)=\"J\",LEFT(H1557,2),LEFT(H1557,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1557,1)=\"J\",RIGHT(H1557,LEN(H1557)-4),RIGHT(H1557,LEN(H1557)-6)),\"\"))","v":""}]
[50001275,"SolarMax","2500SP",2.5,2.75,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1558,1)=\"J\",LEFT(H1558,2),LEFT(H1558,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1558,1)=\"J\",RIGHT(H1558,LEN(H1558)-4),RIGHT(H1558,LEN(H1558)-6)),\"\"))","v":""}]
[50001276,"SolarMax","3000ES",3,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1559,1)=\"J\",LEFT(H1559,2),LEFT(H1559,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1559,1)=\"J\",RIGHT(H1559,LEN(H1559)-4),RIGHT(H1559,LEN(H1559)-6)),\"\"))","v":""}]
[50001277,"SolarMax","3000ES-AC",3,3,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1560,1)=\"J\",LEFT(H1560,2),LEFT(H1560,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1560,1)=\"J\",RIGHT(H1560,LEN(H1560)-4),RIGHT(H1560,LEN(H1560)-6)),\"\"))","v":""}]
[50001278,"SolarMax","3000SP",3,3.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1561,1)=\"J\",LEFT(H1561,2),LEFT(H1561,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1561,1)=\"J\",RIGHT(H1561,LEN(H1561)-4),RIGHT(H1561,LEN(H1561)-6)),\"\"))","v":""}]
[50001279,"SolarMax","3600SP",3.6,3.68,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1562,1)=\"J\",LEFT(H1562,2),LEFT(H1562,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1562,1)=\"J\",RIGHT(H1562,LEN(H1562)-4),RIGHT(H1562,LEN(H1562)-6)),\"\"))","v":""}]
[50001280,"SolarMax","4000SP",4,4.4000000000000004,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1563,1)=\"J\",LEFT(H1563,2),LEFT(H1563,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1563,1)=\"J\",RIGHT(H1563,LEN(H1563)-4),RIGHT(H1563,LEN(H1563)-6)),\"\"))","v":""}]
[50001281,"SolarMax","4500ES",4.5,4.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1564,1)=\"J\",LEFT(H1564,2),LEFT(H1564,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1564,1)=\"J\",RIGHT(H1564,LEN(H1564)-4),RIGHT(H1564,LEN(H1564)-6)),\"\"))","v":""}]
[50001282,"SolarMax","4500ES-AC",4.5,4.5,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1565,1)=\"J\",LEFT(H1565,2),LEFT(H1565,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1565,1)=\"J\",RIGHT(H1565,LEN(H1565)-4),RIGHT(H1565,LEN(H1565)-6)),\"\"))","v":""}]
[50001283,"SolarMax","4600SP",4.5999999999999996,4.5999999999999996,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1566,1)=\"J\",LEFT(H1566,2),LEFT(H1566,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1566,1)=\"J\",RIGHT(H1566,LEN(H1566)-4),RIGHT(H1566,LEN(H1566)-6)),\"\"))","v":""}]
[50001284,"SolarMax","5000SP",5,5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1567,1)=\"J\",LEFT(H1567,2),LEFT(H1567,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1567,1)=\"J\",RIGHT(H1567,LEN(H1567)-4),RIGHT(H1567,LEN(H1567)-6)),\"\"))","v":""}]
[50001285,"SolarMax","5ES-T",5,5,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1568,1)=\"J\",LEFT(H1568,2),LEFT(H1568,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1568,1)=\"J\",RIGHT(H1568,LEN(H1568)-4),RIGHT(H1568,LEN(H1568)-6)),\"\"))","v":""}]
[50001286,"SolarMax","6000ES",6,6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1569,1)=\"J\",LEFT(H1569,2),LEFT(H1569,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1569,1)=\"J\",RIGHT(H1569,LEN(H1569)-4),RIGHT(H1569,LEN(H1569)-6)),\"\"))","v":""}]
[50001287,"SolarMax","6ES-T",6,6,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1570,1)=\"J\",LEFT(H1570,2),LEFT(H1570,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1570,1)=\"J\",RIGHT(H1570,LEN(H1570)-4),RIGHT(H1570,LEN(H1570)-6)),\"\"))","v":""}]
[50001288,"SolarMax","MAX.STORAGE 6",6,6,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1571,1)=\"J\",LEFT(H1571,2),LEFT(H1571,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1571,1)=\"J\",RIGHT(H1571,LEN(H1571)-4),RIGHT(H1571,LEN(H1571)-6)),\"\"))","v":""}]
[50001289,"SolarMax","6SMT",6,6.6,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1572,1)=\"J\",LEFT(H1572,2),LEFT(H1572,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1572,1)=\"J\",RIGHT(H1572,LEN(H1572)-4),RIGHT(H1572,LEN(H1572)-6)),\"\"))","v":""}]
[50001290,"SolarMax","MAX.STORAGE ULTIMATE 6",6,6.6,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1573,1)=\"J\",LEFT(H1573,2),LEFT(H1573,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1573,1)=\"J\",RIGHT(H1573,LEN(H1573)-4),RIGHT(H1573,LEN(H1573)-6)),\"\"))","v":""}]
[50001291,"SolarMax","8ES-T",8,8,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1574,1)=\"J\",LEFT(H1574,2),LEFT(H1574,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1574,1)=\"J\",RIGHT(H1574,LEN(H1574)-4),RIGHT(H1574,LEN(H1574)-6)),\"\"))","v":""}]
[50001292,"SolarMax","8SMT",8,8.8000000000000007,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1575,1)=\"J\",LEFT(H1575,2),LEFT(H1575,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1575,1)=\"J\",RIGHT(H1575,LEN(H1575)-4),RIGHT(H1575,LEN(H1575)-6)),\"\"))","v":""}]
[50001293,"SolarMax","MAX.STORAGE 8",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1576,1)=\"J\",LEFT(H1576,2),LEFT(H1576,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1576,1)=\"J\",RIGHT(H1576,LEN(H1576)-4),RIGHT(H1576,LEN(H1576)-6)),\"\"))","v":""}]
[50001294,"SolarMax","MAX.STORAGE ULTIMATE 8",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1577,1)=\"J\",LEFT(H1577,2),LEFT(H1577,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1577,1)=\"J\",RIGHT(H1577,LEN(H1577)-4),RIGHT(H1577,LEN(H1577)-6)),\"\"))","v":""}]
[50001295,"SolarMax","10ES-T",10,10,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1578,1)=\"J\",LEFT(H1578,2),LEFT(H1578,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1578,1)=\"J\",RIGHT(H1578,LEN(H1578)-4),RIGHT(H1578,LEN(H1578)-6)),\"\"))","v":""}]
[50001296,"SolarMax","10SMT",10,11,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1579,1)=\"J\",LEFT(H1579,2),LEFT(H1579,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1579,1)=\"J\",RIGHT(H1579,LEN(H1579)-4),RIGHT(H1579,LEN(H1579)-6)),\"\"))","v":""}]
[50001297,"SolarMax","MAX.STORAGE 10",10,11,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1580,1)=\"J\",LEFT(H1580,2),LEFT(H1580,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1580,1)=\"J\",RIGHT(H1580,LEN(H1580)-4),RIGHT(H1580,LEN(H1580)-6)),\"\"))","v":""}]
[50001298,"SolarMax","MAX.STORAGE ULTIMATE 10",10,11,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1581,1)=\"J\",LEFT(H1581,2),LEFT(H1581,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1581,1)=\"J\",RIGHT(H1581,LEN(H1581)-4),RIGHT(H1581,LEN(H1581)-6)),\"\"))","v":""}]
[50001299,"SolarMax","13SMT",12,13.2,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1582,1)=\"J\",LEFT(H1582,2),LEFT(H1582,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1582,1)=\"J\",RIGHT(H1582,LEN(H1582)-4),RIGHT(H1582,LEN(H1582)-6)),\"\"))","v":""}]
[50001300,"SolarMax","MAX.STORAGE 12",12,13.2,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1583,1)=\"J\",LEFT(H1583,2),LEFT(H1583,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1583,1)=\"J\",RIGHT(H1583,LEN(H1583)-4),RIGHT(H1583,LEN(H1583)-6)),\"\"))","v":""}]
[50001301,"SolarMax","MAX.STORAGE ULTIMATE 12",12,13.2,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1584,1)=\"J\",LEFT(H1584,2),LEFT(H1584,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1584,1)=\"J\",RIGHT(H1584,LEN(H1584)-4),RIGHT(H1584,LEN(H1584)-6)),\"\"))","v":""}]
[50001302,"SolarMax","15SMT",15,16.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1585,1)=\"J\",LEFT(H1585,2),LEFT(H1585,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1585,1)=\"J\",RIGHT(H1585,LEN(H1585)-4),RIGHT(H1585,LEN(H1585)-6)),\"\"))","v":""}]
[50001303,"SolarMax","MAX.STORAGE 15",15,16.5,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1586,1)=\"J\",LEFT(H1586,2),LEFT(H1586,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1586,1)=\"J\",RIGHT(H1586,LEN(H1586)-4),RIGHT(H1586,LEN(H1586)-6)),\"\"))","v":""}]
[50001304,"SolarMax","MAX.STORAGE ULTIMATE 15",15,16.5,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1587,1)=\"J\",LEFT(H1587,2),LEFT(H1587,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1587,1)=\"J\",RIGHT(H1587,LEN(H1587)-4),RIGHT(H1587,LEN(H1587)-6)),\"\"))","v":""}]
[50001305,"SolarMax","17SHT",17,18.7,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,"Prüfbericht von Kostal Piko IQ 4.2",null,{"$f":"IF(LEFT(H1588,1)=\"J\",LEFT(H1588,2),LEFT(H1588,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1588,1)=\"J\",RIGHT(H1588,LEN(H1588)-4),RIGHT(H1588,LEN(H1588)-6)),\"\"))","v":""}]
[50001306,"SolarMax","20SHT",20,22,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,"Prüfbericht von Kostal Piko IQ 8.5",null,{"$f":"IF(LEFT(H1589,1)=\"J\",LEFT(H1589,2),LEFT(H1589,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1589,1)=\"J\",RIGHT(H1589,LEN(H1589)-4),RIGHT(H1589,LEN(H1589)-6)),\"\"))","v":""}]
[50001307,"SolarMax","22SHT",22,24.2,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1590,1)=\"J\",LEFT(H1590,2),LEFT(H1590,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1590,1)=\"J\",RIGHT(H1590,LEN(H1590)-4),RIGHT(H1590,LEN(H1590)-6)),\"\"))","v":""}]
[50001308,"SolarMax","25SHT",25,27.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1591,1)=\"J\",LEFT(H1591,2),LEFT(H1591,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1591,1)=\"J\",RIGHT(H1591,LEN(H1591)-4),RIGHT(H1591,LEN(H1591)-6)),\"\"))","v":""}]
[50001309,"SolarMax","30SHT-S",30,30,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1592,1)=\"J\",LEFT(H1592,2),LEFT(H1592,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1592,1)=\"J\",RIGHT(H1592,LEN(H1592)-4),RIGHT(H1592,LEN(H1592)-6)),\"\"))","v":""}]
[50001310,"SolarMax","28SHT",28,30.8,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1593,1)=\"J\",LEFT(H1593,2),LEFT(H1593,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1593,1)=\"J\",RIGHT(H1593,LEN(H1593)-4),RIGHT(H1593,LEN(H1593)-6)),\"\"))","v":""}]
[50001311,"SolarMax","30SHT",30,33,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1594,1)=\"J\",LEFT(H1594,2),LEFT(H1594,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1594,1)=\"J\",RIGHT(H1594,LEN(H1594)-4),RIGHT(H1594,LEN(H1594)-6)),\"\"))","v":""}]
[50001312,"SolarMax","35SHT",35,35,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1595,1)=\"J\",LEFT(H1595,2),LEFT(H1595,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1595,1)=\"J\",RIGHT(H1595,LEN(H1595)-4),RIGHT(H1595,LEN(H1595)-6)),\"\"))","v":""}]
[50001313,"SolarMax","35SHT-S",35,35,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1596,1)=\"J\",LEFT(H1596,2),LEFT(H1596,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1596,1)=\"J\",RIGHT(H1596,LEN(H1596)-4),RIGHT(H1596,LEN(H1596)-6)),\"\"))","v":""}]
[50001314,"SolarMax","50SHT",55,55,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1597,1)=\"J\",LEFT(H1597,2),LEFT(H1597,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1597,1)=\"J\",RIGHT(H1597,LEN(H1597)-4),RIGHT(H1597,LEN(H1597)-6)),\"\"))","v":""}]
[50001315,"SolarMax","50SHT-S",50,55,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1598,1)=\"J\",LEFT(H1598,2),LEFT(H1598,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1598,1)=\"J\",RIGHT(H1598,LEN(H1598)-4),RIGHT(H1598,LEN(H1598)-6)),\"\"))","v":""}]
[50001316,"SolarMax","60SHT",66,66,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1599,1)=\"J\",LEFT(H1599,2),LEFT(H1599,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1599,1)=\"J\",RIGHT(H1599,LEN(H1599)-4),RIGHT(H1599,LEN(H1599)-6)),\"\"))","v":""}]
[50001317,"SolarMax","60SHT-S",60,66,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1600,1)=\"J\",LEFT(H1600,2),LEFT(H1600,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1600,1)=\"J\",RIGHT(H1600,LEN(H1600)-4),RIGHT(H1600,LEN(H1600)-6)),\"\"))","v":""}]
[50001318,"SolarMax","110SXT",110,121,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1601,1)=\"J\",LEFT(H1601,2),LEFT(H1601,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1601,1)=\"J\",RIGHT(H1601,LEN(H1601)-4),RIGHT(H1601,LEN(H1601)-6)),\"\"))","v":""}]
[50002145,"Solarnative","PSB-350-10",0.35,0.35,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-04-23","Martin Bertsch","2024-04-23",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"DE243C0M 001","2024-04-10","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1602,1)=\"J\",LEFT(H1602,2),LEFT(H1602,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1602,1)=\"J\",RIGHT(H1602,LEN(H1602)-4),RIGHT(H1602,LEN(H1602)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001319,"Solarwatt","Battery flex base AC-1 1.3",6,6,1,"AC-Batteriewechselrichter","Ja","2022-07-26","Christian Elbs","2022-07-26",null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"DE219P21 001","2021-11-09",null,"OK",null,"Vorhanden",null,null,"Schieflastüberwachung wurde zusätzlich überprüft und nachgewiesen. Netzwirksame Leistung 0, da Batteriewechselrichter.",null,null,null,null,{"$f":"IF(LEFT(H1603,1)=\"J\",LEFT(H1603,2),LEFT(H1603,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1603,1)=\"J\",RIGHT(H1603,LEN(H1603)-4),RIGHT(H1603,LEN(H1603)-6)),\"\"))","v":""}]
[50001320,"Solax Power","X1-0,6-S-D(L)",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1604,1)=\"J\",LEFT(H1604,2),LEFT(H1604,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1604,1)=\"J\",RIGHT(H1604,LEN(H1604)-4),RIGHT(H1604,LEN(H1604)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001321,"Solax Power","X1-0,6-S-N(L)",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1605,1)=\"J\",LEFT(H1605,2),LEFT(H1605,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1605,1)=\"J\",RIGHT(H1605,LEN(H1605)-4),RIGHT(H1605,LEN(H1605)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002121,"Solax Power","X1-MINI-0.6K-G4",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1606,1)=\"J\",LEFT(H1606,2),LEFT(H1606,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1606,1)=\"J\",RIGHT(H1606,LEN(H1606)-4),RIGHT(H1606,LEN(H1606)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001322,"Solax Power","X1-0.7-S-D(L)",0.7,0.77,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1607,1)=\"J\",LEFT(H1607,2),LEFT(H1607,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1607,1)=\"J\",RIGHT(H1607,LEN(H1607)-4),RIGHT(H1607,LEN(H1607)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001323,"Solax Power","X1-0.7-S-N(L)",0.7,0.77,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1608,1)=\"J\",LEFT(H1608,2),LEFT(H1608,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1608,1)=\"J\",RIGHT(H1608,LEN(H1608)-4),RIGHT(H1608,LEN(H1608)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002122,"Solax Power","X1-MINI-0.7K-G4",0.7,0.77,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1609,1)=\"J\",LEFT(H1609,2),LEFT(H1609,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1609,1)=\"J\",RIGHT(H1609,LEN(H1609)-4),RIGHT(H1609,LEN(H1609)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002123,"Solax Power","X1-MINI-0.8K-G4",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1610,1)=\"J\",LEFT(H1610,2),LEFT(H1610,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1610,1)=\"J\",RIGHT(H1610,LEN(H1610)-4),RIGHT(H1610,LEN(H1610)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001324,"Solax Power","X1-1.1-S-D(L)",1.1000000000000001,1.21,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1611,1)=\"J\",LEFT(H1611,2),LEFT(H1611,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1611,1)=\"J\",RIGHT(H1611,LEN(H1611)-4),RIGHT(H1611,LEN(H1611)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001325,"Solax Power","X1-1.1-S-N(L)",1.1000000000000001,1.21,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1612,1)=\"J\",LEFT(H1612,2),LEFT(H1612,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1612,1)=\"J\",RIGHT(H1612,LEN(H1612)-4),RIGHT(H1612,LEN(H1612)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002124,"Solax Power","X1-MINI-1.1K-G4",1.1000000000000001,1.21,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1613,1)=\"J\",LEFT(H1613,2),LEFT(H1613,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1613,1)=\"J\",RIGHT(H1613,LEN(H1613)-4),RIGHT(H1613,LEN(H1613)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001326,"Solax Power","X1-1.5-S-D(L)",1.5,1.65,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1614,1)=\"J\",LEFT(H1614,2),LEFT(H1614,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1614,1)=\"J\",RIGHT(H1614,LEN(H1614)-4),RIGHT(H1614,LEN(H1614)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001327,"Solax Power","X1-1.5-S-N(L)",1.5,1.65,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1615,1)=\"J\",LEFT(H1615,2),LEFT(H1615,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1615,1)=\"J\",RIGHT(H1615,LEN(H1615)-4),RIGHT(H1615,LEN(H1615)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002125,"Solax Power","X1-MINI-1.5K-G4",1.5,1.65,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1616,1)=\"J\",LEFT(H1616,2),LEFT(H1616,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1616,1)=\"J\",RIGHT(H1616,LEN(H1616)-4),RIGHT(H1616,LEN(H1616)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001328,"Solax Power","X1-2.0-S-D(L)",2,2.2000000000000002,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1617,1)=\"J\",LEFT(H1617,2),LEFT(H1617,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1617,1)=\"J\",RIGHT(H1617,LEN(H1617)-4),RIGHT(H1617,LEN(H1617)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001329,"Solax Power","X1-2.0-S-N(L)",2,2.2000000000000002,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25 ","F","F",null,null,{"$f":"IF(LEFT(H1618,1)=\"J\",LEFT(H1618,2),LEFT(H1618,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1618,1)=\"J\",RIGHT(H1618,LEN(H1618)-4),RIGHT(H1618,LEN(H1618)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002126,"Solax Power","X1-MINI-2.0K-G4",2,2.2000000000000002,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1619,1)=\"J\",LEFT(H1619,2),LEFT(H1619,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1619,1)=\"J\",RIGHT(H1619,LEN(H1619)-4),RIGHT(H1619,LEN(H1619)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001330,"Solax Power","X1 AIR X1-2.5-S ",2.5,2.75,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,60408611001,"2020-08-14",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1620,1)=\"J\",LEFT(H1620,2),LEFT(H1620,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1620,1)=\"J\",RIGHT(H1620,LEN(H1620)-4),RIGHT(H1620,LEN(H1620)-6)),\"\"))","v":""}]
[50001331,"Solax Power","X1-2.5K-S-D(L)",2.5,2.75,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1621,1)=\"J\",LEFT(H1621,2),LEFT(H1621,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1621,1)=\"J\",RIGHT(H1621,LEN(H1621)-4),RIGHT(H1621,LEN(H1621)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001332,"Solax Power","X1-2.5K-S-N(L)",2.5,2.75,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1622,1)=\"J\",LEFT(H1622,2),LEFT(H1622,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1622,1)=\"J\",RIGHT(H1622,LEN(H1622)-4),RIGHT(H1622,LEN(H1622)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002032,"Solax Power","X1-BOOST-2.5K-G4",2.5,2.75,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23YAC2 001","2023-11-21",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1623,1)=\"J\",LEFT(H1623,2),LEFT(H1623,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1623,1)=\"J\",RIGHT(H1623,LEN(H1623)-4),RIGHT(H1623,LEN(H1623)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002127,"Solax Power","X1-MINI-2.5K-G4",2.5,2.75,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1624,1)=\"J\",LEFT(H1624,2),LEFT(H1624,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1624,1)=\"J\",RIGHT(H1624,LEN(H1624)-4),RIGHT(H1624,LEN(H1624)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001970,"Solax Power","X3-MIC-3K-G2",3,3,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 001","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1625,1)=\"J\",LEFT(H1625,2),LEFT(H1625,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1625,1)=\"J\",RIGHT(H1625,LEN(H1625)-4),RIGHT(H1625,LEN(H1625)-6)),\"\"))","v":""}]
[50001335,"Solax Power","X1 AIR X1-3.0-S ",3.3,3.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,60408611001,"2020-08-14",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1626,1)=\"J\",LEFT(H1626,2),LEFT(H1626,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1626,1)=\"J\",RIGHT(H1626,LEN(H1626)-4),RIGHT(H1626,LEN(H1626)-6)),\"\"))","v":""}]
[50001333,"Solax Power","X1 BOOST X1-3.0-T ",3,3.3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,60408586001,"2020-08-14",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1627,1)=\"J\",LEFT(H1627,2),LEFT(H1627,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1627,1)=\"J\",RIGHT(H1627,LEN(H1627)-4),RIGHT(H1627,LEN(H1627)-6)),\"\"))","v":""}]
[50001336,"Solax Power","X1-3.0K-S-D(L)",3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1628,1)=\"J\",LEFT(H1628,2),LEFT(H1628,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1628,1)=\"J\",RIGHT(H1628,LEN(H1628)-4),RIGHT(H1628,LEN(H1628)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001337,"Solax Power","X1-3.0K-S-N(L)",3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1629,1)=\"J\",LEFT(H1629,2),LEFT(H1629,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1629,1)=\"J\",RIGHT(H1629,LEN(H1629)-4),RIGHT(H1629,LEN(H1629)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001338,"Solax Power","X1-3.3K-S-D(L)",3.3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1630,1)=\"J\",LEFT(H1630,2),LEFT(H1630,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1630,1)=\"J\",RIGHT(H1630,LEN(H1630)-4),RIGHT(H1630,LEN(H1630)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001339,"Solax Power","X1-3.3K-S-N(L)",3.3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1631,1)=\"J\",LEFT(H1631,2),LEFT(H1631,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1631,1)=\"J\",RIGHT(H1631,LEN(H1631)-4),RIGHT(H1631,LEN(H1631)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001334,"Solax Power","X1-AC-3.0",3.3,3.3,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1632,1)=\"J\",LEFT(H1632,2),LEFT(H1632,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1632,1)=\"J\",RIGHT(H1632,LEN(H1632)-4),RIGHT(H1632,LEN(H1632)-6)),\"\"))","v":""}]
[50002033,"Solax Power","X1-BOOST-3K-G4",3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23YAC2 001","2023-11-21",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1633,1)=\"J\",LEFT(H1633,2),LEFT(H1633,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1633,1)=\"J\",RIGHT(H1633,LEN(H1633)-4),RIGHT(H1633,LEN(H1633)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001340,"Solax Power","X1-HYBRID-3.0T ",3.3,3.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1634,1)=\"J\",LEFT(H1634,2),LEFT(H1634,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1634,1)=\"J\",RIGHT(H1634,LEN(H1634)-4),RIGHT(H1634,LEN(H1634)-6)),\"\"))","v":""}]
[50001341,"Solax Power","X1-HYBRID-G4-3.0-D/M",3,3.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1635,1)=\"J\",LEFT(H1635,2),LEFT(H1635,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1635,1)=\"J\",RIGHT(H1635,LEN(H1635)-4),RIGHT(H1635,LEN(H1635)-6)),\"\"))","v":""}]
[50002128,"Solax Power","X1-MINI-3.0K-G4",3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1636,1)=\"J\",LEFT(H1636,2),LEFT(H1636,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1636,1)=\"J\",RIGHT(H1636,LEN(H1636)-4),RIGHT(H1636,LEN(H1636)-6)),\"\"))","v":"<= 16A Anlage"}]
[50002129,"Solax Power","X1-MINI-3.3K-G4",3.3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-04-15","Martin Bertsch","2024-04-15",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1637,1)=\"J\",LEFT(H1637,2),LEFT(H1637,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1637,1)=\"J\",RIGHT(H1637,LEN(H1637)-4),RIGHT(H1637,LEN(H1637)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001342,"Solax Power","X1 AIR X1-3.3-S ",3.3,3.63,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,60408611001,"2020-08-14",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1638,1)=\"J\",LEFT(H1638,2),LEFT(H1638,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1638,1)=\"J\",RIGHT(H1638,LEN(H1638)-4),RIGHT(H1638,LEN(H1638)-6)),\"\"))","v":""}]
[50001343,"Solax Power","X1 BOOST X1-3.3-T ",3.3,3.63,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,60408586001,"2020-08-14",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1639,1)=\"J\",LEFT(H1639,2),LEFT(H1639,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1639,1)=\"J\",RIGHT(H1639,LEN(H1639)-4),RIGHT(H1639,LEN(H1639)-6)),\"\"))","v":""}]
[50002034,"Solax Power","X1-BOOST-3.3K-G4",3.3,3.63,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23YAC2 001","2023-11-21",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1640,1)=\"J\",LEFT(H1640,2),LEFT(H1640,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1640,1)=\"J\",RIGHT(H1640,LEN(H1640)-4),RIGHT(H1640,LEN(H1640)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001344,"Solax Power","X1 BOOST X1-3.6-T ",3.68,3.68,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,60408586001,"2020-08-14",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1641,1)=\"J\",LEFT(H1641,2),LEFT(H1641,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1641,1)=\"J\",RIGHT(H1641,LEN(H1641)-4),RIGHT(H1641,LEN(H1641)-6)),\"\"))","v":""}]
[50001345,"Solax Power","X1-3.6K-S-D(L)",3.68,3.68,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1642,1)=\"J\",LEFT(H1642,2),LEFT(H1642,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1642,1)=\"J\",RIGHT(H1642,LEN(H1642)-4),RIGHT(H1642,LEN(H1642)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001346,"Solax Power","X1-3.6K-S-N(L)",3.68,3.68,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-12","Martin Bertsch","2022-10-24",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 002","2023-03-01","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1643,1)=\"J\",LEFT(H1643,2),LEFT(H1643,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1643,1)=\"J\",RIGHT(H1643,LEN(H1643)-4),RIGHT(H1643,LEN(H1643)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001347,"Solax Power","X1-AC-3.6",3.68,3.68,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1644,1)=\"J\",LEFT(H1644,2),LEFT(H1644,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1644,1)=\"J\",RIGHT(H1644,LEN(H1644)-4),RIGHT(H1644,LEN(H1644)-6)),\"\"))","v":""}]
[50002035,"Solax Power","X1-BOOST-3.6K-G4",3.68,3.68,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-01-03","Martin Bertsch","2024-01-03",null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23YAC2 001","2023-11-21",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1645,1)=\"J\",LEFT(H1645,2),LEFT(H1645,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1645,1)=\"J\",RIGHT(H1645,LEN(H1645)-4),RIGHT(H1645,LEN(H1645)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001348,"Solax Power","X1-FIT-3.7T",3.68,3.68,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1646,1)=\"J\",LEFT(H1646,2),LEFT(H1646,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1646,1)=\"J\",RIGHT(H1646,LEN(H1646)-4),RIGHT(H1646,LEN(H1646)-6)),\"\"))","v":""}]
[50001349,"Solax Power","X1-HYBRID-3.7T ",3.68,3.68,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1647,1)=\"J\",LEFT(H1647,2),LEFT(H1647,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1647,1)=\"J\",RIGHT(H1647,LEN(H1647)-4),RIGHT(H1647,LEN(H1647)-6)),\"\"))","v":""}]
[50001350,"Solax Power","X1-HYBRID-G4-3.7-D/M",3.68,3.68,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1648,1)=\"J\",LEFT(H1648,2),LEFT(H1648,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1648,1)=\"J\",RIGHT(H1648,LEN(H1648)-4),RIGHT(H1648,LEN(H1648)-6)),\"\"))","v":""}]
[50002290,"Solax Power","X3-IES-4K",4,4,3,"Hybrid-Wechselrichter","Ja","2024-06-04","Martin Bertsch","2024-06-04",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN2488CO 001","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1649,1)=\"J\",LEFT(H1649,2),LEFT(H1649,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1649,1)=\"J\",RIGHT(H1649,LEN(H1649)-4),RIGHT(H1649,LEN(H1649)-6)),\"\"))","v":""}]
[50001351,"Solax Power","X3-MIC-4K-G2",4,4,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 001","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1650,1)=\"J\",LEFT(H1650,2),LEFT(H1650,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1650,1)=\"J\",RIGHT(H1650,LEN(H1650)-4),RIGHT(H1650,LEN(H1650)-6)),\"\"))","v":""}]
[50002130,"Solax Power","X1-MINI-3.7K-G4",3.7,4.07,1,"PV-Wechselrichter","Nein","2024-04-15","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1651,1)=\"J\",LEFT(H1651,2),LEFT(H1651,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1651,1)=\"J\",RIGHT(H1651,LEN(H1651)-4),RIGHT(H1651,LEN(H1651)-6)),\"\"))","v":""}]
[50002131,"Solax Power","X1-MINI-4.0K-G4",4,4.4000000000000004,1,"PV-Wechselrichter","Nein","2024-04-15","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24RFBC 001","2024-03-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1652,1)=\"J\",LEFT(H1652,2),LEFT(H1652,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1652,1)=\"J\",RIGHT(H1652,LEN(H1652)-4),RIGHT(H1652,LEN(H1652)-6)),\"\"))","v":""}]
[50001352,"Solax Power","X3-MIC-4.0-S",null,4.4000000000000004,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1653,1)=\"J\",LEFT(H1653,2),LEFT(H1653,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1653,1)=\"J\",RIGHT(H1653,LEN(H1653)-4),RIGHT(H1653,LEN(H1653)-6)),\"\"))","v":""}]
[50001353,"Solax Power","X3-MIC-4.0-T",null,4.4000000000000004,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1654,1)=\"J\",LEFT(H1654,2),LEFT(H1654,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1654,1)=\"J\",RIGHT(H1654,LEN(H1654)-4),RIGHT(H1654,LEN(H1654)-6)),\"\"))","v":""}]
[50001354,"Solax Power","X1-AC-4.6",null,4.5999999999999996,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1655,1)=\"J\",LEFT(H1655,2),LEFT(H1655,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1655,1)=\"J\",RIGHT(H1655,LEN(H1655)-4),RIGHT(H1655,LEN(H1655)-6)),\"\"))","v":""}]
[50001355,"Solax Power","X1-FIT-4.6T",null,4.5999999999999996,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1656,1)=\"J\",LEFT(H1656,2),LEFT(H1656,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1656,1)=\"J\",RIGHT(H1656,LEN(H1656)-4),RIGHT(H1656,LEN(H1656)-6)),\"\"))","v":""}]
[50001356,"Solax Power","X1-HYBRID-5.0T ",null,4.5999999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 1~ - nur 3~ Anschluss gestattet - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1657,1)=\"J\",LEFT(H1657,2),LEFT(H1657,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1657,1)=\"J\",RIGHT(H1657,LEN(H1657)-4),RIGHT(H1657,LEN(H1657)-6)),\"\"))","v":""}]
[50001357,"Solax Power","X1 BOOST X1-4.2-T ",4.2,4.62,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,60408586001,"2020-08-14",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ nur 3~ Anschluss gestattet - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1658,1)=\"J\",LEFT(H1658,2),LEFT(H1658,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1658,1)=\"J\",RIGHT(H1658,LEN(H1658)-4),RIGHT(H1658,LEN(H1658)-6)),\"\"))","v":""}]
[50001358,"Solax Power","X1-AC-5.0",null,5,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1659,1)=\"J\",LEFT(H1659,2),LEFT(H1659,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1659,1)=\"J\",RIGHT(H1659,LEN(H1659)-4),RIGHT(H1659,LEN(H1659)-6)),\"\"))","v":""}]
[50001359,"Solax Power","X1-FIT-5.0T",null,5,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1660,1)=\"J\",LEFT(H1660,2),LEFT(H1660,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1660,1)=\"J\",RIGHT(H1660,LEN(H1660)-4),RIGHT(H1660,LEN(H1660)-6)),\"\"))","v":""}]
[50001360,"Solax Power","X3-Hybrid-5.0-D-C",5,5,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1661,1)=\"J\",LEFT(H1661,2),LEFT(H1661,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1661,1)=\"J\",RIGHT(H1661,LEN(H1661)-4),RIGHT(H1661,LEN(H1661)-6)),\"\"))","v":""}]
[50001361,"Solax Power","X3-Hybrid-5.0-D-E ( E = mit EPS)",5,5,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1662,1)=\"J\",LEFT(H1662,2),LEFT(H1662,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1662,1)=\"J\",RIGHT(H1662,LEN(H1662)-4),RIGHT(H1662,LEN(H1662)-6)),\"\"))","v":""}]
[50001362,"Solax Power","X3-Hybrid-5.0-N-C",5,5,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1663,1)=\"J\",LEFT(H1663,2),LEFT(H1663,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1663,1)=\"J\",RIGHT(H1663,LEN(H1663)-4),RIGHT(H1663,LEN(H1663)-6)),\"\"))","v":""}]
[50001363,"Solax Power","X3-Hybrid-5.0-N-E",5,5,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1664,1)=\"J\",LEFT(H1664,2),LEFT(H1664,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1664,1)=\"J\",RIGHT(H1664,LEN(H1664)-4),RIGHT(H1664,LEN(H1664)-6)),\"\"))","v":""}]
[50001364,"Solax Power","X3-Hybrid-5.0T ",null,5,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1665,1)=\"J\",LEFT(H1665,2),LEFT(H1665,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1665,1)=\"J\",RIGHT(H1665,LEN(H1665)-4),RIGHT(H1665,LEN(H1665)-6)),\"\"))","v":""}]
[50001365,"Solax Power","X3-MIC-5K-G2",5,5,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 001","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1666,1)=\"J\",LEFT(H1666,2),LEFT(H1666,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1666,1)=\"J\",RIGHT(H1666,LEN(H1666)-4),RIGHT(H1666,LEN(H1666)-6)),\"\"))","v":""}]
[50001366,"Solax Power","X1 BOOST X1-4.6-T ",4.5999999999999996,5.0599999999999996,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,60408586001,"2020-08-14",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ nur 3~ Anschluss gestattet - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1667,1)=\"J\",LEFT(H1667,2),LEFT(H1667,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1667,1)=\"J\",RIGHT(H1667,LEN(H1667)-4),RIGHT(H1667,LEN(H1667)-6)),\"\"))","v":""}]
[50001367,"Solax Power","X1-HYBRID-4.6T ",null,5.0599999999999996,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 1~ - nur 3~ Anschluss gestattet - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1668,1)=\"J\",LEFT(H1668,2),LEFT(H1668,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1668,1)=\"J\",RIGHT(H1668,LEN(H1668)-4),RIGHT(H1668,LEN(H1668)-6)),\"\"))","v":""}]
[50001368,"Solax Power","X1 BOOST X1-5.0-T ",null,5.5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,60408586001,"2020-08-14",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ nur 3~ Anschluss gestattet - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1669,1)=\"J\",LEFT(H1669,2),LEFT(H1669,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1669,1)=\"J\",RIGHT(H1669,LEN(H1669)-4),RIGHT(H1669,LEN(H1669)-6)),\"\"))","v":""}]
[50001369,"Solax Power","X1-HYBRID-G4-5.0-D/M",5,5.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1670,1)=\"J\",LEFT(H1670,2),LEFT(H1670,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1670,1)=\"J\",RIGHT(H1670,LEN(H1670)-4),RIGHT(H1670,LEN(H1670)-6)),\"\"))","v":""}]
[50001370,"Solax Power","X3-HYBRID-G4-5.0-D/M",5,5.5,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 001","2021-07-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1671,1)=\"J\",LEFT(H1671,2),LEFT(H1671,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1671,1)=\"J\",RIGHT(H1671,LEN(H1671)-4),RIGHT(H1671,LEN(H1671)-6)),\"\"))","v":""}]
[50002284,"Solax Power","X3-IES-5K",5,5.5,3,"Hybrid-Wechselrichter","Ja","2024-06-04","Martin Bertsch","2024-06-04",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN2488CO 001","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1672,1)=\"J\",LEFT(H1672,2),LEFT(H1672,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1672,1)=\"J\",RIGHT(H1672,LEN(H1672)-4),RIGHT(H1672,LEN(H1672)-6)),\"\"))","v":""}]
[50001371,"Solax Power","X3-MIC-5.0-S",null,5.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1673,1)=\"J\",LEFT(H1673,2),LEFT(H1673,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1673,1)=\"J\",RIGHT(H1673,LEN(H1673)-4),RIGHT(H1673,LEN(H1673)-6)),\"\"))","v":""}]
[50001372,"Solax Power","X3-MIC-5.0-T",null,5.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1674,1)=\"J\",LEFT(H1674,2),LEFT(H1674,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1674,1)=\"J\",RIGHT(H1674,LEN(H1674)-4),RIGHT(H1674,LEN(H1674)-6)),\"\"))","v":""}]
[50001373,"Solax Power","X1-SMART-6.0-T",6,6,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1675,1)=\"J\",LEFT(H1675,2),LEFT(H1675,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1675,1)=\"J\",RIGHT(H1675,LEN(H1675)-4),RIGHT(H1675,LEN(H1675)-6)),\"\"))","v":""}]
[50001374,"Solax Power","X3-Hybrid-6.0-D-C",6,6,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1676,1)=\"J\",LEFT(H1676,2),LEFT(H1676,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1676,1)=\"J\",RIGHT(H1676,LEN(H1676)-4),RIGHT(H1676,LEN(H1676)-6)),\"\"))","v":""}]
[50001375,"Solax Power","X3-Hybrid-6.0-D-E",6,6,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1677,1)=\"J\",LEFT(H1677,2),LEFT(H1677,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1677,1)=\"J\",RIGHT(H1677,LEN(H1677)-4),RIGHT(H1677,LEN(H1677)-6)),\"\"))","v":""}]
[50001376,"Solax Power","X3-Hybrid-6.0-N-C",6,6,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1678,1)=\"J\",LEFT(H1678,2),LEFT(H1678,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1678,1)=\"J\",RIGHT(H1678,LEN(H1678)-4),RIGHT(H1678,LEN(H1678)-6)),\"\"))","v":""}]
[50001377,"Solax Power","X3-Hybrid-6.0-N-E",6,6,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1679,1)=\"J\",LEFT(H1679,2),LEFT(H1679,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1679,1)=\"J\",RIGHT(H1679,LEN(H1679)-4),RIGHT(H1679,LEN(H1679)-6)),\"\"))","v":""}]
[50001378,"Solax Power","X3-Hybrid-6.0T ",null,6,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1680,1)=\"J\",LEFT(H1680,2),LEFT(H1680,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1680,1)=\"J\",RIGHT(H1680,LEN(H1680)-4),RIGHT(H1680,LEN(H1680)-6)),\"\"))","v":""}]
[50001379,"Solax Power","X3-MIC-6K-G2",6,6,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 001","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1681,1)=\"J\",LEFT(H1681,2),LEFT(H1681,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1681,1)=\"J\",RIGHT(H1681,LEN(H1681)-4),RIGHT(H1681,LEN(H1681)-6)),\"\"))","v":""}]
[50001380,"Solax Power","X1 BOOST X1-5.5K-T ",5.5,6.05,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ nur 3~ Anschluss gestattet - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1682,1)=\"J\",LEFT(H1682,2),LEFT(H1682,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1682,1)=\"J\",RIGHT(H1682,LEN(H1682)-4),RIGHT(H1682,LEN(H1682)-6)),\"\"))","v":""}]
[50001381,"Solax Power","X1 BOOST X1-6K-T ",6,6.6,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ nur 3~ Anschluss gestattet - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1683,1)=\"J\",LEFT(H1683,2),LEFT(H1683,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1683,1)=\"J\",RIGHT(H1683,LEN(H1683)-4),RIGHT(H1683,LEN(H1683)-6)),\"\"))","v":""}]
[50001382,"Solax Power","X1-HYBRID-G4-6.0-D/M",6,6.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1684,1)=\"J\",LEFT(H1684,2),LEFT(H1684,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1684,1)=\"J\",RIGHT(H1684,LEN(H1684)-4),RIGHT(H1684,LEN(H1684)-6)),\"\"))","v":""}]
[50001383,"Solax Power","X3-Fit-G4-6.0-M/W",6,6.6,3,"AC-Batteriewechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2182YH 001","2021-07-19",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H1685,1)=\"J\",LEFT(H1685,2),LEFT(H1685,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1685,1)=\"J\",RIGHT(H1685,LEN(H1685)-4),RIGHT(H1685,LEN(H1685)-6)),\"\"))","v":""}]
[50001384,"Solax Power","X3-HYBRID-G4-6.0-D/M",6,6.6,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 001","2021-07-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1686,1)=\"J\",LEFT(H1686,2),LEFT(H1686,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1686,1)=\"J\",RIGHT(H1686,LEN(H1686)-4),RIGHT(H1686,LEN(H1686)-6)),\"\"))","v":""}]
[50002285,"Solax Power","X3-IES-6K",6,6.6,3,"Hybrid-Wechselrichter","Ja","2024-06-04","Martin Bertsch","2024-06-04",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN2488CO 001","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1687,1)=\"J\",LEFT(H1687,2),LEFT(H1687,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1687,1)=\"J\",RIGHT(H1687,LEN(H1687)-4),RIGHT(H1687,LEN(H1687)-6)),\"\"))","v":""}]
[50001385,"Solax Power","X3-MIC-6.0-T",null,6.6,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1688,1)=\"J\",LEFT(H1688,2),LEFT(H1688,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1688,1)=\"J\",RIGHT(H1688,LEN(H1688)-4),RIGHT(H1688,LEN(H1688)-6)),\"\"))","v":""}]
[50001386,"Solax Power","X1-SMART-7.0-T",7,7,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1689,1)=\"J\",LEFT(H1689,2),LEFT(H1689,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1689,1)=\"J\",RIGHT(H1689,LEN(H1689)-4),RIGHT(H1689,LEN(H1689)-6)),\"\"))","v":""}]
[50001387,"Solax Power","X1-HYBRID-G4-7.5-D/M",7.5,7.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1690,1)=\"J\",LEFT(H1690,2),LEFT(H1690,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1690,1)=\"J\",RIGHT(H1690,LEN(H1690)-4),RIGHT(H1690,LEN(H1690)-6)),\"\"))","v":""}]
[50001388,"Solax Power","X3-MIC-7.0-T",null,7.7,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1691,1)=\"J\",LEFT(H1691,2),LEFT(H1691,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1691,1)=\"J\",RIGHT(H1691,LEN(H1691)-4),RIGHT(H1691,LEN(H1691)-6)),\"\"))","v":""}]
[50001389,"Solax Power","X1-SMART-8.0-T",8,8,1,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1692,1)=\"J\",LEFT(H1692,2),LEFT(H1692,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1692,1)=\"J\",RIGHT(H1692,LEN(H1692)-4),RIGHT(H1692,LEN(H1692)-6)),\"\"))","v":""}]
[50001390,"Solax Power","X3-Fit-8.0C",8,8,3,"AC-Batteriewechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1693,1)=\"J\",LEFT(H1693,2),LEFT(H1693,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1693,1)=\"J\",RIGHT(H1693,LEN(H1693)-4),RIGHT(H1693,LEN(H1693)-6)),\"\"))","v":""}]
[50001391,"Solax Power","X3-Fit-8.0E",8,8,3,"AC-Batteriewechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1694,1)=\"J\",LEFT(H1694,2),LEFT(H1694,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1694,1)=\"J\",RIGHT(H1694,LEN(H1694)-4),RIGHT(H1694,LEN(H1694)-6)),\"\"))","v":""}]
[50001392,"Solax Power","X3-Hybrid-8.0-D-C",8,8,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1695,1)=\"J\",LEFT(H1695,2),LEFT(H1695,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1695,1)=\"J\",RIGHT(H1695,LEN(H1695)-4),RIGHT(H1695,LEN(H1695)-6)),\"\"))","v":""}]
[50001393,"Solax Power","X3-Hybrid-8.0-D-E",8,8,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1696,1)=\"J\",LEFT(H1696,2),LEFT(H1696,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1696,1)=\"J\",RIGHT(H1696,LEN(H1696)-4),RIGHT(H1696,LEN(H1696)-6)),\"\"))","v":""}]
[50001394,"Solax Power","X3-Hybrid-8.0-N-C",8,8,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1697,1)=\"J\",LEFT(H1697,2),LEFT(H1697,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1697,1)=\"J\",RIGHT(H1697,LEN(H1697)-4),RIGHT(H1697,LEN(H1697)-6)),\"\"))","v":""}]
[50001395,"Solax Power","X3-Hybrid-8.0-N-E",8,8,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1698,1)=\"J\",LEFT(H1698,2),LEFT(H1698,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1698,1)=\"J\",RIGHT(H1698,LEN(H1698)-4),RIGHT(H1698,LEN(H1698)-6)),\"\"))","v":""}]
[50001396,"Solax Power","X3-Hybrid-8.0T ",null,8,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1699,1)=\"J\",LEFT(H1699,2),LEFT(H1699,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1699,1)=\"J\",RIGHT(H1699,LEN(H1699)-4),RIGHT(H1699,LEN(H1699)-6)),\"\"))","v":""}]
[50001397,"Solax Power","X3-MIC-8K-G2",8,8,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 001","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1700,1)=\"J\",LEFT(H1700,2),LEFT(H1700,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1700,1)=\"J\",RIGHT(H1700,LEN(H1700)-4),RIGHT(H1700,LEN(H1700)-6)),\"\"))","v":""}]
[50001398,"Solax Power","X3-Fit-8.0T ",null,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1701,1)=\"J\",LEFT(H1701,2),LEFT(H1701,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1701,1)=\"J\",RIGHT(H1701,LEN(H1701)-4),RIGHT(H1701,LEN(H1701)-6)),\"\"))","v":""}]
[50001399,"Solax Power","X3-Fit-G4-8.0-M/W",8,8.8000000000000007,3,"AC-Batteriewechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2182YH 001","2021-07-19",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H1702,1)=\"J\",LEFT(H1702,2),LEFT(H1702,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1702,1)=\"J\",RIGHT(H1702,LEN(H1702)-4),RIGHT(H1702,LEN(H1702)-6)),\"\"))","v":""}]
[50001400,"Solax Power","X3-HYBRID-G4-8.0-D/M",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 001","2021-07-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1703,1)=\"J\",LEFT(H1703,2),LEFT(H1703,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1703,1)=\"J\",RIGHT(H1703,LEN(H1703)-4),RIGHT(H1703,LEN(H1703)-6)),\"\"))","v":""}]
[50002286,"Solax Power","X3-IES-8K",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2024-06-04","Martin Bertsch","2024-06-04",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN2488CO 001","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1704,1)=\"J\",LEFT(H1704,2),LEFT(H1704,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1704,1)=\"J\",RIGHT(H1704,LEN(H1704)-4),RIGHT(H1704,LEN(H1704)-6)),\"\"))","v":""}]
[50001401,"Solax Power","X3-MIC-8.0-T",null,8.8000000000000007,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1705,1)=\"J\",LEFT(H1705,2),LEFT(H1705,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1705,1)=\"J\",RIGHT(H1705,LEN(H1705)-4),RIGHT(H1705,LEN(H1705)-6)),\"\"))","v":""}]
[50001402,"Solax Power","X3-PRO-8.0P",null,8.8000000000000007,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1706,1)=\"J\",LEFT(H1706,2),LEFT(H1706,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1706,1)=\"J\",RIGHT(H1706,LEN(H1706)-4),RIGHT(H1706,LEN(H1706)-6)),\"\"))","v":""}]
[50001403,"Solax Power","X3-PRO-8K-G2",8,8.8000000000000007,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2023-03-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN22J5CM 001","2023-07-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1707,1)=\"J\",LEFT(H1707,2),LEFT(H1707,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1707,1)=\"J\",RIGHT(H1707,LEN(H1707)-4),RIGHT(H1707,LEN(H1707)-6)),\"\"))","v":""}]
[50001404,"Solax Power","X3-MIC-9.0-T",null,9.9,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1708,1)=\"J\",LEFT(H1708,2),LEFT(H1708,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1708,1)=\"J\",RIGHT(H1708,LEN(H1708)-4),RIGHT(H1708,LEN(H1708)-6)),\"\"))","v":""}]
[50001405,"Solax Power","X3-Fit-10.0C",10,10,3,"AC-Batteriewechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1709,1)=\"J\",LEFT(H1709,2),LEFT(H1709,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1709,1)=\"J\",RIGHT(H1709,LEN(H1709)-4),RIGHT(H1709,LEN(H1709)-6)),\"\"))","v":""}]
[50001406,"Solax Power","X3-Fit-10.0E ",10,10,3,"AC-Batteriewechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1710,1)=\"J\",LEFT(H1710,2),LEFT(H1710,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1710,1)=\"J\",RIGHT(H1710,LEN(H1710)-4),RIGHT(H1710,LEN(H1710)-6)),\"\"))","v":""}]
[50001407,"Solax Power","X3-Hybrid-10.0-D-C",10,10,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1711,1)=\"J\",LEFT(H1711,2),LEFT(H1711,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1711,1)=\"J\",RIGHT(H1711,LEN(H1711)-4),RIGHT(H1711,LEN(H1711)-6)),\"\"))","v":""}]
[50001408,"Solax Power","X3-Hybrid-10.0-D-E",10,10,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1712,1)=\"J\",LEFT(H1712,2),LEFT(H1712,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1712,1)=\"J\",RIGHT(H1712,LEN(H1712)-4),RIGHT(H1712,LEN(H1712)-6)),\"\"))","v":""}]
[50001409,"Solax Power","X3-Hybrid-10.0-N-C",10,10,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1713,1)=\"J\",LEFT(H1713,2),LEFT(H1713,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1713,1)=\"J\",RIGHT(H1713,LEN(H1713)-4),RIGHT(H1713,LEN(H1713)-6)),\"\"))","v":""}]
[50001410,"Solax Power","X3-Hybrid-10.0-N-E",10,10,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,null,null,null,"Vorhanden",null,50368718002,"2020-03-06",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1714,1)=\"J\",LEFT(H1714,2),LEFT(H1714,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1714,1)=\"J\",RIGHT(H1714,LEN(H1714)-4),RIGHT(H1714,LEN(H1714)-6)),\"\"))","v":""}]
[50001411,"Solax Power","X3-Hybrid-10.0T ",null,10,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1715,1)=\"J\",LEFT(H1715,2),LEFT(H1715,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1715,1)=\"J\",RIGHT(H1715,LEN(H1715)-4),RIGHT(H1715,LEN(H1715)-6)),\"\"))","v":""}]
[50002287,"Solax Power","X3-IES-10K",10,10,3,"Hybrid-Wechselrichter","Ja","2024-06-04","Martin Bertsch","2024-06-04",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN2488CO 001","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1716,1)=\"J\",LEFT(H1716,2),LEFT(H1716,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1716,1)=\"J\",RIGHT(H1716,LEN(H1716)-4),RIGHT(H1716,LEN(H1716)-6)),\"\"))","v":""}]
[50001412,"Solax Power","X3-MIC-10K-G2",10,10,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 001","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1717,1)=\"J\",LEFT(H1717,2),LEFT(H1717,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1717,1)=\"J\",RIGHT(H1717,LEN(H1717)-4),RIGHT(H1717,LEN(H1717)-6)),\"\"))","v":""}]
[50001413,"Solax Power","X3-Fit-10.0T ",null,11,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1718,1)=\"J\",LEFT(H1718,2),LEFT(H1718,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1718,1)=\"J\",RIGHT(H1718,LEN(H1718)-4),RIGHT(H1718,LEN(H1718)-6)),\"\"))","v":""}]
[50001414,"Solax Power","X3-Fit-G4-10.0-M/W",10,11,3,"AC-Batteriewechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2182YH 001","2021-07-19",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H1719,1)=\"J\",LEFT(H1719,2),LEFT(H1719,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1719,1)=\"J\",RIGHT(H1719,LEN(H1719)-4),RIGHT(H1719,LEN(H1719)-6)),\"\"))","v":""}]
[50001415,"Solax Power","X3-HYBRID-G4-10.0-D/M",10,11,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 001","2021-07-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1720,1)=\"J\",LEFT(H1720,2),LEFT(H1720,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1720,1)=\"J\",RIGHT(H1720,LEN(H1720)-4),RIGHT(H1720,LEN(H1720)-6)),\"\"))","v":""}]
[50001416,"Solax Power","X3-MIC-10.0-T",null,11,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1721,1)=\"J\",LEFT(H1721,2),LEFT(H1721,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1721,1)=\"J\",RIGHT(H1721,LEN(H1721)-4),RIGHT(H1721,LEN(H1721)-6)),\"\"))","v":""}]
[50001417,"Solax Power","X3-PRO-10.0P",null,11,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1722,1)=\"J\",LEFT(H1722,2),LEFT(H1722,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1722,1)=\"J\",RIGHT(H1722,LEN(H1722)-4),RIGHT(H1722,LEN(H1722)-6)),\"\"))","v":""}]
[50001418,"Solax Power","X3-PRO-10K-G2",10,11,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2023-03-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN22J5CM 001","2023-07-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1723,1)=\"J\",LEFT(H1723,2),LEFT(H1723,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1723,1)=\"J\",RIGHT(H1723,LEN(H1723)-4),RIGHT(H1723,LEN(H1723)-6)),\"\"))","v":""}]
[50001419,"Solax Power","X3-MIC-12K-G2",12,12,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 001","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1724,1)=\"J\",LEFT(H1724,2),LEFT(H1724,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1724,1)=\"J\",RIGHT(H1724,LEN(H1724)-4),RIGHT(H1724,LEN(H1724)-6)),\"\"))","v":""}]
[50001420,"Solax Power","X3-HYBRID-G4-12.0-D/M",12,13.2,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 001","2021-07-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1725,1)=\"J\",LEFT(H1725,2),LEFT(H1725,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1725,1)=\"J\",RIGHT(H1725,LEN(H1725)-4),RIGHT(H1725,LEN(H1725)-6)),\"\"))","v":""}]
[50002288,"Solax Power","X3-IES-12K",12,13.2,3,"Hybrid-Wechselrichter","Ja","2024-06-04","Martin Bertsch","2024-06-04",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN2488CO 001","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1726,1)=\"J\",LEFT(H1726,2),LEFT(H1726,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1726,1)=\"J\",RIGHT(H1726,LEN(H1726)-4),RIGHT(H1726,LEN(H1726)-6)),\"\"))","v":""}]
[50001421,"Solax Power","X3-PRO-12.0P",null,13.2,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1727,1)=\"J\",LEFT(H1727,2),LEFT(H1727,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1727,1)=\"J\",RIGHT(H1727,LEN(H1727)-4),RIGHT(H1727,LEN(H1727)-6)),\"\"))","v":""}]
[50001422,"Solax Power","X3-PRO-12K-G2",12,13.2,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2023-03-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN22J5CM 001","2023-07-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1728,1)=\"J\",LEFT(H1728,2),LEFT(H1728,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1728,1)=\"J\",RIGHT(H1728,LEN(H1728)-4),RIGHT(H1728,LEN(H1728)-6)),\"\"))","v":""}]
[50001423,"Solax Power","X3-Fit-G4-15.0-M/W",15,15,3,"AC-Batteriewechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2182YH 001","2021-07-19",null,"nicht vorhanden",null,null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25",null,null,null,null,{"$f":"IF(LEFT(H1729,1)=\"J\",LEFT(H1729,2),LEFT(H1729,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1729,1)=\"J\",RIGHT(H1729,LEN(H1729)-4),RIGHT(H1729,LEN(H1729)-6)),\"\"))","v":""}]
[50001424,"Solax Power","X3-HYBRID-G4-15.0-D/M",15,15,3,"Hybrid-Wechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 001","2021-07-19","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1730,1)=\"J\",LEFT(H1730,2),LEFT(H1730,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1730,1)=\"J\",RIGHT(H1730,LEN(H1730)-4),RIGHT(H1730,LEN(H1730)-6)),\"\"))","v":""}]
[50001425,"Solax Power","X3-MIC-15K-G2",15,15,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2022-11-16",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 001","2023-07-04","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1731,1)=\"J\",LEFT(H1731,2),LEFT(H1731,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1731,1)=\"J\",RIGHT(H1731,LEN(H1731)-4),RIGHT(H1731,LEN(H1731)-6)),\"\"))","v":""}]
[50002289,"Solax Power","X3-IES-15K",15,16.5,3,"Hybrid-Wechselrichter","Ja","2024-06-04","Martin Bertsch","2024-06-04",null,null,null,null,"Ja","Nein","Nein","Vorhanden",null,"CN2488CO 001","2024-05-08","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1732,1)=\"J\",LEFT(H1732,2),LEFT(H1732,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1732,1)=\"J\",RIGHT(H1732,LEN(H1732)-4),RIGHT(H1732,LEN(H1732)-6)),\"\"))","v":""}]
[50001426,"Solax Power","X3-PRO-15.0P",null,16.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1733,1)=\"J\",LEFT(H1733,2),LEFT(H1733,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1733,1)=\"J\",RIGHT(H1733,LEN(H1733)-4),RIGHT(H1733,LEN(H1733)-6)),\"\"))","v":""}]
[50001427,"Solax Power","X3-PRO-15K-G2",15,16.5,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2023-03-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN22J5CM 001","2023-07-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1734,1)=\"J\",LEFT(H1734,2),LEFT(H1734,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1734,1)=\"J\",RIGHT(H1734,LEN(H1734)-4),RIGHT(H1734,LEN(H1734)-6)),\"\"))","v":""}]
[50002084,"Solax Power","X3-ULT-15K",15,16.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-02-06",null,"2024-09-30",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN247N59 001","2024-01-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1735,1)=\"J\",LEFT(H1735,2),LEFT(H1735,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1735,1)=\"J\",RIGHT(H1735,LEN(H1735)-4),RIGHT(H1735,LEN(H1735)-6)),\"\"))","v":"befristet"}]
[50002085,"Solax Power","X3-ULT-15KP",15,16.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-02-06",null,"2024-09-30",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN247N59 001","2024-01-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1736,1)=\"J\",LEFT(H1736,2),LEFT(H1736,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1736,1)=\"J\",RIGHT(H1736,LEN(H1736)-4),RIGHT(H1736,LEN(H1736)-6)),\"\"))","v":"befristet"}]
[50001428,"Solax Power","X3-PRO-17K-G2",17,18.7,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2023-03-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN22J5CM 001","2023-07-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1737,1)=\"J\",LEFT(H1737,2),LEFT(H1737,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1737,1)=\"J\",RIGHT(H1737,LEN(H1737)-4),RIGHT(H1737,LEN(H1737)-6)),\"\"))","v":""}]
[50002086,"Solax Power","X3-ULT-19.9K",19.989999999999998,19.989999999999998,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-02-06",null,"2024-09-30",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN247N59 001","2024-01-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1738,1)=\"J\",LEFT(H1738,2),LEFT(H1738,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1738,1)=\"J\",RIGHT(H1738,LEN(H1738)-4),RIGHT(H1738,LEN(H1738)-6)),\"\"))","v":"befristet"}]
[50001429,"Solax Power","X3-MAX-20K-TL",22,22,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1739,1)=\"J\",LEFT(H1739,2),LEFT(H1739,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1739,1)=\"J\",RIGHT(H1739,LEN(H1739)-4),RIGHT(H1739,LEN(H1739)-6)),\"\"))","v":""}]
[50001430,"Solax Power","X3-PRO-20K-G2",20,22,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2023-03-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN22J5CM 001","2023-07-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1740,1)=\"J\",LEFT(H1740,2),LEFT(H1740,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1740,1)=\"J\",RIGHT(H1740,LEN(H1740)-4),RIGHT(H1740,LEN(H1740)-6)),\"\"))","v":""}]
[50002087,"Solax Power","X3-ULT-20K",20,22,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-02-06",null,"2024-09-30",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN247N59 001","2024-01-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1741,1)=\"J\",LEFT(H1741,2),LEFT(H1741,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1741,1)=\"J\",RIGHT(H1741,LEN(H1741)-4),RIGHT(H1741,LEN(H1741)-6)),\"\"))","v":"befristet"}]
[50001431,"Solax Power","X3-MAX-25K-TL",27.5,27.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1742,1)=\"J\",LEFT(H1742,2),LEFT(H1742,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1742,1)=\"J\",RIGHT(H1742,LEN(H1742)-4),RIGHT(H1742,LEN(H1742)-6)),\"\"))","v":""}]
[50001432,"Solax Power","X3-PRO-25K-G2",25,27.5,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2023-03-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN22J5CM 001","2023-07-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1743,1)=\"J\",LEFT(H1743,2),LEFT(H1743,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1743,1)=\"J\",RIGHT(H1743,LEN(H1743)-4),RIGHT(H1743,LEN(H1743)-6)),\"\"))","v":""}]
[50002088,"Solax Power","X3-ULT-25K",25,27.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-02-06",null,"2024-09-30",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN247N59 001","2024-01-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1744,1)=\"J\",LEFT(H1744,2),LEFT(H1744,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1744,1)=\"J\",RIGHT(H1744,LEN(H1744)-4),RIGHT(H1744,LEN(H1744)-6)),\"\"))","v":"befristet"}]
[50001433,"Solax Power","X3-PRO-30K-G2",30,30,3,"PV-Wechselrichter","Ja","2023-10-12","Martin Bertsch","2023-03-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","CN22J5CM 001","2023-07-05","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1745,1)=\"J\",LEFT(H1745,2),LEFT(H1745,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1745,1)=\"J\",RIGHT(H1745,LEN(H1745)-4),RIGHT(H1745,LEN(H1745)-6)),\"\"))","v":""}]
[50002089,"Solax Power","X3-ULT-30K",30,30,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2024-02-06",null,"2024-09-30",null,null,"Ja","Nein","Nein","Vorhanden",null,"CN247N59 001","2024-01-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1746,1)=\"J\",LEFT(H1746,2),LEFT(H1746,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1746,1)=\"J\",RIGHT(H1746,LEN(H1746)-4),RIGHT(H1746,LEN(H1746)-6)),\"\"))","v":"befristet"}]
[50001434,"Solax Power","X3-MAX-30K-TL",33,33,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1747,1)=\"J\",LEFT(H1747,2),LEFT(H1747,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1747,1)=\"J\",RIGHT(H1747,LEN(H1747)-4),RIGHT(H1747,LEN(H1747)-6)),\"\"))","v":""}]
[50001435,"Solax Power","X3-MGA-40K-G2",40,44,3,"PV-Wechselrichter","Ja","2023-10-25","Martin Bertsch",null,"Master: V003.00, Slave: V003.00, Manager: V003.00",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN22YGKL 001","2023-01-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1748,1)=\"J\",LEFT(H1748,2),LEFT(H1748,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1748,1)=\"J\",RIGHT(H1748,LEN(H1748)-4),RIGHT(H1748,LEN(H1748)-6)),\"\"))","v":""}]
[50001436,"Solax Power","X3-MEGA-50K-TL",55,55,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1749,1)=\"J\",LEFT(H1749,2),LEFT(H1749,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1749,1)=\"J\",RIGHT(H1749,LEN(H1749)-4),RIGHT(H1749,LEN(H1749)-6)),\"\"))","v":""}]
[50001437,"Solax Power","X3-MGA-50K-G2",50,55,3,"PV-Wechselrichter","Ja","2023-10-25","Martin Bertsch",null,"Master: V003.00, Slave: V003.00, Manager: V003.00",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN22YGKL 001","2023-01-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1750,1)=\"J\",LEFT(H1750,2),LEFT(H1750,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1750,1)=\"J\",RIGHT(H1750,LEN(H1750)-4),RIGHT(H1750,LEN(H1750)-6)),\"\"))","v":""}]
[50001438,"Solax Power","X3-MEGA-60K-TL",66,66,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1751,1)=\"J\",LEFT(H1751,2),LEFT(H1751,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1751,1)=\"J\",RIGHT(H1751,LEN(H1751)-4),RIGHT(H1751,LEN(H1751)-6)),\"\"))","v":""}]
[50001439,"Solax Power","X3-MGA-60K-G2",60,66,3,"PV-Wechselrichter","Ja","2023-10-25","Martin Bertsch",null,"Master: V003.00, Slave: V003.00, Manager: V003.00",null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN22YGKL 001","2023-01-13","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1752,1)=\"J\",LEFT(H1752,2),LEFT(H1752,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1752,1)=\"J\",RIGHT(H1752,LEN(H1752)-4),RIGHT(H1752,LEN(H1752)-6)),\"\"))","v":""}]
[50002038,"Solax Power","X3-FTH-75K",75,75,3,"PV-Wechselrichter","Nein - In Prüfung","2024-01-05","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23NOXB 001","2023-10-25",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1753,1)=\"J\",LEFT(H1753,2),LEFT(H1753,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1753,1)=\"J\",RIGHT(H1753,LEN(H1753)-4),RIGHT(H1753,LEN(H1753)-6)),\"\"))","v":"In Prüfung"}]
[50002039,"Solax Power","X3-FTH-80K",80,88,3,"PV-Wechselrichter","Nein - In Prüfung","2024-01-05","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23NOXB 001","2023-10-25",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1754,1)=\"J\",LEFT(H1754,2),LEFT(H1754,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1754,1)=\"J\",RIGHT(H1754,LEN(H1754)-4),RIGHT(H1754,LEN(H1754)-6)),\"\"))","v":"In Prüfung"}]
[50002040,"Solax Power","X3-FTH-100K",100,110,3,"PV-Wechselrichter","Nein - In Prüfung","2024-01-05","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23NOXB 001","2023-10-25",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1755,1)=\"J\",LEFT(H1755,2),LEFT(H1755,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1755,1)=\"J\",RIGHT(H1755,LEN(H1755)-4),RIGHT(H1755,LEN(H1755)-6)),\"\"))","v":"In Prüfung"}]
[50002041,"Solax Power","X3-FTH-110K",110,121,3,"PV-Wechselrichter","Nein - In Prüfung","2024-01-05","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23NOXB 001","2023-10-25",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1756,1)=\"J\",LEFT(H1756,2),LEFT(H1756,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1756,1)=\"J\",RIGHT(H1756,LEN(H1756)-4),RIGHT(H1756,LEN(H1756)-6)),\"\"))","v":"In Prüfung"}]
[50002042,"Solax Power","X3-FTH-120K",120,132,3,"PV-Wechselrichter","Nein - In Prüfung","2024-01-05","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23NOXB 001","2023-10-25",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1757,1)=\"J\",LEFT(H1757,2),LEFT(H1757,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1757,1)=\"J\",RIGHT(H1757,LEN(H1757)-4),RIGHT(H1757,LEN(H1757)-6)),\"\"))","v":"In Prüfung"}]
[50002043,"Solax Power","X3-FTH-125K",125,132,3,"PV-Wechselrichter","Nein - In Prüfung","2024-01-05","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN23NOXB 001","2023-10-25",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1758,1)=\"J\",LEFT(H1758,2),LEFT(H1758,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1758,1)=\"J\",RIGHT(H1758,LEN(H1758)-4),RIGHT(H1758,LEN(H1758)-6)),\"\"))","v":"In Prüfung"}]
[50002036,"Solax Power","X3-FTH-136K-MV",136,149.6,3,"PV-Wechselrichter","Nein - Typ B","2024-01-05","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht vorhanden",null,null,null,"Vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1759,1)=\"J\",LEFT(H1759,2),LEFT(H1759,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1759,1)=\"J\",RIGHT(H1759,LEN(H1759)-4),RIGHT(H1759,LEN(H1759)-6)),\"\"))","v":"Typ B"}]
[50002037,"Solax Power","X3-FTH-150K-MV",150,165,3,"PV-Wechselrichter","Nein - Typ B","2024-01-05","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","nicht vorhanden",null,null,null,"Vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1760,1)=\"J\",LEFT(H1760,2),LEFT(H1760,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1760,1)=\"J\",RIGHT(H1760,LEN(H1760)-4),RIGHT(H1760,LEN(H1760)-6)),\"\"))","v":"Typ B"}]
[50001440,"SOLINTEG","MHT-4K-25",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1761,1)=\"J\",LEFT(H1761,2),LEFT(H1761,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1761,1)=\"J\",RIGHT(H1761,LEN(H1761)-4),RIGHT(H1761,LEN(H1761)-6)),\"\"))","v":"mit Einschränkung"}]
[50002097,"SOLINTEG","OGT-5K",5,5,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1762,1)=\"J\",LEFT(H1762,2),LEFT(H1762,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1762,1)=\"J\",RIGHT(H1762,LEN(H1762)-4),RIGHT(H1762,LEN(H1762)-6)),\"\"))","v":"In Prüfung"}]
[50001441,"SOLINTEG","MHT-5K-25",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1763,1)=\"J\",LEFT(H1763,2),LEFT(H1763,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1763,1)=\"J\",RIGHT(H1763,LEN(H1763)-4),RIGHT(H1763,LEN(H1763)-6)),\"\"))","v":"mit Einschränkung"}]
[50002098,"SOLINTEG","OGT-6K",6,6,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1764,1)=\"J\",LEFT(H1764,2),LEFT(H1764,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1764,1)=\"J\",RIGHT(H1764,LEN(H1764)-4),RIGHT(H1764,LEN(H1764)-6)),\"\"))","v":"In Prüfung"}]
[50001442,"SOLINTEG","MHT-6K-25",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1765,1)=\"J\",LEFT(H1765,2),LEFT(H1765,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1765,1)=\"J\",RIGHT(H1765,LEN(H1765)-4),RIGHT(H1765,LEN(H1765)-6)),\"\"))","v":"mit Einschränkung"}]
[50002099,"SOLINTEG","OGT-8K",8,8,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1766,1)=\"J\",LEFT(H1766,2),LEFT(H1766,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1766,1)=\"J\",RIGHT(H1766,LEN(H1766)-4),RIGHT(H1766,LEN(H1766)-6)),\"\"))","v":"In Prüfung"}]
[50002100,"SOLINTEG","OGT-8K-P",8,8,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1767,1)=\"J\",LEFT(H1767,2),LEFT(H1767,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1767,1)=\"J\",RIGHT(H1767,LEN(H1767)-4),RIGHT(H1767,LEN(H1767)-6)),\"\"))","v":"In Prüfung"}]
[50001443,"SOLINTEG","MHT-8K-25",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1768,1)=\"J\",LEFT(H1768,2),LEFT(H1768,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1768,1)=\"J\",RIGHT(H1768,LEN(H1768)-4),RIGHT(H1768,LEN(H1768)-6)),\"\"))","v":"mit Einschränkung"}]
[50002101,"SOLINTEG","OGT-10K",10,10,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1769,1)=\"J\",LEFT(H1769,2),LEFT(H1769,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1769,1)=\"J\",RIGHT(H1769,LEN(H1769)-4),RIGHT(H1769,LEN(H1769)-6)),\"\"))","v":"In Prüfung"}]
[50002102,"SOLINTEG","OGT-10K-P",10,10,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1770,1)=\"J\",LEFT(H1770,2),LEFT(H1770,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1770,1)=\"J\",RIGHT(H1770,LEN(H1770)-4),RIGHT(H1770,LEN(H1770)-6)),\"\"))","v":"In Prüfung"}]
[50001444,"SOLINTEG","MHT-10K-25",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1771,1)=\"J\",LEFT(H1771,2),LEFT(H1771,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1771,1)=\"J\",RIGHT(H1771,LEN(H1771)-4),RIGHT(H1771,LEN(H1771)-6)),\"\"))","v":"mit Einschränkung"}]
[50001445,"SOLINTEG","MHT-10K-40",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1772,1)=\"J\",LEFT(H1772,2),LEFT(H1772,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1772,1)=\"J\",RIGHT(H1772,LEN(H1772)-4),RIGHT(H1772,LEN(H1772)-6)),\"\"))","v":"mit Einschränkung"}]
[50002103,"SOLINTEG","OGT-12K",12,12,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1773,1)=\"J\",LEFT(H1773,2),LEFT(H1773,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1773,1)=\"J\",RIGHT(H1773,LEN(H1773)-4),RIGHT(H1773,LEN(H1773)-6)),\"\"))","v":"In Prüfung"}]
[50002104,"SOLINTEG","OGT-12K-P",12,12,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1774,1)=\"J\",LEFT(H1774,2),LEFT(H1774,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1774,1)=\"J\",RIGHT(H1774,LEN(H1774)-4),RIGHT(H1774,LEN(H1774)-6)),\"\"))","v":"In Prüfung"}]
[50001446,"SOLINTEG","MHT-12K-25",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1775,1)=\"J\",LEFT(H1775,2),LEFT(H1775,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1775,1)=\"J\",RIGHT(H1775,LEN(H1775)-4),RIGHT(H1775,LEN(H1775)-6)),\"\"))","v":"mit Einschränkung"}]
[50001447,"SOLINTEG","MHT-12K-40",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1776,1)=\"J\",LEFT(H1776,2),LEFT(H1776,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1776,1)=\"J\",RIGHT(H1776,LEN(H1776)-4),RIGHT(H1776,LEN(H1776)-6)),\"\"))","v":"mit Einschränkung"}]
[50002105,"SOLINTEG","OGT-15K",15,15,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1777,1)=\"J\",LEFT(H1777,2),LEFT(H1777,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1777,1)=\"J\",RIGHT(H1777,LEN(H1777)-4),RIGHT(H1777,LEN(H1777)-6)),\"\"))","v":"In Prüfung"}]
[50002106,"SOLINTEG","OGT-15K-P",15,15,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1778,1)=\"J\",LEFT(H1778,2),LEFT(H1778,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1778,1)=\"J\",RIGHT(H1778,LEN(H1778)-4),RIGHT(H1778,LEN(H1778)-6)),\"\"))","v":"In Prüfung"}]
[50001448,"SOLINTEG","MHT-15K-40",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1779,1)=\"J\",LEFT(H1779,2),LEFT(H1779,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1779,1)=\"J\",RIGHT(H1779,LEN(H1779)-4),RIGHT(H1779,LEN(H1779)-6)),\"\"))","v":"mit Einschränkung"}]
[50002107,"SOLINTEG","OGT-20K",20,20,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1780,1)=\"J\",LEFT(H1780,2),LEFT(H1780,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1780,1)=\"J\",RIGHT(H1780,LEN(H1780)-4),RIGHT(H1780,LEN(H1780)-6)),\"\"))","v":"In Prüfung"}]
[50002108,"SOLINTEG","OGT-25K",20,20,3,"PV-Wechselrichter","Nein - In Prüfung","2024-04-10","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden",null,"CN24WHGG 001","2024-03-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1781,1)=\"J\",LEFT(H1781,2),LEFT(H1781,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1781,1)=\"J\",RIGHT(H1781,LEN(H1781)-4),RIGHT(H1781,LEN(H1781)-6)),\"\"))","v":"In Prüfung"}]
[50001449,"SOLINTEG","MHT-20K-40",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-30","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220422BW002-EG-AT-002","2023-04-14","nicht vorhanden","OK",null,null,null,null,"ident zu Wattsonic",null,null,null,null,{"$f":"IF(LEFT(H1782,1)=\"J\",LEFT(H1782,2),LEFT(H1782,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1782,1)=\"J\",RIGHT(H1782,LEN(H1782)-4),RIGHT(H1782,LEN(H1782)-6)),\"\"))","v":"mit Einschränkung"}]
[50001829,"SOLIS","S6-EH3P5K2-H",5,5.5,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1783,1)=\"J\",LEFT(H1783,2),LEFT(H1783,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1783,1)=\"J\",RIGHT(H1783,LEN(H1783)-4),RIGHT(H1783,LEN(H1783)-6)),\"\"))","v":"In Prüfung"}]
[50001821,"SOLIS","S6-EH3P5K2-H-OD",5,5.5,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1784,1)=\"J\",LEFT(H1784,2),LEFT(H1784,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1784,1)=\"J\",RIGHT(H1784,LEN(H1784)-4),RIGHT(H1784,LEN(H1784)-6)),\"\"))","v":"In Prüfung"}]
[50001816,"SOLIS","S6-EH3P5K-H-EU",5,5.5,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1785,1)=\"J\",LEFT(H1785,2),LEFT(H1785,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1785,1)=\"J\",RIGHT(H1785,LEN(H1785)-4),RIGHT(H1785,LEN(H1785)-6)),\"\"))","v":"In Prüfung"}]
[50001825,"SOLIS","S6-EH3P5K-H-EU-OD",5,5.5,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1786,1)=\"J\",LEFT(H1786,2),LEFT(H1786,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1786,1)=\"J\",RIGHT(H1786,LEN(H1786)-4),RIGHT(H1786,LEN(H1786)-6)),\"\"))","v":"In Prüfung"}]
[50001830,"SOLIS","S6-EH3P6K2-H",6,6.6,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1787,1)=\"J\",LEFT(H1787,2),LEFT(H1787,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1787,1)=\"J\",RIGHT(H1787,LEN(H1787)-4),RIGHT(H1787,LEN(H1787)-6)),\"\"))","v":"In Prüfung"}]
[50001822,"SOLIS","S6-EH3P6K2-H-OD",6,6.6,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1788,1)=\"J\",LEFT(H1788,2),LEFT(H1788,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1788,1)=\"J\",RIGHT(H1788,LEN(H1788)-4),RIGHT(H1788,LEN(H1788)-6)),\"\"))","v":"In Prüfung"}]
[50001818,"SOLIS","S6-EH3P6K-H-EU",6,6.6,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1789,1)=\"J\",LEFT(H1789,2),LEFT(H1789,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1789,1)=\"J\",RIGHT(H1789,LEN(H1789)-4),RIGHT(H1789,LEN(H1789)-6)),\"\"))","v":"In Prüfung"}]
[50001826,"SOLIS","S6-EH3P6K-H-EU-OD",6,6.6,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1790,1)=\"J\",LEFT(H1790,2),LEFT(H1790,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1790,1)=\"J\",RIGHT(H1790,LEN(H1790)-4),RIGHT(H1790,LEN(H1790)-6)),\"\"))","v":"In Prüfung"}]
[50001831,"SOLIS","S6-EH3P8K2-H",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1791,1)=\"J\",LEFT(H1791,2),LEFT(H1791,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1791,1)=\"J\",RIGHT(H1791,LEN(H1791)-4),RIGHT(H1791,LEN(H1791)-6)),\"\"))","v":"In Prüfung"}]
[50001823,"SOLIS","S6-EH3P8K2-H-OD",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1792,1)=\"J\",LEFT(H1792,2),LEFT(H1792,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1792,1)=\"J\",RIGHT(H1792,LEN(H1792)-4),RIGHT(H1792,LEN(H1792)-6)),\"\"))","v":"In Prüfung"}]
[50001819,"SOLIS","S6-EH3P8K-H-EU",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1793,1)=\"J\",LEFT(H1793,2),LEFT(H1793,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1793,1)=\"J\",RIGHT(H1793,LEN(H1793)-4),RIGHT(H1793,LEN(H1793)-6)),\"\"))","v":"In Prüfung"}]
[50001827,"SOLIS","S6-EH3P8K-H-EU-OD",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1794,1)=\"J\",LEFT(H1794,2),LEFT(H1794,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1794,1)=\"J\",RIGHT(H1794,LEN(H1794)-4),RIGHT(H1794,LEN(H1794)-6)),\"\"))","v":"In Prüfung"}]
[50001832,"SOLIS","S6-EH3P10K2-H",10,11,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1795,1)=\"J\",LEFT(H1795,2),LEFT(H1795,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1795,1)=\"J\",RIGHT(H1795,LEN(H1795)-4),RIGHT(H1795,LEN(H1795)-6)),\"\"))","v":"In Prüfung"}]
[50001824,"SOLIS","S6-EH3P10K2-H-OD",10,11,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1796,1)=\"J\",LEFT(H1796,2),LEFT(H1796,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1796,1)=\"J\",RIGHT(H1796,LEN(H1796)-4),RIGHT(H1796,LEN(H1796)-6)),\"\"))","v":"In Prüfung"}]
[50001820,"SOLIS","S6-EH3P10K-H-EU",10,11,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1797,1)=\"J\",LEFT(H1797,2),LEFT(H1797,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1797,1)=\"J\",RIGHT(H1797,LEN(H1797)-4),RIGHT(H1797,LEN(H1797)-6)),\"\"))","v":"In Prüfung"}]
[50001828,"SOLIS","S6-EH3P10K-H-EU-OD",10,11,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1798,1)=\"J\",LEFT(H1798,2),LEFT(H1798,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1798,1)=\"J\",RIGHT(H1798,LEN(H1798)-4),RIGHT(H1798,LEN(H1798)-6)),\"\"))","v":"In Prüfung"}]
[50001833,"SOLIS","S6-EH3P10K-H-EU-PRO",10,11,3,"Hybrid-Wechselrichter","Nein - In Prüfung","2023-09-13","Martin Bertsch",null,null,null,null,null,"Ja","Nein",null,"Vorhanden",null,"CN2227ZM 002","2023-06-01",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1799,1)=\"J\",LEFT(H1799,2),LEFT(H1799,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1799,1)=\"J\",RIGHT(H1799,LEN(H1799)-4),RIGHT(H1799,LEN(H1799)-6)),\"\"))","v":"In Prüfung"}]
[50001875,"Solplanet","ASW3000-S-G2",3,3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-09","Martin Bertsch","2023-10-09",null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2304WDG0118-1","2023-08-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1800,1)=\"J\",LEFT(H1800,2),LEFT(H1800,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1800,1)=\"J\",RIGHT(H1800,LEN(H1800)-4),RIGHT(H1800,LEN(H1800)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001721,"Solplanet","ASW3K-LT-G2 Pro",3,3,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1801,1)=\"J\",LEFT(H1801,2),LEFT(H1801,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1801,1)=\"J\",RIGHT(H1801,LEN(H1801)-4),RIGHT(H1801,LEN(H1801)-6)),\"\"))","v":"befristet"}]
[50001876,"Solplanet","ASW3680-S-G2",3.68,3.68,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2023-10-09","Martin Bertsch","2023-10-09",null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2304WDG0118-1","2023-08-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1802,1)=\"J\",LEFT(H1802,2),LEFT(H1802,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1802,1)=\"J\",RIGHT(H1802,LEN(H1802)-4),RIGHT(H1802,LEN(H1802)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001877,"Solplanet","ASW4000-S-G2",4,4,1,"PV-Wechselrichter","Nein","2023-10-09","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2304WDG0118-1","2023-08-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1803,1)=\"J\",LEFT(H1803,2),LEFT(H1803,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1803,1)=\"J\",RIGHT(H1803,LEN(H1803)-4),RIGHT(H1803,LEN(H1803)-6)),\"\"))","v":""}]
[50001722,"Solplanet","ASW4K-LT-G2 Pro",4,4,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1804,1)=\"J\",LEFT(H1804,2),LEFT(H1804,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1804,1)=\"J\",RIGHT(H1804,LEN(H1804)-4),RIGHT(H1804,LEN(H1804)-6)),\"\"))","v":"befristet"}]
[50001878,"Solplanet","ASW5000-S-G2",5,5,1,"PV-Wechselrichter","Nein","2023-10-09","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2304WDG0118-1","2023-08-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1805,1)=\"J\",LEFT(H1805,2),LEFT(H1805,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1805,1)=\"J\",RIGHT(H1805,LEN(H1805)-4),RIGHT(H1805,LEN(H1805)-6)),\"\"))","v":""}]
[50001723,"Solplanet","ASW5K-LT-G2 Pro",5,5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1806,1)=\"J\",LEFT(H1806,2),LEFT(H1806,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1806,1)=\"J\",RIGHT(H1806,LEN(H1806)-4),RIGHT(H1806,LEN(H1806)-6)),\"\"))","v":"befristet"}]
[50001879,"Solplanet","ASW6000-S-G2",6,6,1,"PV-Wechselrichter","Nein","2023-10-09","Martin Bertsch",null,null,null,null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","PVAT2304WDG0118-1","2023-08-31","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1807,1)=\"J\",LEFT(H1807,2),LEFT(H1807,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1807,1)=\"J\",RIGHT(H1807,LEN(H1807)-4),RIGHT(H1807,LEN(H1807)-6)),\"\"))","v":""}]
[50001724,"Solplanet","ASW6K-LT-G2 Pro",6,6,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1808,1)=\"J\",LEFT(H1808,2),LEFT(H1808,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1808,1)=\"J\",RIGHT(H1808,LEN(H1808)-4),RIGHT(H1808,LEN(H1808)-6)),\"\"))","v":"befristet"}]
[50001725,"Solplanet","ASW8K-LT-G2 Pro",8,8,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1809,1)=\"J\",LEFT(H1809,2),LEFT(H1809,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1809,1)=\"J\",RIGHT(H1809,LEN(H1809)-4),RIGHT(H1809,LEN(H1809)-6)),\"\"))","v":"befristet"}]
[50001726,"Solplanet","ASW10K-LT-G2 Pro",10,10,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1810,1)=\"J\",LEFT(H1810,2),LEFT(H1810,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1810,1)=\"J\",RIGHT(H1810,LEN(H1810)-4),RIGHT(H1810,LEN(H1810)-6)),\"\"))","v":"befristet"}]
[50001727,"Solplanet","ASW12K-LT-G2 Pro",12,12,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1811,1)=\"J\",LEFT(H1811,2),LEFT(H1811,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1811,1)=\"J\",RIGHT(H1811,LEN(H1811)-4),RIGHT(H1811,LEN(H1811)-6)),\"\"))","v":"befristet"}]
[50001728,"Solplanet","ASW13K-LT-G2 Pro",13,13,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1812,1)=\"J\",LEFT(H1812,2),LEFT(H1812,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1812,1)=\"J\",RIGHT(H1812,LEN(H1812)-4),RIGHT(H1812,LEN(H1812)-6)),\"\"))","v":"befristet"}]
[50001729,"Solplanet","ASW15K-LT-G2 Pro",15,15,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1813,1)=\"J\",LEFT(H1813,2),LEFT(H1813,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1813,1)=\"J\",RIGHT(H1813,LEN(H1813)-4),RIGHT(H1813,LEN(H1813)-6)),\"\"))","v":"befristet"}]
[50001730,"Solplanet","ASW17K-LT-G2 Pro",17,17,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1814,1)=\"J\",LEFT(H1814,2),LEFT(H1814,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1814,1)=\"J\",RIGHT(H1814,LEN(H1814)-4),RIGHT(H1814,LEN(H1814)-6)),\"\"))","v":"befristet"}]
[50001731,"Solplanet","ASW20K-LT-G2 Pro",20,20,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001398-00","2023-09-18","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1815,1)=\"J\",LEFT(H1815,2),LEFT(H1815,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1815,1)=\"J\",RIGHT(H1815,LEN(H1815)-4),RIGHT(H1815,LEN(H1815)-6)),\"\"))","v":"befristet"}]
[50001735,"Solplanet","ASW25K-LT-G3",25,25,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001399-00","2023-09-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1816,1)=\"J\",LEFT(H1816,2),LEFT(H1816,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1816,1)=\"J\",RIGHT(H1816,LEN(H1816)-4),RIGHT(H1816,LEN(H1816)-6)),\"\"))","v":"befristet"}]
[50001733,"Solplanet","ASW27K-LT-G3",27,27,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001399-00","2023-09-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1817,1)=\"J\",LEFT(H1817,2),LEFT(H1817,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1817,1)=\"J\",RIGHT(H1817,LEN(H1817)-4),RIGHT(H1817,LEN(H1817)-6)),\"\"))","v":"befristet"}]
[50001736,"Solplanet","ASW30K-LT-G3",30,30,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001399-00","2023-09-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1818,1)=\"J\",LEFT(H1818,2),LEFT(H1818,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1818,1)=\"J\",RIGHT(H1818,LEN(H1818)-4),RIGHT(H1818,LEN(H1818)-6)),\"\"))","v":"befristet"}]
[50001737,"Solplanet","ASW33K-LTG3",33,33,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001399-00","2023-09-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1819,1)=\"J\",LEFT(H1819,2),LEFT(H1819,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1819,1)=\"J\",RIGHT(H1819,LEN(H1819)-4),RIGHT(H1819,LEN(H1819)-6)),\"\"))","v":"befristet"}]
[50001738,"Solplanet","ASW36K-LT-G3",36,36,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001399-00","2023-09-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1820,1)=\"J\",LEFT(H1820,2),LEFT(H1820,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1820,1)=\"J\",RIGHT(H1820,LEN(H1820)-4),RIGHT(H1820,LEN(H1820)-6)),\"\"))","v":"befristet"}]
[50001739,"Solplanet","ASW40K-LT-G3",40,40,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-10-09",null,"2024-09-30",null,null,"Nein","Nein","Nein","Vorhanden","Martin Bertsch (OE)","5040923001399-00","2023-09-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1821,1)=\"J\",LEFT(H1821,2),LEFT(H1821,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1821,1)=\"J\",RIGHT(H1821,LEN(H1821)-4),RIGHT(H1821,LEN(H1821)-6)),\"\"))","v":"befristet"}]
[50001450,"sonnen GmbH","sonnenBatterie 10 performance (10p/11) Art-Nr: 3000364",7,7,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-04-27","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein",null,"OK","Roland Bründlinger","20PP126-07_3","2023-04-11","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1822,1)=\"J\",LEFT(H1822,2),LEFT(H1822,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1822,1)=\"J\",RIGHT(H1822,LEN(H1822)-4),RIGHT(H1822,LEN(H1822)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001451,"sonnen GmbH","sonnenBatterie 10 performance (10p/22, 10p/33, 10p/44, 10p/55) Art-Nr: 3000364",9.9,9.9,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-04-27","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein",null,"OK","Roland Bründlinger","20PP126-07_3","2023-04-11","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1823,1)=\"J\",LEFT(H1823,2),LEFT(H1823,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1823,1)=\"J\",RIGHT(H1823,LEN(H1823)-4),RIGHT(H1823,LEN(H1823)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001452,"sonnen GmbH","sonnenBatterie 10 performance (10p/11) Art-Nr: 3000158",7,12,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-04-27","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein",null,"OK","Roland Bründlinger","20PP126-07_3","2023-04-11","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1824,1)=\"J\",LEFT(H1824,2),LEFT(H1824,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1824,1)=\"J\",RIGHT(H1824,LEN(H1824)-4),RIGHT(H1824,LEN(H1824)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001453,"sonnen GmbH","sonnenBatterie 10 performance (10p/22, 10p/33, 10p/44, 10p/55) Art-Nr: 3000158",8,12,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch","2023-04-27","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein",null,"OK","Roland Bründlinger","20PP126-07_3","2023-04-11","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1825,1)=\"J\",LEFT(H1825,2),LEFT(H1825,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1825,1)=\"J\",RIGHT(H1825,LEN(H1825)-4),RIGHT(H1825,LEN(H1825)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001454,"SONNENKRAFT","SK-HWR-5",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-04-12","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365","2022-11-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1826,1)=\"J\",LEFT(H1826,2),LEFT(H1826,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1826,1)=\"J\",RIGHT(H1826,LEN(H1826)-4),RIGHT(H1826,LEN(H1826)-6)),\"\"))","v":"mit Einschränkung"}]
[50001455,"SONNENKRAFT","SK-HWR-6",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-04-12","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365","2022-11-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1827,1)=\"J\",LEFT(H1827,2),LEFT(H1827,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1827,1)=\"J\",RIGHT(H1827,LEN(H1827)-4),RIGHT(H1827,LEN(H1827)-6)),\"\"))","v":"mit Einschränkung"}]
[50001456,"SONNENKRAFT","SK-HWR-8",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-04-12","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365","2022-11-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1828,1)=\"J\",LEFT(H1828,2),LEFT(H1828,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1828,1)=\"J\",RIGHT(H1828,LEN(H1828)-4),RIGHT(H1828,LEN(H1828)-6)),\"\"))","v":"mit Einschränkung"}]
[50001457,"SONNENKRAFT","SK-HWR-10",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-04-12","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365","2022-11-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1829,1)=\"J\",LEFT(H1829,2),LEFT(H1829,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1829,1)=\"J\",RIGHT(H1829,LEN(H1829)-4),RIGHT(H1829,LEN(H1829)-6)),\"\"))","v":"mit Einschränkung"}]
[50001458,"SONNENKRAFT","SK-HWR-12",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-04-04","Martin Bertsch","2023-04-12","1.96 (Master)",null,null,null,"Ja","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CGDY-ESH-P22100365","2022-11-14","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1830,1)=\"J\",LEFT(H1830,2),LEFT(H1830,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1830,1)=\"J\",RIGHT(H1830,LEN(H1830)-4),RIGHT(H1830,LEN(H1830)-6)),\"\"))","v":"mit Einschränkung"}]
[50002207,"SOSSEN","SOSSEN-600",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-13","Martin Bertsch","2024-05-13",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"PVDE2304WDG0196-1","2024-04-08",null,"VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1831,1)=\"J\",LEFT(H1831,2),LEFT(H1831,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1831,1)=\"J\",RIGHT(H1831,LEN(H1831)-4),RIGHT(H1831,LEN(H1831)-6)),\"\"))","v":"<= 800W Anlage"}]
[50002208,"SOSSEN","SOSSEN-800",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-05-13","Martin Bertsch","2024-05-13",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"PVDE2304WDG0196-1","2024-04-08",null,"VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1832,1)=\"J\",LEFT(H1832,2),LEFT(H1832,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1832,1)=\"J\",RIGHT(H1832,LEN(H1832)-4),RIGHT(H1832,LEN(H1832)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001746,"STABL","SI 100",67.5,67.5,3,"AC-Batteriewechselrichter","Ja","2023-09-21","Martin Bertsch","2023-09-21",null,null,null,null,null,null,null,"OK","Martin Bertsch (OE)","20TH0292-OVE-directive R25_0","2023-09-11",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1833,1)=\"J\",LEFT(H1833,2),LEFT(H1833,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1833,1)=\"J\",RIGHT(H1833,LEN(H1833)-4),RIGHT(H1833,LEN(H1833)-6)),\"\"))","v":""}]
[50001740,"STRONGENERGY","CVT1ST-5K3P",5,5.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-09-05",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"OK","Roland Bründlinger (AIT)","230725161GZU-005","2023-07-27",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1834,1)=\"J\",LEFT(H1834,2),LEFT(H1834,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1834,1)=\"J\",RIGHT(H1834,LEN(H1834)-4),RIGHT(H1834,LEN(H1834)-6)),\"\"))","v":"befristet"}]
[50001741,"STRONGENERGY","CVT2ST-6K3P",6,6.6,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-09-05",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"OK","Roland Bründlinger (AIT)","230725161GZU-005","2023-07-27",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1835,1)=\"J\",LEFT(H1835,2),LEFT(H1835,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1835,1)=\"J\",RIGHT(H1835,LEN(H1835)-4),RIGHT(H1835,LEN(H1835)-6)),\"\"))","v":"befristet"}]
[50001742,"STRONGENERGY","CVT3ST-8K3P",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-09-05",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"OK","Roland Bründlinger (AIT)","230725161GZU-005","2023-07-27",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1836,1)=\"J\",LEFT(H1836,2),LEFT(H1836,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1836,1)=\"J\",RIGHT(H1836,LEN(H1836)-4),RIGHT(H1836,LEN(H1836)-6)),\"\"))","v":"befristet"}]
[50001743,"STRONGENERGY","CVT4ST-10K3P",10,11,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-09-05",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"OK","Roland Bründlinger (AIT)","230725161GZU-005","2023-07-27",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1837,1)=\"J\",LEFT(H1837,2),LEFT(H1837,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1837,1)=\"J\",RIGHT(H1837,LEN(H1837)-4),RIGHT(H1837,LEN(H1837)-6)),\"\"))","v":"befristet"}]
[50001744,"STRONGENERGY","CVT5ST-15K3P",15,16.5,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-09-05",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"OK","Roland Bründlinger (AIT)","230725161GZU-005","2023-07-27",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1838,1)=\"J\",LEFT(H1838,2),LEFT(H1838,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1838,1)=\"J\",RIGHT(H1838,LEN(H1838)-4),RIGHT(H1838,LEN(H1838)-6)),\"\"))","v":"befristet"}]
[50001745,"STRONGENERGY","CVT6ST-20K3P",20,22,3,"Hybrid-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-09-05",null,"2024-09-30",null,"Fehler in der FW",null,null,null,"OK","Roland Bründlinger (AIT)","230725161GZU-005","2023-07-27",null,"Vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1839,1)=\"J\",LEFT(H1839,2),LEFT(H1839,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1839,1)=\"J\",RIGHT(H1839,LEN(H1839)-4),RIGHT(H1839,LEN(H1839)-6)),\"\"))","v":"befristet"}]
[50001459,"STUDER INNOTEC","nx3 16000-48 st",15,15,3,"Hybrid-Wechselrichter","Ja","2024-05-17","Christian Elbs","2022-11-16",null,null,null,null,null,null,null,"OK","RB","21PP474-05_2","2022-02-23",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1840,1)=\"J\",LEFT(H1840,2),LEFT(H1840,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1840,1)=\"J\",RIGHT(H1840,LEN(H1840)-4),RIGHT(H1840,LEN(H1840)-6)),\"\"))","v":""}]
[50001460,"STUDER INNOTEC","nx3 16000-48 t",15,15,3,"Hybrid-Wechselrichter","Ja","2024-05-17","Christian Elbs","2022-11-16",null,null,null,null,null,null,null,"OK","RB","21PP474-05_2","2022-02-23",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1841,1)=\"J\",LEFT(H1841,2),LEFT(H1841,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1841,1)=\"J\",RIGHT(H1841,LEN(H1841)-4),RIGHT(H1841,LEN(H1841)-6)),\"\"))","v":""}]
[50001461,"Sungrow","SH5.0RT",5,5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2023-07-27","Martin Bertsch","2023-07-27","LCD: SAPPHIRE-H_01011.51.04 MDSP: SAPPHIRE-H_03011.51.03 SDSP: SUBCTL-S_04011.01.01",null,null,null,"Ja","Nein","Ja","OK","Christian Elbs","SGR-ESH-P20120741-R1\r","2022-03-02","nicht vorhanden","OK",null,"nicht vorhanden",null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1842,1)=\"J\",LEFT(H1842,2),LEFT(H1842,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1842,1)=\"J\",RIGHT(H1842,LEN(H1842)-4),RIGHT(H1842,LEN(H1842)-6)),\"\"))","v":"mit Einschränkung"}]
[50001462,"Sungrow","SG5.0RT",5,5.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1843,1)=\"J\",LEFT(H1843,2),LEFT(H1843,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1843,1)=\"J\",RIGHT(H1843,LEN(H1843)-4),RIGHT(H1843,LEN(H1843)-6)),\"\"))","v":""}]
[50001463,"Sungrow","SH6.0RT",6,6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2023-07-27","Martin Bertsch","2023-07-27","LCD:SAPPHIRE-H_01011.51.04 MDSP:SAPPHIRE-H_03011.51.03 SDSP: SUBCTL-S_04011.01.01",null,null,null,"Ja","Nein","Ja","OK","Christian Elbs","SGR-ESH-P20120741-R1\r","2022-03-02","nicht vorhanden","OK",null,"nicht vorhanden",null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1844,1)=\"J\",LEFT(H1844,2),LEFT(H1844,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1844,1)=\"J\",RIGHT(H1844,LEN(H1844)-4),RIGHT(H1844,LEN(H1844)-6)),\"\"))","v":"mit Einschränkung"}]
[50001464,"Sungrow","SG6.0RT",6,6.6,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1845,1)=\"J\",LEFT(H1845,2),LEFT(H1845,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1845,1)=\"J\",RIGHT(H1845,LEN(H1845)-4),RIGHT(H1845,LEN(H1845)-6)),\"\"))","v":""}]
[50001465,"Sungrow","SG7.0RT",7,7.7,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1846,1)=\"J\",LEFT(H1846,2),LEFT(H1846,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1846,1)=\"J\",RIGHT(H1846,LEN(H1846)-4),RIGHT(H1846,LEN(H1846)-6)),\"\"))","v":""}]
[50001466,"Sungrow","SH8.0RT",8,8,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2023-07-27","Martin Bertsch","2023-07-27","LCD:SAPPHIRE-H_01011.51.04 MDSP:SAPPHIRE-H_03011.51.03 SDSP: SUBCTL-S_04011.01.01",null,null,null,"Ja","Nein","Ja","OK","Christian Elbs","SGR-ESH-P20120741-R1\r","2022-03-02","nicht vorhanden","OK",null,"nicht vorhanden",null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1847,1)=\"J\",LEFT(H1847,2),LEFT(H1847,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1847,1)=\"J\",RIGHT(H1847,LEN(H1847)-4),RIGHT(H1847,LEN(H1847)-6)),\"\"))","v":"mit Einschränkung"}]
[50001467,"Sungrow","SG8.0RT",8,8.8000000000000007,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1848,1)=\"J\",LEFT(H1848,2),LEFT(H1848,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1848,1)=\"J\",RIGHT(H1848,LEN(H1848)-4),RIGHT(H1848,LEN(H1848)-6)),\"\"))","v":""}]
[50001468,"Sungrow","SH10RT",10,10,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2023-10-23","Martin Bertsch","2023-07-27","LCD:SAPPHIRE-H_01011.51.04 MDSP:SAPPHIRE-H_03011.51.03 SDSP: SUBCTL-S_04011.01.01",null,null,null,"Ja","Nein","Ja","OK","Christian Elbs","SGR-ESH-P20120741-R1\r","2022-03-02","nicht vorhanden","OK",null,"nicht vorhanden",null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1849,1)=\"J\",LEFT(H1849,2),LEFT(H1849,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1849,1)=\"J\",RIGHT(H1849,LEN(H1849)-4),RIGHT(H1849,LEN(H1849)-6)),\"\"))","v":"mit Einschränkung"}]
[50001469,"Sungrow","SG10RT",10,11,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1850,1)=\"J\",LEFT(H1850,2),LEFT(H1850,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1850,1)=\"J\",RIGHT(H1850,LEN(H1850)-4),RIGHT(H1850,LEN(H1850)-6)),\"\"))","v":""}]
[50001470,"Sungrow","SG12RT",12,13.2,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,"Prüfbericht von Kostal Piko IQ 7.0",null,{"$f":"IF(LEFT(H1851,1)=\"J\",LEFT(H1851,2),LEFT(H1851,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1851,1)=\"J\",RIGHT(H1851,LEN(H1851)-4),RIGHT(H1851,LEN(H1851)-6)),\"\"))","v":""}]
[50001471,"Sungrow","SG15RT",15,16.5,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1852,1)=\"J\",LEFT(H1852,2),LEFT(H1852,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1852,1)=\"J\",RIGHT(H1852,LEN(H1852)-4),RIGHT(H1852,LEN(H1852)-6)),\"\"))","v":""}]
[50001472,"Sungrow","SG17RT",17,18.7,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1853,1)=\"J\",LEFT(H1853,2),LEFT(H1853,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1853,1)=\"J\",RIGHT(H1853,LEN(H1853)-4),RIGHT(H1853,LEN(H1853)-6)),\"\"))","v":""}]
[50001473,"Sungrow","SG20RT",20,22,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1854,1)=\"J\",LEFT(H1854,2),LEFT(H1854,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1854,1)=\"J\",RIGHT(H1854,LEN(H1854)-4),RIGHT(H1854,LEN(H1854)-6)),\"\"))","v":""}]
[50001474,"Sungrow","SG33CX ",36.299999999999997,36.299999999999997,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"CN21AJ2P 001","2021-01-25",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1855,1)=\"J\",LEFT(H1855,2),LEFT(H1855,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1855,1)=\"J\",RIGHT(H1855,LEN(H1855)-4),RIGHT(H1855,LEN(H1855)-6)),\"\"))","v":""}]
[50001475,"Sungrow","SG40CX ",44,44,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"CN21AJ2P 001","2021-01-25",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1856,1)=\"J\",LEFT(H1856,2),LEFT(H1856,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1856,1)=\"J\",RIGHT(H1856,LEN(H1856)-4),RIGHT(H1856,LEN(H1856)-6)),\"\"))","v":""}]
[50001476,"Sungrow","SG50CX ",55,55,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,"Nein","Nein",null,"Vorhanden",null,"CN21AJ2P 001","2021-01-25",null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H1857,1)=\"J\",LEFT(H1857,2),LEFT(H1857,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1857,1)=\"J\",RIGHT(H1857,LEN(H1857)-4),RIGHT(H1857,LEN(H1857)-6)),\"\"))","v":""}]
[50001477,"Sungrow","SG110CX",null,110,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,"Vorhanden",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1858,1)=\"J\",LEFT(H1858,2),LEFT(H1858,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1858,1)=\"J\",RIGHT(H1858,LEN(H1858)-4),RIGHT(H1858,LEN(H1858)-6)),\"\"))","v":""}]
[50001478,"Sungrow","SG125HV",null,125,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1859,1)=\"J\",LEFT(H1859,2),LEFT(H1859,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1859,1)=\"J\",RIGHT(H1859,LEN(H1859)-4),RIGHT(H1859,LEN(H1859)-6)),\"\"))","v":""}]
[50001479,"Sungrow","SG125HX",null,125,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1860,1)=\"J\",LEFT(H1860,2),LEFT(H1860,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1860,1)=\"J\",RIGHT(H1860,LEN(H1860)-4),RIGHT(H1860,LEN(H1860)-6)),\"\"))","v":""}]
[50001480,"Sungrow","SG250HX",null,250,3,"PV-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1861,1)=\"J\",LEFT(H1861,2),LEFT(H1861,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1861,1)=\"J\",RIGHT(H1861,LEN(H1861)-4),RIGHT(H1861,LEN(H1861)-6)),\"\"))","v":""}]
[50001481,"SUNMASTER","SMMI-600W",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-04-19","Martin Bertsch","2023-04-19",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"221212ST4158-EG-DE-001","2023-01-18",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1862,1)=\"J\",LEFT(H1862,2),LEFT(H1862,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1862,1)=\"J\",RIGHT(H1862,LEN(H1862)-4),RIGHT(H1862,LEN(H1862)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001482,"SUNMASTER","SMMI-700W",0.7,0.7,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-04-19","Martin Bertsch","2023-04-19",null,null,null,null,null,null,null,null,null,"221212ST4158-EG-DE-001","2023-01-18",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1863,1)=\"J\",LEFT(H1863,2),LEFT(H1863,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1863,1)=\"J\",RIGHT(H1863,LEN(H1863)-4),RIGHT(H1863,LEN(H1863)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001483,"SUNMASTER","SMMI-800W",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-04-19","Martin Bertsch","2023-04-19",null,null,null,null,null,null,null,null,null,"221212ST4158-EG-DE-001","2023-01-18",null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1864,1)=\"J\",LEFT(H1864,2),LEFT(H1864,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1864,1)=\"J\",RIGHT(H1864,LEN(H1864)-4),RIGHT(H1864,LEN(H1864)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001484,"SUNWAYS","STH-4KTL-HT",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1865,1)=\"J\",LEFT(H1865,2),LEFT(H1865,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1865,1)=\"J\",RIGHT(H1865,LEN(H1865)-4),RIGHT(H1865,LEN(H1865)-6)),\"\"))","v":"mit Einschränkung"}]
[50001977,"SUNWAYS","STH-4KTL-HT-P",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1866,1)=\"J\",LEFT(H1866,2),LEFT(H1866,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1866,1)=\"J\",RIGHT(H1866,LEN(H1866)-4),RIGHT(H1866,LEN(H1866)-6)),\"\"))","v":"mit Einschränkung"}]
[50001485,"SUNWAYS","STH-5KTL-HT",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1867,1)=\"J\",LEFT(H1867,2),LEFT(H1867,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1867,1)=\"J\",RIGHT(H1867,LEN(H1867)-4),RIGHT(H1867,LEN(H1867)-6)),\"\"))","v":"mit Einschränkung"}]
[50001978,"SUNWAYS","STH-5KTL-HT-P",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1868,1)=\"J\",LEFT(H1868,2),LEFT(H1868,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1868,1)=\"J\",RIGHT(H1868,LEN(H1868)-4),RIGHT(H1868,LEN(H1868)-6)),\"\"))","v":"mit Einschränkung"}]
[50001486,"SUNWAYS","STH-6KTL-HT",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1869,1)=\"J\",LEFT(H1869,2),LEFT(H1869,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1869,1)=\"J\",RIGHT(H1869,LEN(H1869)-4),RIGHT(H1869,LEN(H1869)-6)),\"\"))","v":"mit Einschränkung"}]
[50001979,"SUNWAYS","STH-6KTL-HT-P",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1870,1)=\"J\",LEFT(H1870,2),LEFT(H1870,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1870,1)=\"J\",RIGHT(H1870,LEN(H1870)-4),RIGHT(H1870,LEN(H1870)-6)),\"\"))","v":"mit Einschränkung"}]
[50001487,"SUNWAYS","STH-8KTL-HT",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1871,1)=\"J\",LEFT(H1871,2),LEFT(H1871,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1871,1)=\"J\",RIGHT(H1871,LEN(H1871)-4),RIGHT(H1871,LEN(H1871)-6)),\"\"))","v":"mit Einschränkung"}]
[50001980,"SUNWAYS","STH-8KTL-HT-P",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1872,1)=\"J\",LEFT(H1872,2),LEFT(H1872,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1872,1)=\"J\",RIGHT(H1872,LEN(H1872)-4),RIGHT(H1872,LEN(H1872)-6)),\"\"))","v":"mit Einschränkung"}]
[50001488,"SUNWAYS","STH-10KTL-HT",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1873,1)=\"J\",LEFT(H1873,2),LEFT(H1873,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1873,1)=\"J\",RIGHT(H1873,LEN(H1873)-4),RIGHT(H1873,LEN(H1873)-6)),\"\"))","v":"mit Einschränkung"}]
[50001981,"SUNWAYS","STH-10KTL-HT-P",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1874,1)=\"J\",LEFT(H1874,2),LEFT(H1874,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1874,1)=\"J\",RIGHT(H1874,LEN(H1874)-4),RIGHT(H1874,LEN(H1874)-6)),\"\"))","v":"mit Einschränkung"}]
[50001489,"SUNWAYS","STH-12KTL-HT",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1875,1)=\"J\",LEFT(H1875,2),LEFT(H1875,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1875,1)=\"J\",RIGHT(H1875,LEN(H1875)-4),RIGHT(H1875,LEN(H1875)-6)),\"\"))","v":"mit Einschränkung"}]
[50001982,"SUNWAYS","STH-12KTL-HT-P",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-15","Martin Bertsch","2024-01-03","V1.6.0.0",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6442730.50","2023-11-15",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1876,1)=\"J\",LEFT(H1876,2),LEFT(H1876,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1876,1)=\"J\",RIGHT(H1876,LEN(H1876)-4),RIGHT(H1876,LEN(H1876)-6)),\"\"))","v":"mit Einschränkung"}]
[50001983,"Swatten","SiH-5kW-TH",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-02-22","Martin Bertsch","2024-02-22","Software_Master_Version: SIHXXTH_01_1_ARM.01.011 Main_DSP_Software_Version: SIHXXTH_01_1_MDSP.01.014",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6179237.50","2023-12-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1877,1)=\"J\",LEFT(H1877,2),LEFT(H1877,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1877,1)=\"J\",RIGHT(H1877,LEN(H1877)-4),RIGHT(H1877,LEN(H1877)-6)),\"\"))","v":"mit Einschränkung"}]
[50001984,"Swatten","SiH-6kW-TH",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-02-22","Martin Bertsch","2024-02-22","Software_Master_Version: SIHXXTH_01_1_ARM.01.011 Main_DSP_Software_Version: SIHXXTH_01_1_MDSP.01.014",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6179237.50","2023-12-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1878,1)=\"J\",LEFT(H1878,2),LEFT(H1878,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1878,1)=\"J\",RIGHT(H1878,LEN(H1878)-4),RIGHT(H1878,LEN(H1878)-6)),\"\"))","v":"mit Einschränkung"}]
[50001985,"Swatten","SiH-8kW-TH",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-02-22","Martin Bertsch","2024-02-22","Software_Master_Version: SIHXXTH_01_1_ARM.01.011 Main_DSP_Software_Version: SIHXXTH_01_1_MDSP.01.014",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6179237.50","2023-12-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1879,1)=\"J\",LEFT(H1879,2),LEFT(H1879,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1879,1)=\"J\",RIGHT(H1879,LEN(H1879)-4),RIGHT(H1879,LEN(H1879)-6)),\"\"))","v":"mit Einschränkung"}]
[50001986,"Swatten","SiH-10kW-TH",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-02-22","Martin Bertsch","2024-02-22","Software_Master_Version: SIHXXTH_01_1_ARM.01.011 Main_DSP_Software_Version: SIHXXTH_01_1_MDSP.01.014",null,null,null,"Ja","Nein","Nein","Vorhanden",null,"6179237.50","2023-12-20","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1880,1)=\"J\",LEFT(H1880,2),LEFT(H1880,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1880,1)=\"J\",RIGHT(H1880,LEN(H1880)-4),RIGHT(H1880,LEN(H1880)-6)),\"\"))","v":"mit Einschränkung"}]
[50001490,"TIGO","TSI-5K3D",5,5.5,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1881,1)=\"J\",LEFT(H1881,2),LEFT(H1881,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1881,1)=\"J\",RIGHT(H1881,LEN(H1881)-4),RIGHT(H1881,LEN(H1881)-6)),\"\"))","v":""}]
[50001491,"TIGO","TSI-6K3A",6,6.6,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1882,1)=\"J\",LEFT(H1882,2),LEFT(H1882,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1882,1)=\"J\",RIGHT(H1882,LEN(H1882)-4),RIGHT(H1882,LEN(H1882)-6)),\"\"))","v":""}]
[50001492,"TIGO","TSI-6K3D",6,6.6,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1883,1)=\"J\",LEFT(H1883,2),LEFT(H1883,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1883,1)=\"J\",RIGHT(H1883,LEN(H1883)-4),RIGHT(H1883,LEN(H1883)-6)),\"\"))","v":""}]
[50001493,"TIGO","TSI-8K3A",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1884,1)=\"J\",LEFT(H1884,2),LEFT(H1884,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1884,1)=\"J\",RIGHT(H1884,LEN(H1884)-4),RIGHT(H1884,LEN(H1884)-6)),\"\"))","v":""}]
[50001494,"TIGO","TSI-8K3D",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1885,1)=\"J\",LEFT(H1885,2),LEFT(H1885,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1885,1)=\"J\",RIGHT(H1885,LEN(H1885)-4),RIGHT(H1885,LEN(H1885)-6)),\"\"))","v":""}]
[50001495,"TIGO","TSI-10K3A",10,11,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1886,1)=\"J\",LEFT(H1886,2),LEFT(H1886,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1886,1)=\"J\",RIGHT(H1886,LEN(H1886)-4),RIGHT(H1886,LEN(H1886)-6)),\"\"))","v":""}]
[50001496,"TIGO","TSI-10K3D",10,11,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1887,1)=\"J\",LEFT(H1887,2),LEFT(H1887,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1887,1)=\"J\",RIGHT(H1887,LEN(H1887)-4),RIGHT(H1887,LEN(H1887)-6)),\"\"))","v":""}]
[50001497,"TIGO","TSI-12K3D",12,13.2,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1888,1)=\"J\",LEFT(H1888,2),LEFT(H1888,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1888,1)=\"J\",RIGHT(H1888,LEN(H1888)-4),RIGHT(H1888,LEN(H1888)-6)),\"\"))","v":""}]
[50001498,"TIGO","TSI-15K3A",15,15,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1889,1)=\"J\",LEFT(H1889,2),LEFT(H1889,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1889,1)=\"J\",RIGHT(H1889,LEN(H1889)-4),RIGHT(H1889,LEN(H1889)-6)),\"\"))","v":""}]
[50001499,"TIGO","TSI-15K3D",15,15,3,"Hybrid-Wechselrichter","Ja","2022-12-19","Martin Bertsch","2022-12-14",null,null,null,null,"Ja",null,"Nein","Vorhanden",null,"CN2182YH 003","2022-06-24",null,"Vorhanden",null,null,null,null,"ident zu SOLAX X3 HYBRID G4",null,null,null,null,{"$f":"IF(LEFT(H1890,1)=\"J\",LEFT(H1890,2),LEFT(H1890,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1890,1)=\"J\",RIGHT(H1890,LEN(H1890)-4),RIGHT(H1890,LEN(H1890)-6)),\"\"))","v":""}]
[50001784,"TOMMATECH","Uno-A-0.6-S-D(L)",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1891,1)=\"J\",LEFT(H1891,2),LEFT(H1891,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1891,1)=\"J\",RIGHT(H1891,LEN(H1891)-4),RIGHT(H1891,LEN(H1891)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001790,"TOMMATECH","Uno-A-0.6-S-N(L)",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1892,1)=\"J\",LEFT(H1892,2),LEFT(H1892,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1892,1)=\"J\",RIGHT(H1892,LEN(H1892)-4),RIGHT(H1892,LEN(H1892)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001779,"TOMMATECH","Uno-A-0.7-S-D(L)",0.7,0.77,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1893,1)=\"J\",LEFT(H1893,2),LEFT(H1893,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1893,1)=\"J\",RIGHT(H1893,LEN(H1893)-4),RIGHT(H1893,LEN(H1893)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001791,"TOMMATECH","Uno-A-0.7-S-N(L)",0.7,0.77,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1894,1)=\"J\",LEFT(H1894,2),LEFT(H1894,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1894,1)=\"J\",RIGHT(H1894,LEN(H1894)-4),RIGHT(H1894,LEN(H1894)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001780,"TOMMATECH","Uno-A-1.1-S-D(L)",1.1000000000000001,1.21,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1895,1)=\"J\",LEFT(H1895,2),LEFT(H1895,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1895,1)=\"J\",RIGHT(H1895,LEN(H1895)-4),RIGHT(H1895,LEN(H1895)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001792,"TOMMATECH","Uno-A-1.1-S-N(L)",1.1000000000000001,1.21,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1896,1)=\"J\",LEFT(H1896,2),LEFT(H1896,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1896,1)=\"J\",RIGHT(H1896,LEN(H1896)-4),RIGHT(H1896,LEN(H1896)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001781,"TOMMATECH","Uno-A-1.5-S-D(L)",1.5,1.65,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1897,1)=\"J\",LEFT(H1897,2),LEFT(H1897,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1897,1)=\"J\",RIGHT(H1897,LEN(H1897)-4),RIGHT(H1897,LEN(H1897)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001793,"TOMMATECH","Uno-A-1.5-S-N(L)",1.5,1.65,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1898,1)=\"J\",LEFT(H1898,2),LEFT(H1898,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1898,1)=\"J\",RIGHT(H1898,LEN(H1898)-4),RIGHT(H1898,LEN(H1898)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001785,"TOMMATECH","Uno-A-2.0-S-D(L)",2,2.2000000000000002,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1899,1)=\"J\",LEFT(H1899,2),LEFT(H1899,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1899,1)=\"J\",RIGHT(H1899,LEN(H1899)-4),RIGHT(H1899,LEN(H1899)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001794,"TOMMATECH","Uno-A-2.0-S-N(L)",2,2.2000000000000002,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1900,1)=\"J\",LEFT(H1900,2),LEFT(H1900,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1900,1)=\"J\",RIGHT(H1900,LEN(H1900)-4),RIGHT(H1900,LEN(H1900)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001786,"TOMMATECH","Uno-A-2.5K-S-D(L)",2.5,2.75,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1901,1)=\"J\",LEFT(H1901,2),LEFT(H1901,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1901,1)=\"J\",RIGHT(H1901,LEN(H1901)-4),RIGHT(H1901,LEN(H1901)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001795,"TOMMATECH","Uno-A-2.5K-S-N(L)",2.5,2.75,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1902,1)=\"J\",LEFT(H1902,2),LEFT(H1902,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1902,1)=\"J\",RIGHT(H1902,LEN(H1902)-4),RIGHT(H1902,LEN(H1902)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001760,"TOMMATECH","Trio-Atom 3.0K",3,3.3,3,"PV-Wechselrichter","Ja","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 002","2023-02-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1903,1)=\"J\",LEFT(H1903,2),LEFT(H1903,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1903,1)=\"J\",RIGHT(H1903,LEN(H1903)-4),RIGHT(H1903,LEN(H1903)-6)),\"\"))","v":""}]
[50001788,"TOMMATECH","Uno-A-3.3K-S-D(L)",3.3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1904,1)=\"J\",LEFT(H1904,2),LEFT(H1904,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1904,1)=\"J\",RIGHT(H1904,LEN(H1904)-4),RIGHT(H1904,LEN(H1904)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001797,"TOMMATECH","Uno-A-3.3K-S-N(L)",3.3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1905,1)=\"J\",LEFT(H1905,2),LEFT(H1905,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1905,1)=\"J\",RIGHT(H1905,LEN(H1905)-4),RIGHT(H1905,LEN(H1905)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001787,"TOMMATECH","Uno-A-3K-S-D(L)",3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1906,1)=\"J\",LEFT(H1906,2),LEFT(H1906,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1906,1)=\"J\",RIGHT(H1906,LEN(H1906)-4),RIGHT(H1906,LEN(H1906)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001796,"TOMMATECH","Uno-A-3K-S-N(L)",3,3.3,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1907,1)=\"J\",LEFT(H1907,2),LEFT(H1907,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1907,1)=\"J\",RIGHT(H1907,LEN(H1907)-4),RIGHT(H1907,LEN(H1907)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001789,"TOMMATECH","Uno-A-3.6K-S-D(L)",3.68,3.68,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1908,1)=\"J\",LEFT(H1908,2),LEFT(H1908,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1908,1)=\"J\",RIGHT(H1908,LEN(H1908)-4),RIGHT(H1908,LEN(H1908)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001798,"TOMMATECH","Uno-A-3.6K-S-N(L)",3.68,3.68,1,"PV-Wechselrichter","Ja - <= 16A Anlage","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Moustafa Mohamed (Netz NÖ)","CN22NLCH 003","2023-03-09","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1909,1)=\"J\",LEFT(H1909,2),LEFT(H1909,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1909,1)=\"J\",RIGHT(H1909,LEN(H1909)-4),RIGHT(H1909,LEN(H1909)-6)),\"\"))","v":"<= 16A Anlage"}]
[50001761,"TOMMATECH","Trio-Atom 4.0K",4,4.4000000000000004,3,"PV-Wechselrichter","Ja","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 002","2023-02-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1910,1)=\"J\",LEFT(H1910,2),LEFT(H1910,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1910,1)=\"J\",RIGHT(H1910,LEN(H1910)-4),RIGHT(H1910,LEN(H1910)-6)),\"\"))","v":""}]
[50001762,"TOMMATECH","Trio-Atom 5.0K",5,5.5,3,"PV-Wechselrichter","Ja","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 002","2023-02-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1911,1)=\"J\",LEFT(H1911,2),LEFT(H1911,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1911,1)=\"J\",RIGHT(H1911,LEN(H1911)-4),RIGHT(H1911,LEN(H1911)-6)),\"\"))","v":""}]
[50001768,"TOMMATECH","Trio-Hybrid 5.0K",5,5.5,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1912,1)=\"J\",LEFT(H1912,2),LEFT(H1912,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1912,1)=\"J\",RIGHT(H1912,LEN(H1912)-4),RIGHT(H1912,LEN(H1912)-6)),\"\"))","v":""}]
[50001763,"TOMMATECH","Trio-Atom 6.0K",6,6.6,3,"PV-Wechselrichter","Ja","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 002","2023-02-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1913,1)=\"J\",LEFT(H1913,2),LEFT(H1913,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1913,1)=\"J\",RIGHT(H1913,LEN(H1913)-4),RIGHT(H1913,LEN(H1913)-6)),\"\"))","v":""}]
[50001774,"TOMMATECH","Trio-BackUp 6.0K",6,6.6,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1914,1)=\"J\",LEFT(H1914,2),LEFT(H1914,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1914,1)=\"J\",RIGHT(H1914,LEN(H1914)-4),RIGHT(H1914,LEN(H1914)-6)),\"\"))","v":""}]
[50001769,"TOMMATECH","Trio-Hybrid 6.0K",6,6.6,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1915,1)=\"J\",LEFT(H1915,2),LEFT(H1915,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1915,1)=\"J\",RIGHT(H1915,LEN(H1915)-4),RIGHT(H1915,LEN(H1915)-6)),\"\"))","v":""}]
[50001764,"TOMMATECH","Trio-Atom 8.0K",8,8.8000000000000007,3,"PV-Wechselrichter","Ja","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 002","2023-02-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1916,1)=\"J\",LEFT(H1916,2),LEFT(H1916,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1916,1)=\"J\",RIGHT(H1916,LEN(H1916)-4),RIGHT(H1916,LEN(H1916)-6)),\"\"))","v":""}]
[50001775,"TOMMATECH","Trio-BackUp 8.0K",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1917,1)=\"J\",LEFT(H1917,2),LEFT(H1917,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1917,1)=\"J\",RIGHT(H1917,LEN(H1917)-4),RIGHT(H1917,LEN(H1917)-6)),\"\"))","v":""}]
[50001770,"TOMMATECH","Trio-Hybrid 8.0K",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1918,1)=\"J\",LEFT(H1918,2),LEFT(H1918,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1918,1)=\"J\",RIGHT(H1918,LEN(H1918)-4),RIGHT(H1918,LEN(H1918)-6)),\"\"))","v":""}]
[50001765,"TOMMATECH","Trio-Atom 10.0K",10,11,3,"PV-Wechselrichter","Ja","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 002","2023-02-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1919,1)=\"J\",LEFT(H1919,2),LEFT(H1919,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1919,1)=\"J\",RIGHT(H1919,LEN(H1919)-4),RIGHT(H1919,LEN(H1919)-6)),\"\"))","v":""}]
[50001776,"TOMMATECH","Trio-BackUp 10.0K",10,11,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1920,1)=\"J\",LEFT(H1920,2),LEFT(H1920,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1920,1)=\"J\",RIGHT(H1920,LEN(H1920)-4),RIGHT(H1920,LEN(H1920)-6)),\"\"))","v":""}]
[50001771,"TOMMATECH","Trio-Hybrid 10.0K",10,11,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1921,1)=\"J\",LEFT(H1921,2),LEFT(H1921,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1921,1)=\"J\",RIGHT(H1921,LEN(H1921)-4),RIGHT(H1921,LEN(H1921)-6)),\"\"))","v":""}]
[50001766,"TOMMATECH","Trio-Atom 12.0K",12,13.2,3,"PV-Wechselrichter","Ja","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 002","2023-02-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1922,1)=\"J\",LEFT(H1922,2),LEFT(H1922,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1922,1)=\"J\",RIGHT(H1922,LEN(H1922)-4),RIGHT(H1922,LEN(H1922)-6)),\"\"))","v":""}]
[50001772,"TOMMATECH","Trio-Hybrid 12.0K",12,13.2,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1923,1)=\"J\",LEFT(H1923,2),LEFT(H1923,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1923,1)=\"J\",RIGHT(H1923,LEN(H1923)-4),RIGHT(H1923,LEN(H1923)-6)),\"\"))","v":""}]
[50001767,"TOMMATECH","Trio-Atom 15.0K",15,15,3,"PV-Wechselrichter","Ja","2024-03-14","Martin Bertsch","2023-09-13",null,null,null,null,"Nein","Nein","Nein","OK","Martin Bertsch","CN225LEG 002","2023-02-17","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1924,1)=\"J\",LEFT(H1924,2),LEFT(H1924,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1924,1)=\"J\",RIGHT(H1924,LEN(H1924)-4),RIGHT(H1924,LEN(H1924)-6)),\"\"))","v":""}]
[50001777,"TOMMATECH","Trio-BackUp 15.0K",15,15,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1925,1)=\"J\",LEFT(H1925,2),LEFT(H1925,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1925,1)=\"J\",RIGHT(H1925,LEN(H1925)-4),RIGHT(H1925,LEN(H1925)-6)),\"\"))","v":""}]
[50001773,"TOMMATECH","Trio-Hybrid 15.0K",15,15,3,"Hybrid-Wechselrichter","Ja","2023-09-13","Martin Bertsch","2023-09-13",null,null,null,null,"Ja","Nein","Nein","Vorhanden","Markus Radauer","CN2182YH 005","2023-03-16","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1926,1)=\"J\",LEFT(H1926,2),LEFT(H1926,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1926,1)=\"J\",RIGHT(H1926,LEN(H1926)-4),RIGHT(H1926,LEN(H1926)-6)),\"\"))","v":""}]
[50001500,"Trumpf Hüttinger GmbH","TruConvert AC 3025",25,25,3,"AC-Batteriewechselrichter","Ja","2023-10-17","Martin Bertsch","2022-06-30",null,null,null,null,"Ja","Ja","Nein","OK","Roland Bründlinger","19TH0414-OVE-directive R25_4","2023-10-16",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1927,1)=\"J\",LEFT(H1927,2),LEFT(H1927,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1927,1)=\"J\",RIGHT(H1927,LEN(H1927)-4),RIGHT(H1927,LEN(H1927)-6)),\"\"))","v":""}]
[50001501,"TSUN","TSOL-MS300",0.3,0.3,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-06-27","Martin Bertsch","2023-06-27",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"221101454SHA-006","2023-05-29","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1928,1)=\"J\",LEFT(H1928,2),LEFT(H1928,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1928,1)=\"J\",RIGHT(H1928,LEN(H1928)-4),RIGHT(H1928,LEN(H1928)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001502,"TSUN","TSOL-M350",0.35,0.35,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-03-23","Martin Bertsch","2023-03-23",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"AQRN-19SE2405FCSHP-6","2020-04-08","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1929,1)=\"J\",LEFT(H1929,2),LEFT(H1929,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1929,1)=\"J\",RIGHT(H1929,LEN(H1929)-4),RIGHT(H1929,LEN(H1929)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001503,"TSUN","TSOL-MS350",0.35,0.35,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-06-27","Martin Bertsch","2023-06-27",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"221101454SHA-006","2023-05-29","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1930,1)=\"J\",LEFT(H1930,2),LEFT(H1930,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1930,1)=\"J\",RIGHT(H1930,LEN(H1930)-4),RIGHT(H1930,LEN(H1930)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001504,"TSUN","TSOL-M400",0.4,0.4,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-03-23","Martin Bertsch","2023-03-23",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"AQRN-19SE2405FCSHP-6","2020-04-08","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1931,1)=\"J\",LEFT(H1931,2),LEFT(H1931,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1931,1)=\"J\",RIGHT(H1931,LEN(H1931)-4),RIGHT(H1931,LEN(H1931)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001505,"TSUN","TSOL-MS400",0.4,0.4,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-06-27","Martin Bertsch","2023-06-27",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"221101454SHA-006","2023-05-29","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1932,1)=\"J\",LEFT(H1932,2),LEFT(H1932,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1932,1)=\"J\",RIGHT(H1932,LEN(H1932)-4),RIGHT(H1932,LEN(H1932)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001506,"TSUN","TSOL-MS600",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-06-27","Martin Bertsch","2023-06-27",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"221101454SHA-006","2023-05-29","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1933,1)=\"J\",LEFT(H1933,2),LEFT(H1933,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1933,1)=\"J\",RIGHT(H1933,LEN(H1933)-4),RIGHT(H1933,LEN(H1933)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001507,"TSUN","TSOL-M800",0.7,0.7,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-06-29","Martin Bertsch","2023-06-29",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"AQRN-19SE2405FCSHP-5","2020-04-07","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1934,1)=\"J\",LEFT(H1934,2),LEFT(H1934,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1934,1)=\"J\",RIGHT(H1934,LEN(H1934)-4),RIGHT(H1934,LEN(H1934)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001508,"TSUN","TSOL-MS700",0.7,0.7,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-06-27","Martin Bertsch","2023-06-27",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"221101454SHA-006","2023-05-29","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1935,1)=\"J\",LEFT(H1935,2),LEFT(H1935,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1935,1)=\"J\",RIGHT(H1935,LEN(H1935)-4),RIGHT(H1935,LEN(H1935)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001509,"TSUN","TSOL-MS800",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-06-27","Martin Bertsch","2023-06-27",null,null,null,null,"Nein","Nein","Nein","VDE4105/4110",null,"221101454SHA-006","2023-05-29","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1936,1)=\"J\",LEFT(H1936,2),LEFT(H1936,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1936,1)=\"J\",RIGHT(H1936,LEN(H1936)-4),RIGHT(H1936,LEN(H1936)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001510,"Vaillant","VPVI 3000/1 ",3.2,3.2,3,"PV-Wechselrichter","Ja",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"13TH0511-OVE-directive R25_1",null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - gleich wie Steca/Katek ","F","F",null,null,{"$f":"IF(LEFT(H1937,1)=\"J\",LEFT(H1937,2),LEFT(H1937,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1937,1)=\"J\",RIGHT(H1937,LEN(H1937)-4),RIGHT(H1937,LEN(H1937)-6)),\"\"))","v":""}]
[50001511,"Vaillant","VPVI 4000/1 ",4,4,3,"PV-Wechselrichter","Ja",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"13TH0511-OVE-directive R25_1",null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - gleich wie Steca/Katek ","F","F",null,null,{"$f":"IF(LEFT(H1938,1)=\"J\",LEFT(H1938,2),LEFT(H1938,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1938,1)=\"J\",RIGHT(H1938,LEN(H1938)-4),RIGHT(H1938,LEN(H1938)-6)),\"\"))","v":""}]
[50001512,"Vaillant","VPVI 5000/1 ",5,5,3,"PV-Wechselrichter","Ja",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"13TH0511-OVE-directive R25_1",null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - gleich wie Steca/Katek ","F","F",null,null,{"$f":"IF(LEFT(H1939,1)=\"J\",LEFT(H1939,2),LEFT(H1939,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1939,1)=\"J\",RIGHT(H1939,LEN(H1939)-4),RIGHT(H1939,LEN(H1939)-6)),\"\"))","v":""}]
[50001513,"Vaillant","VPVI 6000/1 ",6,6,3,"PV-Wechselrichter","Ja",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"Vorhanden",null,"13TH0511-OVE-directive R25_1",null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 3~ - gleich wie Steca/Katek ","F","F",null,null,{"$f":"IF(LEFT(H1940,1)=\"J\",LEFT(H1940,2),LEFT(H1940,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1940,1)=\"J\",RIGHT(H1940,LEN(H1940)-4),RIGHT(H1940,LEN(H1940)-6)),\"\"))","v":""}]
[50001514,"Varta","PULSE NEO 3",null,1.6,1,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - VDE 4105","F","F",null,null,{"$f":"IF(LEFT(H1941,1)=\"J\",LEFT(H1941,2),LEFT(H1941,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1941,1)=\"J\",RIGHT(H1941,LEN(H1941)-4),RIGHT(H1941,LEN(H1941)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001515,"Varta","Element Backup 6/S5",null,1.8,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,null,null,null,null,null,"Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - NICHT einspeiserelevant- KONFORM TOR Erzeuger A","F","F",null,null,{"$f":"IF(LEFT(H1942,1)=\"J\",LEFT(H1942,2),LEFT(H1942,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1942,1)=\"J\",RIGHT(H1942,LEN(H1942)-4),RIGHT(H1942,LEN(H1942)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001516,"Varta","ELEMENT 6/S4",null,2.2000000000000002,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - VDE 4105","F","F",null,null,{"$f":"IF(LEFT(H1943,1)=\"J\",LEFT(H1943,2),LEFT(H1943,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1943,1)=\"J\",RIGHT(H1943,LEN(H1943)-4),RIGHT(H1943,LEN(H1943)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001517,"Varta","PULSE NEO 6",null,2.5,1,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - VDE 4105","F","F",null,null,{"$f":"IF(LEFT(H1944,1)=\"J\",LEFT(H1944,2),LEFT(H1944,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1944,1)=\"J\",RIGHT(H1944,LEN(H1944)-4),RIGHT(H1944,LEN(H1944)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001518,"Varta","ELEMENT 9/S4",null,3.4,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - VDE 4105","F","F",null,null,{"$f":"IF(LEFT(H1945,1)=\"J\",LEFT(H1945,2),LEFT(H1945,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1945,1)=\"J\",RIGHT(H1945,LEN(H1945)-4),RIGHT(H1945,LEN(H1945)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001519,"Varta","Element Backup 12/S5",null,3.7,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,null,null,null,null,null,"Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - NICHT einspeiserelevant- KONFORM TOR Erzeuger A","F","F",null,null,{"$f":"IF(LEFT(H1946,1)=\"J\",LEFT(H1946,2),LEFT(H1946,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1946,1)=\"J\",RIGHT(H1946,LEN(H1946)-4),RIGHT(H1946,LEN(H1946)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001520,"Varta","ELEMENT 12/S4",null,4,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,"2021-05-06",null,null,null,null,"Nein","Nein",null,"nicht vorhanden",null,null,null,null,"OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - VDE 4105","F","F",null,null,{"$f":"IF(LEFT(H1947,1)=\"J\",LEFT(H1947,2),LEFT(H1947,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1947,1)=\"J\",RIGHT(H1947,LEN(H1947)-4),RIGHT(H1947,LEN(H1947)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001521,"Varta","Element Backup 18/S5",null,4,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,null,null,null,null,null,"Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - NICHT einspeiserelevant- KONFORM TOR Erzeuger A","F","F",null,null,{"$f":"IF(LEFT(H1948,1)=\"J\",LEFT(H1948,2),LEFT(H1948,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1948,1)=\"J\",RIGHT(H1948,LEN(H1948)-4),RIGHT(H1948,LEN(H1948)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001522,"Varta","FLEX STORAGE E (36 kVA)",null,36,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,null,null,null,"2021-03-01",null,"Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - NICHT einspeiserelevant- KONFORM TOR Erzeuger A+B","F","F",null,null,{"$f":"IF(LEFT(H1949,1)=\"J\",LEFT(H1949,2),LEFT(H1949,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1949,1)=\"J\",RIGHT(H1949,LEN(H1949)-4),RIGHT(H1949,LEN(H1949)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001523,"Varta","FLEX STORAGE E (80 kVA)",null,80,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,null,null,null,"2021-03-02",null,"Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - NICHT einspeiserelevant- KONFORM TOR Erzeuger A+B","F","F",null,null,{"$f":"IF(LEFT(H1950,1)=\"J\",LEFT(H1950,2),LEFT(H1950,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1950,1)=\"J\",RIGHT(H1950,LEN(H1950)-4),RIGHT(H1950,LEN(H1950)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001524,"Varta","FLEX STORAGE E (120 kVA)",null,120,3,"AC-Batteriewechselrichter","Ja - nur für Eigenverbrauch",null,null,null,null,null,"2021-03-01",null,"Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - NICHT einspeiserelevant- KONFORM TOR Erzeuger A+B","F","F",null,null,{"$f":"IF(LEFT(H1951,1)=\"J\",LEFT(H1951,2),LEFT(H1951,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1951,1)=\"J\",RIGHT(H1951,LEN(H1951)-4),RIGHT(H1951,LEN(H1951)-6)),\"\"))","v":"nur für Eigenverbrauch"}]
[50001525,"Victron Energy","MultiPlus 12/500/20",0.43,0.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1952,1)=\"J\",LEFT(H1952,2),LEFT(H1952,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1952,1)=\"J\",RIGHT(H1952,LEN(H1952)-4),RIGHT(H1952,LEN(H1952)-6)),\"\"))","v":""}]
[50001526,"Victron Energy","MultiPlus 24/500/10",0.43,0.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1953,1)=\"J\",LEFT(H1953,2),LEFT(H1953,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1953,1)=\"J\",RIGHT(H1953,LEN(H1953)-4),RIGHT(H1953,LEN(H1953)-6)),\"\"))","v":""}]
[50001527,"Victron Energy","MultiPlus 48/500/6",0.43,0.5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1954,1)=\"J\",LEFT(H1954,2),LEFT(H1954,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1954,1)=\"J\",RIGHT(H1954,LEN(H1954)-4),RIGHT(H1954,LEN(H1954)-6)),\"\"))","v":""}]
[50001528,"Victron Energy","MultiPlus 12/800/35",0.7,0.8,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1955,1)=\"J\",LEFT(H1955,2),LEFT(H1955,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1955,1)=\"J\",RIGHT(H1955,LEN(H1955)-4),RIGHT(H1955,LEN(H1955)-6)),\"\"))","v":""}]
[50001529,"Victron Energy","MultiPlus 24/800/16",0.7,0.8,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1956,1)=\"J\",LEFT(H1956,2),LEFT(H1956,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1956,1)=\"J\",RIGHT(H1956,LEN(H1956)-4),RIGHT(H1956,LEN(H1956)-6)),\"\"))","v":""}]
[50001530,"Victron Energy","MultiPlus 48/800/9",0.7,0.8,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1957,1)=\"J\",LEFT(H1957,2),LEFT(H1957,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1957,1)=\"J\",RIGHT(H1957,LEN(H1957)-4),RIGHT(H1957,LEN(H1957)-6)),\"\"))","v":""}]
[50001531,"Victron Energy","MultiPlus C 12/800/35",0.7,0.8,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1958,1)=\"J\",LEFT(H1958,2),LEFT(H1958,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1958,1)=\"J\",RIGHT(H1958,LEN(H1958)-4),RIGHT(H1958,LEN(H1958)-6)),\"\"))","v":""}]
[50001532,"Victron Energy","MultiPlus C 24/800/16",0.7,0.8,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1959,1)=\"J\",LEFT(H1959,2),LEFT(H1959,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1959,1)=\"J\",RIGHT(H1959,LEN(H1959)-4),RIGHT(H1959,LEN(H1959)-6)),\"\"))","v":""}]
[50001533,"Victron Energy","MultiPlus 12/1200/50",1,1.2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1960,1)=\"J\",LEFT(H1960,2),LEFT(H1960,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1960,1)=\"J\",RIGHT(H1960,LEN(H1960)-4),RIGHT(H1960,LEN(H1960)-6)),\"\"))","v":""}]
[50001534,"Victron Energy","MultiPlus 24/1200/25",1,1.2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1961,1)=\"J\",LEFT(H1961,2),LEFT(H1961,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1961,1)=\"J\",RIGHT(H1961,LEN(H1961)-4),RIGHT(H1961,LEN(H1961)-6)),\"\"))","v":""}]
[50001535,"Victron Energy","MultiPlus 48/1200/13",1,1.2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1962,1)=\"J\",LEFT(H1962,2),LEFT(H1962,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1962,1)=\"J\",RIGHT(H1962,LEN(H1962)-4),RIGHT(H1962,LEN(H1962)-6)),\"\"))","v":""}]
[50001536,"Victron Energy","MultiPlus C 12/1200/50",1,1.2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1963,1)=\"J\",LEFT(H1963,2),LEFT(H1963,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1963,1)=\"J\",RIGHT(H1963,LEN(H1963)-4),RIGHT(H1963,LEN(H1963)-6)),\"\"))","v":""}]
[50001537,"Victron Energy","MultiPlus C 24/1200/25",1,1.2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1964,1)=\"J\",LEFT(H1964,2),LEFT(H1964,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1964,1)=\"J\",RIGHT(H1964,LEN(H1964)-4),RIGHT(H1964,LEN(H1964)-6)),\"\"))","v":""}]
[50001538,"Victron Energy","EasySolar 12/1600/70",1.3,1.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1965,1)=\"J\",LEFT(H1965,2),LEFT(H1965,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1965,1)=\"J\",RIGHT(H1965,LEN(H1965)-4),RIGHT(H1965,LEN(H1965)-6)),\"\"))","v":""}]
[50001539,"Victron Energy","EasySolar 24/1600/40",1.3,1.3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1966,1)=\"J\",LEFT(H1966,2),LEFT(H1966,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1966,1)=\"J\",RIGHT(H1966,LEN(H1966)-4),RIGHT(H1966,LEN(H1966)-6)),\"\"))","v":""}]
[50001540,"Victron Energy","MultiPlus 12/160070",1.3,1.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1967,1)=\"J\",LEFT(H1967,2),LEFT(H1967,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1967,1)=\"J\",RIGHT(H1967,LEN(H1967)-4),RIGHT(H1967,LEN(H1967)-6)),\"\"))","v":""}]
[50001541,"Victron Energy","MultiPlus 24/1600/40",1.3,1.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1968,1)=\"J\",LEFT(H1968,2),LEFT(H1968,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1968,1)=\"J\",RIGHT(H1968,LEN(H1968)-4),RIGHT(H1968,LEN(H1968)-6)),\"\"))","v":""}]
[50001542,"Victron Energy","MultiPlus 48/1600/20",1.3,1.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1969,1)=\"J\",LEFT(H1969,2),LEFT(H1969,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1969,1)=\"J\",RIGHT(H1969,LEN(H1969)-4),RIGHT(H1969,LEN(H1969)-6)),\"\"))","v":""}]
[50001543,"Victron Energy","MultiPlus C 12/1600/70",null,1.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1970,1)=\"J\",LEFT(H1970,2),LEFT(H1970,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1970,1)=\"J\",RIGHT(H1970,LEN(H1970)-4),RIGHT(H1970,LEN(H1970)-6)),\"\"))","v":""}]
[50001544,"Victron Energy","MultiPlus C 24/1600/40",null,1.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1971,1)=\"J\",LEFT(H1971,2),LEFT(H1971,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1971,1)=\"J\",RIGHT(H1971,LEN(H1971)-4),RIGHT(H1971,LEN(H1971)-6)),\"\"))","v":""}]
[50001545,"Victron Energy","MultiPlus 12/2000/80",1.6,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1972,1)=\"J\",LEFT(H1972,2),LEFT(H1972,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1972,1)=\"J\",RIGHT(H1972,LEN(H1972)-4),RIGHT(H1972,LEN(H1972)-6)),\"\"))","v":""}]
[50001546,"Victron Energy","MultiPlus 24/2000/50",1.6,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1973,1)=\"J\",LEFT(H1973,2),LEFT(H1973,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1973,1)=\"J\",RIGHT(H1973,LEN(H1973)-4),RIGHT(H1973,LEN(H1973)-6)),\"\"))","v":""}]
[50001547,"Victron Energy","MultiPlus 48/2000/25",1.6,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1974,1)=\"J\",LEFT(H1974,2),LEFT(H1974,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1974,1)=\"J\",RIGHT(H1974,LEN(H1974)-4),RIGHT(H1974,LEN(H1974)-6)),\"\"))","v":""}]
[50001548,"Victron Energy","MultiPlus C 12/2000/80",null,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1975,1)=\"J\",LEFT(H1975,2),LEFT(H1975,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1975,1)=\"J\",RIGHT(H1975,LEN(H1975)-4),RIGHT(H1975,LEN(H1975)-6)),\"\"))","v":""}]
[50001549,"Victron Energy","MultiPlus C 24/2000/50",null,2,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1976,1)=\"J\",LEFT(H1976,2),LEFT(H1976,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1976,1)=\"J\",RIGHT(H1976,LEN(H1976)-4),RIGHT(H1976,LEN(H1976)-6)),\"\"))","v":""}]
[50001550,"Victron Energy","MultiPlus-II 24/3000/70-32",2.4700000000000002,2.5,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2022-12-19","Martin Bertsch",null,null,null,"2021-03-01",null,"Ja","Nein","Ja","OK","Meike Gelhart","17PP264-23_1","2021-05-06",null,"OK",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - KONFORM TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H1977,1)=\"J\",LEFT(H1977,2),LEFT(H1977,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1977,1)=\"J\",RIGHT(H1977,LEN(H1977)-4),RIGHT(H1977,LEN(H1977)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001551,"Victron Energy","MultiPlus-II 24/3000/70-32 GX",2.4700000000000002,2.5,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2022-12-19","Martin Bertsch",null,null,null,"2021-03-01",null,"Ja","Nein","Ja","OK","Meike Gelhart","17PP264-23_1","2021-05-06",null,"OK",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - KONFORM TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H1978,1)=\"J\",LEFT(H1978,2),LEFT(H1978,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1978,1)=\"J\",RIGHT(H1978,LEN(H1978)-4),RIGHT(H1978,LEN(H1978)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001552,"Victron Energy","MultiPlus-II 48/3000/35-32",2.4700000000000002,2.5,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2022-12-19","Martin Bertsch",null,null,null,"2021-03-01",null,"Ja","Nein","Ja","OK","Meike Gelhart","17PP264-23_1","2021-05-06",null,"OK",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - KONFORM TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H1979,1)=\"J\",LEFT(H1979,2),LEFT(H1979,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1979,1)=\"J\",RIGHT(H1979,LEN(H1979)-4),RIGHT(H1979,LEN(H1979)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001553,"Victron Energy","MultiPlus-II 48/3000/35-32 GX",2.4700000000000002,2.5,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2022-12-19","Martin Bertsch",null,null,null,"2021-03-01",null,"Ja","Nein","Ja","OK","Meike Gelhart","17PP264-23_1","2021-05-06",null,"OK",null,null,null,null,"Batteriespeicher 1~ - DC gekuppelt - KONFORM TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H1980,1)=\"J\",LEFT(H1980,2),LEFT(H1980,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1980,1)=\"J\",RIGHT(H1980,LEN(H1980)-4),RIGHT(H1980,LEN(H1980)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001554,"Victron Energy","EasySolar 24/3000/70-50",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1981,1)=\"J\",LEFT(H1981,2),LEFT(H1981,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1981,1)=\"J\",RIGHT(H1981,LEN(H1981)-4),RIGHT(H1981,LEN(H1981)-6)),\"\"))","v":""}]
[50001555,"Victron Energy","Easysolar-II 24/3000/70-32 MPPT 250/70GX",2.4,3,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2023-05-08","Martin Bertsch","2023-05-17",null,null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","20PP183-10_1","2023-01-30","nicht vorhanden","OK",null,null,null,null,"Hybridstromrichter 1~ - inselbetriebsfähig - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1982,1)=\"J\",LEFT(H1982,2),LEFT(H1982,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1982,1)=\"J\",RIGHT(H1982,LEN(H1982)-4),RIGHT(H1982,LEN(H1982)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001556,"Victron Energy","Easysolar-II 48/3000/35-32 MPPT 250/70GX",2.4,3,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2023-05-08","Martin Bertsch","2023-05-17",null,null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","20PP183-10_1","2023-01-30","nicht vorhanden","OK",null,null,null,null,"Hybridstromrichter 1~ - inselbetriebsfähig - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1983,1)=\"J\",LEFT(H1983,2),LEFT(H1983,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1983,1)=\"J\",RIGHT(H1983,LEN(H1983)-4),RIGHT(H1983,LEN(H1983)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001557,"Victron Energy","MultiPlus 12/3000/120",null,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1984,1)=\"J\",LEFT(H1984,2),LEFT(H1984,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1984,1)=\"J\",RIGHT(H1984,LEN(H1984)-4),RIGHT(H1984,LEN(H1984)-6)),\"\"))","v":""}]
[50001558,"Victron Energy","MultiPlus 24/3000/70",null,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1985,1)=\"J\",LEFT(H1985,2),LEFT(H1985,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1985,1)=\"J\",RIGHT(H1985,LEN(H1985)-4),RIGHT(H1985,LEN(H1985)-6)),\"\"))","v":""}]
[50001559,"Victron Energy","MultiPlus 48/3000/35",null,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stromrichter 1~ für Batteriespeicher - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1986,1)=\"J\",LEFT(H1986,2),LEFT(H1986,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1986,1)=\"J\",RIGHT(H1986,LEN(H1986)-4),RIGHT(H1986,LEN(H1986)-6)),\"\"))","v":""}]
[50001560,"Victron Energy","MultiPlus-II 12/3000/120-32",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,"Ja","nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1987,1)=\"J\",LEFT(H1987,2),LEFT(H1987,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1987,1)=\"J\",RIGHT(H1987,LEN(H1987)-4),RIGHT(H1987,LEN(H1987)-6)),\"\"))","v":""}]
[50001561,"Victron Energy","MultiPlus-II 12/3000/120-50",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,"Ja","nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1988,1)=\"J\",LEFT(H1988,2),LEFT(H1988,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1988,1)=\"J\",RIGHT(H1988,LEN(H1988)-4),RIGHT(H1988,LEN(H1988)-6)),\"\"))","v":""}]
[50001562,"Victron Energy","MultiPlus-II 24/3000/70-50",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,"Ja","nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1989,1)=\"J\",LEFT(H1989,2),LEFT(H1989,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1989,1)=\"J\",RIGHT(H1989,LEN(H1989)-4),RIGHT(H1989,LEN(H1989)-6)),\"\"))","v":""}]
[50001563,"Victron Energy","MultiPlus-II 48/3000/35-50",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,"Ja","nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1990,1)=\"J\",LEFT(H1990,2),LEFT(H1990,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1990,1)=\"J\",RIGHT(H1990,LEN(H1990)-4),RIGHT(H1990,LEN(H1990)-6)),\"\"))","v":""}]
[50001564,"Victron Energy","Quattro 12/3000/120-50/50",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1991,1)=\"J\",LEFT(H1991,2),LEFT(H1991,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1991,1)=\"J\",RIGHT(H1991,LEN(H1991)-4),RIGHT(H1991,LEN(H1991)-6)),\"\"))","v":""}]
[50001565,"Victron Energy","Quattro 24/3000/70-50/50",2.4,3,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1992,1)=\"J\",LEFT(H1992,2),LEFT(H1992,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1992,1)=\"J\",RIGHT(H1992,LEN(H1992)-4),RIGHT(H1992,LEN(H1992)-6)),\"\"))","v":""}]
[50001566,"Victron Energy","MultiPlus-II 48/5000/70-50",4.4000000000000004,4.5,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2022-12-19","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Ja","OK","Meike Gelhart","17PP264-23_1","2021-05-06",null,"OK",null,null,null,null,"Batteriespeicher 1~ - nur 3~ Anschluss gestattet - DC gekoppelt - inselbetriebsfähig - KONFORM TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H1993,1)=\"J\",LEFT(H1993,2),LEFT(H1993,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1993,1)=\"J\",RIGHT(H1993,LEN(H1993)-4),RIGHT(H1993,LEN(H1993)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001567,"Victron Energy","MultiPlus-II 48/5000/70-50 GX",4.4000000000000004,4.5,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2022-12-19","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Ja","OK","Meike Gelhart","17PP264-23_1","2021-05-06",null,"OK",null,null,null,null,"Batteriespeicher 1~ - nur 3~ Anschluss gestattet - DC gekoppelt - inselbetriebsfähig - KONFORM TOR ERZ A","F","F",null,null,{"$f":"IF(LEFT(H1994,1)=\"J\",LEFT(H1994,2),LEFT(H1994,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1994,1)=\"J\",RIGHT(H1994,LEN(H1994)-4),RIGHT(H1994,LEN(H1994)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50002096,"Victron Energy","Quattro-II 48/5000/70-50/50/230V",4.4000000000000004,4.5,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2024-03-21","Martin Bertsch","2024-03-21",null,null,null,null,"Ja","Nein","Ja","Vorhanden",null,"22PP102-07_0","2024-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1995,1)=\"J\",LEFT(H1995,2),LEFT(H1995,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1995,1)=\"J\",RIGHT(H1995,LEN(H1995)-4),RIGHT(H1995,LEN(H1995)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001568,"Victron Energy","RS Smart Solar 48/6000",4.5,4.5,1,"AC-Batteriewechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1996,1)=\"J\",LEFT(H1996,2),LEFT(H1996,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1996,1)=\"J\",RIGHT(H1996,LEN(H1996)-4),RIGHT(H1996,LEN(H1996)-6)),\"\"))","v":""}]
[50001569,"Victron Energy","EasySolar 48/5000/70-100",4,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H1997,1)=\"J\",LEFT(H1997,2),LEFT(H1997,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1997,1)=\"J\",RIGHT(H1997,LEN(H1997)-4),RIGHT(H1997,LEN(H1997)-6)),\"\"))","v":""}]
[50001570,"Victron Energy","Easysolar-II 48/5000/70-50 MPPT 250/100GX",4,5,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2023-05-08","Martin Bertsch","2023-05-17",null,null,null,null,"Ja","Nein",null,"OK","Martin Bertsch (OE)","20PP183-10_1","2023-01-30","nicht vorhanden","OK",null,null,null,null,"Hybridstromrichter 1~ - inselbetriebsfähig - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1998,1)=\"J\",LEFT(H1998,2),LEFT(H1998,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H1998,1)=\"J\",RIGHT(H1998,LEN(H1998)-4),RIGHT(H1998,LEN(H1998)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001571,"Victron Energy","MultiPlus 24/5000/120",null,5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H1999,1)=\"J\",LEFT(H1999,2),LEFT(H1999,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H1999,1)=\"J\",RIGHT(H1999,LEN(H1999)-4),RIGHT(H1999,LEN(H1999)-6)),\"\"))","v":""}]
[50001572,"Victron Energy","MultiPlus 48/5000/70",null,5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - keine KONFORM","F","F",null,null,{"$f":"IF(LEFT(H2000,1)=\"J\",LEFT(H2000,2),LEFT(H2000,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2000,1)=\"J\",RIGHT(H2000,LEN(H2000)-4),RIGHT(H2000,LEN(H2000)-6)),\"\"))","v":""}]
[50001573,"Victron Energy","MultiPlus-II 24/5000/120-50",4,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,"Ja","nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2001,1)=\"J\",LEFT(H2001,2),LEFT(H2001,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2001,1)=\"J\",RIGHT(H2001,LEN(H2001)-4),RIGHT(H2001,LEN(H2001)-6)),\"\"))","v":""}]
[50001574,"Victron Energy","Quattro 12/5000/220-100/100",4,5,1,"Hybrid-Wechselrichter","Nein","2023-05-23","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2002,1)=\"J\",LEFT(H2002,2),LEFT(H2002,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2002,1)=\"J\",RIGHT(H2002,LEN(H2002)-4),RIGHT(H2002,LEN(H2002)-6)),\"\"))","v":""}]
[50001575,"Victron Energy","Quattro 24/5000/120-100/100",4,5,1,"Hybrid-Wechselrichter","Nein","2023-05-23","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2003,1)=\"J\",LEFT(H2003,2),LEFT(H2003,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2003,1)=\"J\",RIGHT(H2003,LEN(H2003)-4),RIGHT(H2003,LEN(H2003)-6)),\"\"))","v":""}]
[50001576,"Victron Energy","Quattro 48/5000/70-100/100",4,5,1,"Hybrid-Wechselrichter","Nein","2023-05-23","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2004,1)=\"J\",LEFT(H2004,2),LEFT(H2004,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2004,1)=\"J\",RIGHT(H2004,LEN(H2004)-4),RIGHT(H2004,LEN(H2004)-6)),\"\"))","v":""}]
[50001577,"Victron Energy","MultiPlus-II 48/8000/110-100/100",6.4,8,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2024-03-12","Martin Bertsch","2024-03-12",null,null,null,null,"Ja","Nein","Ja","Vorhanden",null,"2222 / 0478 - E","2024-02-16",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2005,1)=\"J\",LEFT(H2005,2),LEFT(H2005,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2005,1)=\"J\",RIGHT(H2005,LEN(H2005)-4),RIGHT(H2005,LEN(H2005)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001578,"Victron Energy","Quattro 24/8000/200-100/100",6.4,8,1,"Hybrid-Wechselrichter","Nein","2023-05-23","Martin Bertsch",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2006,1)=\"J\",LEFT(H2006,2),LEFT(H2006,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2006,1)=\"J\",RIGHT(H2006,LEN(H2006)-4),RIGHT(H2006,LEN(H2006)-6)),\"\"))","v":""}]
[50001579,"Victron Energy","Quattro 48/8000/110-100/100",6.4,8,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2023-05-08","Martin Bertsch","2023-05-17",null,null,null,null,null,null,null,"OK","Roland Bründlinger","2220/0019-K-E2","2023-03-27",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2007,1)=\"J\",LEFT(H2007,2),LEFT(H2007,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2007,1)=\"J\",RIGHT(H2007,LEN(H2007)-4),RIGHT(H2007,LEN(H2007)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001580,"Victron Energy","MultiPlus-II 48/10000/140-100/100",8,10,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2024-03-12","Martin Bertsch","2024-03-12",null,null,null,null,"Ja","Nein","Ja","Vorhanden",null,"2222 / 0478 - E","2024-02-16",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2008,1)=\"J\",LEFT(H2008,2),LEFT(H2008,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2008,1)=\"J\",RIGHT(H2008,LEN(H2008)-4),RIGHT(H2008,LEN(H2008)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001581,"Victron Energy","Quattro 48/10000/140-100/100",8,10,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2023-05-08","Martin Bertsch","2023-05-17",null,null,null,null,null,null,null,"OK","Roland Bründlinger","2220/0019-K-E2","2023-03-27",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2009,1)=\"J\",LEFT(H2009,2),LEFT(H2009,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2009,1)=\"J\",RIGHT(H2009,LEN(H2009)-4),RIGHT(H2009,LEN(H2009)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50002095,"Victron Energy","Multiplus-II 48/15000/200-100 230V",12,15,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2024-03-12","Martin Bertsch","2024-03-12",null,null,null,null,"Ja","Nein","Ja","Vorhanden",null,"2222 / 0478 - E","2024-02-16",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2010,1)=\"J\",LEFT(H2010,2),LEFT(H2010,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2010,1)=\"J\",RIGHT(H2010,LEN(H2010)-4),RIGHT(H2010,LEN(H2010)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001582,"Victron Energy","Quattro 48/15000/200-100/100",12,15,1,"Hybrid-Wechselrichter","Ja - bis 30kW Rückspeisung","2023-05-08","Martin Bertsch","2023-05-17",null,null,null,null,null,null,null,"OK","Roland Bründlinger","2220/0019-K-E2","2023-03-27",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2011,1)=\"J\",LEFT(H2011,2),LEFT(H2011,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2011,1)=\"J\",RIGHT(H2011,LEN(H2011)-4),RIGHT(H2011,LEN(H2011)-6)),\"\"))","v":"bis 30kW Rückspeisung"}]
[50001583,"Viessmann GmbH","Vitocharge VX3 6.0A",6,6,3,"Hybrid-Wechselrichter","Ja","2022-09-08","Martin Bertsch",null,null,null,null,null,"Ja","Ja","Nein","OK","Martin Bertsch (OE)","21TH0320-OVE-directive R25_2","2022-05-10",null,"OK",null,"nicht vorhanden",null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2012,1)=\"J\",LEFT(H2012,2),LEFT(H2012,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2012,1)=\"J\",RIGHT(H2012,LEN(H2012)-4),RIGHT(H2012,LEN(H2012)-6)),\"\"))","v":""}]
[50001584,"Viessmann GmbH","Vitocharge VX3 8.0A",8,8,3,"Hybrid-Wechselrichter","Ja","2022-09-08","Martin Bertsch",null,null,null,null,null,"Ja","Ja","Nein","OK","Martin Bertsch (OE)","21TH0320-OVE-directive R25_2","2022-05-10",null,"OK",null,"nicht vorhanden",null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2013,1)=\"J\",LEFT(H2013,2),LEFT(H2013,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2013,1)=\"J\",RIGHT(H2013,LEN(H2013)-4),RIGHT(H2013,LEN(H2013)-6)),\"\"))","v":""}]
[50002073,"VIRTUS","6 L",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-29","Martin Bertsch","2024-01-29","HMI: 1001-CF41 MAIN: 2005-1143-1807 ARC: Ver0000; PV-Shop Zusatzmodul Treiberversion 2023.04.02-0.9.4 Hardwareversion 4419.0.4097-53057",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CDAN-ESH-P21110559-R1","2022-07-18","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2014,1)=\"J\",LEFT(H2014,2),LEFT(H2014,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2014,1)=\"J\",RIGHT(H2014,LEN(H2014)-4),RIGHT(H2014,LEN(H2014)-6)),\"\"))","v":"mit Einschränkung"}]
[50002074,"VIRTUS","8 L",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-29","Martin Bertsch","2024-01-29","HMI: 1001-CF41 MAIN: 2005-1143-1807 ARC: Ver0000; PV-Shop Zusatzmodul Treiberversion 2023.04.02-0.9.4 Hardwareversion 4419.0.4097-53057",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CDAN-ESH-P21110559-R1","2022-07-18","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2015,1)=\"J\",LEFT(H2015,2),LEFT(H2015,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2015,1)=\"J\",RIGHT(H2015,LEN(H2015)-4),RIGHT(H2015,LEN(H2015)-6)),\"\"))","v":"mit Einschränkung"}]
[50002075,"VIRTUS","10 L",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-29","Martin Bertsch","2024-01-29","HMI: 1001-CF41 MAIN: 2005-1143-1807 ARC: Ver0000; PV-Shop Zusatzmodul Treiberversion 2023.04.02-0.9.4 Hardwareversion 4419.0.4097-53057",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CDAN-ESH-P21110559-R1","2022-07-18","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2016,1)=\"J\",LEFT(H2016,2),LEFT(H2016,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2016,1)=\"J\",RIGHT(H2016,LEN(H2016)-4),RIGHT(H2016,LEN(H2016)-6)),\"\"))","v":"mit Einschränkung"}]
[50002076,"VIRTUS","12 L",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-01-29","Martin Bertsch","2024-01-29","HMI: 1001-CF41 MAIN: 2005-1143-1807 ARC: Ver0000; PV-Shop Zusatzmodul Treiberversion 2023.04.02-0.9.4 Hardwareversion 4419.0.4097-53057",null,null,null,"Ja","Nein","Nein","OK","Martin Bertsch (OE)","CDAN-ESH-P21110559-R1","2022-07-18","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2017,1)=\"J\",LEFT(H2017,2),LEFT(H2017,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2017,1)=\"J\",RIGHT(H2017,LEN(H2017)-4),RIGHT(H2017,LEN(H2017)-6)),\"\"))","v":"mit Einschränkung"}]
[50001585,"Voltronic Power","InfiniSolar 2KW ",null,2,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Nicht mehr am Markt","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - nicht mehr am Markt","T","F",null,null,{"$f":"IF(LEFT(H2018,1)=\"J\",LEFT(H2018,2),LEFT(H2018,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2018,1)=\"J\",RIGHT(H2018,LEN(H2018)-4),RIGHT(H2018,LEN(H2018)-6)),\"\"))","v":""}]
[50001586,"Voltronic Power","InfiniSolar Plus 3kW ",null,3,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Nicht mehr am Markt","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - nicht mehr am Markt","T","F",null,null,{"$f":"IF(LEFT(H2019,1)=\"J\",LEFT(H2019,2),LEFT(H2019,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2019,1)=\"J\",RIGHT(H2019,LEN(H2019)-4),RIGHT(H2019,LEN(H2019)-6)),\"\"))","v":""}]
[50001587,"Voltronic Power","InfiniSolar Plus 5kW ",null,5,1,"PV-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Nicht mehr am Markt","Nein","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Stringwechselrichter 1~ - nicht mehr am Markt","T","F",null,null,{"$f":"IF(LEFT(H2020,1)=\"J\",LEFT(H2020,2),LEFT(H2020,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2020,1)=\"J\",RIGHT(H2020,LEN(H2020)-4),RIGHT(H2020,LEN(H2020)-6)),\"\"))","v":""}]
[50001588,"Voltronic Power","FSP Power Manager 10kW",null,10,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,"Ja","Ja",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - DC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2021,1)=\"J\",LEFT(H2021,2),LEFT(H2021,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2021,1)=\"J\",RIGHT(H2021,LEN(H2021)-4),RIGHT(H2021,LEN(H2021)-6)),\"\"))","v":""}]
[50001589,"Voltronic Power","InfiniSolar 3P 10kW",null,10,3,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,"2021-03-01","Keine Konformitätserklärung","Ja","Nein",null,"nicht vorhanden",null,null,null,null,"nicht vorhanden",null,null,null,null,"Batteriespeicher 3~ - DC gekuppelt - keine KONFORM Individuell KEINE SERIE","F","F",null,null,{"$f":"IF(LEFT(H2022,1)=\"J\",LEFT(H2022,2),LEFT(H2022,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2022,1)=\"J\",RIGHT(H2022,LEN(H2022)-4),RIGHT(H2022,LEN(H2022)-6)),\"\"))","v":""}]
[50001590,"Wattsonic","WTS-3.6KW-HVS",null,3.6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2023,1)=\"J\",LEFT(H2023,2),LEFT(H2023,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2023,1)=\"J\",RIGHT(H2023,LEN(H2023)-4),RIGHT(H2023,LEN(H2023)-6)),\"\"))","v":""}]
[50001591,"Wattsonic","4.0K-25A-3P",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2024,1)=\"J\",LEFT(H2024,2),LEFT(H2024,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2024,1)=\"J\",RIGHT(H2024,LEN(H2024)-4),RIGHT(H2024,LEN(H2024)-6)),\"\"))","v":"mit Einschränkung"}]
[50001592,"Wattsonic","WTS-4KW-3P",4,4.4000000000000004,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch","2022-09-06","V1.05","2023-05-31","2023-06-01","FW hat noch kleinere Fehler: Q(U) geht noch auf Mittelwert, Verzögerungszeit P(U) zu hoch","Ja","Nein","Ja","nicht OK","Christian Elbs","6103826.50 V1.1","2022-04-20",null,"OK",null,"Vorhanden","2022-09-05",null,null,null,null,null,null,{"$f":"IF(LEFT(H2025,1)=\"J\",LEFT(H2025,2),LEFT(H2025,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2025,1)=\"J\",RIGHT(H2025,LEN(H2025)-4),RIGHT(H2025,LEN(H2025)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001593,"Wattsonic","WTS-5.0KW-HVS",null,5,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2026,1)=\"J\",LEFT(H2026,2),LEFT(H2026,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2026,1)=\"J\",RIGHT(H2026,LEN(H2026)-4),RIGHT(H2026,LEN(H2026)-6)),\"\"))","v":""}]
[50001594,"Wattsonic","5.0K-25A-3P",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2027,1)=\"J\",LEFT(H2027,2),LEFT(H2027,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2027,1)=\"J\",RIGHT(H2027,LEN(H2027)-4),RIGHT(H2027,LEN(H2027)-6)),\"\"))","v":"mit Einschränkung"}]
[50001595,"Wattsonic","WTS-5KW-3P",5,5.5,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch","2022-09-06","V1.05","2023-05-31","2023-06-01","FW hat noch kleinere Fehler: Q(U) geht noch auf Mittelwert, Verzögerungszeit P(U) zu hoch","Ja","Nein","Ja","nicht OK","Christian Elbs","6103826.50 V1.1","2022-04-20",null,"OK",null,"Vorhanden","2022-09-05",null,null,null,null,null,null,{"$f":"IF(LEFT(H2028,1)=\"J\",LEFT(H2028,2),LEFT(H2028,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2028,1)=\"J\",RIGHT(H2028,LEN(H2028)-4),RIGHT(H2028,LEN(H2028)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001596,"Wattsonic","WTS-6.0KW-HVS",null,6,1,"Hybrid-Wechselrichter","Nein",null,null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2029,1)=\"J\",LEFT(H2029,2),LEFT(H2029,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2029,1)=\"J\",RIGHT(H2029,LEN(H2029)-4),RIGHT(H2029,LEN(H2029)-6)),\"\"))","v":""}]
[50001597,"Wattsonic","6.0K-25A-3P",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2030,1)=\"J\",LEFT(H2030,2),LEFT(H2030,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2030,1)=\"J\",RIGHT(H2030,LEN(H2030)-4),RIGHT(H2030,LEN(H2030)-6)),\"\"))","v":"mit Einschränkung"}]
[50001598,"Wattsonic","WTS-6KW-3P",6,6.6,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch","2022-09-06","V1.05","2023-05-31","2023-06-01","FW hat noch kleinere Fehler: Q(U) geht noch auf Mittelwert, Verzögerungszeit P(U) zu hoch","Ja","Nein","Ja","nicht OK","Christian Elbs","6103826.50 V1.1","2022-04-20",null,"OK",null,"Vorhanden","2022-09-05",null,null,null,null,null,null,{"$f":"IF(LEFT(H2031,1)=\"J\",LEFT(H2031,2),LEFT(H2031,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2031,1)=\"J\",RIGHT(H2031,LEN(H2031)-4),RIGHT(H2031,LEN(H2031)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001599,"Wattsonic","8.0K-25A-3P",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2032,1)=\"J\",LEFT(H2032,2),LEFT(H2032,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2032,1)=\"J\",RIGHT(H2032,LEN(H2032)-4),RIGHT(H2032,LEN(H2032)-6)),\"\"))","v":"mit Einschränkung"}]
[50001600,"Wattsonic","WTS-8KW-3P",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch","2022-09-06","V1.05","2023-05-31","2023-06-01","FW hat noch kleinere Fehler: Q(U) geht noch auf Mittelwert, Verzögerungszeit P(U) zu hoch","Ja","Nein","Ja","nicht OK","Christian Elbs","6103826.50 V1.1","2022-04-20",null,"OK",null,"Vorhanden","2022-09-05",null,null,null,null,null,null,{"$f":"IF(LEFT(H2033,1)=\"J\",LEFT(H2033,2),LEFT(H2033,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2033,1)=\"J\",RIGHT(H2033,LEN(H2033)-4),RIGHT(H2033,LEN(H2033)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001601,"Wattsonic","10K-25A-3P",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2034,1)=\"J\",LEFT(H2034,2),LEFT(H2034,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2034,1)=\"J\",RIGHT(H2034,LEN(H2034)-4),RIGHT(H2034,LEN(H2034)-6)),\"\"))","v":"mit Einschränkung"}]
[50001602,"Wattsonic","10K-40A-3P",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2035,1)=\"J\",LEFT(H2035,2),LEFT(H2035,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2035,1)=\"J\",RIGHT(H2035,LEN(H2035)-4),RIGHT(H2035,LEN(H2035)-6)),\"\"))","v":"mit Einschränkung"}]
[50001603,"Wattsonic","WTS-10KW-3P",10,11,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch","2022-09-06","V1.05","2023-05-31","2023-06-01","FW hat noch kleinere Fehler: Q(U) geht noch auf Mittelwert, Verzögerungszeit P(U) zu hoch","Ja","Nein","Ja","nicht OK","Christian Elbs","6103826.50 V1.1","2022-04-20",null,"OK",null,"Vorhanden","2022-09-05",null,null,null,null,null,null,{"$f":"IF(LEFT(H2036,1)=\"J\",LEFT(H2036,2),LEFT(H2036,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2036,1)=\"J\",RIGHT(H2036,LEN(H2036)-4),RIGHT(H2036,LEN(H2036)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001604,"Wattsonic","12K-25A-3P",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2037,1)=\"J\",LEFT(H2037,2),LEFT(H2037,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2037,1)=\"J\",RIGHT(H2037,LEN(H2037)-4),RIGHT(H2037,LEN(H2037)-6)),\"\"))","v":"mit Einschränkung"}]
[50001605,"Wattsonic","12K-40A-3P",12,13.2,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2038,1)=\"J\",LEFT(H2038,2),LEFT(H2038,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2038,1)=\"J\",RIGHT(H2038,LEN(H2038)-4),RIGHT(H2038,LEN(H2038)-6)),\"\"))","v":"mit Einschränkung"}]
[50001606,"Wattsonic","WTS-12KW-3P",12,13.2,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-05-31","Martin Bertsch","2022-09-06","V1.05","2023-05-31","2023-06-01","FW hat noch kleinere Fehler: Q(U) geht noch auf Mittelwert, Verzögerungszeit P(U) zu hoch","Ja","Nein","Ja","nicht OK","Christian Elbs","6103826.50 V1.1","2022-04-20",null,"OK",null,"Vorhanden","2022-09-05",null,null,null,null,null,null,{"$f":"IF(LEFT(H2039,1)=\"J\",LEFT(H2039,2),LEFT(H2039,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2039,1)=\"J\",RIGHT(H2039,LEN(H2039)-4),RIGHT(H2039,LEN(H2039)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001607,"Wattsonic","15K-40A-3P",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2040,1)=\"J\",LEFT(H2040,2),LEFT(H2040,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2040,1)=\"J\",RIGHT(H2040,LEN(H2040)-4),RIGHT(H2040,LEN(H2040)-6)),\"\"))","v":"mit Einschränkung"}]
[50001608,"Wattsonic","20K-40A-3P",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-11","Martin Bertsch","2023-01-11","slave version: 27.52.04.00 SW Version(Country Setting): V1.07",null,null,null,"Ja","Nein","Ja","OK","Roland Bründlinger","220618BW001-EG-AT-002","2023-03-23","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2041,1)=\"J\",LEFT(H2041,2),LEFT(H2041,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2041,1)=\"J\",RIGHT(H2041,LEN(H2041)-4),RIGHT(H2041,LEN(H2041)-6)),\"\"))","v":"mit Einschränkung"}]
[50001711,"Xelectrix Power GmbH","XPB-B11",11,11,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2023-08-28",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2042,1)=\"J\",LEFT(H2042,2),LEFT(H2042,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2042,1)=\"J\",RIGHT(H2042,LEN(H2042)-4),RIGHT(H2042,LEN(H2042)-6)),\"\"))","v":""}]
[50001706,"Xelectrix Power GmbH","XPB-P11",11,11,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2023-08-28",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2043,1)=\"J\",LEFT(H2043,2),LEFT(H2043,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2043,1)=\"J\",RIGHT(H2043,LEN(H2043)-4),RIGHT(H2043,LEN(H2043)-6)),\"\"))","v":""}]
[50001612,"Xelectrix Power GmbH","XPB-W11",11,11,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2044,1)=\"J\",LEFT(H2044,2),LEFT(H2044,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2044,1)=\"J\",RIGHT(H2044,LEN(H2044)-4),RIGHT(H2044,LEN(H2044)-6)),\"\"))","v":""}]
[50001615,"Xelectrix Power GmbH","XPB-B35",35,35,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2045,1)=\"J\",LEFT(H2045,2),LEFT(H2045,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2045,1)=\"J\",RIGHT(H2045,LEN(H2045)-4),RIGHT(H2045,LEN(H2045)-6)),\"\"))","v":""}]
[50001617,"Xelectrix Power GmbH","XPB-P35",35,35,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2046,1)=\"J\",LEFT(H2046,2),LEFT(H2046,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2046,1)=\"J\",RIGHT(H2046,LEN(H2046)-4),RIGHT(H2046,LEN(H2046)-6)),\"\"))","v":""}]
[50001618,"Xelectrix Power GmbH","XPB-U35",35,35,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2047,1)=\"J\",LEFT(H2047,2),LEFT(H2047,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2047,1)=\"J\",RIGHT(H2047,LEN(H2047)-4),RIGHT(H2047,LEN(H2047)-6)),\"\"))","v":""}]
[50001619,"Xelectrix Power GmbH","XPB-W35",35,35,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2048,1)=\"J\",LEFT(H2048,2),LEFT(H2048,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2048,1)=\"J\",RIGHT(H2048,LEN(H2048)-4),RIGHT(H2048,LEN(H2048)-6)),\"\"))","v":""}]
[50001620,"Xelectrix Power GmbH","XBP-U80",80,80,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2049,1)=\"J\",LEFT(H2049,2),LEFT(H2049,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2049,1)=\"J\",RIGHT(H2049,LEN(H2049)-4),RIGHT(H2049,LEN(H2049)-6)),\"\"))","v":""}]
[50001621,"Xelectrix Power GmbH","XPB-B80",80,80,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2050,1)=\"J\",LEFT(H2050,2),LEFT(H2050,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2050,1)=\"J\",RIGHT(H2050,LEN(H2050)-4),RIGHT(H2050,LEN(H2050)-6)),\"\"))","v":""}]
[50001707,"Xelectrix Power GmbH","XPB-P80",80,80,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2023-08-28",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2051,1)=\"J\",LEFT(H2051,2),LEFT(H2051,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2051,1)=\"J\",RIGHT(H2051,LEN(H2051)-4),RIGHT(H2051,LEN(H2051)-6)),\"\"))","v":""}]
[50001714,"Xelectrix Power GmbH","XBP-B150",150,150,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2023-08-28",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2052,1)=\"J\",LEFT(H2052,2),LEFT(H2052,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2052,1)=\"J\",RIGHT(H2052,LEN(H2052)-4),RIGHT(H2052,LEN(H2052)-6)),\"\"))","v":""}]
[50001712,"Xelectrix Power GmbH","XPB-B150",150,150,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2023-08-28",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2053,1)=\"J\",LEFT(H2053,2),LEFT(H2053,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2053,1)=\"J\",RIGHT(H2053,LEN(H2053)-4),RIGHT(H2053,LEN(H2053)-6)),\"\"))","v":""}]
[50001623,"Xelectrix Power GmbH","XPB-U150",150,150,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2021-05-06",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,"Batteriespeicher 3~ - AC gekuppelt - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2054,1)=\"J\",LEFT(H2054,2),LEFT(H2054,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2054,1)=\"J\",RIGHT(H2054,LEN(H2054)-4),RIGHT(H2054,LEN(H2054)-6)),\"\"))","v":""}]
[50001713,"Xelectrix Power GmbH","XPB-B250",250,250,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2023-08-28",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2055,1)=\"J\",LEFT(H2055,2),LEFT(H2055,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2055,1)=\"J\",RIGHT(H2055,LEN(H2055)-4),RIGHT(H2055,LEN(H2055)-6)),\"\"))","v":""}]
[50001716,"Xelectrix Power GmbH","XPB-U250",250,250,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2023-08-28",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2056,1)=\"J\",LEFT(H2056,2),LEFT(H2056,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2056,1)=\"J\",RIGHT(H2056,LEN(H2056)-4),RIGHT(H2056,LEN(H2056)-6)),\"\"))","v":""}]
[50001715,"Xelectrix Power GmbH","XPB-B500",500,500,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2023-08-28",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2057,1)=\"J\",LEFT(H2057,2),LEFT(H2057,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2057,1)=\"J\",RIGHT(H2057,LEN(H2057)-4),RIGHT(H2057,LEN(H2057)-6)),\"\"))","v":""}]
[50001717,"Xelectrix Power GmbH","XPB-U500",500,500,3,"AC-Batteriewechselrichter","Ja","2023-08-28","Martin Bertsch","2023-08-28",null,null,null,null,"Ja","Nein","Nein","OK","Roland Bründlinger (AIT)","SGP-18617_01_R1","2020-10-12","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2058,1)=\"J\",LEFT(H2058,2),LEFT(H2058,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2058,1)=\"J\",RIGHT(H2058,LEN(H2058)-4),RIGHT(H2058,LEN(H2058)-6)),\"\"))","v":""}]
[50002279,"Xiamen E-star Energy","HERF-300",0.3,0.3,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-06-03","Martin Bertsch","2024-06-03",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"BMH-ESH-P22091070","2023-01-11","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2059,1)=\"J\",LEFT(H2059,2),LEFT(H2059,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2059,1)=\"J\",RIGHT(H2059,LEN(H2059)-4),RIGHT(H2059,LEN(H2059)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001710,"Xiamen E-star Energy","HT-300",0.3,0.3,1,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2060,1)=\"J\",LEFT(H2060,2),LEFT(H2060,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2060,1)=\"J\",RIGHT(H2060,LEN(H2060)-4),RIGHT(H2060,LEN(H2060)-6)),\"\"))","v":""}]
[50001625,"Xiamen E-star Energy","HT-350",0.35,0.35,1,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2061,1)=\"J\",LEFT(H2061,2),LEFT(H2061,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2061,1)=\"J\",RIGHT(H2061,LEN(H2061)-4),RIGHT(H2061,LEN(H2061)-6)),\"\"))","v":""}]
[50002280,"Xiamen E-star Energy","HERF-400",0.4,0.4,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-06-03","Martin Bertsch","2024-06-03",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"BMH-ESH-P22091070","2023-01-11","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2062,1)=\"J\",LEFT(H2062,2),LEFT(H2062,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2062,1)=\"J\",RIGHT(H2062,LEN(H2062)-4),RIGHT(H2062,LEN(H2062)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001626,"Xiamen E-star Energy","HT-400",0.4,0.4,1,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2063,1)=\"J\",LEFT(H2063,2),LEFT(H2063,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2063,1)=\"J\",RIGHT(H2063,LEN(H2063)-4),RIGHT(H2063,LEN(H2063)-6)),\"\"))","v":""}]
[50002281,"Xiamen E-star Energy","HERF-500",0.49,0.49,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2024-06-03","Martin Bertsch","2024-06-03",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"BMH-ESH-P22091070","2023-01-11","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2064,1)=\"J\",LEFT(H2064,2),LEFT(H2064,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2064,1)=\"J\",RIGHT(H2064,LEN(H2064)-4),RIGHT(H2064,LEN(H2064)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001627,"Xiamen E-star Energy","HERF-600",0.6,0.6,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-01-16","Martin Bertsch","2023-01-16",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"BMH-ESH-P22091069","2022-12-14","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2065,1)=\"J\",LEFT(H2065,2),LEFT(H2065,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2065,1)=\"J\",RIGHT(H2065,LEN(H2065)-4),RIGHT(H2065,LEN(H2065)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001628,"Xiamen E-star Energy","HT-600",0.6,0.6,1,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2066,1)=\"J\",LEFT(H2066,2),LEFT(H2066,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2066,1)=\"J\",RIGHT(H2066,LEN(H2066)-4),RIGHT(H2066,LEN(H2066)-6)),\"\"))","v":""}]
[50001629,"Xiamen E-star Energy","HT-700",0.7,0.7,1,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2067,1)=\"J\",LEFT(H2067,2),LEFT(H2067,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2067,1)=\"J\",RIGHT(H2067,LEN(H2067)-4),RIGHT(H2067,LEN(H2067)-6)),\"\"))","v":""}]
[50001630,"Xiamen E-star Energy","HERF-800",0.8,0.8,1,"PV-Wechselrichter","Ja - <= 800W Anlage","2023-01-16","Martin Bertsch","2023-01-16",null,null,null,null,"Nein","Nein","Nein","VDE4105",null,"BMH-ESH-P22091069","2022-12-14","nicht vorhanden","VDE4105/4110",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2068,1)=\"J\",LEFT(H2068,2),LEFT(H2068,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2068,1)=\"J\",RIGHT(H2068,LEN(H2068)-4),RIGHT(H2068,LEN(H2068)-6)),\"\"))","v":"<= 800W Anlage"}]
[50001631,"Xiamen E-star Energy","HT-800",0.8,0.8,1,"PV-Wechselrichter","Nein","2022-09-08","Christian Elbs",null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2069,1)=\"J\",LEFT(H2069,2),LEFT(H2069,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2069,1)=\"J\",RIGHT(H2069,LEN(H2069)-4),RIGHT(H2069,LEN(H2069)-6)),\"\"))","v":""}]
[50001632,"Xiamen E-star Energy","HT-1200",1.2,1.2,1,"PV-Wechselrichter","Nein","2022-06-30",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2070,1)=\"J\",LEFT(H2070,2),LEFT(H2070,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2070,1)=\"J\",RIGHT(H2070,LEN(H2070)-4),RIGHT(H2070,LEN(H2070)-6)),\"\"))","v":""}]
[50001633,"Xiamen E-star Energy","HT-1400",1.4,1.4,1,"PV-Wechselrichter","Nein","2022-06-30",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2071,1)=\"J\",LEFT(H2071,2),LEFT(H2071,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2071,1)=\"J\",RIGHT(H2071,LEN(H2071)-4),RIGHT(H2071,LEN(H2071)-6)),\"\"))","v":""}]
[50001634,"Xiamen E-star Energy","HT-1600",1.6,1.6,1,"PV-Wechselrichter","Nein","2022-06-30",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2072,1)=\"J\",LEFT(H2072,2),LEFT(H2072,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2072,1)=\"J\",RIGHT(H2072,LEN(H2072)-4),RIGHT(H2072,LEN(H2072)-6)),\"\"))","v":""}]
[50001635,"Xiamen E-star Energy","HT-2000",2,2,1,"PV-Wechselrichter","Nein","2022-06-30",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2073,1)=\"J\",LEFT(H2073,2),LEFT(H2073,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2073,1)=\"J\",RIGHT(H2073,LEN(H2073)-4),RIGHT(H2073,LEN(H2073)-6)),\"\"))","v":""}]
[50001636,"YOSHOPO","Y1-H3P6K-H",6,6.6,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-10-16","Martin Bertsch","2023-07-26","V1.04 ","2023-10-16","2023-10-16","Gerät wurde im Auftrag von OE beim AIT überprüft. Schwere Fehler gefunden.","Ja","Nein",null,"Vorhanden","Martin Bertsch (OE)","ABRE-ESH-P22120410","2023-07-20","nicht vorhanden","OK",null,null,null,null,"ident zu RENAC",null,null,null,null,{"$f":"IF(LEFT(H2074,1)=\"J\",LEFT(H2074,2),LEFT(H2074,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2074,1)=\"J\",RIGHT(H2074,LEN(H2074)-4),RIGHT(H2074,LEN(H2074)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001637,"YOSHOPO","Y1-H3P8K-H",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-10-16","Martin Bertsch","2023-07-26","V1.04 ","2023-10-16","2023-10-16","Gerät wurde im Auftrag von OE beim AIT überprüft. Schwere Fehler gefunden.","Ja","Nein",null,"Vorhanden","Martin Bertsch (OE)","ABRE-ESH-P22120410","2023-07-20","nicht vorhanden","OK",null,null,null,null,"ident zu RENAC",null,null,null,null,{"$f":"IF(LEFT(H2075,1)=\"J\",LEFT(H2075,2),LEFT(H2075,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2075,1)=\"J\",RIGHT(H2075,LEN(H2075)-4),RIGHT(H2075,LEN(H2075)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001638,"YOSHOPO","Y1-H3P10K-H",10,11,3,"Hybrid-Wechselrichter","Nein - Befristung abgelaufen","2023-10-16","Martin Bertsch","2023-07-26","V1.04 ","2023-10-16","2023-10-16","Gerät wurde im Auftrag von OE beim AIT überprüft. Schwere Fehler gefunden.","Ja","Nein",null,"Vorhanden","Martin Bertsch (OE)","ABRE-ESH-P22120410","2023-07-20","nicht vorhanden","OK",null,null,null,null,"ident zu RENAC",null,null,null,null,{"$f":"IF(LEFT(H2076,1)=\"J\",LEFT(H2076,2),LEFT(H2076,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2076,1)=\"J\",RIGHT(H2076,LEN(H2076)-4),RIGHT(H2076,LEN(H2076)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001639,"ZCS Zucchetti Centro Sistemi","1PH 3000-TLM-V3",3,3,1,"PV-Wechselrichter","Nein","2022-11-21",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2077,1)=\"J\",LEFT(H2077,2),LEFT(H2077,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2077,1)=\"J\",RIGHT(H2077,LEN(H2077)-4),RIGHT(H2077,LEN(H2077)-6)),\"\"))","v":""}]
[50001640,"ZCS Zucchetti Centro Sistemi","1PH HYD 3000 ZSS HP",3,3.3,1,"Hybrid-Wechselrichter","Nein","2022-11-21",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2078,1)=\"J\",LEFT(H2078,2),LEFT(H2078,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2078,1)=\"J\",RIGHT(H2078,LEN(H2078)-4),RIGHT(H2078,LEN(H2078)-6)),\"\"))","v":""}]
[50001641,"ZCS Zucchetti Centro Sistemi","3PH 3.3KTL-V3",3,3.3,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-002","2023-02-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2079,1)=\"J\",LEFT(H2079,2),LEFT(H2079,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2079,1)=\"J\",RIGHT(H2079,LEN(H2079)-4),RIGHT(H2079,LEN(H2079)-6)),\"\"))","v":"befristet"}]
[50001642,"ZCS Zucchetti Centro Sistemi","1PH 3680-TLM-V3",3.68,3.68,1,"PV-Wechselrichter","Nein","2022-11-21",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2080,1)=\"J\",LEFT(H2080,2),LEFT(H2080,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2080,1)=\"J\",RIGHT(H2080,LEN(H2080)-4),RIGHT(H2080,LEN(H2080)-6)),\"\"))","v":""}]
[50001643,"ZCS Zucchetti Centro Sistemi","1PH HYD 3600 ZSS HP",3.68,3.68,1,"Hybrid-Wechselrichter","Nein","2022-11-21",null,null,null,null,null,null,null,null,null,"nicht vorhanden",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2081,1)=\"J\",LEFT(H2081,2),LEFT(H2081,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2081,1)=\"J\",RIGHT(H2081,LEN(H2081)-4),RIGHT(H2081,LEN(H2081)-6)),\"\"))","v":""}]
[50001644,"ZCS Zucchetti Centro Sistemi","3PH 4.4KTL-V3",4,4.4000000000000004,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-002","2023-02-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2082,1)=\"J\",LEFT(H2082,2),LEFT(H2082,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2082,1)=\"J\",RIGHT(H2082,LEN(H2082)-4),RIGHT(H2082,LEN(H2082)-6)),\"\"))","v":"befristet"}]
[50001645,"ZCS Zucchetti Centro Sistemi","3PH 5.5KTL-V3",5,5.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-002","2023-02-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2083,1)=\"J\",LEFT(H2083,2),LEFT(H2083,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2083,1)=\"J\",RIGHT(H2083,LEN(H2083)-4),RIGHT(H2083,LEN(H2083)-6)),\"\"))","v":"befristet"}]
[50001646,"ZCS Zucchetti Centro Sistemi","AZZURRO 3PH HYD5000 ZSS ",5,5.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2022-07-08","Firmware Version: V112351_51_51",null,null,"Fehler in der FW","Ja","Nein",null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"Vorhanden","Vorhanden",null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R25","F","F",null,null,{"$f":"IF(LEFT(H2084,1)=\"J\",LEFT(H2084,2),LEFT(H2084,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2084,1)=\"J\",RIGHT(H2084,LEN(H2084)-4),RIGHT(H2084,LEN(H2084)-6)),\"\"))","v":"mit Einschränkung"}]
[50001647,"ZCS Zucchetti Centro Sistemi","3PH 6.6KTL-V3",6,6.6,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-002","2023-02-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2085,1)=\"J\",LEFT(H2085,2),LEFT(H2085,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2085,1)=\"J\",RIGHT(H2085,LEN(H2085)-4),RIGHT(H2085,LEN(H2085)-6)),\"\"))","v":"befristet"}]
[50001648,"ZCS Zucchetti Centro Sistemi","AZZURRO 3PH HYD6000 ZSS ",6,6.6,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2022-07-08","Firmware Version: V112351_51_51",null,null,"Fehler in der FW","Ja","Nein",null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"Vorhanden","Vorhanden",null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R26","F","F",null,null,{"$f":"IF(LEFT(H2086,1)=\"J\",LEFT(H2086,2),LEFT(H2086,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2086,1)=\"J\",RIGHT(H2086,LEN(H2086)-4),RIGHT(H2086,LEN(H2086)-6)),\"\"))","v":"mit Einschränkung"}]
[50001649,"ZCS Zucchetti Centro Sistemi","3PH 8.8KTL-V3",8,8.8000000000000007,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-002","2023-02-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2087,1)=\"J\",LEFT(H2087,2),LEFT(H2087,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2087,1)=\"J\",RIGHT(H2087,LEN(H2087)-4),RIGHT(H2087,LEN(H2087)-6)),\"\"))","v":"befristet"}]
[50001650,"ZCS Zucchetti Centro Sistemi","AZZURRO 3PH HYD8000 ZSS ",8,8.8000000000000007,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2022-07-08","Firmware Version: V112351_51_51",null,null,"Fehler in der FW","Ja","Nein",null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"Vorhanden","Vorhanden",null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R27","F","F",null,null,{"$f":"IF(LEFT(H2088,1)=\"J\",LEFT(H2088,2),LEFT(H2088,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2088,1)=\"J\",RIGHT(H2088,LEN(H2088)-4),RIGHT(H2088,LEN(H2088)-6)),\"\"))","v":"mit Einschränkung"}]
[50001651,"ZCS Zucchetti Centro Sistemi","3PH 11KTL-V3",10,11,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-002","2023-02-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2089,1)=\"J\",LEFT(H2089,2),LEFT(H2089,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2089,1)=\"J\",RIGHT(H2089,LEN(H2089)-4),RIGHT(H2089,LEN(H2089)-6)),\"\"))","v":"befristet"}]
[50001652,"ZCS Zucchetti Centro Sistemi","AZZURRO 3PH HYD10000 ZSS ",10,11,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2022-07-08","Firmware Version: V112351_51_51",null,null,"Fehler in der FW","Ja","Nein",null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"Vorhanden","Vorhanden",null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R28","F","F",null,null,{"$f":"IF(LEFT(H2090,1)=\"J\",LEFT(H2090,2),LEFT(H2090,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2090,1)=\"J\",RIGHT(H2090,LEN(H2090)-4),RIGHT(H2090,LEN(H2090)-6)),\"\"))","v":"mit Einschränkung"}]
[50001653,"ZCS Zucchetti Centro Sistemi","3PH 12KTL-V3",12,13.2,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","230116067GZU-002","2023-02-26","nicht vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2091,1)=\"J\",LEFT(H2091,2),LEFT(H2091,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2091,1)=\"J\",RIGHT(H2091,LEN(H2091)-4),RIGHT(H2091,LEN(H2091)-6)),\"\"))","v":"befristet"}]
[50001654,"ZCS Zucchetti Centro Sistemi","3PH 15000TL-V3",15,16.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-30",null,"2024-09-30",null,null,null,null,null,"OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2092,1)=\"J\",LEFT(H2092,2),LEFT(H2092,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2092,1)=\"J\",RIGHT(H2092,LEN(H2092)-4),RIGHT(H2092,LEN(H2092)-6)),\"\"))","v":"befristet"}]
[50001655,"ZCS Zucchetti Centro Sistemi","AZZURRO 3PH HYD15000 ZSS ",15,16.5,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2022-07-08","Firmware Version: V112351_51_51",null,null,"Fehler in der FW","Ja","Nein",null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"Vorhanden","Vorhanden",null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R29","F","F",null,null,{"$f":"IF(LEFT(H2093,1)=\"J\",LEFT(H2093,2),LEFT(H2093,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2093,1)=\"J\",RIGHT(H2093,LEN(H2093)-4),RIGHT(H2093,LEN(H2093)-6)),\"\"))","v":"mit Einschränkung"}]
[50001656,"ZCS Zucchetti Centro Sistemi","3PH 17000TL-V3",17,18.7,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-12-01",null,"2024-09-30",null,null,null,null,null,"OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2094,1)=\"J\",LEFT(H2094,2),LEFT(H2094,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2094,1)=\"J\",RIGHT(H2094,LEN(H2094)-4),RIGHT(H2094,LEN(H2094)-6)),\"\"))","v":"befristet"}]
[50001657,"ZCS Zucchetti Centro Sistemi","3PH 20000TL-V3",20,22,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-12-01",null,"2024-09-30",null,null,null,null,null,"OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2095,1)=\"J\",LEFT(H2095,2),LEFT(H2095,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2095,1)=\"J\",RIGHT(H2095,LEN(H2095)-4),RIGHT(H2095,LEN(H2095)-6)),\"\"))","v":"befristet"}]
[50001658,"ZCS Zucchetti Centro Sistemi","AZZURRO 3PH HYD20000 ZSS ",20,22,3,"Hybrid-Wechselrichter","Ja - mit Einschränkung","2024-06-17","Martin Bertsch","2022-07-08","Firmware Version: V112351_51_51",null,null,"Fehler in der FW","Ja","Nein",null,"OK","Roland Bründlinger (AIT)","210526211GZU-003","2022-07-14",null,"Vorhanden","Vorhanden",null,null,null,"Hybridstromrichter 3~ - inselbetriebsfähig - KONFORM TOR ERZ A+R30","F","F",null,null,{"$f":"IF(LEFT(H2096,1)=\"J\",LEFT(H2096,2),LEFT(H2096,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2096,1)=\"J\",RIGHT(H2096,LEN(H2096)-4),RIGHT(H2096,LEN(H2096)-6)),\"\"))","v":"mit Einschränkung"}]
[50001659,"ZCS Zucchetti Centro Sistemi","3PH 22000TL-V3",22,24.2,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-12-01",null,"2024-09-30",null,null,null,null,null,"OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2097,1)=\"J\",LEFT(H2097,2),LEFT(H2097,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2097,1)=\"J\",RIGHT(H2097,LEN(H2097)-4),RIGHT(H2097,LEN(H2097)-6)),\"\"))","v":"befristet"}]
[50001660,"ZCS Zucchetti Centro Sistemi","3PH 24000TL-V3",24,26.4,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2022-12-01",null,"2024-09-30",null,null,null,null,null,"OK","Martin Bertsch (OE)","210526211GZU-002","2023-01-02",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2098,1)=\"J\",LEFT(H2098,2),LEFT(H2098,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2098,1)=\"J\",RIGHT(H2098,LEN(H2098)-4),RIGHT(H2098,LEN(H2098)-6)),\"\"))","v":"befristet"}]
[50001661,"ZCS Zucchetti Centro Sistemi","3PH 25KTL-V3",25,27.5,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,null,null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2099,1)=\"J\",LEFT(H2099,2),LEFT(H2099,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2099,1)=\"J\",RIGHT(H2099,LEN(H2099)-4),RIGHT(H2099,LEN(H2099)-6)),\"\"))","v":"befristet"}]
[50001662,"ZCS Zucchetti Centro Sistemi","3PH 30KTL-V3",30,33,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,null,null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2100,1)=\"J\",LEFT(H2100,2),LEFT(H2100,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2100,1)=\"J\",RIGHT(H2100,LEN(H2100)-4),RIGHT(H2100,LEN(H2100)-6)),\"\"))","v":"befristet"}]
[50001663,"ZCS Zucchetti Centro Sistemi","3PH 33KTL-V3",33,36.299999999999997,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,null,null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2101,1)=\"J\",LEFT(H2101,2),LEFT(H2101,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2101,1)=\"J\",RIGHT(H2101,LEN(H2101)-4),RIGHT(H2101,LEN(H2101)-6)),\"\"))","v":"befristet"}]
[50001664,"ZCS Zucchetti Centro Sistemi","3PH 36KTL-V3",36,40,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,null,null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2102,1)=\"J\",LEFT(H2102,2),LEFT(H2102,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2102,1)=\"J\",RIGHT(H2102,LEN(H2102)-4),RIGHT(H2102,LEN(H2102)-6)),\"\"))","v":"befristet"}]
[50001665,"ZCS Zucchetti Centro Sistemi","3PH 40KTL-V3",40,44,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,null,null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2103,1)=\"J\",LEFT(H2103,2),LEFT(H2103,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2103,1)=\"J\",RIGHT(H2103,LEN(H2103)-4),RIGHT(H2103,LEN(H2103)-6)),\"\"))","v":"befristet"}]
[50001666,"ZCS Zucchetti Centro Sistemi","3PH 45KTL-V3",45,50,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,null,null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2104,1)=\"J\",LEFT(H2104,2),LEFT(H2104,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2104,1)=\"J\",RIGHT(H2104,LEN(H2104)-4),RIGHT(H2104,LEN(H2104)-6)),\"\"))","v":"befristet"}]
[50001667,"ZCS Zucchetti Centro Sistemi","3PH 50KTL-V3",50,50,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-03-23",null,"2024-09-30",null,null,null,null,null,"OK","KS und MAB","210819144GZU-001","2023-03-09",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2105,1)=\"J\",LEFT(H2105,2),LEFT(H2105,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2105,1)=\"J\",RIGHT(H2105,LEN(H2105)-4),RIGHT(H2105,LEN(H2105)-6)),\"\"))","v":"befristet"}]
[50001668,"ZCS Zucchetti Centro Sistemi","3PH 60KTL-V3",60,66,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,"Nein","Nein","Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12","Vorhanden","OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2106,1)=\"J\",LEFT(H2106,2),LEFT(H2106,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2106,1)=\"J\",RIGHT(H2106,LEN(H2106)-4),RIGHT(H2106,LEN(H2106)-6)),\"\"))","v":"befristet"}]
[50001669,"ZCS Zucchetti Centro Sistemi","3PH 75KTL-V3",75,75,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,null,null,"Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2107,1)=\"J\",LEFT(H2107,2),LEFT(H2107,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2107,1)=\"J\",RIGHT(H2107,LEN(H2107)-4),RIGHT(H2107,LEN(H2107)-6)),\"\"))","v":"befristet"}]
[50001670,"ZCS Zucchetti Centro Sistemi","3PH 70KTL-V3",70,77,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,null,null,"Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2108,1)=\"J\",LEFT(H2108,2),LEFT(H2108,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2108,1)=\"J\",RIGHT(H2108,LEN(H2108)-4),RIGHT(H2108,LEN(H2108)-6)),\"\"))","v":"befristet"}]
[50001671,"ZCS Zucchetti Centro Sistemi","3PH 80KTL-LV",80,88,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-12-01",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2109,1)=\"J\",LEFT(H2109,2),LEFT(H2109,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2109,1)=\"J\",RIGHT(H2109,LEN(H2109)-4),RIGHT(H2109,LEN(H2109)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001672,"ZCS Zucchetti Centro Sistemi","3PH 80KTL-V3",80,88,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,null,null,"Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2110,1)=\"J\",LEFT(H2110,2),LEFT(H2110,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2110,1)=\"J\",RIGHT(H2110,LEN(H2110)-4),RIGHT(H2110,LEN(H2110)-6)),\"\"))","v":"befristet"}]
[50001673,"ZCS Zucchetti Centro Sistemi","3PH 100KTL-V4",100,100,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,null,null,"Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2111,1)=\"J\",LEFT(H2111,2),LEFT(H2111,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2111,1)=\"J\",RIGHT(H2111,LEN(H2111)-4),RIGHT(H2111,LEN(H2111)-6)),\"\"))","v":"befristet"}]
[50001674,"ZCS Zucchetti Centro Sistemi","3PH 100KTL-LV",100,110,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-12-01",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2112,1)=\"J\",LEFT(H2112,2),LEFT(H2112,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2112,1)=\"J\",RIGHT(H2112,LEN(H2112)-4),RIGHT(H2112,LEN(H2112)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001675,"ZCS Zucchetti Centro Sistemi","3PH 110KTL-V4",100,110,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,null,null,"Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2113,1)=\"J\",LEFT(H2113,2),LEFT(H2113,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2113,1)=\"J\",RIGHT(H2113,LEN(H2113)-4),RIGHT(H2113,LEN(H2113)-6)),\"\"))","v":"befristet"}]
[50001676,"ZCS Zucchetti Centro Sistemi","3PH 110KTL-LV",110,121,3,"PV-Wechselrichter","Nein - Befristung abgelaufen","2023-04-24","Martin Bertsch","2022-12-01",null,"2023-03-31",null,null,null,null,null,"nicht OK","Moustafa Mohamed (Netz NÖ)","210526211GZU-004","2021-06-21",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2114,1)=\"J\",LEFT(H2114,2),LEFT(H2114,4))","v":"Nein"},{"$f":"TRIM(IFERROR(IF(LEFT(H2114,1)=\"J\",RIGHT(H2114,LEN(H2114)-4),RIGHT(H2114,LEN(H2114)-6)),\"\"))","v":"Befristung abgelaufen"}]
[50001677,"ZCS Zucchetti Centro Sistemi","3PH 125KTL-V4",110,125,3,"PV-Wechselrichter","Ja, befristet","2024-05-26","Martin Bertsch","2023-05-31",null,"2024-09-30",null,null,null,null,"Nein","OK","Martin Bertsch (OE)","220606147GZU-013","2023-05-12",null,"OK",null,null,null,null,null,null,null,null,null,{"$f":"IF(LEFT(H2115,1)=\"J\",LEFT(H2115,2),LEFT(H2115,4))","v":"Ja"},{"$f":"TRIM(IFERROR(IF(LEFT(H2115,1)=\"J\",RIGHT(H2115,LEN(H2115)-4),RIGHT(H2115,LEN(H2115)-6)),\"\"))","v":"befristet"}]

{"sheet":"Datenüberprüfung","index":1,"n_rows":19,"n_cols":32,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
[]
["Hersteller","Type","Nennwirkleistung\n(Maximalleistung)","Nennscheinleistung\n(Maximalleistung)","Phasenzahl","Art Betriebsmittel","Zulässig ","Datum letzte Änderung","Geändert von","Datum Zulassung","ab Firmware","Datum befristet bis","Datum Entzug Zulassung","Grund nicht zulässig","Notstrom-/Inselbetriebsfähig","Externe Notstromumschaltung notwendig","USV-Fähig","OVE R25 Prüfbericht","Geprüft von","Nummer Prüfbericht","Datum OVE R25 Prüfbericht","VDE-AR-N 4110 Zertifikat","AUT Setting Typ A vorhanden","Hersteller Parametrieranleitung","Musterreport vorhanden","Datum Musterreport","Nur mit externem Entkupplungsschutz","Info","Produktion ausgelaufen","E-Mobilität","Kommentar für HP","Kommentar intern"]
[null,null,null,null,1,"AC-Batteriewechselrichter","Ja",null,null,null,null,null,null,null,"Ja","Ja","Ja","Vorhanden",null,null,null,"Vorhanden","Vorhanden","Vorhanden","Vorhanden",null,"Ja, keine N-Überwachung durch ENS",null,"T","T"]
[null,null,null,null,2,"PV-Wechselrichter","Ja - <= 16A Anlage",null,null,null,null,null,null,null,"Nein","Nein","Nein","nicht vorhanden",null,null,null,"nicht vorhanden","nicht vorhanden","nicht vorhanden","nicht vorhanden",null,null,null,"F","F"]
[null,null,null,null,3,"Hybrid-Wechselrichter","Ja - <= 800W Anlage",null,null,null,null,null,null,null,null,null,null,"OK",null,null,null,null,"OK","OK"]
[null,null,null,null,null,"Frequenzumformer","Ja - mit Einschränkung",null,null,null,null,null,null,null,null,null,null,"nicht OK",null,null,null,null,"nicht OK","nicht OK"]
[null,null,null,null,null,"Windenergie-Wechselrichter","Ja - nur für Eigenverbrauch",null,null,null,null,null,null,null,null,null,null,"VDE4105",null,null,null,null,"VDE4105/4110","VDE4105/4110"]
[null,null,null,null,null,"USV-Anwendung","Ja - bis 30kW Rückspeisung"]
[null,null,null,null,null,null,"Ja, befristet"]
[null,null,null,null,null,null,"Ja - <= 16A Anlage, befristet"]
[null,null,null,null,null,null,"Ja - <= 800W Anlage, befristet"]
[null,null,null,null,null,null,"Ja - mit Einschränkung, befristet"]
[null,null,null,null,null,null,"Ja - nur für Eigenverbrauch, befristet"]
[null,null,null,null,null,null,"Ja - bis 30kW Rückspeisung, befristet"]
[null,null,null,null,null,null,"Ja - <= 16A Anlage, mit Einschränkung"]
[null,null,null,null,null,null,"Nein"]
[null,null,null,null,null,null,"Nein - Typ B"]
[null,null,null,null,null,null,"Nein - In Prüfung"]
[null,null,null,null,null,null,"Nein - Befristung abgelaufen"]